From 2db8d1cd04d98a3cfba1b800ce031c6dd97e1ac9 Mon Sep 17 00:00:00 2001
From: Jonathan Bell <jonathan@raspberrypi.com>
Date: Wed, 20 Mar 2024 11:58:49 +0000
Subject: [PATCH 0982/1085] DTS: bcm2712: emmc2 clock frequency is 200MHz

The bootloader sets this as the controller base clock.

Signed-off-by: Jonathan Bell <jonathan@raspberrypi.com>
---
 arch/arm/boot/dts/broadcom/bcm2712.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/broadcom/bcm2712.dtsi
+++ b/arch/arm/boot/dts/broadcom/bcm2712.dtsi
@@ -1214,7 +1214,7 @@
 		clk_emmc2: clk_emmc2 {
 			#clock-cells = <0>;
 			compatible = "fixed-clock";
-			clock-frequency = <54000000>;
+			clock-frequency = <200000000>;
 			clock-output-names = "emmc2-clock";
 		};
 	};
