From d6e7ddb03b509147af9d21b0d544f76f014e4b92 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Tue, 5 Mar 2019 09:51:22 +0000
Subject: [PATCH] lan78xx: EEE support is now a PHY property

Now that EEE support is a property of the PHY, use the PHY's DT node
when querying the EEE-related properties.

See: https://github.com/raspberrypi/linux/issues/2882

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 drivers/net/usb/lan78xx.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/usb/lan78xx.c
+++ b/drivers/net/usb/lan78xx.c
@@ -2188,7 +2188,7 @@ static int lan78xx_phy_init(struct lan78
 	mii_adv_to_linkmode_adv_t(fc, mii_adv);
 	linkmode_or(phydev->advertising, fc, phydev->advertising);
 
-	if (of_property_read_bool(dev->udev->dev.of_node,
+	if (of_property_read_bool(phydev->mdio.dev.of_node,
 				  "microchip,eee-enabled")) {
 		struct ethtool_eee edata;
 		memset(&edata, 0, sizeof(edata));
