From 078d5cda5fc94e1d40d8d44bc4a0067341f02e72 Mon Sep 17 00:00:00 2001
From: Yangbo Lu <yangbo.lu@nxp.com>
Date: Thu, 1 Nov 2018 12:10:59 +0800
Subject: [PATCH] sdk_fman: share the event interrupt

This patch is to share fman event interrupt because
the 1588 timer driver will also use this interrupt.

Signed-off-by: Yangbo Lu <yangbo.lu@nxp.com>
---
 drivers/net/ethernet/freescale/sdk_fman/src/wrapper/lnxwrp_fm.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/ethernet/freescale/sdk_fman/src/wrapper/lnxwrp_fm.c
+++ b/drivers/net/ethernet/freescale/sdk_fman/src/wrapper/lnxwrp_fm.c
@@ -883,7 +883,7 @@ static t_Error ConfigureFmDev(t_LnxWrpFm
     if (unlikely(_errno < 0))
         RETURN_ERROR(MAJOR, E_INVALID_STATE, ("can_request_irq() = %d", _errno));
 #endif
-    _errno = devm_request_irq(p_LnxWrpFmDev->dev, p_LnxWrpFmDev->irq, fm_irq, 0, "fman", p_LnxWrpFmDev);
+    _errno = devm_request_irq(p_LnxWrpFmDev->dev, p_LnxWrpFmDev->irq, fm_irq, IRQF_SHARED, "fman", p_LnxWrpFmDev);
     if (unlikely(_errno < 0))
         RETURN_ERROR(MAJOR, E_INVALID_STATE, ("request_irq(%d) = %d", p_LnxWrpFmDev->irq, _errno));
 
