--- a/include/uapi/linux/nl80211.h
+++ b/include/uapi/linux/nl80211.h
@@ -655,6 +655,9 @@
  *	When a security association was established on an 802.1X network using
  *	fast transition, this event should be followed by an
  *	%NL80211_CMD_PORT_AUTHORIZED event.
+ *	Following a %NL80211_CMD_ROAM event userspace can issue
+ *	%NL80211_CMD_GET_SCAN in order to obtain the scan information for the
+ *	new BSS the card/driver roamed to.
  * @NL80211_CMD_DISCONNECT: drop a given connection; also used to notify
  *	userspace that a connection was dropped by the AP or due to other
  *	reasons, for this the %NL80211_ATTR_DISCONNECTED_BY_AP and
@@ -757,7 +760,8 @@
  *	of any other interfaces, and other interfaces will again take
  *	precedence when they are used.
  *
- * @NL80211_CMD_SET_WDS_PEER: Set the MAC address of the peer on a WDS interface.
+ * @NL80211_CMD_SET_WDS_PEER: Set the MAC address of the peer on a WDS interface
+ *	(no longer supported).
  *
  * @NL80211_CMD_SET_MULTICAST_TO_UNICAST: Configure if this AP should perform
  *	multicast to unicast conversion. When enabled, all multicast packets
@@ -1177,6 +1181,10 @@
  *	includes the contents of the frame. %NL80211_ATTR_ACK flag is included
  *	if the recipient acknowledged the frame.
  *
+ * @NL80211_CMD_SET_SAR_SPECS: SAR power limitation configuration is
+ *	passed using %NL80211_ATTR_SAR_SPEC. %NL80211_ATTR_WIPHY is used to
+ *	specify the wiphy index to be applied to.
+ *
  * @NL80211_CMD_MAX: highest used command number
  * @__NL80211_CMD_AFTER_LAST: internal use
  */
@@ -1407,6 +1415,8 @@ enum nl80211_commands {
 
 	NL80211_CMD_CONTROL_PORT_FRAME_TX_STATUS,
 
+	NL80211_CMD_SET_SAR_SPECS,
+
 	/* add new commands above here */
 
 	/* used to define NL80211_CMD_MAX below */
@@ -1750,8 +1760,9 @@ enum nl80211_commands {
  *	specify just a single bitrate, which is to be used for the beacon.
  *	The driver must also specify support for this with the extended
  *	features NL80211_EXT_FEATURE_BEACON_RATE_LEGACY,
- *	NL80211_EXT_FEATURE_BEACON_RATE_HT and
- *	NL80211_EXT_FEATURE_BEACON_RATE_VHT.
+ *	NL80211_EXT_FEATURE_BEACON_RATE_HT,
+ *	NL80211_EXT_FEATURE_BEACON_RATE_VHT and
+ *	NL80211_EXT_FEATURE_BEACON_RATE_HE.
  *
  * @NL80211_ATTR_FRAME_MATCH: A binary attribute which typically must contain
  *	at least one byte, currently used with @NL80211_CMD_REGISTER_FRAME.
@@ -1955,8 +1966,15 @@ enum nl80211_commands {
  * @NL80211_ATTR_PROBE_RESP: Probe Response template data. Contains the entire
  *	probe-response frame. The DA field in the 802.11 header is zero-ed out,
  *	to be filled by the FW.
- * @NL80211_ATTR_DISABLE_HT:  Force HT capable interfaces to disable
- *      this feature.  Currently, only supported in mac80211 drivers.
+ * @NL80211_ATTR_DISABLE_HT: Force HT capable interfaces to disable
+ *      this feature during association. This is a flag attribute.
+ *	Currently only supported in mac80211 drivers.
+ * @NL80211_ATTR_DISABLE_VHT: Force VHT capable interfaces to disable
+ *      this feature during association. This is a flag attribute.
+ *	Currently only supported in mac80211 drivers.
+ * @NL80211_ATTR_DISABLE_HE: Force HE capable interfaces to disable
+ *      this feature during association. This is a flag attribute.
+ *	Currently only supported in mac80211 drivers.
  * @NL80211_ATTR_HT_CAPABILITY_MASK: Specify which bits of the
  *      ATTR_HT_CAPABILITY to which attention should be paid.
  *      Currently, only mac80211 NICs support this feature.
@@ -2077,7 +2095,8 @@ enum nl80211_commands {
  *	until the channel switch event.
  * @NL80211_ATTR_CH_SWITCH_BLOCK_TX: flag attribute specifying that transmission
  *	must be blocked on the current channel (before the channel switch
- *	operation).
+ *	operation). Also included in the channel switch started event if quiet
+ *	was requested by the AP.
  * @NL80211_ATTR_CSA_IES: Nested set of attributes containing the IE information
  *	for the time while performing a channel switch.
  * @NL80211_ATTR_CNTDWN_OFFS_BEACON: An array of offsets (u16) to the channel
@@ -2527,6 +2546,20 @@ enum nl80211_commands {
  *	override mask. Used with NL80211_ATTR_S1G_CAPABILITY in
  *	NL80211_CMD_ASSOCIATE or NL80211_CMD_CONNECT.
  *
+ * @NL80211_ATTR_SAE_PWE: Indicates the mechanism(s) allowed for SAE PWE
+ *	derivation in WPA3-Personal networks which are using SAE authentication.
+ *	This is a u8 attribute that encapsulates one of the values from
+ *	&enum nl80211_sae_pwe_mechanism.
+ *
+ * @NL80211_ATTR_SAR_SPEC: SAR power limitation specification when
+ *	used with %NL80211_CMD_SET_SAR_SPECS. The message contains fields
+ *	of %nl80211_sar_attrs which specifies the sar type and related
+ *	sar specs. Sar specs contains array of %nl80211_sar_specs_attrs.
+ *
+ * @NL80211_ATTR_RECONNECT_REQUESTED: flag attribute, used with deauth and
+ *	disassoc events to indicate that an immediate reconnect to the AP
+ *	is desired.
+ *
  * @NUM_NL80211_ATTR: total number of nl80211_attrs available
  * @NL80211_ATTR_MAX: highest attribute number currently defined
  * @__NL80211_ATTR_AFTER_LAST: internal use
@@ -3016,6 +3049,14 @@ enum nl80211_attrs {
 	NL80211_ATTR_S1G_CAPABILITY,
 	NL80211_ATTR_S1G_CAPABILITY_MASK,
 
+	NL80211_ATTR_SAE_PWE,
+
+	NL80211_ATTR_RECONNECT_REQUESTED,
+
+	NL80211_ATTR_SAR_SPEC,
+
+	NL80211_ATTR_DISABLE_HE,
+
 	/* add attributes here, update the policy in nl80211.c */
 
 	__NL80211_ATTR_AFTER_LAST,
@@ -5896,6 +5937,19 @@ enum nl80211_feature_flags {
  * @NL80211_EXT_FEATURE_UNSOL_BCAST_PROBE_RESP: Driver/device supports
  *	unsolicited broadcast probe response transmission
  *
+ * @NL80211_EXT_FEATURE_BEACON_RATE_HE: Driver supports beacon rate
+ *	configuration (AP/mesh) with HE rates.
+ *
+ * @NL80211_EXT_FEATURE_SECURE_LTF: Device supports secure LTF measurement
+ *      exchange protocol.
+ *
+ * @NL80211_EXT_FEATURE_SECURE_RTT: Device supports secure RTT measurement
+ *      exchange protocol.
+ *
+ * @NL80211_EXT_FEATURE_PROT_RANGE_NEGO_AND_MEASURE: Device supports management
+ *      frame protection for all management frames exchanged during the
+ *      negotiation and range measurement procedure.
+ *
  * @NUM_NL80211_EXT_FEATURES: number of extended features.
  * @MAX_NL80211_EXT_FEATURES: highest extended feature index.
  */
@@ -5956,6 +6010,10 @@ enum nl80211_ext_feature_index {
 	NL80211_EXT_FEATURE_SAE_OFFLOAD_AP,
 	NL80211_EXT_FEATURE_FILS_DISCOVERY,
 	NL80211_EXT_FEATURE_UNSOL_BCAST_PROBE_RESP,
+	NL80211_EXT_FEATURE_BEACON_RATE_HE,
+	NL80211_EXT_FEATURE_SECURE_LTF,
+	NL80211_EXT_FEATURE_SECURE_RTT,
+	NL80211_EXT_FEATURE_PROT_RANGE_NEGO_AND_MEASURE,
 
 	/* add new features before the definition below */
 	NUM_NL80211_EXT_FEATURES,
@@ -6253,11 +6311,13 @@ struct nl80211_vendor_cmd_info {
  * @NL80211_TDLS_PEER_HT: TDLS peer is HT capable.
  * @NL80211_TDLS_PEER_VHT: TDLS peer is VHT capable.
  * @NL80211_TDLS_PEER_WMM: TDLS peer is WMM capable.
+ * @NL80211_TDLS_PEER_HE: TDLS peer is HE capable.
  */
 enum nl80211_tdls_peer_capability {
 	NL80211_TDLS_PEER_HT = 1<<0,
 	NL80211_TDLS_PEER_VHT = 1<<1,
 	NL80211_TDLS_PEER_WMM = 1<<2,
+	NL80211_TDLS_PEER_HE = 1<<3,
 };
 
 /**
@@ -6849,6 +6909,9 @@ enum nl80211_peer_measurement_ftm_capa {
  *      if neither %NL80211_PMSR_FTM_REQ_ATTR_TRIGGER_BASED nor
  *	%NL80211_PMSR_FTM_REQ_ATTR_NON_TRIGGER_BASED is set, EDCA based
  *	ranging will be used.
+ * @NL80211_PMSR_FTM_REQ_ATTR_LMR_FEEDBACK: negotiate for LMR feedback. Only
+ *	valid if either %NL80211_PMSR_FTM_REQ_ATTR_TRIGGER_BASED or
+ *	%NL80211_PMSR_FTM_REQ_ATTR_NON_TRIGGER_BASED is set.
  *
  * @NUM_NL80211_PMSR_FTM_REQ_ATTR: internal
  * @NL80211_PMSR_FTM_REQ_ATTR_MAX: highest attribute number
@@ -6867,6 +6930,7 @@ enum nl80211_peer_measurement_ftm_req {
 	NL80211_PMSR_FTM_REQ_ATTR_REQUEST_CIVICLOC,
 	NL80211_PMSR_FTM_REQ_ATTR_TRIGGER_BASED,
 	NL80211_PMSR_FTM_REQ_ATTR_NON_TRIGGER_BASED,
+	NL80211_PMSR_FTM_REQ_ATTR_LMR_FEEDBACK,
 
 	/* keep last */
 	NUM_NL80211_PMSR_FTM_REQ_ATTR,
@@ -7124,4 +7188,115 @@ enum nl80211_unsol_bcast_probe_resp_attr
 	NL80211_UNSOL_BCAST_PROBE_RESP_ATTR_MAX =
 		__NL80211_UNSOL_BCAST_PROBE_RESP_ATTR_LAST - 1
 };
+
+/**
+ * enum nl80211_sae_pwe_mechanism - The mechanism(s) allowed for SAE PWE
+ *	derivation. Applicable only when WPA3-Personal SAE authentication is
+ *	used.
+ *
+ * @NL80211_SAE_PWE_UNSPECIFIED: not specified, used internally to indicate that
+ *	attribute is not present from userspace.
+ * @NL80211_SAE_PWE_HUNT_AND_PECK: hunting-and-pecking loop only
+ * @NL80211_SAE_PWE_HASH_TO_ELEMENT: hash-to-element only
+ * @NL80211_SAE_PWE_BOTH: both hunting-and-pecking loop and hash-to-element
+ *	can be used.
+ */
+enum nl80211_sae_pwe_mechanism {
+	NL80211_SAE_PWE_UNSPECIFIED,
+	NL80211_SAE_PWE_HUNT_AND_PECK,
+	NL80211_SAE_PWE_HASH_TO_ELEMENT,
+	NL80211_SAE_PWE_BOTH,
+};
+
+/**
+ * enum nl80211_sar_type - type of SAR specs
+ *
+ * @NL80211_SAR_TYPE_POWER: power limitation specified in 0.25dBm unit
+ *
+ */
+enum nl80211_sar_type {
+	NL80211_SAR_TYPE_POWER,
+
+	/* add new type here */
+
+	/* Keep last */
+	NUM_NL80211_SAR_TYPE,
+};
+
+/**
+ * enum nl80211_sar_attrs - Attributes for SAR spec
+ *
+ * @NL80211_SAR_ATTR_TYPE: the SAR type as defined in &enum nl80211_sar_type.
+ *
+ * @NL80211_SAR_ATTR_SPECS: Nested array of SAR power
+ *	limit specifications. Each specification contains a set
+ *	of %nl80211_sar_specs_attrs.
+ *
+ *	For SET operation, it contains array of %NL80211_SAR_ATTR_SPECS_POWER
+ *	and %NL80211_SAR_ATTR_SPECS_RANGE_INDEX.
+ *
+ *	For sar_capa dump, it contains array of
+ *	%NL80211_SAR_ATTR_SPECS_START_FREQ
+ *	and %NL80211_SAR_ATTR_SPECS_END_FREQ.
+ *
+ * @__NL80211_SAR_ATTR_LAST: Internal
+ * @NL80211_SAR_ATTR_MAX: highest sar attribute
+ *
+ * These attributes are used with %NL80211_CMD_SET_SAR_SPEC
+ */
+enum nl80211_sar_attrs {
+	__NL80211_SAR_ATTR_INVALID,
+
+	NL80211_SAR_ATTR_TYPE,
+	NL80211_SAR_ATTR_SPECS,
+
+	__NL80211_SAR_ATTR_LAST,
+	NL80211_SAR_ATTR_MAX = __NL80211_SAR_ATTR_LAST - 1,
+};
+
+/**
+ * enum nl80211_sar_specs_attrs - Attributes for SAR power limit specs
+ *
+ * @NL80211_SAR_ATTR_SPECS_POWER: Required (s32)value to specify the actual
+ *	power limit value in units of 0.25 dBm if type is
+ *	NL80211_SAR_TYPE_POWER. (i.e., a value of 44 represents 11 dBm).
+ *	0 means userspace doesn't have SAR limitation on this associated range.
+ *
+ * @NL80211_SAR_ATTR_SPECS_RANGE_INDEX: Required (u32) value to specify the
+ *	index of exported freq range table and the associated power limitation
+ *	is applied to this range.
+ *
+ *	Userspace isn't required to set all the ranges advertised by WLAN driver,
+ *	and userspace can skip some certain ranges. These skipped ranges don't
+ *	have SAR limitations, and they are same as setting the
+ *	%NL80211_SAR_ATTR_SPECS_POWER to any unreasonable high value because any
+ *	value higher than regulatory allowed value just means SAR power
+ *	limitation is removed, but it's required to set at least one range.
+ *	It's not allowed to set duplicated range in one SET operation.
+ *
+ *	Every SET operation overwrites previous SET operation.
+ *
+ * @NL80211_SAR_ATTR_SPECS_START_FREQ: Required (u32) value to specify the start
+ *	frequency of this range edge when registering SAR capability to wiphy.
+ *	It's not a channel center frequency. The unit is kHz.
+ *
+ * @NL80211_SAR_ATTR_SPECS_END_FREQ: Required (u32) value to specify the end
+ *	frequency of this range edge when registering SAR capability to wiphy.
+ *	It's not a channel center frequency. The unit is kHz.
+ *
+ * @__NL80211_SAR_ATTR_SPECS_LAST: Internal
+ * @NL80211_SAR_ATTR_SPECS_MAX: highest sar specs attribute
+ */
+enum nl80211_sar_specs_attrs {
+	__NL80211_SAR_ATTR_SPECS_INVALID,
+
+	NL80211_SAR_ATTR_SPECS_POWER,
+	NL80211_SAR_ATTR_SPECS_RANGE_INDEX,
+	NL80211_SAR_ATTR_SPECS_START_FREQ,
+	NL80211_SAR_ATTR_SPECS_END_FREQ,
+
+	__NL80211_SAR_ATTR_SPECS_LAST,
+	NL80211_SAR_ATTR_SPECS_MAX = __NL80211_SAR_ATTR_SPECS_LAST - 1,
+};
+
 #endif /* __LINUX_NL80211_H */
