From b9801549748233e71a5c0dd76351e02a125505b4 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Mon, 21 Sep 2020 20:45:46 +0100
Subject: [PATCH] overlays: adafruit18,sainsmart18: default bgr to
 off

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 arch/arm/boot/dts/overlays/README                  | 4 ++--
 arch/arm/boot/dts/overlays/adafruit18-overlay.dts  | 1 -
 arch/arm/boot/dts/overlays/sainsmart18-overlay.dts | 1 -
 3 files changed, 2 insertions(+), 4 deletions(-)

--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -269,7 +269,7 @@ Params: green                   Use the
         rotate                  Display rotation {0,90,180,270}
         speed                   SPI bus speed in Hz (default 4000000)
         fps                     Display frame rate in Hz
-        bgr                     Enable BGR mode (default on)
+        bgr                     Enable BGR mode (default off)
         debug                   Debug output level {0-7}
         dc_pin                  GPIO pin for D/C (default 24)
         reset_pin               GPIO pin for RESET (default 25)
@@ -2284,7 +2284,7 @@ Load:   dtoverlay=sainsmart18,<param>=<v
 Params: rotate                  Display rotation {0,90,180,270}
         speed                   SPI bus speed in Hz (default 4000000)
         fps                     Display frame rate in Hz
-        bgr                     Enable BGR mode (default on)
+        bgr                     Enable BGR mode (default off)
         debug                   Debug output level {0-7}
         dc_pin                  GPIO pin for D/C (default 24)
         reset_pin               GPIO pin for RESET (default 25)
--- a/arch/arm/boot/dts/overlays/adafruit18-overlay.dts
+++ b/arch/arm/boot/dts/overlays/adafruit18-overlay.dts
@@ -36,7 +36,6 @@
 				reset-gpios = <&gpio 25 1>;
 				dc-gpios = <&gpio 24 0>;
 				led-gpios = <&gpio 18 0>;
-				bgr;
 				debug = <0>;
 			};
 		};
--- a/arch/arm/boot/dts/overlays/sainsmart18-overlay.dts
+++ b/arch/arm/boot/dts/overlays/sainsmart18-overlay.dts
@@ -35,7 +35,6 @@
 				width = <128>;
 				reset-gpios = <&gpio 25 1>;
 				dc-gpios = <&gpio 24 0>;
-				bgr;
 				debug = <0>;
 			};
 		};
