From dde4afa87452e8499c611c9a889f4c5f35d9e2bb Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Thu, 3 Sep 2020 17:36:00 +0100
Subject: [PATCH] overlays: Add adafruit18 and sainsmart18 overlays

Add support for three ST7735R-based displays - adafruit18,
adafruit18_green and sainsmart18.

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 arch/arm/boot/dts/overlays/Makefile           |  2 +
 arch/arm/boot/dts/overlays/README             | 15 ++++++
 .../boot/dts/overlays/adafruit18-overlay.dts  | 49 +++++++++++++++++++
 .../boot/dts/overlays/sainsmart18-overlay.dts | 47 ++++++++++++++++++
 4 files changed, 113 insertions(+)
 create mode 100644 arch/arm/boot/dts/overlays/adafruit18-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/sainsmart18-overlay.dts

--- a/arch/arm/boot/dts/overlays/Makefile
+++ b/arch/arm/boot/dts/overlays/Makefile
@@ -4,6 +4,7 @@ dtb-$(CONFIG_ARCH_BCM2835) += overlay_ma
 
 dtbo-$(CONFIG_ARCH_BCM2835) += \
 	act-led.dtbo \
+	adafruit18.dtbo \
 	adau1977-adc.dtbo \
 	adau7002-simple.dtbo \
 	ads1015.dtbo \
@@ -147,6 +148,7 @@ dtbo-$(CONFIG_ARCH_BCM2835) += \
 	rpi-tv.dtbo \
 	rpivid-v4l2.dtbo \
 	rra-digidac1-wm8741-audio.dtbo \
+	sainsmart18.dtbo \
 	sc16is750-i2c.dtbo \
 	sc16is752-i2c.dtbo \
 	sc16is752-spi0.dtbo \
--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -261,6 +261,14 @@ Params: activelow               Set to "
                                 REQUIRED
 
 
+Name:   adafruit18
+Info:   Overlay for the SPI-connected Adafruit 1.8" display (based on the
+        ST7735R chip). It includes support for the "green tab" version.
+Load:   dtoverlay=adafruit18,<param>=<val>
+Params: green                   Use the adafruit18_green variant.
+        rotate                  Display rotation {0,90,180,270}
+
+
 Name:   adau1977-adc
 Info:   Overlay for activation of ADAU1977 ADC codec over I2C for control
         and I2S for data.
@@ -2251,6 +2259,13 @@ Load:   dtoverlay=rra-digidac1-wm8741-au
 Params: <None>
 
 
+Name:   sainsmart18
+Info:   Overlay for the SPI-connected Sainsmart 1.8" display (based on the
+        ST7735R chip).
+Load:   dtoverlay=sainsmart18,<param>=<val>
+Params: rotate                  Display rotation {0,90,180,270}
+
+
 Name:   sc16is750-i2c
 Info:   Overlay for the NXP SC16IS750 UART with I2C Interface
         Enables the chip on I2C1 at 0x48 (or the "addr" parameter value). To
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/adafruit18-overlay.dts
@@ -0,0 +1,49 @@
+/*
+ * Device Tree overlay for Adafruit 1.8" TFT LCD with ST7735R chip 160x128
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			af18: adafruit18@0 {
+				compatible = "fbtft,adafruit18";
+				reg = <0>;
+				pinctrl-names = "default";
+				spi-max-frequency = <40000000>;
+				rotate = <90>;
+				buswidth = <8>;
+				fps = <50>;
+				height = <160>;
+				width = <128>;
+				reset-gpios = <&gpio 25 0>;
+				dc-gpios = <&gpio 24 0>;
+				led-gpios = <&gpio 18 0>;
+				bgr;
+				debug = <0>;
+			};
+		};
+	};
+
+	__overrides__ {
+		green = <&af18>, "compatible=fbtft,adafruit18_green";
+		rotate = <&af18>, "rotate:0";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/sainsmart18-overlay.dts
@@ -0,0 +1,47 @@
+/*
+ * Device Tree overlay for the Sainsmart 1.8" TFT LCD with ST7735R chip 160x128
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ss18: sainsmart18@0 {
+				compatible = "fbtft,sainsmart18";
+				reg = <0>;
+				pinctrl-names = "default";
+				spi-max-frequency = <40000000>;
+				rotate = <90>;
+				buswidth = <8>;
+				fps = <50>;
+				height = <160>;
+				width = <128>;
+				reset-gpios = <&gpio 25 0>;
+				dc-gpios = <&gpio 24 0>;
+				bgr;
+				debug = <0>;
+			};
+		};
+	};
+
+	__overrides__ {
+		rotate = <&ss18>, "rotate:0";
+	};
+};
