From 4fc22765b3888cf6575015b904718bfd36d1f49c Mon Sep 17 00:00:00 2001
From: Christian Marangi <ansuelsmth@gmail.com>
Date: Wed, 11 Dec 2024 12:22:38 +0100
Subject: [PATCH 4/4] clk: en7523: Add clock for eMMC for EN7581

Add clock for eMMC for EN7581. This is used to give info of the current
eMMC source clock and to switch it from 200MHz or 150MHz.

Signed-off-by: Christian Marangi <ansuelsmth@gmail.com>
---
 drivers/clk/clk-en7523.c | 10 ++++++++++
 1 file changed, 10 insertions(+)

--- a/drivers/clk/clk-en7523.c
+++ b/drivers/clk/clk-en7523.c
@@ -91,6 +91,7 @@ static const u32 emi7581_base[] = { 5400
 static const u32 bus7581_base[] = { 600000000, 540000000 };
 static const u32 npu7581_base[] = { 800000000, 750000000, 720000000, 600000000 };
 static const u32 crypto_base[] = { 540000000, 480000000 };
+static const u32 emmc7581_base[] = { 200000000, 150000000 };
 
 static const struct en_clk_desc en7523_base_clks[] = {
 	{
@@ -281,6 +282,15 @@ static const struct en_clk_desc en7581_b
 		.base_shift = 0,
 		.base_values = crypto_base,
 		.n_base_values = ARRAY_SIZE(crypto_base),
+	}, {
+		.id = EN7581_CLK_EMMC,
+		.name = "emmc",
+
+		.base_reg = REG_CRYPTO_CLKSRC2,
+		.base_bits = 1,
+		.base_shift = 12,
+		.base_values = emmc7581_base,
+		.n_base_values = ARRAY_SIZE(emmc7581_base),
 	}
 };
 
