#!/bin/sh
if [ -e "/sys/bus/mdio_bus/drivers/IC+ IP175C/0:00" -o \
     -e "/sys/bus/mdio_bus/drivers/IC+ IP17xx/0:00" ] && \
   [ -x /sbin/swconfig ];
then
	uci batch <<EOF
set network.eth0=switch
set network.eth0.name=eth0
set network.eth0.reset=1
set network.eth0.enable_vlan=1
set network.eth0_1=switch_vlan
set network.eth0_1.device=eth0
set network.eth0_1.vlan=1
set network.eth0_1.ports="0 1 2 3 5t"
set network.eth0_2=switch_vlan
set network.eth0_2.device=eth0
set network.eth0_2.vlan=2
set network.eth0_2.ports="4 5t"
EOF
	HAS_SWITCH=1
fi

if [ -n "$HAS_SWITCH" -o \
	-e "/sys/bus/mdio_bus/drivers/Infineon ADM6996/0:00" -o \
	-e "/sys/bus/mdio_bus/drivers/Marvell 88E6060/0:10" ]; then
	uci batch <<EOF
set network.lan.ifname=eth0.1
set network.wan=interface
set network.wan.ifname=eth0.2
set network.wan.proto=dhcp
commit network
EOF
	HAS_SWITCH=1
fi

[ -z "$HAS_SWITCH" -a -d /sys/class/net/eth1 ] && {
	uci batch <<EOF
set network.wan=interface
set network.wan.ifname=eth1
set network.wan.proto=dhcp
commit network
EOF
}

uci commit network
