--- a/arch/mips/ath79/Kconfig
+++ b/arch/mips/ath79/Kconfig
@@ -762,6 +762,16 @@ config ATH79_MACH_UBNT_XM
 	  Say 'Y' here if you want your kernel to support the
 	  Ubiquiti Networks XM (rev 1.0) board.
 
+config ATH79_MACH_MYNET_N600
+	bool "WD My Net N600 board support"
+	select SOC_AR934X
+	select ATH79_DEV_ETH
+	select ATH79_DEV_GPIO_BUTTONS
+	select ATH79_DEV_LEDS_GPIO
+	select ATH79_DEV_M25P80
+	select ATH79_DEV_WMAC
+	select ATH79_NVRAM
+
 config ATH79_MACH_ZCN_1523H
 	bool "Zcomax ZCN-1523H support"
 	select SOC_AR724X
--- a/arch/mips/ath79/machtypes.h
+++ b/arch/mips/ath79/machtypes.h
@@ -53,6 +53,7 @@ enum ath79_mach_type {
 	ATH79_MACH_HORNET_UB,		/* ALFA Networks Hornet-UB */
 	ATH79_MACH_MR600V2,		/* OpenMesh MR600v2 */
 	ATH79_MACH_MR600,		/* OpenMesh MR600 */
+	ATH79_MACH_MYNET_N600,		/* WD My Net N600 */
 	ATH79_MACH_MZK_W04NU,		/* Planex MZK-W04NU */
 	ATH79_MACH_MZK_W300NH,		/* Planex MZK-W300NH */
 	ATH79_MACH_NBG460N,		/* Zyxel NBG460N/550N/550NH */
--- a/arch/mips/ath79/Makefile
+++ b/arch/mips/ath79/Makefile
@@ -64,6 +64,7 @@ obj-$(CONFIG_ATH79_MACH_JA76PF)		+= mach
 obj-$(CONFIG_ATH79_MACH_JWAP003)	+= mach-jwap003.o
 obj-$(CONFIG_ATH79_MACH_HORNET_UB)	+= mach-hornet-ub.o
 obj-$(CONFIG_ATH79_MACH_MR600)		+= mach-mr600.o
+obj-$(CONFIG_ATH79_MACH_MYNET_N600)	+= mach-mynet-n600.o
 obj-$(CONFIG_ATH79_MACH_MZK_W04NU)	+= mach-mzk-w04nu.o
 obj-$(CONFIG_ATH79_MACH_MZK_W300NH)	+= mach-mzk-w300nh.o
 obj-$(CONFIG_ATH79_MACH_NBG460N)	+= mach-nbg460n.o
