From b12363b0a393e2751395af002bf9ab192c1140c1 Mon Sep 17 00:00:00 2001
From: Thomas Petazzoni <thomas.petazzoni@free-electrons.com>
Date: Wed, 15 May 2013 15:36:58 +0200
Subject: [PATCH 13/29] arm: kirkwood: convert MPL CEC4 to use DT for the PCIe
 interface

Now that the PCIe mvebu driver is usable on Kirkwood, use it instead
of the legacy PCIe code, since it allows to describe the PCIe
interfaces in the Device Tree.

Signed-off-by: Thomas Petazzoni <thomas.petazzoni@free-electrons.com>
Signed-off-by: Jason Cooper <jason@lakedaemon.net>
---
 arch/arm/boot/dts/kirkwood-mplcec4.dts | 8 ++++++++
 arch/arm/mach-kirkwood/board-mplcec4.c | 1 -
 2 files changed, 8 insertions(+), 1 deletion(-)

--- a/arch/arm/boot/dts/kirkwood-mplcec4.dts
+++ b/arch/arm/boot/dts/kirkwood-mplcec4.dts
@@ -139,6 +139,14 @@
 			cd-gpios = <&gpio1 15 0>;
 			/* No WP GPIO */
 		};
+
+		pcie-controller {
+			status = "okay";
+
+			pcie@1,0 {
+				status = "okay";
+			};
+		};
 	};
 
 	gpio-leds {
--- a/arch/arm/mach-kirkwood/board-mplcec4.c
+++ b/arch/arm/mach-kirkwood/board-mplcec4.c
@@ -29,7 +29,6 @@ void __init mplcec4_init(void)
 	 */
 	kirkwood_ge00_init(&mplcec4_ge00_data);
 	kirkwood_ge01_init(&mplcec4_ge01_data);
-	kirkwood_pcie_init(KW_PCIE0);
 }
 
 
