--- a/drivers/net/ethernet/freescale/gianfar.c
+++ b/drivers/net/ethernet/freescale/gianfar.c
@@ -132,7 +132,7 @@ static int gfar_poll(struct napi_struct
 static void gfar_netpoll(struct net_device *dev);
 #endif
 int gfar_clean_rx_ring(struct gfar_priv_rx_q *rx_queue, int rx_work_limit);
-static void gfar_clean_tx_ring(struct gfar_priv_tx_q *tx_queue);
+static int gfar_clean_tx_ring(struct gfar_priv_tx_q *tx_queue);
 static void gfar_process_frame(struct net_device *dev, struct sk_buff *skb,
 			       int amount_pull, struct napi_struct *napi);
 void gfar_halt(struct net_device *dev);
@@ -2475,7 +2475,7 @@ static void gfar_align_skb(struct sk_buf
 }
 
 /* Interrupt Handler for Transmit complete */
-static void gfar_clean_tx_ring(struct gfar_priv_tx_q *tx_queue)
+static int gfar_clean_tx_ring(struct gfar_priv_tx_q *tx_queue)
 {
 	struct net_device *dev = tx_queue->dev;
 	struct netdev_queue *txq;
@@ -2575,6 +2575,8 @@ static void gfar_clean_tx_ring(struct gf
 	tx_queue->dirty_tx = bdp;
 
 	netdev_tx_completed_queue(txq, howmany, bytes_sent);
+
+	return howmany;
 }
 
 static void gfar_schedule_cleanup(struct gfar_priv_grp *gfargrp)
@@ -2833,82 +2835,62 @@ static int gfar_poll(struct napi_struct
 	struct gfar __iomem *regs = gfargrp->regs;
 	struct gfar_priv_tx_q *tx_queue = NULL;
 	struct gfar_priv_rx_q *rx_queue = NULL;
-	int work_done = 0, work_done_per_q = 0;
-	int i, budget_per_q = 0;
-	int has_tx_work;
-	unsigned long rstat_rxf;
-	int num_act_queues;
+	int rx_cleaned = 0, budget_per_queue = 0, rx_cleaned_per_queue = 0;
+	int tx_cleaned = 0, i, left_over_budget = budget;
+	unsigned long serviced_queues = 0;
+	int num_queues = 0;
+
+	num_queues = gfargrp->num_rx_queues;
+	budget_per_queue = budget/num_queues;
 
 	/* Clear IEVENT, so interrupts aren't called again
 	 * because of the packets that have already arrived
 	 */
 	gfar_write(&regs->ievent, IEVENT_RTX_MASK);
 
-	rstat_rxf = gfar_read(&regs->rstat) & RSTAT_RXF_MASK;
-
-	num_act_queues = bitmap_weight(&rstat_rxf, MAX_RX_QS);
-	if (num_act_queues)
-		budget_per_q = budget/num_act_queues;
-
-	while (1) {
-		has_tx_work = 0;
-		for_each_set_bit(i, &gfargrp->tx_bit_map, priv->num_tx_queues) {
-			tx_queue = priv->tx_queue[i];
-			/* run Tx cleanup to completion */
-			if (tx_queue->tx_skbuff[tx_queue->skb_dirtytx]) {
-				gfar_clean_tx_ring(tx_queue);
-				has_tx_work = 1;
-			}
-		}
+	while (num_queues && left_over_budget) {
+		budget_per_queue = left_over_budget/num_queues;
+		left_over_budget = 0;
 
 		for_each_set_bit(i, &gfargrp->rx_bit_map, priv->num_rx_queues) {
-			/* skip queue if not active */
-			if (!(rstat_rxf & (RSTAT_CLEAR_RXF0 >> i)))
+			if (test_bit(i, &serviced_queues))
 				continue;
-
 			rx_queue = priv->rx_queue[i];
-			work_done_per_q =
-				gfar_clean_rx_ring(rx_queue, budget_per_q);
-			work_done += work_done_per_q;
-
-			/* finished processing this queue */
-			if (work_done_per_q < budget_per_q) {
-				/* clear active queue hw indication */
-				gfar_write(&regs->rstat,
-					   RSTAT_CLEAR_RXF0 >> i);
-				rstat_rxf &= ~(RSTAT_CLEAR_RXF0 >> i);
-				num_act_queues--;
-
-				if (!num_act_queues)
-					break;
-				/* recompute budget per Rx queue */
-				budget_per_q =
-					(budget - work_done) / num_act_queues;
+			tx_queue = priv->tx_queue[rx_queue->qindex];
+
+			tx_cleaned += gfar_clean_tx_ring(tx_queue);
+			rx_cleaned_per_queue =
+				gfar_clean_rx_ring(rx_queue, budget_per_queue);
+			rx_cleaned += rx_cleaned_per_queue;
+			if (rx_cleaned_per_queue < budget_per_queue) {
+				left_over_budget = left_over_budget +
+					(budget_per_queue -
+					 rx_cleaned_per_queue);
+				set_bit(i, &serviced_queues);
+				num_queues--;
 			}
 		}
+	}
 
-		if (work_done >= budget)
-			break;
-
-		if (!num_act_queues && !has_tx_work) {
+	if (tx_cleaned)
+		return budget;
 
-			napi_complete(napi);
+	if (rx_cleaned < budget) {
+		napi_complete(napi);
 
-			/* Clear the halt bit in RSTAT */
-			gfar_write(&regs->rstat, gfargrp->rstat);
+		/* Clear the halt bit in RSTAT */
+		gfar_write(&regs->rstat, gfargrp->rstat);
 
-			gfar_write(&regs->imask, IMASK_DEFAULT);
+		gfar_write(&regs->imask, IMASK_DEFAULT);
 
-			/* If we are coalescing interrupts, update the timer
-			 * Otherwise, clear it
-			 */
-			gfar_configure_coalescing(priv, gfargrp->rx_bit_map,
-						  gfargrp->tx_bit_map);
-			break;
-		}
+		/* If we are coalescing interrupts, update the timer
+		 * Otherwise, clear it
+		 */
+		gfar_configure_coalescing(priv, gfargrp->rx_bit_map,
+					  gfargrp->tx_bit_map);
 	}
 
-	return work_done;
+	return rx_cleaned;
 }
 
 #ifdef CONFIG_NET_POLL_CONTROLLER
--- a/drivers/net/ethernet/freescale/gianfar.h
+++ b/drivers/net/ethernet/freescale/gianfar.h
@@ -291,9 +291,7 @@ extern const char gfar_driver_version[];
 #define RCTRL_PADDING(x)	((x << 16) & RCTRL_PAL_MASK)
 
 
-#define RSTAT_CLEAR_RHALT	0x00800000
-#define RSTAT_CLEAR_RXF0	0x00000080
-#define RSTAT_RXF_MASK		0x000000ff
+#define RSTAT_CLEAR_RHALT       0x00800000
 
 #define TCTRL_IPCSEN		0x00004000
 #define TCTRL_TUCSEN		0x00002000
