--- a/drivers/leds/Kconfig
+++ b/drivers/leds/Kconfig
@@ -582,4 +582,11 @@ config LEDS_TRIGGER_NETDEV
 	  This allows LEDs to be controlled by network device activity.
 	  If unsure, say Y.
 
+config LEDS_TRIGGER_USBDEV
+	tristate "LED USB device Trigger"
+	depends on USB && LEDS_TRIGGERS
+	help
+	  This allows LEDs to be controlled by the presence/activity of
+	  an USB device. If unsure, say N.
+
 endif # NEW_LEDS
--- a/drivers/leds/Makefile
+++ b/drivers/leds/Makefile
@@ -68,3 +68,4 @@ obj-$(CONFIG_LEDS_TRIGGER_DEFAULT_ON)	+=
 obj-$(CONFIG_LEDS_TRIGGER_TRANSIENT)	+= ledtrig-transient.o
 obj-$(CONFIG_LEDS_TRIGGER_MORSE)	+= ledtrig-morse.o
 obj-$(CONFIG_LEDS_TRIGGER_NETDEV)	+= ledtrig-netdev.o
+obj-$(CONFIG_LEDS_TRIGGER_USBDEV)	+= ledtrig-usbdev.o
--- a/drivers/leds/ledtrig-usbdev.c
+++ b/drivers/leds/ledtrig-usbdev.c
@@ -24,7 +24,6 @@
 #include <linux/list.h>
 #include <linux/spinlock.h>
 #include <linux/device.h>
-#include <linux/sysdev.h>
 #include <linux/timer.h>
 #include <linux/ctype.h>
 #include <linux/slab.h>
