--- a/drivers/usb/host/Kconfig
+++ b/drivers/usb/host/Kconfig
@@ -403,6 +403,16 @@ config USB_OHCI_HCD_PLATFORM
 
 	  If unsure, say N.
 
+config USB_EHCI_HCD_PLATFORM
+	bool "Generic EHCI driver for a platform device"
+	depends on USB_EHCI_HCD && EXPERIMENTAL
+	default n
+	---help---
+	  Adds an EHCI host driver for a generic platform device, which
+	  provieds a memory space and an irq.
+
+	  If unsure, say N.
+
 config USB_OHCI_BIG_ENDIAN_DESC
 	bool
 	depends on USB_OHCI_HCD
--- a/drivers/usb/host/ehci-hcd.c
+++ b/drivers/usb/host/ehci-hcd.c
@@ -1381,6 +1381,11 @@ MODULE_LICENSE ("GPL");
 #define        PLATFORM_DRIVER         ehci_mv_driver
 #endif
 
+#ifdef CONFIG_USB_EHCI_HCD_PLATFORM
+#include "ehci-platform.c"
+#define PLATFORM_DRIVER		ehci_platform_driver
+#endif
+
 #if !defined(PCI_DRIVER) && !defined(PLATFORM_DRIVER) && \
     !defined(PS3_SYSTEM_BUS_DRIVER) && !defined(OF_PLATFORM_DRIVER) && \
     !defined(XILINX_OF_PLATFORM_DRIVER)
--- /dev/null
+++ b/drivers/usb/host/ehci-platform.c
@@ -0,0 +1,198 @@
+/*
+ * Generic platform ehci driver
+ *
+ * Copyright 2007 Steven Brown <sbrown@cortland.com>
+ * Copyright 2010-2012 Hauke Mehrtens <hauke@hauke-m.de>
+ *
+ * Derived from the ohci-ssb driver
+ * Copyright 2007 Michael Buesch <m@bues.ch>
+ *
+ * Derived from the EHCI-PCI driver
+ * Copyright (c) 2000-2004 by David Brownell
+ *
+ * Derived from the ohci-pci driver
+ * Copyright 1999 Roman Weissgaerber
+ * Copyright 2000-2002 David Brownell
+ * Copyright 1999 Linus Torvalds
+ * Copyright 1999 Gregory P. Smith
+ *
+ * Licensed under the GNU/GPL. See COPYING for details.
+ */
+#include <linux/platform_device.h>
+#include <linux/usb/ehci_pdriver.h>
+
+static int ehci_platform_reset(struct usb_hcd *hcd)
+{
+	struct platform_device *pdev = to_platform_device(hcd->self.controller);
+	struct usb_ehci_pdata *pdata = pdev->dev.platform_data;
+	struct ehci_hcd *ehci = hcd_to_ehci(hcd);
+	int retval;
+
+	hcd->has_tt = pdata->has_tt;
+	ehci->has_synopsys_hc_bug = pdata->has_synopsys_hc_bug;
+	ehci->big_endian_desc = pdata->big_endian_desc;
+	ehci->big_endian_mmio = pdata->big_endian_mmio;
+
+	ehci->caps = hcd->regs + pdata->caps_offset;
+	retval = ehci_setup(hcd);
+	if (retval)
+		return retval;
+
+	if (pdata->port_power_on)
+		ehci_port_power(ehci, 1);
+	if (pdata->port_power_off)
+		ehci_port_power(ehci, 0);
+
+	return 0;
+}
+
+static const struct hc_driver ehci_platform_hc_driver = {
+	.description		= hcd_name,
+	.product_desc		= "Generic Platform EHCI Controller",
+	.hcd_priv_size		= sizeof(struct ehci_hcd),
+
+	.irq			= ehci_irq,
+	.flags			= HCD_MEMORY | HCD_USB2,
+
+	.reset			= ehci_platform_reset,
+	.start			= ehci_run,
+	.stop			= ehci_stop,
+	.shutdown		= ehci_shutdown,
+
+	.urb_enqueue		= ehci_urb_enqueue,
+	.urb_dequeue		= ehci_urb_dequeue,
+	.endpoint_disable	= ehci_endpoint_disable,
+	.endpoint_reset		= ehci_endpoint_reset,
+
+	.get_frame_number	= ehci_get_frame,
+
+	.hub_status_data	= ehci_hub_status_data,
+	.hub_control		= ehci_hub_control,
+#if defined(CONFIG_PM)
+	.bus_suspend		= ehci_bus_suspend,
+	.bus_resume		= ehci_bus_resume,
+#endif
+	.relinquish_port	= ehci_relinquish_port,
+	.port_handed_over	= ehci_port_handed_over,
+
+	.update_device		= ehci_update_device,
+
+	.clear_tt_buffer_complete = ehci_clear_tt_buffer_complete,
+};
+
+static int __devinit ehci_platform_probe(struct platform_device *dev)
+{
+	struct usb_hcd *hcd;
+	struct resource *res_mem;
+	int irq;
+	int err = -ENOMEM;
+
+	BUG_ON(!dev->dev.platform_data);
+
+	if (usb_disabled())
+		return -ENODEV;
+
+	irq = platform_get_irq(dev, 0);
+	if (irq < 0) {
+		pr_err("no irq provieded");
+		return irq;
+	}
+	res_mem = platform_get_resource(dev, IORESOURCE_MEM, 0);
+	if (!res_mem) {
+		pr_err("no memory recourse provieded");
+		return -ENXIO;
+	}
+
+	hcd = usb_create_hcd(&ehci_platform_hc_driver, &dev->dev,
+			     dev_name(&dev->dev));
+	if (!hcd)
+		return -ENOMEM;
+
+	hcd->rsrc_start = res_mem->start;
+	hcd->rsrc_len = resource_size(res_mem);
+
+	if (!request_mem_region(hcd->rsrc_start, hcd->rsrc_len, hcd_name)) {
+		pr_err("controller already in use");
+		err = -EBUSY;
+		goto err_put_hcd;
+	}
+
+	hcd->regs = ioremap_nocache(hcd->rsrc_start, hcd->rsrc_len);
+	if (!hcd->regs)
+		goto err_release_region;
+	err = usb_add_hcd(hcd, irq, IRQF_SHARED);
+	if (err)
+		goto err_iounmap;
+
+	platform_set_drvdata(dev, hcd);
+
+	return err;
+
+err_iounmap:
+	iounmap(hcd->regs);
+err_release_region:
+	release_mem_region(hcd->rsrc_start, hcd->rsrc_len);
+err_put_hcd:
+	usb_put_hcd(hcd);
+	return err;
+}
+
+static int __devexit ehci_platform_remove(struct platform_device *dev)
+{
+	struct usb_hcd *hcd = platform_get_drvdata(dev);
+
+	usb_remove_hcd(hcd);
+	iounmap(hcd->regs);
+	release_mem_region(hcd->rsrc_start, hcd->rsrc_len);
+	usb_put_hcd(hcd);
+	platform_set_drvdata(dev, NULL);
+
+	return 0;
+}
+
+#ifdef CONFIG_PM
+
+static int ehci_platform_suspend(struct device *dev)
+{
+	struct usb_hcd *hcd = dev_get_drvdata(dev);
+	bool wakeup = device_may_wakeup(dev);
+
+	ehci_prepare_ports_for_controller_suspend(hcd_to_ehci(hcd), wakeup);
+	return 0;
+}
+
+static int ehci_platform_resume(struct device *dev)
+{
+	struct usb_hcd *hcd = dev_get_drvdata(dev);
+
+	ehci_prepare_ports_for_controller_resume(hcd_to_ehci(hcd));
+	return 0;
+}
+
+#else /* !CONFIG_PM */
+#define ehci_platform_suspend	NULL
+#define ehci_platform_resume	NULL
+#endif /* CONFIG_PM */
+
+static const struct platform_device_id ehci_platform_table[] = {
+	{ "ehci-platform", 0 },
+	{ }
+};
+MODULE_DEVICE_TABLE(platform, ehci_platform_table);
+
+static const struct dev_pm_ops ehci_platform_pm_ops = {
+	.suspend	= ehci_platform_suspend,
+	.resume		= ehci_platform_resume,
+};
+
+static struct platform_driver ehci_platform_driver = {
+	.id_table	= ehci_platform_table,
+	.probe		= ehci_platform_probe,
+	.remove		= __devexit_p(ehci_platform_remove),
+	.shutdown	= usb_hcd_platform_shutdown,
+	.driver		= {
+		.owner	= THIS_MODULE,
+		.name	= "ehci-platform",
+		.pm	= &ehci_platform_pm_ops,
+	}
+};
--- /dev/null
+++ b/include/linux/usb/ehci_pdriver.h
@@ -0,0 +1,46 @@
+/*
+ * Copyright (C) 2012 Hauke Mehrtens <hauke@hauke-m.de>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful, but
+ * WITHOUT ANY WARRANTY; without even the implied warranty of MERCHANTABILITY
+ * or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public License
+ * for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software Foundation,
+ * Inc., 675 Mass Ave, Cambridge, MA 02139, USA.
+ */
+
+#ifndef __USB_CORE_EHCI_PDRIVER_H
+#define __USB_CORE_EHCI_PDRIVER_H
+
+/**
+ * struct usb_ehci_pdata - platform_data for generic ehci driver
+ *
+ * @caps_offset:	offset of the EHCI Capability Registers to the start of
+ *			the io memory region provided to the driver.
+ * @has_tt:		set to 1 if TT is integrated in root hub.
+ * @port_power_on:	set to 1 if the controller needs a power up after
+ *			initialization.
+ * @port_power_off:	set to 1 if the controller needs to be powered down
+ *			after initialization.
+ *
+ * These are general configuration options for the EHCI controller. All of
+ * these options are activating more or less workarounds for some hardware.
+ */
+struct usb_ehci_pdata {
+	int		caps_offset;
+	unsigned	has_tt:1;
+	unsigned	has_synopsys_hc_bug:1;
+	unsigned	big_endian_desc:1;
+	unsigned	big_endian_mmio:1;
+	unsigned	port_power_on:1;
+	unsigned	port_power_off:1;
+};
+
+#endif /* __USB_CORE_EHCI_PDRIVER_H */
