From 60e8a35f0efa5a7e5d797a3f239971c84061ef11 Mon Sep 17 00:00:00 2001
From: Daniel Schwierzeck <daniel.schwierzeck@gmail.com>
Date: Tue, 6 Nov 2012 21:39:47 +0100
Subject: sf: handle CONFIG_MANUAL_RELOC

Signed-off-by: Daniel Schwierzeck <daniel.schwierzeck@gmail.com>

--- a/drivers/mtd/spi/spi_flash.c
+++ b/drivers/mtd/spi/spi_flash.c
@@ -293,7 +293,7 @@ int spi_flash_cmd_write_status(struct sp
  */
 #define IDCODE_CONT_LEN 0
 #define IDCODE_PART_LEN 5
-static const struct {
+static struct {
 	const u8 shift;
 	const u8 idcode;
 	struct spi_flash *(*probe) (struct spi_slave *spi, u8 *idcode);
@@ -335,6 +335,10 @@ static const struct {
 };
 #define IDCODE_LEN (IDCODE_CONT_LEN + IDCODE_PART_LEN)
 
+#ifdef CONFIG_NEEDS_MANUAL_RELOC
+DECLARE_GLOBAL_DATA_PTR;
+#endif
+
 struct spi_flash *spi_flash_probe(unsigned int bus, unsigned int cs,
 		unsigned int max_hz, unsigned int spi_mode)
 {
@@ -342,6 +346,16 @@ struct spi_flash *spi_flash_probe(unsign
 	struct spi_flash *flash = NULL;
 	int ret, i, shift;
 	u8 idcode[IDCODE_LEN], *idp;
+#ifdef CONFIG_NEEDS_MANUAL_RELOC
+	static int relocated;
+
+	if (!relocated) {
+		for (i = 0; i < ARRAY_SIZE(flashes); i++)
+			flashes[i].probe += gd->reloc_off;
+
+		relocated = 1;
+	}
+#endif
 
 	spi = spi_setup_slave(bus, cs, max_hz, spi_mode);
 	if (!spi) {
