From 12594762fcbec024cb424c9b77efb28402651667 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Thu, 27 Jun 2013 21:33:56 +0200
Subject: [PATCH 04/10] MIPS: bmips: change compile time checks to runtime
 checks

Allow building for all bmips cpus at the same time by changing ifdefs
to checks for the cpu type, or adding appropriate checks to the
assembly.

Signed-off-by: Jonas Gorski <jogo@openwrt.org>
---
 arch/mips/kernel/bmips_vec.S |   55 +++++++---
 arch/mips/kernel/smp-bmips.c |  241 ++++++++++++++++++++++--------------------
 2 files changed, 172 insertions(+), 124 deletions(-)

--- a/arch/mips/kernel/bmips_vec.S
+++ b/arch/mips/kernel/bmips_vec.S
@@ -13,6 +13,7 @@
 #include <asm/asm.h>
 #include <asm/asmmacro.h>
 #include <asm/cacheops.h>
+#include <asm/cpu.h>
 #include <asm/regdef.h>
 #include <asm/mipsregs.h>
 #include <asm/stackframe.h>
@@ -89,12 +90,18 @@ NESTED(bmips_reset_nmi_vec, PT_SIZE, sp)
 	beqz	k0, bmips_smp_entry
 
 #if defined(CONFIG_CPU_BMIPS5000)
+	mfc0	k0, CP0_PRID
+	li	k1, PRID_IMP_BMIPS5000
+	andi	k0, 0xff00
+	bne	k0, k1, 1f
+
 	/* if we're not on core 0, this must be the SMP boot signal */
 	li	k1, (3 << 25)
 	mfc0	k0, $22
 	and	k0, k1
 	bnez	k0, bmips_smp_entry
-#endif
+1:
+#endif /* CONFIG_CPU_BMIPS5000 */
 #endif /* CONFIG_SMP */
 
 	/* nope, it's just a regular NMI */
@@ -137,7 +144,12 @@ bmips_smp_entry:
 	xori	k0, 0x04
 	mtc0	k0, CP0_CONFIG
 
+	mfc0	k0, CP0_PRID
+	andi	k0, 0xff00
 #if defined(CONFIG_CPU_BMIPS4350) || defined(CONFIG_CPU_BMIPS4380)
+	li	k1, PRID_IMP_BMIPS43XX
+	bne	k0, k1, 2f
+
 	/* initialize CPU1's local I-cache */
 	li	k0, 0x80000000
 	li	k1, 0x80010000
@@ -148,14 +160,21 @@ bmips_smp_entry:
 1:	cache	Index_Store_Tag_I, 0(k0)
 	addiu	k0, 16
 	bne	k0, k1, 1b
-#elif defined(CONFIG_CPU_BMIPS5000)
+
+	b	3f
+2:
+#endif /* CONFIG_CPU_BMIPS4350 || CONFIG_CPU_BMIPS4380 */
+#if defined(CONFIG_CPU_BMIPS5000)
 	/* set exception vector base */
+	li	k1, PRID_IMP_BMIPS5000
+	bne	k0, k1, 3f
+
 	la	k0, ebase
 	lw	k0, 0(k0)
 	mtc0	k0, $15, 1
 	BARRIER
-#endif
-
+#endif /* CONFIG_CPU_BMIPS5000 */
+3:
 	/* jump back to kseg0 in case we need to remap the kseg1 area */
 	la	k0, 1f
 	jr	k0
@@ -221,8 +240,18 @@ END(bmips_smp_int_vec)
 LEAF(bmips_enable_xks01)
 
 #if defined(CONFIG_XKS01)
-
+	mfc0	t0, CP0_PRID
+	andi	t2, t0, 0xff00
 #if defined(CONFIG_CPU_BMIPS4380)
+	li	t1, PRID_IMP_BMIPS43XX
+	bne	t2, t1, 1f
+
+	andi	t0, 0xff
+	addiu	t1, t0, -PRID_REV_BMIPS4380_HI
+	bgtz	t1, 2f
+	addiu	t0, -PRID_REV_BMIPS4380_LO
+	bltz	t0, 2f
+
 	mfc0	t0, $22, 3
 	li	t1, 0x1ff0
 	li	t2, (1 << 12) | (1 << 9)
@@ -231,7 +260,13 @@ LEAF(bmips_enable_xks01)
 	or	t0, t2
 	mtc0	t0, $22, 3
 	BARRIER
-#elif defined(CONFIG_CPU_BMIPS5000)
+	b	2f
+1:
+#endif /* CONFIG_CPU_BMIPS4380 */
+#if defined(CONFIG_CPU_BMIPS5000)
+	li	t1, PRID_IMP_BMIPS5000
+	bne	t2, t1, 2f
+
 	mfc0	t0, $22, 5
 	li	t1, 0x01ff
 	li	t2, (1 << 8) | (1 << 5)
@@ -240,12 +275,8 @@ LEAF(bmips_enable_xks01)
 	or	t0, t2
 	mtc0	t0, $22, 5
 	BARRIER
-#else
-
-#error Missing XKS01 setup
-
-#endif
-
+#endif /* CONFIG_CPU_BMIPS5000 */
+2:
 #endif /* defined(CONFIG_XKS01) */
 
 	jr	ra
--- a/arch/mips/kernel/smp-bmips.c
+++ b/arch/mips/kernel/smp-bmips.c
@@ -49,8 +49,11 @@ cpumask_t bmips_booted_mask;
 unsigned long bmips_smp_boot_sp;
 unsigned long bmips_smp_boot_gp;
 
+static void bmips43xx_send_ipi_single(int cpu, unsigned int action);
+static void bmips5000_send_ipi_single(int cpu, unsigned int action);
 static void bmips_send_ipi_single(int cpu, unsigned int action);
-static irqreturn_t bmips_ipi_interrupt(int irq, void *dev_id);
+static irqreturn_t bmips43xx_ipi_interrupt(int irq, void *dev_id);
+static irqreturn_t bmips5000_ipi_interrupt(int irq, void *dev_id);
 
 /* SW interrupts 0,1 are used for interprocessor signaling */
 #define IPI0_IRQ			(MIPS_CPU_IRQ_BASE + 0)
@@ -65,48 +68,49 @@ static void __init bmips_smp_setup(void)
 {
 	int i, cpu = 1, boot_cpu = 0;
 
-#if defined(CONFIG_CPU_BMIPS4350) || defined(CONFIG_CPU_BMIPS4380)
-	/* arbitration priority */
-	clear_c0_brcm_cmt_ctrl(0x30);
-
-	/* NBK and weak order flags */
-	set_c0_brcm_config_0(0x30000);
-
-	/* Find out if we are running on TP0 or TP1 */
-	boot_cpu = !!(read_c0_brcm_cmt_local() & (1 << 31));
-
-	/*
-	 * MIPS interrupts 0,1 (SW INT 0,1) cross over to the other thread
-	 * MIPS interrupt 2 (HW INT 0) is the CPU0 L1 controller output
-	 * MIPS interrupt 3 (HW INT 1) is the CPU1 L1 controller output
-	 *
-	 * If booting from TP1, leave the existing CMT interrupt routing
-	 * such that TP0 responds to SW1 and TP1 responds to SW0.
-	 */
-	if (boot_cpu == 0)
-		change_c0_brcm_cmt_intr(0xf8018000,
+	if (cpu_is_bmips4350() || cpu_is_bmips4380()) {
+		/* arbitration priority */
+		clear_c0_brcm_cmt_ctrl(0x30);
+
+		/* NBK and weak order flags */
+		set_c0_brcm_config_0(0x30000);
+
+		/* Find out if we are running on TP0 or TP1 */
+		boot_cpu = !!(read_c0_brcm_cmt_local() & (1 << 31));
+
+		/*
+		 * MIPS interrupts 0,1 (SW INT 0,1) cross over to the other
+		 * thread
+		 * MIPS interrupt 2 (HW INT 0) is the CPU0 L1 controller output
+		 * MIPS interrupt 3 (HW INT 1) is the CPU1 L1 controller output
+		 *
+		 * If booting from TP1, leave the existing CMT interrupt routing
+		 * such that TP0 responds to SW1 and TP1 responds to SW0.
+		 */
+		if (boot_cpu == 0)
+			change_c0_brcm_cmt_intr(0xf8018000,
 					(0x02 << 27) | (0x03 << 15));
-	else
-		change_c0_brcm_cmt_intr(0xf8018000, (0x1d << 27));
-
-	/* single core, 2 threads (2 pipelines) */
-	max_cpus = 2;
-#elif defined(CONFIG_CPU_BMIPS5000)
-	/* enable raceless SW interrupts */
-	set_c0_brcm_config(0x03 << 22);
-
-	/* route HW interrupt 0 to CPU0, HW interrupt 1 to CPU1 */
-	change_c0_brcm_mode(0x1f << 27, 0x02 << 27);
+		else
+			change_c0_brcm_cmt_intr(0xf8018000, (0x1d << 27));
 
-	/* N cores, 2 threads per core */
-	max_cpus = (((read_c0_brcm_config() >> 6) & 0x03) + 1) << 1;
-
-	/* clear any pending SW interrupts */
-	for (i = 0; i < max_cpus; i++) {
-		write_c0_brcm_action(ACTION_CLR_IPI(i, 0));
-		write_c0_brcm_action(ACTION_CLR_IPI(i, 1));
+		/* single core, 2 threads (2 pipelines) */
+		max_cpus = 2;
+	} else if (cpu_is_bmips5000()) {
+		/* enable raceless SW interrupts */
+		set_c0_brcm_config(0x03 << 22);
+
+		/* route HW interrupt 0 to CPU0, HW interrupt 1 to CPU1 */
+		change_c0_brcm_mode(0x1f << 27, 0x02 << 27);
+
+		/* N cores, 2 threads per core */
+		max_cpus = (((read_c0_brcm_config() >> 6) & 0x03) + 1) << 1;
+
+		/* clear any pending SW interrupts */
+		for (i = 0; i < max_cpus; i++) {
+			write_c0_brcm_action(ACTION_CLR_IPI(i, 0));
+			write_c0_brcm_action(ACTION_CLR_IPI(i, 1));
+		}
 	}
-#endif
 
 	if (!bmips_smp_enabled)
 		max_cpus = 1;
@@ -134,6 +138,15 @@ static void __init bmips_smp_setup(void)
  */
 static void bmips_prepare_cpus(unsigned int max_cpus)
 {
+	irqreturn_t (*bmips_ipi_interrupt)(int irq, void *dev_id);
+
+	if (cpu_is_bmips4350() || cpu_is_bmips4380())
+		bmips_ipi_interrupt = bmips43xx_ipi_interrupt;
+	else if (cpu_is_bmips5000())
+		bmips_ipi_interrupt = bmips5000_ipi_interrupt;
+	else
+		return;
+
 	if (request_irq(IPI0_IRQ, bmips_ipi_interrupt, IRQF_PERCPU,
 			"smp_ipi0", NULL))
 		panic("Can't request IPI0 interrupt\n");
@@ -168,26 +181,26 @@ static void bmips_boot_secondary(int cpu
 
 	pr_info("SMP: Booting CPU%d...\n", cpu);
 
-	if (cpumask_test_cpu(cpu, &bmips_booted_mask))
+	if (cpumask_test_cpu(cpu, &bmips_booted_mask)) {
 		bmips_send_ipi_single(cpu, 0);
-	else {
-#if defined(CONFIG_CPU_BMIPS4350) || defined(CONFIG_CPU_BMIPS4380)
-		/* Reset slave TP1 if booting from TP0 */
-		if (cpu_logical_map(cpu) == 0)
-			set_c0_brcm_cmt_ctrl(0x01);
-#elif defined(CONFIG_CPU_BMIPS5000)
-		if (cpu & 0x01)
-			write_c0_brcm_action(ACTION_BOOT_THREAD(cpu));
-		else {
-			/*
-			 * core N thread 0 was already booted; just
-			 * pulse the NMI line
-			 */
-			bmips_write_zscm_reg(0x210, 0xc0000000);
-			udelay(10);
-			bmips_write_zscm_reg(0x210, 0x00);
+	} else {
+		if (cpu_is_bmips4350() || cpu_is_bmips4380()) {
+			/* Reset slave TP1 if booting from TP0 */
+			if (cpu_logical_map(cpu) == 0)
+				set_c0_brcm_cmt_ctrl(0x01);
+		} else if (cpu_is_bmips5000()) {
+			if (cpu & 0x01)
+				write_c0_brcm_action(ACTION_BOOT_THREAD(cpu));
+			else {
+				/*
+				 * core N thread 0 was already booted; just
+				 * pulse the NMI line
+				 */
+				bmips_write_zscm_reg(0x210, 0xc0000000);
+				udelay(10);
+				bmips_write_zscm_reg(0x210, 0x00);
+			}
 		}
-#endif
 		cpumask_set_cpu(cpu, &bmips_booted_mask);
 	}
 }
@@ -199,20 +212,21 @@ static void bmips_init_secondary(void)
 {
 	/* move NMI vector to kseg0, in case XKS01 is enabled */
 
-#if defined(CONFIG_CPU_BMIPS4350) || defined(CONFIG_CPU_BMIPS4380)
-	void __iomem *cbr = BMIPS_GET_CBR();
-	unsigned long old_vec;
-
-	old_vec = __raw_readl(cbr + BMIPS_RELO_VECTOR_CONTROL_1);
-	__raw_writel(old_vec & ~0x20000000, cbr + BMIPS_RELO_VECTOR_CONTROL_1);
-
-	clear_c0_cause(smp_processor_id() ? C_SW1 : C_SW0);
-#elif defined(CONFIG_CPU_BMIPS5000)
-	write_c0_brcm_bootvec(read_c0_brcm_bootvec() &
-		(smp_processor_id() & 0x01 ? ~0x20000000 : ~0x2000));
+	if (cpu_is_bmips4350() || cpu_is_bmips4380()) {
+		void __iomem *cbr = BMIPS_GET_CBR();
+		unsigned long old_vec;
+
+		old_vec = __raw_readl(cbr + BMIPS_RELO_VECTOR_CONTROL_1);
+		__raw_writel(old_vec & ~0x20000000,
+			cbr + BMIPS_RELO_VECTOR_CONTROL_1);
+
+		clear_c0_cause(smp_processor_id() ? C_SW1 : C_SW0);
+	} else if (cpu_is_bmips5000()) {
+		write_c0_brcm_bootvec(read_c0_brcm_bootvec() &
+			(smp_processor_id() & 0x01 ? ~0x20000000 : ~0x2000));
 
-	write_c0_brcm_action(ACTION_CLR_IPI(smp_processor_id(), 0));
-#endif
+		write_c0_brcm_action(ACTION_CLR_IPI(smp_processor_id(), 0));
+	}
 }
 
 /*
@@ -237,8 +251,6 @@ static void bmips_cpus_done(void)
 {
 }
 
-#if defined(CONFIG_CPU_BMIPS5000)
-
 /*
  * BMIPS5000 raceless IPIs
  *
@@ -247,12 +259,12 @@ static void bmips_cpus_done(void)
  * IPI1 is used for SMP_CALL_FUNCTION
  */
 
-static void bmips_send_ipi_single(int cpu, unsigned int action)
+static void bmips5000_send_ipi_single(int cpu, unsigned int action)
 {
 	write_c0_brcm_action(ACTION_SET_IPI(cpu, action == SMP_CALL_FUNCTION));
 }
 
-static irqreturn_t bmips_ipi_interrupt(int irq, void *dev_id)
+static irqreturn_t bmips5000_ipi_interrupt(int irq, void *dev_id)
 {
 	int action = irq - IPI0_IRQ;
 
@@ -266,8 +278,6 @@ static irqreturn_t bmips_ipi_interrupt(i
 	return IRQ_HANDLED;
 }
 
-#else
-
 /*
  * BMIPS43xx racey IPIs
  *
@@ -281,7 +291,7 @@ static irqreturn_t bmips_ipi_interrupt(i
 static DEFINE_SPINLOCK(ipi_lock);
 static DEFINE_PER_CPU(int, ipi_action_mask);
 
-static void bmips_send_ipi_single(int cpu, unsigned int action)
+static void bmips43xx_send_ipi_single(int cpu, unsigned int action)
 {
 	unsigned long flags;
 
@@ -292,7 +302,7 @@ static void bmips_send_ipi_single(int cp
 	spin_unlock_irqrestore(&ipi_lock, flags);
 }
 
-static irqreturn_t bmips_ipi_interrupt(int irq, void *dev_id)
+static irqreturn_t bmips43xx_ipi_interrupt(int irq, void *dev_id)
 {
 	unsigned long flags;
 	int action, cpu = irq - IPI0_IRQ;
@@ -311,7 +321,13 @@ static irqreturn_t bmips_ipi_interrupt(i
 	return IRQ_HANDLED;
 }
 
-#endif /* BMIPS type */
+static void bmips_send_ipi_single(int cpu, unsigned int action)
+{
+	if (cpu_is_bmips4350() || cpu_is_bmips4380())
+		bmips43xx_send_ipi_single(cpu, action);
+	else if (cpu_is_bmips5000())
+		bmips5000_send_ipi_single(cpu, action);
+}
 
 static void bmips_send_ipi_mask(const struct cpumask *mask,
 	unsigned int action)
@@ -421,43 +437,44 @@ void __cpuinit bmips_ebase_setup(void)
 
 	BUG_ON(ebase != CKSEG0);
 
-#if defined(CONFIG_CPU_BMIPS4350)
-	/*
-	 * BMIPS4350 cannot relocate the normal vectors, but it
-	 * can relocate the BEV=1 vectors.  So CPU1 starts up at
-	 * the relocated BEV=1, IV=0 general exception vector @
-	 * 0xa000_0380.
-	 *
-	 * set_uncached_handler() is used here because:
-	 *  - CPU1 will run this from uncached space
-	 *  - None of the cacheflush functions are set up yet
-	 */
-	set_uncached_handler(BMIPS_WARM_RESTART_VEC - CKSEG0,
-		&bmips_smp_int_vec, 0x80);
-	__sync();
-	return;
-#elif defined(CONFIG_CPU_BMIPS4380)
-	/*
-	 * 0x8000_0000: reset/NMI (initially in kseg1)
-	 * 0x8000_0400: normal vectors
-	 */
-	new_ebase = 0x80000400;
-	cbr = BMIPS_GET_CBR();
-	__raw_writel(0x80080800, cbr + BMIPS_RELO_VECTOR_CONTROL_0);
-	__raw_writel(0xa0080800, cbr + BMIPS_RELO_VECTOR_CONTROL_1);
-#elif defined(CONFIG_CPU_BMIPS5000)
-	/*
-	 * 0x8000_0000: reset/NMI (initially in kseg1)
-	 * 0x8000_1000: normal vectors
-	 */
-	new_ebase = 0x80001000;
-	write_c0_brcm_bootvec(0xa0088008);
-	write_c0_ebase(new_ebase);
-	if (max_cpus > 2)
-		bmips_write_zscm_reg(0xa0, 0xa008a008);
-#else
-	return;
-#endif
+	if (cpu_is_bmips4350()) {
+		/*
+		 * BMIPS4350 cannot relocate the normal vectors, but it
+		 * can relocate the BEV=1 vectors.  So CPU1 starts up at
+		 * the relocated BEV=1, IV=0 general exception vector @
+		 * 0xa000_0380.
+		 *
+		 * set_uncached_handler() is used here because:
+		 *  - CPU1 will run this from uncached space
+		 *  - None of the cacheflush functions are set up yet
+		 */
+		set_uncached_handler(BMIPS_WARM_RESTART_VEC - CKSEG0,
+			&bmips_smp_int_vec, 0x80);
+		__sync();
+		return;
+	} else if (cpu_is_bmips4380()) {
+		/*
+		 * 0x8000_0000: reset/NMI (initially in kseg1)
+		 * 0x8000_0400: normal vectors
+		 */
+		new_ebase = 0x80000400;
+		cbr = BMIPS_GET_CBR();
+		__raw_writel(0x80080800, cbr + BMIPS_RELO_VECTOR_CONTROL_0);
+		__raw_writel(0xa0080800, cbr + BMIPS_RELO_VECTOR_CONTROL_1);
+	} else if (cpu_is_bmips5000()) {
+		/*
+		 * 0x8000_0000: reset/NMI (initially in kseg1)
+		 * 0x8000_1000: normal vectors
+		 */
+		new_ebase = 0x80001000;
+		write_c0_brcm_bootvec(0xa0088008);
+		write_c0_ebase(new_ebase);
+		if (max_cpus > 2)
+			bmips_write_zscm_reg(0xa0, 0xa008a008);
+	} else {
+		return;
+	}
+
 	board_nmi_handler_setup = &bmips_nmi_handler_setup;
 	ebase = new_ebase;
 }
