
config custom-commands
	option description '****************通用****************'
	option command 'ATI'

config custom-commands
	option description '模组信息 > ATI'
	option command 'ATI'

config custom-commands
	option description '查询SIM卡状态 > AT+CPIN?'
	option command 'AT+CPIN?'

config custom-commands
	option description '查询网络信号质量（4G） > AT+CSQ'
	option command 'AT+CSQ'

config custom-commands
	option description '查询网络信号质量（5G） > AT+CESQ'
	option command 'AT+CESQ'

config custom-commands
	option description '查询网络信息 > AT+COPS?'
	option command 'AT+COPS?'

config custom-commands
	option description '查询PDP信息 > AT+CGDCONT?'
	option command 'AT+CGDCONT?'

config custom-commands
	option description '查询PDP地址 > AT+CGPADDR'
	option command 'AT+CGPADDR'

config custom-commands
	option description '查询模组IMEI > AT+CGSN'
	option command 'AT+CGSN'

config custom-commands
	option description '查询模组IMEI > AT+GSN'
	option command 'AT+GSN'

config custom-commands
	option description '查看当前电压'
	option command 'AT+CBC'

config custom-commands
	option description '最小功能模式 > AT+CFUN=0'
	option command 'AT+CFUN=0'

config custom-commands
	option description '全功能模式 > AT+CFUN=1'
	option command 'AT+CFUN=1'

config custom-commands
	option description '重启模组 > AT+CFUN=1,1'
	option command 'AT+CFUN=1,1'

config custom-commands
	option description '****************移远****************'
	option command 'ATI'

config custom-commands
	option description 'SIM卡状态上报 > AT+QSIMSTAT?'
	option command 'AT+QSIMSTAT?'

config custom-commands
	option description '设置当前使用的为卡1 > AT+QUIMSLOT=1'
	option command 'AT+QUIMSLOT=1'

config custom-commands
	option description '设置当前使用的为卡2 > AT+QUIMSLOT=2'
	option command 'AT+QUIMSLOT=2'

config custom-commands
	option description '查询网络信息 > AT+QNWINFO'
	option command 'AT+QNWINFO'

config custom-commands
	option description '查询SIM卡签约速率 > AT+QNWCFG="nr5g_ambr"'
	option command 'AT+QNWCFG="nr5g_ambr"'

config custom-commands
	option description '查询载波聚合参数 > AT+QCAINFO'
	option command 'AT+QCAINFO'

config custom-commands
	option description '查询当前拨号模式 > AT+QCFG="usbnet"'
	option command 'AT+QCFG="usbnet"'

config custom-commands
	option description 'QMI/GobiNet拨号 > AT+QCFG="usbnet",0'
	option command 'AT+QCFG="usbnet",0'

config custom-commands
	option description 'ECM拨号 > AT+QCFG="usbnet",1'
	option command 'AT+QCFG="usbnet",1'

config custom-commands
	option description 'MBIM拨号 > AT+QCFG="usbnet",2'
	option command 'AT+QCFG="usbnet",2'

config custom-commands
	option description 'RNDIS拨号 > AT+QCFG="usbnet",3'
	option command 'AT+QCFG="usbnet",3'

config custom-commands
	option description 'NCM拨号 > AT+QCFG="usbnet",5'
	option command 'AT+QCFG="usbnet",5'

config custom-commands
	option description '锁4G > AT+QNWPREFCFG="mode_pref",LTE'
	option command 'AT+QNWPREFCFG="mode_pref",LTE'

config custom-commands
	option description '锁5G > AT+QNWPREFCFG="mode_pref",NR5G'
	option command 'AT+QNWPREFCFG="mode_pref",NR5G'

config custom-commands
	option description '锁5G NSA > AT+QNWPREFCFG="mode_pref",NR5G-NSA'
	option command 'AT+QNWPREFCFG="mode_pref",NR5G-NSA'

config custom-commands
	option description '锁5G SA > AT+QNWPREFCFG="mode_pref",NR5G-SA'
	option command 'AT+QNWPREFCFG="mode_pref",NR5G-SA'

config custom-commands
	option description '恢复自动搜索网络 > AT+QNWPREFCFG="mode_pref",AUTO'
	option command 'AT+QNWPREFCFG="mode_pref",AUTO'

config custom-commands
	option description '查询模组IMEI > AT+EGMR=0,7'
	option command 'AT+EGMR=0,7'

config custom-commands
	option description '更改模组IMEI > AT+EGMR=1,7,"IMEI"'
	option command 'AT+EGMR=1,7,"在此设置IMEI"'

config custom-commands
	option description '获取模组温度 > AT+QTEMP'
	option command 'AT+QTEMP'

config custom-commands
	option description '切换为USB通信端口 > AT+QCFG="data_interface",0,0'
	option command 'AT+QCFG="data_interface",0,0'

config custom-commands
	option description '切换为PCIE通信端口 > AT+QCFG="data_interface",1,0'
	option command 'AT+QCFG="data_interface",1,0'

config custom-commands
	option description '查看当前USB速率 > AT+QCFG="usbspeed"'
	option command 'AT+QCFG="usbspeed"'

config custom-commands
	option description '切换为USB2.0 > AT+QCFG="usbspeed","20"'
	option command 'AT+QCFG="usbspeed","20"'

config custom-commands
	option description '切换为USB3.1 Gen1（5Gbps） > AT+QCFG="usbspeed","311"'
	option command 'AT+QCFG="usbspeed","311"'

config custom-commands
	option description '切换为USB3.1 Gen1（10Gbps） > AT+QCFG="usbspeed","312"'
	option command 'AT+QCFG="usbspeed","312"'

config custom-commands
	option description '重置模组 > AT+QCFG="ResetFactory"'
	option command 'AT+QCFG="ResetFactory"'

config custom-commands
	option description '****************广和通****************'
	option command 'ATI'

config custom-commands
	option description '设置当前使用的为卡1 > AT+GTDUALSIM=0'
	option command 'AT+GTDUALSIM=0'

config custom-commands
	option description '设置当前使用的为卡2 > AT+GTDUALSIM=1'
	option command 'AT+GTDUALSIM=1'

config custom-commands
	option description 'ECM手动拨号 > AT+GTRNDIS=1,1'
	option command 'AT+GTRNDIS=1,1'

config custom-commands
	option description 'ECM拨号断开 > AT+GTRNDIS=0,1'
	option command 'AT+GTRNDIS=0,1'

config custom-commands
	option description '查询当前端口模式 > AT+GTUSBMODE?'
	option command 'AT+GTUSBMODE?'

config custom-commands
	option description 'QMI/GobiNet拨号 > AT+GTUSBMODE=32'
	option command 'AT+GTUSBMODE=32'

config custom-commands
	option description 'ECM拨号 > AT+GTUSBMODE=18'
	option command 'AT+GTUSBMODE=18'

config custom-commands
	option description 'MBIM拨号 > AT+GTUSBMODE=30'
	option command 'AT+GTUSBMODE=30'

config custom-commands
	option description 'RNDIS拨号 > AT+GTUSBMODE=24'
	option command 'AT+GTUSBMODE=24'

config custom-commands
	option description 'NCM拨号 > AT+GTUSBMODE=18'
	option command 'AT+GTUSBMODE=18'

config custom-commands
	option description '锁4G > AT+GTACT=2'
	option command 'AT+GTACT=2'

config custom-commands
	option description '锁5G > AT+GTACT=14'
	option command 'AT+GTACT=14'

config custom-commands
	option description '恢复自动搜索网络 > AT+GTACT=20'
	option command 'AT+GTACT=20'

config custom-commands
	option description '查询当前连接的网络类型 > AT+PSRAT?'
	option command 'AT+PSRAT?'

config custom-commands
	option description '查询模组IMEI > AT+GTSN=0,7'
	option command 'AT+GTSN=0,7'

config custom-commands
	option description '更改模组IMEI > AT+GTSN=1,7,"IMEI"'
	option command 'AT+GTSN=1,7,"在此设置IMEI"'

config custom-commands
	option description '报告一次当前BBIC的温度 > AT+MTSM=1,6'
	option command 'AT+MTSM=1,6'

config custom-commands
	option description '报告一次当前射频的温度 > AT+MTSM=1,7'
	option command 'AT+MTSM=1,7'

config custom-commands
	option description '获取当前温度 > AT+GTLADC'
	option command 'AT+GTLADC'

config custom-commands
	option description '重启模组 > AT+CFUN=15'
	option command 'AT+CFUN=15'

config custom-commands
	option description '****************美格****************'
	option command 'ATI'

config custom-commands
	option description 'SIM卡状态上报 > AT^SIMSLOTURC=1'
	option command 'AT^SIMSLOTURC=1'

config custom-commands
	option description '获取SIM卡卡槽状态 > AT^SIMSLOT?'
	option command 'AT^SIMSLOT?'

config custom-commands
	option description '设置当前使用的为卡1 > AT^SIMSLOT=1'
	option command 'AT^SIMSLOT=1'

config custom-commands
	option description '设置当前使用的为卡2 > AT^SIMSLOT=2'
	option command 'AT^SIMSLOT=2'

config custom-commands
	option description '查询网络信息 > AT^SYSINFOEX'
	option command 'AT^SYSINFOEX'

config custom-commands
	option description '查询载波聚合小区信息 > AT^CELLINFO=3'
	option command 'AT^CELLINFO=3'

config custom-commands
	option description '查询当前拨号模式 > AT+SER?'
	option command 'AT+SER?'

config custom-commands
	option description 'QMI/GobiNet拨号 > AT+SER=1,1'
	option command 'AT+SER=1,1'

config custom-commands
	option description 'ECM拨号 > AT+SER=2,1'
	option command 'AT+SER=2,1'

config custom-commands
	option description 'MBIM拨号 > AT+SER=3,1'
	option command 'AT+SER=3,1'

config custom-commands
	option description 'RNDIS拨号 > AT+SER=3,1'
	option command 'AT+SER=3,1'

config custom-commands
	option description 'NCM拨号 > AT+SER=2,1'
	option command 'AT+SER=2,1'

config custom-commands
	option description '锁4G > AT^SYSCFGEX="03",all,0,2,all,all,all,all,1'
	option command 'AT^SYSCFGEX="03",all,0,2,all,all,all,all,1'

config custom-commands
	option description '锁5G > AT^SYSCFGEX="04",all,0,2,all,all,all,all,1'
	option command 'AT^SYSCFGEX="04",all,0,2,all,all,all,all,1'

config custom-commands
	option description '恢复自动搜索网络 > AT^SYSCFGEX="00",all,0,2,all,all,all,all,1'
	option command 'AT^SYSCFGEX="00",all,0,2,all,all,all,all,1'

config custom-commands
	option description '查询模组IMEI > AT+LCTSN=0,7'
	option command 'AT+LCTSN=0,7'

config custom-commands
	option description '更改模组IMEI > AT+LCTSN=1,7,"IMEI"'
	option command 'AT+LCTSN=1,7,"在此设置IMEI"'

config custom-commands
	option description '获取模组温度 > AT+TEMP'
	option command 'AT+TEMP'

config custom-commands
	option description '重启模组 > AT+RESET'
	option command 'AT+RESET'

config custom-commands
	option description '****************华为****************'
	option command 'ATI'

config custom-commands
	option description '获取SIM卡卡槽状态 > AT^SIMSLOT?'
	option command 'AT^SIMSLOT?'

config custom-commands
	option description '设置当前使用的为卡1 > AT^SIMSWITCH=1'
	option command 'AT^SIMSWITCH=1'

config custom-commands
	option description '设置当前使用的为卡2 > AT^SIMSWITCH=0'
	option command 'AT^SIMSWITCH=0'

config custom-commands
	option description '查询网络信息 > AT^SYSINFOEX'
	option command 'AT^SYSINFOEX'

config custom-commands
	option description '查询当前拨号模式 > AT^SETMODE?'
	option command 'AT^SETMODE?'

config custom-commands
	option description 'ECM拨号模式（Linux） > AT^SETMODE=0'
	option command 'AT^SETMODE=0'

config custom-commands
	option description 'NCM拨号模式（Windows） > AT^SETMODE=1'
	option command 'AT^SETMODE=1'

config custom-commands
	option description 'ECM拨号模式（Linux，Debug） > AT^SETMODE=2'
	option command 'AT^SETMODE=2'

config custom-commands
	option description 'NCM拨号模式（Windows,Debug） > AT^SETMODE=3'
	option command 'AT^SETMODE=3'

config custom-commands
	option description '锁4G > AT^SYSCFGEX="03",40000000,1,2,7FFFFFFFFFFFFFFF,,'
	option command 'AT^SYSCFGEX="03",40000000,1,2,7FFFFFFFFFFFFFFF,,'

config custom-commands
	option description '锁5G > AT^SYSCFGEX="08",40000000,1,2,7FFFFFFFFFFFFFFF,,'
	option command 'AT^SYSCFGEX="08",40000000,1,2,7FFFFFFFFFFFFFFF,,'

config custom-commands
	option description '恢复自动搜索网络 > AT^SYSCFGEX="00",3FFFFFFF,1,2,7FFFFFFFFFFFFFFF,,'
	option command 'AT^SYSCFGEX="00",3FFFFFFF,1,2,7FFFFFFFFFFFFFFF,,'

config custom-commands
	option description '获取模组温度 > AT^CHIPTEMP?'
	option command 'AT^CHIPTEMP?'

config custom-commands
	option description '重启模组 > AT^RESET'
	option command 'AT^RESET'

config custom-commands
	option description '****************鼎桥****************'
	option command 'ATI'

config custom-commands
	option description '获取SIM卡卡槽状态 > AT^HVSST?'
	option command 'AT^HVSST?'

config custom-commands
	option description '设置当前使用的为卡1 > AT^SCICHG=0,1'
	option command 'AT^SCICHG=0,1'

config custom-commands
	option description '设置当前使用的为卡2 > AT^SCICHG=1,0'
	option command 'AT^SCICHG=1,0'

config custom-commands
	option description '查询网络信息 > AT^SYSINFOEX'
	option command 'AT^SYSINFOEX'

config custom-commands
	option description '查询当前拨号模式 > AT^SETMODE?'
	option command 'AT^SETMODE?'

config custom-commands
	option description 'ECM拨号模式（Linux） > AT^SETMODE=0'
	option command 'AT^SETMODE=0'

config custom-commands
	option description 'NCM拨号模式（Windows） > AT^SETMODE=1'
	option command 'AT^SETMODE=1'

config custom-commands
	option description 'ECM拨号模式（Linux，Debug） > AT^SETMODE=2'
	option command 'AT^SETMODE=2'

config custom-commands
	option description 'NCM拨号模式（Windows,Debug） > AT^SETMODE=3'
	option command 'AT^SETMODE=3'

config custom-commands
	option description '锁4G > AT^SYSCFGEX="03",40000000,1,2,7FFFFFFFFFFFFFFF,,'
	option command 'AT^SYSCFGEX="03",40000000,1,2,7FFFFFFFFFFFFFFF,,'

config custom-commands
	option description '锁5G > AT^SYSCFGEX="08",40000000,1,2,7FFFFFFFFFFFFFFF,,'
	option command 'AT^SYSCFGEX="08",40000000,1,2,7FFFFFFFFFFFFFFF,,'

config custom-commands
	option description '恢复自动搜索网络 > AT^SYSCFGEX="080302",3FFFFFFF,1,2,7FFFFFFFFFFFFFFF,,'
	option command 'AT^SYSCFGEX="080302",3FFFFFFF,1,2,7FFFFFFFFFFFFFFF,,'

config custom-commands
	option description '获取模组温度 > AT^CHIPTEMP?'
	option command 'AT^CHIPTEMP?'

config custom-commands
	option description '重启模组 > AT^RESET'
	option command 'AT^RESET'