From f3f0945b19a90b194b2886a4fe5b092b4a3f7b3b Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.org>
Date: Mon, 24 Sep 2018 18:26:02 +0100
Subject: [PATCH] staging: vc04_services: Support sending data to MMAL
 ports

Add the ability to send data to ports. This only supports
zero copy mode as the required bulk transfer setup calls
are not done.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.org>
---
 .../vc04_services/vchiq-mmal/mmal-vchiq.c      | 18 +++++++++++++-----
 1 file changed, 13 insertions(+), 5 deletions(-)

--- a/drivers/staging/vc04_services/vchiq-mmal/mmal-vchiq.c
+++ b/drivers/staging/vc04_services/vchiq-mmal/mmal-vchiq.c
@@ -427,11 +427,19 @@ buffer_from_host(struct vchiq_mmal_insta
 	m.u.buffer_from_host.buffer_header.data =
 		(u32)(unsigned long)buf->buffer;
 	m.u.buffer_from_host.buffer_header.alloc_size = buf->buffer_size;
-	m.u.buffer_from_host.buffer_header.length = 0;	/* nothing used yet */
-	m.u.buffer_from_host.buffer_header.offset = 0;	/* no offset */
-	m.u.buffer_from_host.buffer_header.flags = 0;	/* no flags */
-	m.u.buffer_from_host.buffer_header.pts = MMAL_TIME_UNKNOWN;
-	m.u.buffer_from_host.buffer_header.dts = MMAL_TIME_UNKNOWN;
+	if (port->type == MMAL_PORT_TYPE_OUTPUT) {
+		m.u.buffer_from_host.buffer_header.length = 0;
+		m.u.buffer_from_host.buffer_header.offset = 0;
+		m.u.buffer_from_host.buffer_header.flags = 0;
+		m.u.buffer_from_host.buffer_header.pts = MMAL_TIME_UNKNOWN;
+		m.u.buffer_from_host.buffer_header.dts = MMAL_TIME_UNKNOWN;
+	} else {
+		m.u.buffer_from_host.buffer_header.length = buf->length;
+		m.u.buffer_from_host.buffer_header.offset = 0;
+		m.u.buffer_from_host.buffer_header.flags = buf->mmal_flags;
+		m.u.buffer_from_host.buffer_header.pts = buf->pts;
+		m.u.buffer_from_host.buffer_header.dts = buf->dts;
+	}
 
 	/* clear buffer type sepecific data */
 	memset(&m.u.buffer_from_host.buffer_header_type_specific, 0,
