From eae83133532e44adae2f632b2168119a4c7249a2 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Wed, 11 Mar 2020 12:07:57 +0000
Subject: [PATCH] overlays: imx219: Correct link frequency to match the
 upstream driver

The upstream driver is checking the link frequency parameter, and
the overlay had the wrong value.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 arch/arm/boot/dts/overlays/imx219-overlay.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/overlays/imx219-overlay.dts
+++ b/arch/arm/boot/dts/overlays/imx219-overlay.dts
@@ -40,7 +40,7 @@
 						data-lanes = <1 2>;
 						clock-noncontinuous;
 						link-frequencies =
-							/bits/ 64 <297000000>;
+							/bits/ 64 <456000000>;
 					};
 				};
 			};
