From 79d32025a54899fe7d82c88906c1e3ad911c498d Mon Sep 17 00:00:00 2001
From: Sandor Yu <Sandor.yu@nxp.com>
Date: Thu, 26 Sep 2019 15:46:43 +0800
Subject: [PATCH] drm: bridge: cdns dp: Remove link rate/lanes set by device
 tree

Get the link rate and lanes from sink device.
Remove user specific set by device tree.

Signed-off-by: Sandor Yu <Sandor.yu@nxp.com>
---
 drivers/gpu/drm/bridge/cadence/cdns-dp-core.c     | 56 ++++++-----------------
 drivers/gpu/drm/bridge/cadence/cdns-mhdp-common.c |  6 +--
 drivers/gpu/drm/rockchip/cdn-dp-core.c            | 27 ++++++-----
 drivers/gpu/drm/rockchip/cdn-dp-core.h            |  1 -
 include/drm/bridge/cdns-mhdp-common.h             |  6 +--
 5 files changed, 35 insertions(+), 61 deletions(-)

--- a/drivers/gpu/drm/bridge/cadence/cdns-dp-core.c
+++ b/drivers/gpu/drm/bridge/cadence/cdns-dp-core.c
@@ -111,10 +111,10 @@ static void dp_pixel_clk_reset(struct cd
 static void cdns_dp_mode_set(struct cdns_mhdp_device *mhdp,
 			const struct drm_display_mode *mode)
 {
-	struct drm_dp_link link;
 	u32 lane_mapping = mhdp->lane_mapping;
-	int ret;
+	struct drm_dp_link *link = &mhdp->dp.link;
 	char linkid[6];
+	int ret;
 
 	memcpy(&mhdp->mode, mode, sizeof(struct drm_display_mode));
 
@@ -125,8 +125,6 @@ static void cdns_dp_mode_set(struct cdns
 
 	cdns_mhdp_plat_call(mhdp, pclk_rate);
 
-	cdns_mhdp_plat_call(mhdp, phy_set);
-
 	ret = drm_dp_downstream_id(&mhdp->dp.aux, linkid);
 	if (ret < 0) {
 		DRM_INFO("Failed to Get DP link ID: %d\n", ret);
@@ -137,35 +135,28 @@ static void cdns_dp_mode_set(struct cdns
 		 linkid[5]);
 
 	/* Check dp link */
-	ret = drm_dp_link_probe(&mhdp->dp.aux, &link);
+	ret = drm_dp_link_probe(&mhdp->dp.aux, link);
 	if (ret < 0) {
 		DRM_INFO("Failed to probe DP link: %d\n", ret);
 		return;
 	}
-	DRM_INFO("DP revision: 0x%x\n", link.revision);
-	DRM_INFO("DP rate: %d Mbps\n", link.rate);
-	DRM_INFO("DP number of lanes: %d\n", link.num_lanes);
-	DRM_INFO("DP capabilities: 0x%lx\n", link.capabilities);
+	DRM_INFO("DP revision: 0x%x\n", link->revision);
+	DRM_INFO("DP rate: %d Mbps\n", link->rate);
+	DRM_INFO("DP number of lanes: %d\n", link->num_lanes);
+	DRM_INFO("DP capabilities: 0x%lx\n", link->capabilities);
+
+	/* check the max link rate */
+	if (link->rate > CDNS_DP_MAX_LINK_RATE)
+		link->rate = CDNS_DP_MAX_LINK_RATE;
 
-	drm_dp_link_power_up(&mhdp->dp.aux, &mhdp->dp.link);
+	drm_dp_link_power_up(&mhdp->dp.aux, link);
 	if (ret < 0) {
 		DRM_INFO("Failed to power DP link: %d\n", ret);
 		return;
 	}
 
-	/* always use the number of lanes from the display*/
-	mhdp->dp.link.num_lanes = link.num_lanes;
-
-	/* Use the lower link rate */
-	if (mhdp->dp.link_rate != 0) {
-		mhdp->dp.link.rate = min(mhdp->dp.link_rate, (u32)link.rate);
-		DRM_DEBUG("DP actual link rate:  0x%x\n", link.rate);
-	}
-
-	/* initialize phy if lanes or link rate differnt */
-	if (mhdp->dp.link.num_lanes != mhdp->dp.num_lanes ||
-			mhdp->dp.link.rate != mhdp->dp.link_rate)
-		cdns_mhdp_plat_call(mhdp, phy_set);
+	/* Initialize link rate/num_lanes as panel max link rate/max_num_lanes */
+	cdns_mhdp_plat_call(mhdp, phy_set);
 
 	/* Video off */
 	ret = cdns_mhdp_set_video_status(mhdp, CONTROL_VIDEO_IDLE);
@@ -178,7 +169,7 @@ static void cdns_dp_mode_set(struct cdns
 	cdns_mhdp_reg_write(mhdp, LANES_CONFIG, 0x00400000 | lane_mapping);
 
 	/* Set DP host capability */
-	ret = cdns_mhdp_set_host_cap(mhdp, mhdp->dp.link.num_lanes, false);
+	ret = cdns_mhdp_set_host_cap(mhdp, false);
 	if (ret) {
 		DRM_DEV_ERROR(mhdp->dev, "Failed to set host cap %d\n", ret);
 		return;
@@ -412,23 +403,6 @@ static void cdns_dp_parse_dt(struct cdns
 		dev_warn(mhdp->dev, "Failed to get lane_mapping - using default 0xc6\n");
 	}
 	dev_info(mhdp->dev, "lane-mapping 0x%02x\n", mhdp->lane_mapping);
-
-	ret = of_property_read_u32(of_node, "link-rate", &mhdp->dp.link_rate);
-	if (ret) {
-		mhdp->dp.link_rate = 162000 ;
-		dev_warn(mhdp->dev, "Failed to get link-rate, use default 1620MHz\n");
-	}
-	dev_info(mhdp->dev, "link-rate %d\n", mhdp->dp.link_rate);
-	
-	ret = of_property_read_u32(of_node, "num-lanes", &mhdp->dp.num_lanes);
-	if (ret) {
-		mhdp->dp.num_lanes = 4;
-		dev_warn(mhdp->dev, "Failed to get num_lanes - using default\n");
-	}
-	dev_info(mhdp->dev, "dp_num_lanes 0x%02x\n", mhdp->dp.num_lanes);
-
-	mhdp->dp.link.num_lanes = mhdp->dp.num_lanes;
-	mhdp->dp.link.rate= mhdp->dp.link_rate;
 }
 
 static int __cdns_dp_probe(struct platform_device *pdev,
--- a/drivers/gpu/drm/bridge/cadence/cdns-mhdp-common.c
+++ b/drivers/gpu/drm/bridge/cadence/cdns-mhdp-common.c
@@ -494,13 +494,13 @@ err_set_firmware_active:
 }
 EXPORT_SYMBOL(cdns_mhdp_set_firmware_active);
 
-int cdns_mhdp_set_host_cap(struct cdns_mhdp_device *mhdp, u8 lanes, bool flip)
+int cdns_mhdp_set_host_cap(struct cdns_mhdp_device *mhdp, bool flip)
 {
 	u8 msg[8];
 	int ret;
 
-	msg[0] = CDNS_DP_MAX_LINK_RATE;
-	msg[1] = lanes | SCRAMBLER_EN;
+	msg[0] = drm_dp_link_rate_to_bw_code(mhdp->dp.link.rate);
+	msg[1] = mhdp->dp.link.num_lanes | SCRAMBLER_EN;
 	msg[2] = VOLTAGE_LEVEL_2;
 	msg[3] = PRE_EMPHASIS_LEVEL_3;
 	msg[4] = PTS1 | PTS2 | PTS3 | PTS4;
--- a/drivers/gpu/drm/rockchip/cdn-dp-core.c
+++ b/drivers/gpu/drm/rockchip/cdn-dp-core.c
@@ -305,12 +305,10 @@ static int cdn_dp_connector_mode_valid(s
 	requested = mode->clock * bpc * 3 / 1000;
 
 	source_max = dp->lanes;
-	sink_max = drm_dp_max_lane_count(dp->dpcd);
+	sink_max = dp->mhdp.dp.link.num_lanes;
 	lanes = min(source_max, sink_max);
 
-	source_max = drm_dp_bw_code_to_link_rate(CDNS_DP_MAX_LINK_RATE);
-	sink_max = drm_dp_max_link_rate(dp->dpcd);
-	rate = min(source_max, sink_max);
+	rate = dp->mhdp.dp.link.rate;
 
 	actual = rate * lanes / 100;
 
@@ -365,21 +363,25 @@ static int cdn_dp_firmware_init(struct c
 
 static int cdn_dp_get_sink_capability(struct cdn_dp_device *dp)
 {
+	struct cdns_mhdp_device *mhdp = &dp->mhdp;
+	struct drm_dp_link *link = &mhdp->dp.link;
 	int ret;
 
 	if (!cdn_dp_check_sink_connection(dp))
 		return -ENODEV;
 
-	ret = cdns_mhdp_dpcd_read(&dp->mhdp, DP_DPCD_REV, dp->dpcd,
-				  DP_RECEIVER_CAP_SIZE);
+	ret = drm_dp_link_probe(&mhdp->dp.aux, link);
 	if (ret) {
-		DRM_DEV_ERROR(dp->mhdp.dev, "Failed to get caps %d\n", ret);
+		DRM_DEV_ERROR(mhdp->dev, "Failed to get caps %d\n", ret);
 		return ret;
 	}
 
+	if (link->rate > CDNS_DP_MAX_LINK_RATE)
+		link->rate = CDNS_DP_MAX_LINK_RATE;
+
 	kfree(dp->edid);
-	dp->edid = drm_do_get_edid(&dp->mhdp.connector.base,
-				   cdns_mhdp_get_edid_block, &dp->mhdp);
+	dp->edid = drm_do_get_edid(&mhdp->connector.base,
+				   cdns_mhdp_get_edid_block, mhdp);
 	return 0;
 }
 
@@ -421,7 +423,8 @@ static int cdn_dp_enable_phy(struct cdn_
 	}
 
 	port->lanes = cdn_dp_get_port_lanes(port);
-	ret = cdns_mhdp_set_host_cap(&dp->mhdp, port->lanes, property.intval);
+	dp->mhdp.dp.link.num_lanes = port->lanes;
+	ret = cdns_mhdp_set_host_cap(&dp->mhdp, property.intval);
 	if (ret) {
 		DRM_DEV_ERROR(dev, "set host capabilities failed: %d\n",
 			      ret);
@@ -576,9 +579,9 @@ static bool cdn_dp_check_link_status(str
 {
 	u8 link_status[DP_LINK_STATUS_SIZE];
 	struct cdn_dp_port *port = cdn_dp_connected_port(dp);
-	u8 sink_lanes = drm_dp_max_lane_count(dp->dpcd);
+	u8 sink_lanes = dp->mhdp.dp.link.num_lanes;
 
-	if (!port || !dp->mhdp.dp.link.rate || !dp->mhdp.dp.link.num_lanes)
+	if (!port || !dp->mhdp.dp.link.rate || !sink_lanes)
 		return false;
 
 	if (cdns_mhdp_dpcd_read(&dp->mhdp, DP_LANE0_1_STATUS, link_status,
--- a/drivers/gpu/drm/rockchip/cdn-dp-core.h
+++ b/drivers/gpu/drm/rockchip/cdn-dp-core.h
@@ -61,7 +61,6 @@ struct cdn_dp_device {
 	u8 lanes;
 	int active_port;
 
-	u8 dpcd[DP_RECEIVER_CAP_SIZE];
 	bool sink_has_audio;
 };
 #endif  /* _CDN_DP_CORE_H */
--- a/include/drm/bridge/cdns-mhdp-common.h
+++ b/include/drm/bridge/cdns-mhdp-common.h
@@ -436,7 +436,7 @@
 #define HDCP_TX_IS_RECEIVER_ID_VALID_EVENT	BIT(7)
 
 #define TU_SIZE					30
-#define CDNS_DP_MAX_LINK_RATE			DP_LINK_BW_5_4
+#define CDNS_DP_MAX_LINK_RATE	540000
 
 #define F_HDMI_ENCODING(x) (((x) & ((1 << 2) - 1)) << 16)
 #define F_VIF_DATA_WIDTH(x) (((x) & ((1 << 2) - 1)) << 2)
@@ -697,8 +697,6 @@ struct cdns_mhdp_device {
 			struct cdns_mhdp_mst_cbs cbs;
 			bool is_mst;
 			bool can_mst;
-			u32 link_rate;
-			u32 num_lanes;
 		} dp;
 		struct _hdmi_data {
 #ifdef CONFIG_DRM_CDNS_HDMI_CEC
@@ -720,7 +718,7 @@ u32 cdns_mhdp_get_fw_clk(struct cdns_mhd
 int cdns_mhdp_load_firmware(struct cdns_mhdp_device *mhdp, const u32 *i_mem,
 			    u32 i_size, const u32 *d_mem, u32 d_size);
 int cdns_mhdp_set_firmware_active(struct cdns_mhdp_device *mhdp, bool enable);
-int cdns_mhdp_set_host_cap(struct cdns_mhdp_device *mhdp, u8 lanes, bool flip);
+int cdns_mhdp_set_host_cap(struct cdns_mhdp_device *mhdp, bool flip);
 int cdns_mhdp_event_config(struct cdns_mhdp_device *mhdp);
 u32 cdns_mhdp_get_event(struct cdns_mhdp_device *mhdp);
 int cdns_mhdp_get_hpd_status(struct cdns_mhdp_device *mhdp);
