From 4896c33bf9fe61ab62d5f6f93762d7c951a64a49 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Thu, 15 Aug 2019 12:02:34 +0100
Subject: [PATCH] configs: arm64/bcm2711: Enable V3D

Enable the V3D driver, which depends on BCM2835_POWER.

Originally submitted by GitHub user 'phire' in a slightly different
form.

See: https://github.com/raspberrypi/linux/pull/3063

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 drivers/gpu/drm/v3d/Kconfig          | 2 +-
 2 files changed, 2 insertions(+), 1 deletion(-)

--- a/drivers/gpu/drm/v3d/Kconfig
+++ b/drivers/gpu/drm/v3d/Kconfig
@@ -1,7 +1,7 @@
 # SPDX-License-Identifier: GPL-2.0-only
 config DRM_V3D
 	tristate "Broadcom V3D 3.x and newer"
-	depends on ARCH_BCM || ARCH_BCMSTB || COMPILE_TEST
+	depends on ARCH_BCM || ARCH_BCMSTB || ARCH_BCM2835 || COMPILE_TEST
 	depends on DRM
 	depends on COMMON_CLK
 	depends on MMU
