From b2e19dbff471eb6b9b39ff8f21c8d38e4fac8fe6 Mon Sep 17 00:00:00 2001
From: Stefan Wahren <wahrenst@gmx.net>
Date: Wed, 1 Jan 2020 15:01:34 +0100
Subject: [PATCH] Bluetooth: hci_bcm: Drive RTS only for BCM43438
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

commit e601daed271e9eb1b923972a0a1af65f8c7bb77b upstream.

The commit 3347a80965b3 ("Bluetooth: hci_bcm: Fix RTS handling during
startup") is causing at least a regression for AP6256 on Orange Pi 3.
So do the RTS line handing during startup only on the necessary platform.

Fixes: 3347a80965b3 ("Bluetooth: hci_bcm: Fix RTS handling during startup")
Reported-by: Ondřej Jirman <megous@megous.com>
Signed-off-by: Stefan Wahren <wahrenst@gmx.net>
Signed-off-by: Marcel Holtmann <marcel@holtmann.org>
---
 drivers/bluetooth/hci_bcm.c | 21 +++++++++++++++++----
 1 file changed, 17 insertions(+), 4 deletions(-)

--- a/drivers/bluetooth/hci_bcm.c
+++ b/drivers/bluetooth/hci_bcm.c
@@ -53,6 +53,7 @@
  */
 struct bcm_device_data {
 	bool	no_early_set_baudrate;
+	bool	drive_rts_on_open;
 };
 
 /**
@@ -123,6 +124,7 @@ struct bcm_device {
 	bool			is_suspended;
 #endif
 	bool			no_early_set_baudrate;
+	bool			drive_rts_on_open;
 	u8			pcm_int_params[5];
 };
 
@@ -459,7 +461,9 @@ static int bcm_open(struct hci_uart *hu)
 
 out:
 	if (bcm->dev) {
-		hci_uart_set_flow_control(hu, true);
+		if (bcm->dev->drive_rts_on_open)
+			hci_uart_set_flow_control(hu, true);
+
 		hu->init_speed = bcm->dev->init_speed;
 
 		/* If oper_speed is set, ldisc/serdev will set the baudrate
@@ -469,7 +473,10 @@ out:
 			hu->oper_speed = bcm->dev->oper_speed;
 
 		err = bcm_gpio_set_power(bcm->dev, true);
-		hci_uart_set_flow_control(hu, false);
+
+		if (bcm->dev->drive_rts_on_open)
+			hci_uart_set_flow_control(hu, false);
+
 		if (err)
 			goto err_unset_hu;
 	}
@@ -1450,8 +1457,10 @@ static int bcm_serdev_probe(struct serde
 		dev_err(&serdev->dev, "Failed to power down\n");
 
 	data = device_get_match_data(bcmdev->dev);
-	if (data)
+	if (data) {
 		bcmdev->no_early_set_baudrate = data->no_early_set_baudrate;
+		bcmdev->drive_rts_on_open = data->drive_rts_on_open;
+	}
 
 	return hci_uart_register_device(&bcmdev->serdev_hu, &bcm_proto);
 }
@@ -1468,11 +1477,15 @@ static struct bcm_device_data bcm4354_de
 	.no_early_set_baudrate = true,
 };
 
+static struct bcm_device_data bcm43438_device_data = {
+	.drive_rts_on_open = true,
+};
+
 static const struct of_device_id bcm_bluetooth_of_match[] = {
 	{ .compatible = "brcm,bcm20702a1" },
 	{ .compatible = "brcm,bcm4345c5" },
 	{ .compatible = "brcm,bcm4330-bt" },
-	{ .compatible = "brcm,bcm43438-bt" },
+	{ .compatible = "brcm,bcm43438-bt", .data = &bcm43438_device_data },
 	{ .compatible = "brcm,bcm43540-bt", .data = &bcm4354_device_data },
 	{ .compatible = "brcm,bcm4335a0" },
 	{ },
