From 9c08f4ff9f8f9e56011395dc064100ff6f139bdc Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Thu, 29 Oct 2020 14:10:56 +0000
Subject: [PATCH] phy: broadcom: Add bcm54213pe configuration

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 drivers/net/phy/broadcom.c | 9 +++++++++
 1 file changed, 9 insertions(+)

--- a/drivers/net/phy/broadcom.c
+++ b/drivers/net/phy/broadcom.c
@@ -43,6 +43,11 @@ static int bcm54210e_config_init(struct
 	return 0;
 }
 
+static int bcm54213pe_config_init(struct phy_device *phydev)
+{
+	return bcm54210e_config_init(phydev);
+}
+
 static int bcm54612e_config_init(struct phy_device *phydev)
 {
 	int reg;
@@ -304,6 +309,10 @@ static int bcm54xx_config_init(struct ph
 		err = bcm54210e_config_init(phydev);
 		if (err)
 			return err;
+	} else if (BRCM_PHY_MODEL(phydev) == PHY_ID_BCM54213PE) {
+		err = bcm54213pe_config_init(phydev);
+		if (err)
+			return err;
 	} else if (BRCM_PHY_MODEL(phydev) == PHY_ID_BCM54612E) {
 		err = bcm54612e_config_init(phydev);
 		if (err)
