#!/bin/sh

. /lib/functions.sh
. /lib/functions/uci-defaults.sh
. /lib/functions/system.sh

ramips_setup_rt3x5x_vlans()
{
	if [ ! -x /sbin/swconfig ]; then
		# legacy default
		ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		return
	fi
	local wanports=""
	local lanports=""
	for port in 5 4 3 2 1 0; do
		if [ `swconfig dev rt305x port $port get disable` = "1" ]; then
			continue
		fi
		if [ `swconfig dev rt305x port $port get lan` = "0" ]; then
			wanports="$port:wan $wanports"
		else
			lanports="$port:lan $lanports"
		fi
	done
	ucidef_add_switch "rt305x" $lanports $wanports "6t@eth0"
}

ramips_setup_interfaces()
{
	local board="$1"

	case $board in
	11acnas|\
	d-team,newifi-d2|\
	dir-615-h1|\
	w2914nsv2|\
	zbt-we2026)
		ucidef_add_switch "switch0" \
			"0:lan:4" "1:lan:3" "2:lan:2" "3:lan:1" "4:wan:5" "6@eth0"
		;;
	3g150b|\
	3g300m|\
	a5-v11|\
	all0256n-4M|\
	all0256n-8M|\
	all5002|\
	all5003|\
	bocco|\
	broadway|\
	dcs-930|\
	dcs-930l-b1|\
	ht-tm02|\
	kimax,u35wf|\
	linkits7688 | \
	m2m|\
	microwrt|\
	mikrotik,rbm11g|\
	mpr-a2|\
	ncs601w|\
	omega2 | \
	omega2p | \
	timecloud|\
	tplink,tl-wa801nd-v5|\
	w150m|\
	widora,neo-16m|\
	widora,neo-32m|\
	wnce2001|\
	zbt-cpe102|\
	zorlik,zl5900v2|\
	zte-q7)
		ucidef_add_switch "switch0"
		ucidef_add_switch_attr "switch0" "enable" "false"
		ucidef_set_interface_lan "eth0"
		;;
	mlw221|\
	mr-102n)
		ucidef_set_interface_lan "eth0.2"
		;;
	3g-6200n|\
	ai-br100|\
	alfa-network,ac1200rm|\
	mediatek,ap-mt7621a-v60|\
	xzwifi,creativebox-v1|\
	d240|\
	db-wrt01|\
	dir-300-b7|\
	dir-320-b1|\
	dir-610-a1|\
	dir-810l|\
	dlink,dwr-116-a1|\
	dlink,dwr-921-c1|\
	dlink,dwr-922-e2|\
	ew1200|\
	firewrt|\
	hc5661a|\
	hlk-rm04|\
	k2p|\
	kn|\
	kn_rc|\
	mac1200rv2|\
	miwifi-nano|\
	mt7621|\
	mt7628|\
	mtc,wr1201|\
	mzk-750dhp|\
	mzk-w300nh2|\
	nixcore-x1-8M|\
	nixcore-x1-16M|\
	oy-0001|\
	pbr-m1|\
	psg1208|\
	psg1218a|\
	rt-n12p|\
	sap-g3200u3|\
	sk-wb8|\
	telco-electronics,x1|\
	totolink,lr1200|\
	unielec,u7621-06-256m-16m|\
	unielec,u7621-06-512m-64m|\
	vr500|\
	wavlink,wl-wn570ha1|\
	wavlink,wl-wn575a3|\
	wf-2881|\
	whr-g300n|\
	mqmaker,witi-256m|\
	mqmaker,witi-512m|\
	youku-yk1|\
	youku,yk-l2|\
	zbt-ape522ii|\
	zbt-we1326|\
	zbtlink,zbt-we826-e|\
	zbtlink,zbt-we3526|\
	zbt-we826-16M|\
	zbt-we826-32M|\
	zbt-wg2626|\
	zbt-wg3526-16M|\
	zbt-wg3526-32M|\
	zbt-wr8305rt)
		ucidef_add_switch "switch0" \
			"0:lan" "1:lan" "2:lan" "3:lan" "4:wan" "6@eth0"
		;;
	gehua,ghl-r-001)
		ucidef_add_switch "switch0" \
			"0:lan" "1:lan" "2:lan" "4:wan" "6@eth0"
		;;
	alfa-network,awusfree1|\
	alfa-network,tube-e4g|\
	cs-qr10|\
	d105|\
	dlink,dap-1522-a1|\
	dch-m225|\
	ex2700|\
	ex3700|\
	hpm|\
	mzk-ex300np|\
	mzk-ex750np|\
	na930|\
	pbr-d1|\
	ravpower,wd03|\
	tama,w06|\
	tplink,tl-mr3020-v3|\
	tplink,tl-wr802n-v4|\
	u25awf-h1|\
	wli-tx4-ag300n|\
	wmdr-143n|\
	wmr-300|\
	wn3000rpv3|\
	wrh-300cr)
		ucidef_set_interface_lan "eth0"
		;;
	alfa-network,quad-e4g|\
	netgear,r6120|\
	r6220|\
	netgear,r6350|\
	wndr3700v5)
		ucidef_add_switch "switch0" \
			"0:lan:4" "1:lan:3" "2:lan:2" "3:lan:1" "4:wan" "6@eth0"
		;;
	alfa-network,r36m-e4g|\
	wcr-1166ds)
		ucidef_add_switch "switch0" \
			"3:lan" "4:wan" "6@eth0"
		;;
	dlink,dwr-118-a1)
		ucidef_add_switch "switch0" \
			"1:lan:2" "2:lan:3" "3:lan:1" "4:lan:0" "5:wan" "6@eth0"
		;;
	dlink,dwr-118-a2)
		ucidef_add_switch "switch0" \
			"1:lan:2" "2:lan:1" "3:lan:3" "4:lan" "0:wan" "6@eth0"
		;;
	psg1218b)
		ucidef_add_switch "switch0" \
			"0:lan:3" "1:lan:2" "2:lan:1" "3:wan" "6@eth0"
		;;
	whr-300hp2|\
	whr-600d|\
	wsr-1166|\
	wsr-600)
		ucidef_add_switch "switch0" \
			"0:lan:1" "1:lan:2" "2:lan:3" "3:lan:4" "4:wan:5" "6@eth0"
		;;
	ar670w|\
	ar725w|\
	rakwireless,rak633|\
	rt-ac51u)
		ucidef_add_switch "switch0" \
			"0:wan" "1:lan" "2:lan" "3:lan" "4:lan" "6t@eth0"
		;;
	belkin,f9k1109v1|\
	rt-n15|\
	wl-351)
		ucidef_add_switch "switch0" \
			"0:lan" "1:lan" "2:lan" "3:lan" "4:wan" "5@eth0"
		;;
	asl26555-8M|\
	asl26555-16M|\
	rp-n53)
		ucidef_add_switch "switch0" \
			"1:lan" "2:lan" "3:lan" "4:lan" "6t@eth0"
		;;
	asus,rt-ac57u|\
	atp-52b|\
	awm002-evb-4M|\
	awm002-evb-8M|\
	bdcom,wap2100-sk|\
	dir-645|\
	gl-mt300a|\
	gl-mt300n|\
	gl-mt750|\
	hilink,hlk-7628n|\
	hiwifi,hc5861b|\
	jhr-n805r|\
	jhr-n825r|\
	jhr-n926r|\
	mikrotik,rb750gr3|\
	mzk-wdpr|\
	rt-n14u|\
	skylab,skw92a|\
	tplink,c20-v4|\
	tplink,c50-v3|\
	tplink,c50-v4|\
	tplink,tl-mr3420-v5|\
	tplink,tl-wr842n-v5|\
	tl-wr840n-v4|\
	tl-wr840n-v5|\
	tl-wr841n-v13|\
	u7628-01-128M-16M|\
	ubnt-erx|\
	ubnt-erx-sfp|\
	ur-326n4g|\
	wrtnode|\
	wrtnode2p | \
	wrtnode2r | \
	youhua,wr1200js|\
	zbt-wa05|\
	zyxel,keenetic-extra-ii)
		ucidef_add_switch "switch0" \
			"1:lan" "2:lan" "3:lan" "4:lan" "0:wan" "6@eth0"
		;;
	mikrotik,rbm33g)
		ucidef_add_switch "switch0" \
			"1:lan" "2:lan" "0:wan" "6@eth0"
		;;
	c20i|\
	c50|\
	tplink,c20-v1)
		ucidef_add_switch "switch0" \
			"1:lan:3" "2:lan:4" "3:lan:1" "4:lan:2" "0:wan" "6@eth0"
		;;
	dir-860l-b1|\
	elecom,wrc-1167ghbk2-s|\
	elecom,wrc-2533gst|\
	elecom,wrc-1900gst|\
	hg255d|\
	iodata,wn-ax1167gr|\
	iodata,wn-gx300gr)
		ucidef_add_switch "switch0" \
			"1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1" "0:wan" "6@eth0"
		;;
	gnubee,gb-pc1|\
	gnubee,gb-pc2)
		ucidef_add_switch "switch0" \
			"0:lan" "4:lan" "6@eth0"
		;;
	gl-mt300n-v2)
		ucidef_add_switch "switch0" \
			"1:lan" "0:wan" "6@eth0"
		;;
	awapn2403)
		ucidef_add_switch "switch0" \
			"0:lan" "1:wan" "6@eth0"
		;;
	b2c|\
	nw718|\
	psr-680w|\
	sl-r7205|\
	ur-336un|\
	w502u|\
	wr6202)
		ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		;;
	br-6475nd)
		ucidef_add_switch "switch0" \
			"1:lan" "2:lan" "3:lan" "4:lan" "0:wan" "9@eth0"
		;;
	c108|\
	cf-wr800n)
		ucidef_add_switch "switch0" \
			"4:lan" "6t@eth0"
		;;
	cudy,wr1000)
		ucidef_add_switch "switch0" \
			"2:lan:2" "3:lan:1" "4:wan" "6@eth0"
		;;
	cy-swr1100)
		ucidef_add_switch "switch0" \
			"0:lan" "1:lan" "2:lan" "3:lan" "4:wan" "9@eth0"
		;;
	duzun-dm06)
		ucidef_add_switch "switch0" \
			"1:lan" "0:wan" "6@eth0"
		;;
	e1700|\
	mt7620a_mt7530)
		ucidef_add_switch "switch1" \
			"0:lan" "1:lan" "2:lan" "3:lan" "4:wan" "6@eth0"
		;;
	edimax,br-6478ac-v2|\
	tplink,c2-v1)
		ucidef_add_switch "switch1" \
			"1:lan" "2:lan" "3:lan" "4:lan" "0:wan" "6@eth0"
		;;
	hc5661|\
	head-weblink,hdrm200|\
	y1s)
		ucidef_add_switch "switch0" \
			"1:lan" "2:lan" "3:lan" "4:lan" "5:lan" "0:wan" "6@eth0"
		;;
	hc5861)
		ucidef_add_switch "switch0" \
			"0:lan" "1:lan" "5:wan" "6@eth0"
		;;
	hc5962)
		ucidef_add_switch "switch0" \
			"1:lan" "2:lan" "3:lan" "4:wan" "6@eth0"
		;;
	iodata,wn-ac1167gr|\
	iodata,wn-ac733gr3)
		ucidef_add_switch "switch1" \
			"1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1" "0:wan" "6@eth0"
		;;
	kn_rf)
		ucidef_add_switch "switch0" \
			"0:wan" "1:lan" "2:lan" "3:lan" "4:lan" "6@eth0"
		;;
	kng_rc)
		ucidef_add_switch "switch1" \
			"0:lan" "1:lan" "2:lan" "3:lan" "4:wan" "7t@eth0"
		;;
	miwifi-mini|\
	y1|\
	zbtlink,zbt-we1226)
		ucidef_add_switch "switch0" \
			"0:lan:2" "1:lan:1" "4:wan" "6@eth0"
		;;
	mlwg2|\
	wizard8800|\
	wl-330n)
		ucidef_set_interface_lan "eth0.1"
		;;
	mr200)
		ucidef_add_switch "switch0" \
			"0:lan" "1:lan" "2:lan" "3:lan" "6t@eth0"
		ucidef_set_interface_wan "usb0"
		;;
	hc5761)
		ucidef_add_switch "switch0" \
			"1:lan" "4:lan" "0:wan" "6@eth0"
		;;
	mzk-dp150n|\
	vocore-8M|\
	vocore-16M)
		ucidef_add_switch "switch0" \
			"0:lan" "4:lan" "6t@eth0"
		;;
	newifi-d1)
		ucidef_add_switch "switch0" \
		"1:lan:2" "2:lan:1" "4:wan" "6@eth0"
		;;
	phicomm,k2g)
		ucidef_add_switch "switch0" \
			"0:lan:4" "1:lan:3" "2:lan:2" "3:lan:1" "5:wan" "6@eth0"
		;;
	dlink,dir-510l|\
	glinet,vixmini|\
	netgear,ex6150|\
	re350-v1)
		ucidef_add_switch "switch0" \
			"0:lan" "6@eth0"
		;;
	re6500)
		ucidef_add_switch "switch0" \
			"0:lan:1" "1:lan:2" "2:lan:3" "3:lan:4" "6@eth0"
		;;
	rt-n56u)
		ucidef_add_switch "switch0" \
			"0:lan" "1:lan" "2:lan" "3:lan" "4:wan" "8@eth0"
		;;
	tew-638apb-v2)
		ucidef_add_switch "switch0" \
			"4:lan" "6@eth0"
		;;
	lava,lr-25g001|\
	tew-691gr|\
	tew-692gr|\
	wlr-6000)
		ucidef_add_switch "switch0" \
			"1:lan" "2:lan" "3:lan" "4:lan" "5:wan" "0@eth0"
		;;
	tplink,tl-wr902ac-v3)
		ucidef_add_switch "switch0" \
			"4:lan" "6@eth0"
		;;
	vonets,var11n-300|\
	wt1520-4M|\
	wt1520-8M)
		ucidef_add_switch "switch0" \
			"0:lan" "4:wan" "6@eth0"
		;;
	vocore2|\
	vocore2lite)
		ucidef_add_switch "switch0" \
			"0:lan" "2:lan" "6t@eth0"
		;;
	f5d8235-v1|\
	f5d8235-v2|\
	tew-714tru|\
	v11st-fe|\
	wzr-agl300nh)
		ucidef_add_switch "switch0" \
			"1:lan" "2:lan" "3:lan" "4:lan" "0:wan" "5@eth0"
		;;
	wcr-150gn|\
	we1026-5g-16m)
		ucidef_add_switch "switch0" \
			"0:lan" "6t@eth0"
		;;
	whr-1166d)
		ucidef_add_switch "switch0" \
			"0:lan" "1:lan" "2:lan" "3:lan" "5:wan" "6@eth0"
		;;
	wizfi630a)
		ucidef_add_switch "switch0" \
			"0:lan" "1:lan" "2:wan" "6@eth0"
		;;
	wiznet,wizfi630s)
		ucidef_add_switch "switch0" \
			"0:wan" "3:lan" "4:lan" "6@eth0"
		;;
	wt3020-4M|\
	wt3020-8M)
		ucidef_add_switch "switch0" \
			"4:lan" "0:wan" "6@eth0"
		;;
	xiaomi,mir3g)
		ucidef_add_switch "switch0" \
			"2:lan:2" "3:lan:1" "1:wan" "6t@eth0"
		;;
	xiaomi,mir3p)
		ucidef_add_switch "switch0" \
			"1:lan:3" "2:lan:2" "3:lan:1" "4:wan" "6@eth0"
		;;
	xiaomi,mir4a-100m)
		ucidef_add_switch "switch0" \
			"4:lan:1" "2:lan:2" "0:wan" "6@eth0"
		;;
	zyxel,keenetic-start)
		ucidef_add_switch "switch0" \
			"0:lan:3" "1:lan:2" "2:lan:1" "3:lan:0" "4:wan" "6@eth0"
		;;
	*)
		RT3X5X=`cat /proc/cpuinfo | egrep "(RT3.5|RT5350)"`
		if [ -n "${RT3X5X}" ]; then
			ramips_setup_rt3x5x_vlans
		else
			ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		fi
		;;
	esac
}

ramips_setup_macs()
{
	local board="$1"
	local lan_mac=""
	local wan_mac=""

	case $board in
	a5-v11|\
	ht-tm02|\
	wmdr-143n)
		lan_mac=$(cat /sys/class/net/eth0/address)
		;;
	asus,rt-ac57u|\
	vr500)
		lan_mac=$(mtd_get_mac_binary factory 57344)
		wan_mac=$(mtd_get_mac_binary factory 57350)
		;;
	alfa-network,quad-e4g|\
	elecom,wrc-1167ghbk2-s|\
	elecom,wrc-2533gst|\
	elecom,wrc-1900gst|\
	sk-wb8)
		wan_mac=$(mtd_get_mac_binary factory 57350)
		;;
	alfa-network,r36m-e4g|\
	carambola|\
	freestation5|\
	w502u|\
	wnce2001)
		wan_mac=$(mtd_get_mac_binary factory 46)
		;;
	bc2|\
	broadway|\
	d105|\
	dir-300-b7|\
	dir-320-b1|\
	dir-620-a1|\
	esr-9753|\
	hilink,hlk-7628n|\
	hlk-rm04|\
	mpr-a1|\
	psr-680w|\
	sl-r7205|\
	y1|\
	y1s)
		lan_mac=$(cat /sys/class/net/eth0/address)
		lan_mac=$(macaddr_setbit_la "$lan_mac")
		wan_mac=$(macaddr_add "$lan_mac" 1)
		;;
	belkin,f9k1109v1)
		wan_mac=$(mtd_get_mac_ascii uboot-env HW_WAN_MAC)
		lan_mac=$(mtd_get_mac_ascii uboot-env HW_LAN_MAC)
		;;
	br-6475nd)
		lan_mac=$(cat /sys/class/net/eth0/address)
		wan_mac=$(mtd_get_mac_binary devdata 7)
		;;
	cy-swr1100|\
	dir-645)
		lan_mac=$(mtd_get_mac_ascii nvram lanmac)
		wan_mac=$(mtd_get_mac_ascii nvram wanmac)
		;;
	dch-m225)
		lan_mac=$(mtd_get_mac_ascii factory lanmac)
		;;
	dir-860l-b1)
		lan_mac=$(mtd_get_mac_ascii factory lanmac)
		wan_mac=$(mtd_get_mac_ascii factory wanmac)
		;;
	dlink,dir-510l|\
	dlink,dwr-116-a1|\
	dlink,dwr-118-a1|\
	dlink,dwr-118-a2|\
	dlink,dwr-921-c1|\
	dlink,dwr-922-e2|\
	lava,lr-25g001)
		wan_mac=$(jboot_config_read -m -i $(find_mtd_part "config") -o 0xE000)
		lan_mac=$(macaddr_add "$wan_mac" 1)
		;;
	e1700)
		wan_mac=$(mtd_get_mac_ascii config WAN_MAC_ADDR)
		;;
	edimax,br-6478ac-v2|\
	netgear,r6350)
		lan_mac=$(cat /sys/class/net/eth0/address)
		wan_mac=$(macaddr_add "$lan_mac" 2)
		;;
	gl-mt300n-v2|\
	whr-g300n)
		wan_mac=$(mtd_get_mac_binary factory 4)
		;;
	hc5*61|\
	hc5661a|\
	hc5962|\
	hiwifi,hc5861b)
		lan_mac=`mtd_get_mac_ascii bdinfo "Vfac_mac "`
		[ -n "$lan_mac" ] || lan_mac=$(cat /sys/class/net/eth0/address)
		wan_mac=$(macaddr_add "$lan_mac" 1)
		;;
	iodata,wn-ac1167gr|\
	iodata,wn-ac733gr3)
		wan_mac=$(macaddr_add "$(mtd_get_mac_binary Factory 4)" -1)
		;;
	iodata,wn-ax1167gr|\
	iodata,wn-gx300gr)
		wan_mac=$(macaddr_add "$(mtd_get_mac_binary Factory 4)" 1)
		;;
	kn_rc|\
	kn_rf|\
	kng_rc)
		wan_mac=$(mtd_get_mac_binary factory 40)
		;;
	linkits7688)
		wan_mac=$(mtd_get_mac_binary factory 4)
		lan_mac=$(mtd_get_mac_binary factory 46)
		;;
	mac1200rv2)
		lan_mac=$(mtd_get_mac_binary factory_info 13)
		wan_mac=$(macaddr_add "$lan_mac" 1)
		;;
	miwifi-mini)
		wan_mac=$(cat /sys/class/net/eth0/address)
		lan_mac=$(macaddr_setbit_la "$wan_mac")
		;;
	m3|\
	m4-4M|\
	m4-8M|\
	x5|\
	x8)
		lan_mac=$(cat /sys/class/net/eth0/address)
		lan_mac=$(macaddr_add "$lan_mac" -2)
		;;
	newifi-d1)
		lan_mac=$(cat /sys/class/net/eth0/address)
		lan_mac=$(macaddr_add "$lan_mac" 2)
		;;
	omega2|\
	omega2p)
		wan_mac=$(mtd_get_mac_binary factory 4)
		lan_mac=$(mtd_get_mac_binary factory 46)
		;;
	oy-0001|\
	phicomm,k2g)
		lan_mac=$(mtd_get_mac_binary factory 40)
		wan_mac=$(mtd_get_mac_binary factory 46)
		;;
	rt-n56u)
		lan_mac=$(cat /sys/class/net/eth0/address)
		lan_mac=$(macaddr_setbit_la "$lan_mac")
		wan_mac=$(mtd_get_mac_binary factory 32772)
		;;
	skylab,skw92a)
		lan_mac=$(mtd_get_mac_binary factory 40)
		wan_mac=$(mtd_get_mac_binary factory 46)
		;;
	tew-691gr)
		wan_mac=$(macaddr_add "$(mtd_get_mac_binary factory 4)" 3)
		;;
	tew-692gr)
		wan_mac=$(macaddr_add "$(mtd_get_mac_binary factory 4)" 1)
		;;
	tiny-ac)
		lan_mac=$(mtd_get_mac_ascii u-boot-env LAN_MAC_ADDR)
		wan_mac=$(mtd_get_mac_ascii u-boot-env WAN_MAC_ADDR)
		;;
	w306r-v20)
		lan_mac=$(cat /sys/class/net/eth0/address)
		wan_mac=$(macaddr_add "$lan_mac" 5)
		;;
	wcr-1166ds|\
	wsr-1166)
		local index="$(find_mtd_index "board_data")"
		wan_mac="$(grep -m1 mac= "/dev/mtd${index}" | cut -d= -f2)"
		lan_mac=$wan_mac
		;;
	wcr-150gn)
		wan_mac=$(mtd_get_mac_binary factory 40)
		;;
	whr-1166d|\
	whr-300hp2|\
	whr-600d|\
	wsr-600)
		wan_mac=$(mtd_get_mac_binary factory 4)
		lan_mac=$wan_mac
		;;
	wizfi630a)
		lan_mac=$(mtd_get_mac_binary factory 4)
		wan_mac=$(mtd_get_mac_binary factory 40)
		;;
	wlr-6000)
		wan_mac=$(macaddr_add "$(mtd_get_mac_binary factory 32772)" 2)
		;;
	xiaomi,mir3g|\
	xiaomi,mir3p)
		lan_mac=$(mtd_get_mac_binary Factory 0xe006)
		;;
	zyxel,keenetic-start)
		wan_mac=$(mtd_get_mac_binary factory 40)
		;;
	*)
		lan_mac=$(cat /sys/class/net/eth0/address)
		wan_mac=$(macaddr_add "$lan_mac" 1)
		;;
	esac

	[ -n "$lan_mac" ] && ucidef_set_interface_macaddr "lan" $lan_mac
	[ -n "$wan_mac" ] && ucidef_set_interface_macaddr "wan" $wan_mac
}

board_config_update
board=$(board_name)
ramips_setup_interfaces $board
ramips_setup_macs $board
board_config_flush

exit 0
