From b5b405c12536e216476598de4ff56551bf56ad6e Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Tue, 17 Apr 2018 08:59:47 +0100
Subject: [PATCH 275/454] overlays: Fix typo in README

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/overlays/README | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -835,7 +835,7 @@ Params: addr                    Set the
                                 Valid addresses 0x76-0x77, default 0x76
 
         ds1621                  Select the Dallas Semiconductors DS1621 temp
-                                sensor. Valid addresses 0x48-9x4f, default 0x48
+                                sensor. Valid addresses 0x48-0x4f, default 0x48
 
         hdc100x                 Select the Texas Instruments HDC100x temp sensor
                                 Valid addresses 0x40-0x43, default 0x40
