From 0bd446083b4690dfadd835fab60f6eac4c308da1 Mon Sep 17 00:00:00 2001
From: Matt Flax <flatmax@flatmax.org>
Date: Thu, 30 Aug 2018 09:38:01 +1000
Subject: [PATCH 414/454] ASoC: cs4265: Add native 32bit I2S transport

commit be47e75eb1419ffc1d9c26230963fd5fa3055097 upstream.

The cs4265 uses 32 bit transport on the I2S bus. This patch enables native
32 bit mode for machine drivers which use this sound card driver.

Signed-off-by: Matt Flax <flatmax@flatmax.org>
Reviewed-by: Charles Keepax <ckeepax@opensource.cirrus.com>
Signed-off-by: Mark Brown <broonie@kernel.org>
---
 sound/soc/codecs/cs4265.c | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/sound/soc/codecs/cs4265.c
+++ b/sound/soc/codecs/cs4265.c
@@ -497,7 +497,8 @@ static int cs4265_set_bias_level(struct
 			SNDRV_PCM_RATE_176400 | SNDRV_PCM_RATE_192000)
 
 #define CS4265_FORMATS (SNDRV_PCM_FMTBIT_S16_LE | SNDRV_PCM_FMTBIT_U16_LE | \
-			SNDRV_PCM_FMTBIT_S24_LE | SNDRV_PCM_FMTBIT_U24_LE)
+			SNDRV_PCM_FMTBIT_S24_LE | SNDRV_PCM_FMTBIT_U24_LE | \
+			SNDRV_PCM_FMTBIT_S32_LE | SNDRV_PCM_FMTBIT_U32_LE)
 
 static const struct snd_soc_dai_ops cs4265_ops = {
 	.hw_params	= cs4265_pcm_hw_params,
