#include "qcom-ipq8064-v2.0.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "NEC Aterm WG2600HP";
	compatible = "nec,wg2600hp", "qcom,ipq8064";

	memory@0 {
		reg = <0x42000000 0x1e000000>;
		device_type = "memory";
	};

	reserved-memory {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		rsvd@41200000 {
			reg = <0x41200000 0x300000>;
			no-map;
		};
	};

	aliases {
		serial0 = &gsbi4_serial;
		mdio-gpio0 = &mdio0;

		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;
		led-upgrade = &power_green;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	soc {
		mdio0: mdio {
			compatible = "virtual,mdio-gpio";
			#address-cells = <1>;
			#size-cells = <0>;
			gpios = <&qcom_pinmux 1 GPIO_ACTIVE_HIGH &qcom_pinmux 0 GPIO_ACTIVE_HIGH>;
			pinctrl-0 = <&mdio0_pins>;
			pinctrl-names = "default";

			ethernet-phy@0 {
				reg = <0>;
				qca,ar8327-initvals = <
					0x00004 0x06000000  /* PAD0_MODE */
					0x0000c 0x00080080  /* PAD6_MODE */
					0x000e4 0x0006a545  /* MAC_POWER_SEL */
					0x000e0 0xc74164de  /* SGMII_CTRL */
					0x0007c 0x0000004e  /* PORT0_STATUS */
					0x00094 0x0000004e  /* PORT6_STATUS */
					>;
			};

			ethernet-phy@4 {
				reg = <4>;
			};
		};
	};

	keys {
		compatible = "gpio-keys";
		pinctrl-0 = <&button_pins>;
		pinctrl-names = "default";

		wps {
			label = "wps";
			gpios = <&qcom_pinmux 16 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		reset {
			label = "reset";
			gpios = <&qcom_pinmux 54 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		bridge {
			label = "bridge";
			gpios = <&qcom_pinmux 24 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
		};

		converter {
			label = "converter";
			gpios = <&qcom_pinmux 25 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-0 = <&led_pins>;
		pinctrl-names = "default";

		converter_green {
			label = "wg2600hp:green:converter";
			gpios = <&qcom_pinmux 6 GPIO_ACTIVE_HIGH>;
		};

		power_red: power_red {
			label = "wg2600hp:red:power";
			gpios = <&qcom_pinmux 7 GPIO_ACTIVE_HIGH>;
		};

		active_green {
			label = "wg2600hp:green:active";
			gpios = <&qcom_pinmux 8 GPIO_ACTIVE_HIGH>;
		};

		active_red {
			label = "wg2600hp:red:active";
			gpios = <&qcom_pinmux 9 GPIO_ACTIVE_HIGH>;
		};

		power_green: power_green {
			label = "wg2600hp:green:power";
			gpios = <&qcom_pinmux 14 GPIO_ACTIVE_HIGH>;
		};

		converter_red {
			label = "wg2600hp:red:converter";
			gpios = <&qcom_pinmux 15 GPIO_ACTIVE_HIGH>;
		};

		wlan2g_green {
			label = "wg2600hp:green:wlan2g";
			gpios = <&qcom_pinmux 55 GPIO_ACTIVE_HIGH>;
		};

		wlan2g_red {
			label = "wg2600hp:red:wlan2g";
			gpios = <&qcom_pinmux 56 GPIO_ACTIVE_HIGH>;
		};

		wlan5g_green {
			label = "wg2600hp:green:wlan5g";
			gpios = <&qcom_pinmux 57 GPIO_ACTIVE_HIGH>;
		};

		wlan5g_red {
			label = "wg2600hp:red:wlan5g";
			gpios = <&qcom_pinmux 58 GPIO_ACTIVE_HIGH>;
		};

		tv_green {
			label = "wg2600hp:green:tv";
			gpios = <&qcom_pinmux 64 GPIO_ACTIVE_HIGH>;
		};

		tv_red {
			label = "wg2600hp:red:tv";
			gpios = <&qcom_pinmux 65 GPIO_ACTIVE_HIGH>;
		};
	};
};

&adm_dma {
	status = "okay";
};

&gmac1 {
	status = "okay";

	phy-mode = "rgmii";
	qcom,id = <1>;

	pinctrl-0 = <&rgmii2_pins>;
	pinctrl-names = "default";

	mtd-mac-address = <&PRODUCTDATA 6>;

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gmac2 {
	status = "okay";

	phy-mode = "sgmii";
	qcom,id = <2>;

	mtd-mac-address = <&PRODUCTDATA 0>;

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gsbi4 {
	status = "okay";
	qcom,mode = <GSBI_PROT_I2C_UART>;
};

&gsbi4_serial {
	status = "okay";
};

&gsbi5 {
	status = "okay";

	qcom,mode = <GSBI_PROT_SPI>;

	spi@1a280000 {
		status = "okay";

		pinctrl-0 = <&spi_pins>;
		pinctrl-names = "default";

		cs-gpios = <&qcom_pinmux 20 GPIO_ACTIVE_HIGH>;

		flash@0 {
			compatible = "jedec,spi-nor";
			spi-max-frequency = <50000000>;
			reg = <0>;

			partitions {
				compatible = "fixed-partitions";
				#address-cells = <1>;
				#size-cells = <1>;

				SBL1@0 {
					label = "SBL1";
					reg = <0x0 0x20000>;
					read-only;
				};

				MIBIB@20000 {
					label = "MIBIB";
					reg = <0x20000 0x20000>;
					read-only;
				};

				SBL2@40000 {
					label = "SBL2";
					reg = <0x40000 0x40000>;
					read-only;
				};

				SBL3@80000 {
					label = "SBL3";
					reg = <0x80000 0x80000>;
					read-only;
				};

				DDRCONFIG@100000 {
					label = "DDRCONFIG";
					reg = <0x100000 0x10000>;
					read-only;
				};

				SSD@110000 {
					label = "SSD";
					reg = <0x110000 0x10000>;
					read-only;
				};

				TZ@120000 {
					label = "TZ";
					reg = <0x120000 0x80000>;
					read-only;
				};

				RPM@1a0000 {
					label = "RPM";
					reg = <0x1a0000 0x80000>;
					read-only;
				};

				APPSBL@220000 {
					label = "APPSBL";
					reg = <0x220000 0x80000>;
					read-only;
				};

				APPSBLENV@2a0000 {
					label = "APPSBLENV";
					reg = <0x2a0000 0x10000>;
				};

				PRODUCTDATA: PRODUCTDATA@2b0000 {
					label = "PRODUCTDATA";
					reg = <0x2b0000 0x30000>;
					read-only;
				};

				ART@2e0000 {
					label = "ART";
					reg = <0x2e0000 0x40000>;
					read-only;
				};

				TP@320000 {
					label = "TP";
					reg = <0x320000 0x40000>;
					read-only;
				};

				TINY@360000 {
					label = "TINY";
					reg = <0x360000 0x500000>;
					read-only;
				};

				firmware@860000 {
					compatible = "denx,uimage";
					label = "firmware";
					reg = <0x860000 0x17a0000>;
				};
			};
		};
	};
};

&hs_phy_0 {		/* USB3 port 0 HS phy */
	status = "okay";
};

&ss_phy_0 {		/* USB3 port 0 SS phy */
	status = "okay";
};

&hs_phy_1 {		/* USB3 port 1 HS phy */
	status = "okay";
};

&ss_phy_1 {		/* USB3 port 1 SS phy */
	status = "okay";
};

&usb3_0 {
	status = "okay";

	pinctrl-0 = <&usb_pwr_en_pins>;
	pinctrl-names = "default";
};

&usb3_1 {
	status = "okay";
};

&pcie0 {
	status = "okay";
};

&pcie1 {
	status = "okay";
	force_gen1 = <1>;
};

&qcom_pinmux {
	button_pins: button_pins {
		mux {
			pins = "gpio16", "gpio54", "gpio24", "gpio25";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	i2c4_pins: i2c4_pinmux {
		mux {
			pins = "gpio12", "gpio13";
			function = "gsbi4";
			drive-strength = <12>;
			bias-disable;
		};
	};

	led_pins: led_pins {
		mux {
			pins = "gpio6", "gpio7", "gpio8", "gpio9", "gpio14",
				"gpio15", "gpio55", "gpio56", "gpio57", "gpio58",
				"gpio64", "gpio65";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-down;
		};
	};

	spi_pins: spi_pins {
		mux {
			pins = "gpio18", "gpio19", "gpio21";
			function = "gsbi5";
			bias-pull-down;
		};

		data {
			pins = "gpio18", "gpio19";
			drive-strength = <10>;
		};

		cs {
			pins = "gpio20";
			drive-strength = <10>;
			bias-pull-up;
		};

		clk {
			pins = "gpio21";
			drive-strength = <12>;
		};
	};

	mdio0_pins: mdio0_pins {
		mux {
			pins = "gpio0", "gpio1";
			function = "gpio";
			drive-strength = <8>;
			bias-disable;
		};
	};

	rgmii2_pins: rgmii2_pins {
		mux {
			pins = "gpio27", "gpio28", "gpio29", "gpio30", "gpio31", "gpio32",
			       "gpio51", "gpio52", "gpio59", "gpio60", "gpio61", "gpio62" ;
			function = "rgmii2";
			drive-strength = <8>;
			bias-disable;
		};
	};

	usb_pwr_en_pins: usb_pwr_en_pins {
		mux {
			pins = "gpio22";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-down;
			output-high;
		};
	};
};
