--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -1037,6 +1037,7 @@ static const struct flash_info spi_nor_i
 	{ "mx25l12805d", INFO(0xc22018, 0, 64 * 1024, 256, 0) },
 	{ "mx25l12855e", INFO(0xc22618, 0, 64 * 1024, 256, 0) },
 	{ "mx25l25635e", INFO(0xc22019, 0, 64 * 1024, 512, SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ) },
+	{ "mx25l25635f", INFO(0xc22019, 0, 64 * 1024, 512, SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ | SPI_NOR_4B_OPCODES) },
 	{ "mx25u25635f", INFO(0xc22539, 0, 64 * 1024, 512, SECT_4K | SPI_NOR_4B_OPCODES) },
 	{ "mx25l25655e", INFO(0xc22619, 0, 64 * 1024, 512, 0) },
 	{ "mx66l51235l", INFO(0xc2201a, 0, 64 * 1024, 1024, SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ | SPI_NOR_4B_OPCODES) },
@@ -1206,11 +1207,12 @@ static const struct flash_info spi_nor_i
 	{ },
 };
 
-static const struct flash_info *spi_nor_read_id(struct spi_nor *nor)
+static const struct flash_info *spi_nor_read_id(struct spi_nor *nor,
+						const char *name)
 {
 	int			tmp;
 	u8			id[SPI_NOR_MAX_ID_LEN];
-	const struct flash_info	*info;
+	const struct flash_info	*info, *first_match = NULL;
 
 	tmp = nor->read_reg(nor, SPINOR_OP_RDID, id, SPI_NOR_MAX_ID_LEN);
 	if (tmp < 0) {
@@ -1221,10 +1223,16 @@ static const struct flash_info *spi_nor_
 	for (tmp = 0; tmp < ARRAY_SIZE(spi_nor_ids) - 1; tmp++) {
 		info = &spi_nor_ids[tmp];
 		if (info->id_len) {
-			if (!memcmp(info->id, id, info->id_len))
-				return &spi_nor_ids[tmp];
+			if (!memcmp(info->id, id, info->id_len)) {
+				if (!name || !strcmp(name, info->name))
+					return info;
+				if (!first_match)
+					first_match = info;
+			}
 		}
 	}
+	if (first_match)
+		return first_match;
 	dev_err(nor->dev, "unrecognized JEDEC id bytes: %02x, %02x, %02x\n",
 		id[0], id[1], id[2]);
 	return ERR_PTR(-ENODEV);
@@ -2684,7 +2692,7 @@ int spi_nor_scan(struct spi_nor *nor, co
 		info = spi_nor_match_id(name);
 	/* Try to auto-detect if chip name wasn't specified or not found */
 	if (!info)
-		info = spi_nor_read_id(nor);
+		info = spi_nor_read_id(nor, NULL);
 	if (IS_ERR_OR_NULL(info))
 		return -ENOENT;
 
@@ -2695,7 +2703,7 @@ int spi_nor_scan(struct spi_nor *nor, co
 	if (name && info->id_len) {
 		const struct flash_info *jinfo;
 
-		jinfo = spi_nor_read_id(nor);
+		jinfo = spi_nor_read_id(nor, name);
 		if (IS_ERR(jinfo)) {
 			return PTR_ERR(jinfo);
 		} else if (jinfo != info) {
