From 212b50d76ee63b58a59ccb687719583f72ea5e23 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.org>
Date: Thu, 10 May 2018 12:42:17 -0700
Subject: [PATCH 376/454] staging: bcm2835-camera: Fix indentation of tables

commit 6166045e7964067dba0da43a122de27ceb49be7b upstream

As requested by Mauro Carvalho Chehab in review.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.org>
Signed-off-by: Eric Anholt <eric@anholt.net>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 .../bcm2835-camera/bcm2835-camera.c           | 289 +++++++++---------
 1 file changed, 139 insertions(+), 150 deletions(-)

--- a/drivers/staging/vc04_services/bcm2835-camera/bcm2835-camera.c
+++ b/drivers/staging/vc04_services/bcm2835-camera/bcm2835-camera.c
@@ -81,145 +81,132 @@ static const struct v4l2_fract
 /* video formats */
 static struct mmal_fmt formats[] = {
 	{
-	 .name = "4:2:0, planar, YUV",
-	 .fourcc = V4L2_PIX_FMT_YUV420,
-	 .flags = 0,
-	 .mmal = MMAL_ENCODING_I420,
-	 .depth = 12,
-	 .mmal_component = MMAL_COMPONENT_CAMERA,
-	 .ybbp = 1,
-	 .remove_padding = 1,
-	 },
-	{
-	 .name = "4:2:2, packed, YUYV",
-	 .fourcc = V4L2_PIX_FMT_YUYV,
-	 .flags = 0,
-	 .mmal = MMAL_ENCODING_YUYV,
-	 .depth = 16,
-	 .mmal_component = MMAL_COMPONENT_CAMERA,
-	 .ybbp = 2,
-	 .remove_padding = 0,
-	 },
-	{
-	 .name = "RGB24 (LE)",
-	 .fourcc = V4L2_PIX_FMT_RGB24,
-	 .flags = 0,
-	 .mmal = MMAL_ENCODING_RGB24,
-	 .depth = 24,
-	 .mmal_component = MMAL_COMPONENT_CAMERA,
-	 .ybbp = 3,
-	 .remove_padding = 0,
-	 },
-	{
-	 .name = "JPEG",
-	 .fourcc = V4L2_PIX_FMT_JPEG,
-	 .flags = V4L2_FMT_FLAG_COMPRESSED,
-	 .mmal = MMAL_ENCODING_JPEG,
-	 .depth = 8,
-	 .mmal_component = MMAL_COMPONENT_IMAGE_ENCODE,
-	 .ybbp = 0,
-	 .remove_padding = 0,
-	 },
-	{
-	 .name = "H264",
-	 .fourcc = V4L2_PIX_FMT_H264,
-	 .flags = V4L2_FMT_FLAG_COMPRESSED,
-	 .mmal = MMAL_ENCODING_H264,
-	 .depth = 8,
-	 .mmal_component = MMAL_COMPONENT_VIDEO_ENCODE,
-	 .ybbp = 0,
-	 .remove_padding = 0,
-	 },
-	{
-	 .name = "MJPEG",
-	 .fourcc = V4L2_PIX_FMT_MJPEG,
-	 .flags = V4L2_FMT_FLAG_COMPRESSED,
-	 .mmal = MMAL_ENCODING_MJPEG,
-	 .depth = 8,
-	 .mmal_component = MMAL_COMPONENT_VIDEO_ENCODE,
-	 .ybbp = 0,
-	 .remove_padding = 0,
-	 },
-	{
-	 .name = "4:2:2, packed, YVYU",
-	 .fourcc = V4L2_PIX_FMT_YVYU,
-	 .flags = 0,
-	 .mmal = MMAL_ENCODING_YVYU,
-	 .depth = 16,
-	 .mmal_component = MMAL_COMPONENT_CAMERA,
-	 .ybbp = 2,
-	 .remove_padding = 0,
-	 },
-	{
-	 .name = "4:2:2, packed, VYUY",
-	 .fourcc = V4L2_PIX_FMT_VYUY,
-	 .flags = 0,
-	 .mmal = MMAL_ENCODING_VYUY,
-	 .depth = 16,
-	 .mmal_component = MMAL_COMPONENT_CAMERA,
-	 .ybbp = 2,
-	 .remove_padding = 0,
-	 },
-	{
-	 .name = "4:2:2, packed, UYVY",
-	 .fourcc = V4L2_PIX_FMT_UYVY,
-	 .flags = 0,
-	 .mmal = MMAL_ENCODING_UYVY,
-	 .depth = 16,
-	 .mmal_component = MMAL_COMPONENT_CAMERA,
-	 .ybbp = 2,
-	 .remove_padding = 0,
-	 },
-	{
-	 .name = "4:2:0, planar, NV12",
-	 .fourcc = V4L2_PIX_FMT_NV12,
-	 .flags = 0,
-	 .mmal = MMAL_ENCODING_NV12,
-	 .depth = 12,
-	 .mmal_component = MMAL_COMPONENT_CAMERA,
-	 .ybbp = 1,
-	 .remove_padding = 1,
-	 },
-	{
-	 .name = "RGB24 (BE)",
-	 .fourcc = V4L2_PIX_FMT_BGR24,
-	 .flags = 0,
-	 .mmal = MMAL_ENCODING_BGR24,
-	 .depth = 24,
-	 .mmal_component = MMAL_COMPONENT_CAMERA,
-	 .ybbp = 3,
-	 .remove_padding = 0,
-	 },
-	{
-	 .name = "4:2:0, planar, YVU",
-	 .fourcc = V4L2_PIX_FMT_YVU420,
-	 .flags = 0,
-	 .mmal = MMAL_ENCODING_YV12,
-	 .depth = 12,
-	 .mmal_component = MMAL_COMPONENT_CAMERA,
-	 .ybbp = 1,
-	 .remove_padding = 1,
-	 },
-	{
-	 .name = "4:2:0, planar, NV21",
-	 .fourcc = V4L2_PIX_FMT_NV21,
-	 .flags = 0,
-	 .mmal = MMAL_ENCODING_NV21,
-	 .depth = 12,
-	 .mmal_component = MMAL_COMPONENT_CAMERA,
-	 .ybbp = 1,
-	 .remove_padding = 1,
-	 },
-	{
-	 .name = "RGB32 (BE)",
-	 .fourcc = V4L2_PIX_FMT_BGR32,
-	 .flags = 0,
-	 .mmal = MMAL_ENCODING_BGRA,
-	 .depth = 32,
-	 .mmal_component = MMAL_COMPONENT_CAMERA,
-	 .ybbp = 4,
-	 .remove_padding = 0,
-	 },
+		.name = "4:2:0, planar, YUV",
+		.fourcc = V4L2_PIX_FMT_YUV420,
+		.flags = 0,
+		.mmal = MMAL_ENCODING_I420,
+		.depth = 12,
+		.mmal_component = MMAL_COMPONENT_CAMERA,
+		.ybbp = 1,
+		.remove_padding = 1,
+	}, {
+		.name = "4:2:2, packed, YUYV",
+		.fourcc = V4L2_PIX_FMT_YUYV,
+		.flags = 0,
+		.mmal = MMAL_ENCODING_YUYV,
+		.depth = 16,
+		.mmal_component = MMAL_COMPONENT_CAMERA,
+		.ybbp = 2,
+		.remove_padding = 0,
+	}, {
+		.name = "RGB24 (LE)",
+		.fourcc = V4L2_PIX_FMT_RGB24,
+		.flags = 0,
+		.mmal = MMAL_ENCODING_RGB24,
+		.depth = 24,
+		.mmal_component = MMAL_COMPONENT_CAMERA,
+		.ybbp = 3,
+		.remove_padding = 0,
+	}, {
+		.name = "JPEG",
+		.fourcc = V4L2_PIX_FMT_JPEG,
+		.flags = V4L2_FMT_FLAG_COMPRESSED,
+		.mmal = MMAL_ENCODING_JPEG,
+		.depth = 8,
+		.mmal_component = MMAL_COMPONENT_IMAGE_ENCODE,
+		.ybbp = 0,
+		.remove_padding = 0,
+	}, {
+		.name = "H264",
+		.fourcc = V4L2_PIX_FMT_H264,
+		.flags = V4L2_FMT_FLAG_COMPRESSED,
+		.mmal = MMAL_ENCODING_H264,
+		.depth = 8,
+		.mmal_component = MMAL_COMPONENT_VIDEO_ENCODE,
+		.ybbp = 0,
+		.remove_padding = 0,
+	}, {
+		.name = "MJPEG",
+		.fourcc = V4L2_PIX_FMT_MJPEG,
+		.flags = V4L2_FMT_FLAG_COMPRESSED,
+		.mmal = MMAL_ENCODING_MJPEG,
+		.depth = 8,
+		.mmal_component = MMAL_COMPONENT_VIDEO_ENCODE,
+		.ybbp = 0,
+		.remove_padding = 0,
+	}, {
+		.name = "4:2:2, packed, YVYU",
+		.fourcc = V4L2_PIX_FMT_YVYU,
+		.flags = 0,
+		.mmal = MMAL_ENCODING_YVYU,
+		.depth = 16,
+		.mmal_component = MMAL_COMPONENT_CAMERA,
+		.ybbp = 2,
+		.remove_padding = 0,
+	}, {
+		.name = "4:2:2, packed, VYUY",
+		.fourcc = V4L2_PIX_FMT_VYUY,
+		.flags = 0,
+		.mmal = MMAL_ENCODING_VYUY,
+		.depth = 16,
+		.mmal_component = MMAL_COMPONENT_CAMERA,
+		.ybbp = 2,
+		.remove_padding = 0,
+	}, {
+		.name = "4:2:2, packed, UYVY",
+		.fourcc = V4L2_PIX_FMT_UYVY,
+		.flags = 0,
+		.mmal = MMAL_ENCODING_UYVY,
+		.depth = 16,
+		.mmal_component = MMAL_COMPONENT_CAMERA,
+		.ybbp = 2,
+		.remove_padding = 0,
+	}, {
+		.name = "4:2:0, planar, NV12",
+		.fourcc = V4L2_PIX_FMT_NV12,
+		.flags = 0,
+		.mmal = MMAL_ENCODING_NV12,
+		.depth = 12,
+		.mmal_component = MMAL_COMPONENT_CAMERA,
+		.ybbp = 1,
+		.remove_padding = 1,
+	}, {
+		.name = "RGB24 (BE)",
+		.fourcc = V4L2_PIX_FMT_BGR24,
+		.flags = 0,
+		.mmal = MMAL_ENCODING_BGR24,
+		.depth = 24,
+		.mmal_component = MMAL_COMPONENT_CAMERA,
+		.ybbp = 3,
+		.remove_padding = 0,
+	}, {
+		.name = "4:2:0, planar, YVU",
+		.fourcc = V4L2_PIX_FMT_YVU420,
+		.flags = 0,
+		.mmal = MMAL_ENCODING_YV12,
+		.depth = 12,
+		.mmal_component = MMAL_COMPONENT_CAMERA,
+		.ybbp = 1,
+		.remove_padding = 1,
+	}, {
+		.name = "4:2:0, planar, NV21",
+		.fourcc = V4L2_PIX_FMT_NV21,
+		.flags = 0,
+		.mmal = MMAL_ENCODING_NV21,
+		.depth = 12,
+		.mmal_component = MMAL_COMPONENT_CAMERA,
+		.ybbp = 1,
+		.remove_padding = 1,
+	}, {
+		.name = "RGB32 (BE)",
+		.fourcc = V4L2_PIX_FMT_BGR32,
+		.flags = 0,
+		.mmal = MMAL_ENCODING_BGRA,
+		.depth = 32,
+		.mmal_component = MMAL_COMPONENT_CAMERA,
+		.ybbp = 4,
+		.remove_padding = 0,
+	},
 };
 
 static struct mmal_fmt *get_format(struct v4l2_format *f)
@@ -709,17 +696,19 @@ static int set_overlay_params(struct bm2
 			      struct vchiq_mmal_port *port)
 {
 	struct mmal_parameter_displayregion prev_config = {
-	.set = MMAL_DISPLAY_SET_LAYER | MMAL_DISPLAY_SET_ALPHA |
-	    MMAL_DISPLAY_SET_DEST_RECT | MMAL_DISPLAY_SET_FULLSCREEN,
-	.layer = PREVIEW_LAYER,
-	.alpha = dev->overlay.global_alpha,
-	.fullscreen = 0,
-	.dest_rect = {
-		      .x = dev->overlay.w.left,
-		      .y = dev->overlay.w.top,
-		      .width = dev->overlay.w.width,
-		      .height = dev->overlay.w.height,
-		      },
+		.set =	MMAL_DISPLAY_SET_LAYER |
+			MMAL_DISPLAY_SET_ALPHA |
+			MMAL_DISPLAY_SET_DEST_RECT |
+			MMAL_DISPLAY_SET_FULLSCREEN,
+		.layer = PREVIEW_LAYER,
+		.alpha = dev->overlay.global_alpha,
+		.fullscreen = 0,
+		.dest_rect = {
+			.x = dev->overlay.w.left,
+			.y = dev->overlay.w.top,
+			.width = dev->overlay.w.width,
+			.height = dev->overlay.w.height,
+		},
 	};
 	return vchiq_mmal_port_parameter_set(dev->instance, port,
 					     MMAL_PARAMETER_DISPLAYREGION,
