// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "ar7100.dtsi"

/ {
	compatible = "dlink,dir-825-b1", "qca,ar7161";
	model = "D-Link DIR825B1";

	aliases {
		led-boot = &orange_power;
		led-failsafe = &orange_power;
		led-running = &blue_power;
		led-upgrade = &orange_power;
	};

	extosc: ref {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-output-names = "ref";
		clock-frequency = <40000000>;
	};

	leds {
		compatible = "gpio-leds";
		blue_usb {
			label = "d-link:blue:usb";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
			trigger-sources = <&usb_ochi_port>, <&usb_echi_port>;
			linux,default-trigger = "usbport";
		};

		orange_power: orange_power {
			label = "d-link:orange:power";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		blue_power: blue_power {
			label = "d-link:blue:power";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};

		blue_wps {
			label = "d-link:blue:wps";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};

		orange_planet {
			label = "d-link:orange:planet";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};

		blue_planet {
			label = "d-link:blue:planet";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};
	};

	ath9k-leds {
		compatible = "gpio-leds";

		wlan2g {
			label = "d-link:blue:wlan2g";
			gpios = <&ath9k0 5 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wlan5g {
			label = "d-link:blue:wlan5g";
			gpios = <&ath9k1 5 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	rtl8366s {
		compatible = "realtek,rtl8366s";
		gpio-sda = <&gpio 5 GPIO_ACTIVE_HIGH>;
		gpio-sck = <&gpio 7 GPIO_ACTIVE_HIGH>;
		realtek,initvals = <0x06 0x0108>;

		mdio-bus {
			#address-cells = <1>;
			#size-cells = <0>;
			status = "okay";

			phy-mask = <0x10>;

			phy4: ethernet-phy@4 {
				reg = <4>;
				phy-mode = "rgmii";
			};
		};
	};
};


&usb1 {
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";

	usb_ochi_port: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};

&usb2 {
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";

	usb_echi_port: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};

&usb_phy {
	status = "okay";
};

&pcie0 {
	status = "okay";

	ath9k0: wifi@0,11 {
		compatible = "pci168c,0029";
		reg = <0x8800 0 0 0 0>;
		qca,no-eeprom;
		#gpio-cells = <2>;
		gpio-controller;
	};

	ath9k1: wifi@0,12 {
		compatible = "pci168c,0029";
		reg = <0x9000 0 0 0 0>;
		qca,no-eeprom;
		#gpio-cells = <2>;
		gpio-controller;
	};
};

&uart {
	status = "okay";
};

&pll {
	clocks = <&extosc>;
};

&spi {
	status = "okay";
	num-cs = <1>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "config";
				reg = <0x040000 0x010000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x050000 0x610000>;
			};

			caldata: partition@60000 {
				label = "caldata";
				reg = <0x660000 0x010000>;
				read-only;
			};

			partition@670000 {
				label = "unknown";
				reg = <0x670000 0x190000>;
				read-only;
			};
		};
	};
};


&eth0 {
	status = "okay";
	pll-data = <0x11110000 0x00001099 0x00991099>;

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&eth1 {
	status = "okay";
	pll-data = <0x11110000 0x00001099 0x00991099>;

	phy-handle = <&phy4>;
};
