From dd62aee5d2d24199e71e745544e49a1a8b3c6f7a Mon Sep 17 00:00:00 2001
From: Linus Walleij <linus.walleij@linaro.org>
Date: Fri, 21 Apr 2017 20:50:22 +0200
Subject: [PATCH 31/31] ARM: dts: Add the FOTG210 USB host to Gemini

This adds the FOTG210 USB host controller to the Gemini
device trees. In the main SoC DTSI it is flagged as disabled
and then it is selectively enabled on the devices that utilize
it (these per-platform enablements are done on the out-of-tree
OpenWrt patch set). It is not enabled on the Itian SquareOne
NAS/router since this instead has a VIA host controller
soldered on the PCI port, and can gate off these USB host
controllers.

Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
---
USB maintainers: I will merge this through the ARM SoC tree,
the patch is only included in the series for context.
---
 arch/arm/boot/dts/gemini-dlink-dir-685.dts |  8 ++++++++
 arch/arm/boot/dts/gemini-nas4220b.dts      |  8 ++++++++
 arch/arm/boot/dts/gemini-wbd111.dts        | 20 ++++++++++++++++++++
 arch/arm/boot/dts/gemini-wbd222.dts        | 21 +++++++++++++++++++++
 arch/arm/boot/dts/gemini.dtsi              | 26 ++++++++++++++++++++++++++
 6 files changed, 103 insertions(+)

--- a/arch/arm/boot/dts/gemini-dlink-dir-685.dts
+++ b/arch/arm/boot/dts/gemini-dlink-dir-685.dts
@@ -299,5 +299,13 @@
 				};
 			};
 		};
+
+		usb@68000000 {
+			status = "okay";
+		};
+
+		usb@69000000 {
+			status = "okay";
+		};
 	};
 };
--- a/arch/arm/boot/dts/gemini-nas4220b.dts
+++ b/arch/arm/boot/dts/gemini-nas4220b.dts
@@ -146,5 +146,13 @@
 		ata@63000000 {
 			status = "okay";
 		};
+
+		usb@68000000 {
+			status = "okay";
+		};
+
+		usb@69000000 {
+			status = "okay";
+		};
 	};
 };
--- a/arch/arm/boot/dts/gemini-wbd111.dts
+++ b/arch/arm/boot/dts/gemini-wbd111.dts
@@ -160,5 +160,25 @@
 				<0x6000 0 0 3 &pci_intc 1>,
 				<0x6000 0 0 4 &pci_intc 2>;
 		};
+
+		ethernet@60000000 {
+			status = "okay";
+
+			ethernet-port@0 {
+				phy-mode = "rgmii";
+				phy-handle = <&phy0>;
+			};
+			ethernet-port@1 {
+				/* Not used in this platform */
+			};
+		};
+
+		usb@68000000 {
+			status = "okay";
+		};
+
+		usb@69000000 {
+			status = "okay";
+		};
 	};
 };
--- a/arch/arm/boot/dts/gemini-wbd222.dts
+++ b/arch/arm/boot/dts/gemini-wbd222.dts
@@ -165,5 +165,26 @@
 				<0x6000 0 0 3 &pci_intc 1>,
 				<0x6000 0 0 4 &pci_intc 2>;
 		};
+
+		ethernet@60000000 {
+			status = "okay";
+
+			ethernet-port@0 {
+				phy-mode = "rgmii";
+				phy-handle = <&phy0>;
+			};
+			ethernet-port@1 {
+				phy-mode = "rgmii";
+				phy-handle = <&phy1>;
+			};
+		};
+
+		usb@68000000 {
+			status = "okay";
+		};
+
+		usb@69000000 {
+			status = "okay";
+		};
 	};
 };
--- a/arch/arm/boot/dts/gemini.dtsi
+++ b/arch/arm/boot/dts/gemini.dtsi
@@ -411,5 +411,31 @@
 			#size-cells = <0>;
 			status = "disabled";
 		};
+
+		usb@68000000 {
+			compatible = "cortina,gemini-usb", "faraday,fotg210";
+			reg = <0x68000000 0x1000>;
+			interrupts = <10 IRQ_TYPE_LEVEL_HIGH>;
+			resets = <&syscon GEMINI_RESET_USB0>;
+			clocks = <&syscon GEMINI_CLK_GATE_USB0>;
+			clock-names = "PCLK";
+			pinctrl-names = "default";
+			pinctrl-0 = <&usb_default_pins>;
+			syscon = <&syscon>;
+			status = "disabled";
+		};
+
+		usb@69000000 {
+			compatible = "cortina,gemini-usb", "faraday,fotg210";
+			reg = <0x69000000 0x1000>;
+			interrupts = <11 IRQ_TYPE_LEVEL_HIGH>;
+			resets = <&syscon GEMINI_RESET_USB1>;
+			clocks = <&syscon GEMINI_CLK_GATE_USB1>;
+			clock-names = "PCLK";
+			pinctrl-names = "default";
+			pinctrl-0 = <&usb_default_pins>;
+			syscon = <&syscon>;
+			status = "disabled";
+		};
 	};
 };
