From 8c8e60fb86a90a30721bbd797f58f96b3980dcc1 Mon Sep 17 00:00:00 2001
From: Jean-Philippe Brucker <jean-philippe@linaro.org>
Date: Thu, 26 Dec 2019 10:20:33 +0100
Subject: [PATCH] brcmfmac: sdio: Fix OOB interrupt initialization on brcm43362

Commit 262f2b53f679 ("brcmfmac: call brcmf_attach() just before calling
brcmf_bus_started()") changed the initialization order of the brcmfmac
SDIO driver. Unfortunately since brcmf_sdiod_intr_register() is now
called before the sdiodev->bus_if initialization, it reads the wrong
chip ID and fails to initialize the GPIO on brcm43362. Thus the chip
cannot send interrupts and fails to probe:

[   12.517023] brcmfmac: brcmf_sdio_bus_rxctl: resumed on timeout
[   12.531214] ieee80211 phy0: brcmf_bus_started: failed: -110
[   12.536976] ieee80211 phy0: brcmf_attach: dongle is not responding: err=-110
[   12.566467] brcmfmac: brcmf_sdio_firmware_callback: brcmf_attach failed

Initialize the bus interface earlier to ensure that
brcmf_sdiod_intr_register() properly sets up the OOB interrupt.

BugLink: https://bugs.debian.org/cgi-bin/bugreport.cgi?bug=908438
Fixes: 262f2b53f679 ("brcmfmac: call brcmf_attach() just before calling brcmf_bus_started()")
Signed-off-by: Jean-Philippe Brucker <jean-philippe@linaro.org>
Reviewed-by: Arend van Spriel <arend.vanspriel@broadcom.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 .../net/wireless/broadcom/brcm80211/brcmfmac/sdio.c  | 12 ++++++------
 1 file changed, 6 insertions(+), 6 deletions(-)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
@@ -4249,6 +4249,12 @@ static void brcmf_sdio_firmware_callback
 	}
 
 	if (err == 0) {
+		/* Assign bus interface call back */
+		sdiod->bus_if->dev = sdiod->dev;
+		sdiod->bus_if->ops = &brcmf_sdio_bus_ops;
+		sdiod->bus_if->chip = bus->ci->chip;
+		sdiod->bus_if->chiprev = bus->ci->chiprev;
+
 		/* Allow full data communication using DPC from now on. */
 		brcmf_sdiod_change_state(bus->sdiodev, BRCMF_SDIOD_DATA);
 
@@ -4265,12 +4271,6 @@ static void brcmf_sdio_firmware_callback
 
 	sdio_release_host(sdiod->func1);
 
-	/* Assign bus interface call back */
-	sdiod->bus_if->dev = sdiod->dev;
-	sdiod->bus_if->ops = &brcmf_sdio_bus_ops;
-	sdiod->bus_if->chip = bus->ci->chip;
-	sdiod->bus_if->chiprev = bus->ci->chiprev;
-
 	err = brcmf_alloc(sdiod->dev, sdiod->settings);
 	if (err) {
 		brcmf_err("brcmf_alloc failed\n");
