From 0a9850b65c2ad0183684790cb6fefb2f59eca573 Mon Sep 17 00:00:00 2001
From: Gordon Hollingworth <gordon@raspberrypi.org>
Date: Tue, 12 May 2015 14:47:56 +0100
Subject: [PATCH 060/454] rpi-ft5406: Add touchscreen driver for pi LCD display

Fix driver detection failure Check that the buffer response is non-zero meaning the touchscreen was detected

rpi-ft5406: Use firmware API

RPI-FT5406: Enable aarch64 support through explicit iomem interface

Signed-off-by: Gerhard de Clercq <gerharddeclercq@outlook.com>
---
 drivers/input/touchscreen/Kconfig      |   7 +
 drivers/input/touchscreen/Makefile     |   1 +
 drivers/input/touchscreen/rpi-ft5406.c | 292 +++++++++++++++++++++++++
 3 files changed, 300 insertions(+)
 create mode 100644 drivers/input/touchscreen/rpi-ft5406.c

--- a/drivers/input/touchscreen/Kconfig
+++ b/drivers/input/touchscreen/Kconfig
@@ -628,6 +628,13 @@ config TOUCHSCREEN_EDT_FT5X06
 	  To compile this driver as a module, choose M here: the
 	  module will be called edt-ft5x06.
 
+config TOUCHSCREEN_RPI_FT5406
+	tristate "Raspberry Pi FT5406 driver"
+	depends on RASPBERRYPI_FIRMWARE
+	help
+	  Say Y here to enable the Raspberry Pi memory based FT5406 device
+
+
 config TOUCHSCREEN_MIGOR
 	tristate "Renesas MIGO-R touchscreen"
 	depends on (SH_MIGOR || COMPILE_TEST) && I2C
--- a/drivers/input/touchscreen/Makefile
+++ b/drivers/input/touchscreen/Makefile
@@ -30,6 +30,7 @@ obj-$(CONFIG_TOUCHSCREEN_DA9034)	+= da90
 obj-$(CONFIG_TOUCHSCREEN_DA9052)	+= da9052_tsi.o
 obj-$(CONFIG_TOUCHSCREEN_DYNAPRO)	+= dynapro.o
 obj-$(CONFIG_TOUCHSCREEN_EDT_FT5X06)	+= edt-ft5x06.o
+obj-$(CONFIG_TOUCHSCREEN_RPI_FT5406)	+= rpi-ft5406.o
 obj-$(CONFIG_TOUCHSCREEN_HAMPSHIRE)	+= hampshire.o
 obj-$(CONFIG_TOUCHSCREEN_GUNZE)		+= gunze.o
 obj-$(CONFIG_TOUCHSCREEN_EETI)		+= eeti_ts.o
--- /dev/null
+++ b/drivers/input/touchscreen/rpi-ft5406.c
@@ -0,0 +1,292 @@
+/*
+ * Driver for memory based ft5406 touchscreen
+ *
+ * Copyright (C) 2015 Raspberry Pi
+ *
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+
+#include <linux/module.h>
+#include <linux/interrupt.h>
+#include <linux/input.h>
+#include <linux/irq.h>
+#include <linux/delay.h>
+#include <linux/slab.h>
+#include <linux/bitops.h>
+#include <linux/input/mt.h>
+#include <linux/kthread.h>
+#include <linux/platform_device.h>
+#include <linux/stddef.h>
+#include <asm/io.h>
+#include <linux/dma-mapping.h>
+#include <soc/bcm2835/raspberrypi-firmware.h>
+
+#define MAXIMUM_SUPPORTED_POINTS 10
+struct ft5406_regs {
+	uint8_t device_mode;
+	uint8_t gesture_id;
+	uint8_t num_points;
+	struct ft5406_touch {
+		uint8_t xh;
+		uint8_t xl;
+		uint8_t yh;
+		uint8_t yl;
+		uint8_t res1;
+		uint8_t res2;
+	} point[MAXIMUM_SUPPORTED_POINTS];
+};
+
+#define SCREEN_WIDTH  800
+#define SCREEN_HEIGHT 480
+
+struct ft5406 {
+	struct platform_device * pdev;
+	struct input_dev       * input_dev;
+	void __iomem           * ts_base;
+	dma_addr_t		 bus_addr;
+	struct task_struct     * thread;
+};
+
+/* Thread to poll for touchscreen events
+ * 
+ * This thread polls the memory based register copy of the ft5406 registers
+ * using the number of points register to know whether the copy has been
+ * updated (we write 99 to the memory copy, the GPU will write between 
+ * 0 - 10 points)
+ */
+static int ft5406_thread(void *arg)
+{
+	struct ft5406 *ts = (struct ft5406 *) arg;
+	struct ft5406_regs regs;
+	int known_ids = 0;
+	
+	while(!kthread_should_stop())
+	{
+		// 60fps polling
+		msleep_interruptible(17);
+		memcpy_fromio(&regs, ts->ts_base, sizeof(struct ft5406_regs));
+		iowrite8(99, ts->ts_base + offsetof(struct ft5406_regs, num_points));
+		// Do not output if theres no new information (num_points is 99)
+		// or we have no touch points and don't need to release any
+		if(!(regs.num_points == 99 || (regs.num_points == 0 && known_ids == 0)))
+		{
+			int i;
+			int modified_ids = 0, released_ids;
+			for(i = 0; i < regs.num_points; i++)
+			{
+				int x = (((int) regs.point[i].xh & 0xf) << 8) + regs.point[i].xl;
+				int y = (((int) regs.point[i].yh & 0xf) << 8) + regs.point[i].yl;
+				int touchid = (regs.point[i].yh >> 4) & 0xf;
+				
+				modified_ids |= 1 << touchid;
+
+				if(!((1 << touchid) & known_ids))
+					dev_dbg(&ts->pdev->dev, "x = %d, y = %d, touchid = %d\n", x, y, touchid);
+				
+				input_mt_slot(ts->input_dev, touchid);
+				input_mt_report_slot_state(ts->input_dev, MT_TOOL_FINGER, 1);
+
+				input_report_abs(ts->input_dev, ABS_MT_POSITION_X, x);
+				input_report_abs(ts->input_dev, ABS_MT_POSITION_Y, y);
+
+			}
+
+			released_ids = known_ids & ~modified_ids;
+			for(i = 0; released_ids && i < MAXIMUM_SUPPORTED_POINTS; i++)
+			{
+				if(released_ids & (1<<i))
+				{
+					dev_dbg(&ts->pdev->dev, "Released %d, known = %x modified = %x\n", i, known_ids, modified_ids);
+					input_mt_slot(ts->input_dev, i);
+					input_mt_report_slot_state(ts->input_dev, MT_TOOL_FINGER, 0);
+					modified_ids &= ~(1 << i);
+				}
+			}
+			known_ids = modified_ids;
+			
+			input_mt_report_pointer_emulation(ts->input_dev, true);
+			input_sync(ts->input_dev);
+		}
+			
+	}
+	
+	return 0;
+}
+
+static int ft5406_probe(struct platform_device *pdev)
+{
+	int err = 0;
+	struct device *dev = &pdev->dev;
+	struct device_node *np = dev->of_node;
+	struct ft5406 * ts;
+	struct device_node *fw_node;
+	struct rpi_firmware *fw;
+	u32 touchbuf;
+	
+	dev_info(dev, "Probing device\n");
+	
+	fw_node = of_parse_phandle(np, "firmware", 0);
+	if (!fw_node) {
+		dev_err(dev, "Missing firmware node\n");
+		return -ENOENT;
+	}
+
+	fw = rpi_firmware_get(fw_node);
+	if (!fw)
+		return -EPROBE_DEFER;
+
+	ts = devm_kzalloc(dev, sizeof(struct ft5406), GFP_KERNEL);
+	if (!ts) {
+		dev_err(dev, "Failed to allocate memory\n");
+		return -ENOMEM;
+	}
+
+	ts->input_dev = input_allocate_device();
+	if (!ts->input_dev) {
+		dev_err(dev, "Failed to allocate input device\n");
+		return -ENOMEM;
+	}
+
+	ts->ts_base = dma_zalloc_coherent(dev, PAGE_SIZE, &ts->bus_addr, GFP_KERNEL);
+	if (!ts->ts_base) {
+		pr_err("[%s]: failed to dma_alloc_coherent(%ld)\n",
+				__func__, PAGE_SIZE);
+		err = -ENOMEM;
+		goto out;
+	}
+
+	touchbuf = (u32)ts->bus_addr;
+	err = rpi_firmware_property(fw, RPI_FIRMWARE_FRAMEBUFFER_SET_TOUCHBUF,
+				    &touchbuf, sizeof(touchbuf));
+
+	if (err || touchbuf != 0) {
+		dev_warn(dev, "Failed to set touchbuf, trying to get err:%x\n", err);
+		dma_free_coherent(dev, PAGE_SIZE, ts->ts_base, ts->bus_addr);
+		ts->ts_base = 0;
+		ts->bus_addr = 0;
+	}
+
+	if (!ts->ts_base) {
+		dev_warn(dev, "set failed, trying get (err:%d touchbuf:%x virt:%p bus:%x)\n", err, touchbuf, ts->ts_base, ts->bus_addr);
+
+		err = rpi_firmware_property(fw, RPI_FIRMWARE_FRAMEBUFFER_GET_TOUCHBUF,
+				    &touchbuf, sizeof(touchbuf));
+		if (err) {
+			dev_err(dev, "Failed to get touch buffer\n");
+			goto out;
+		}
+
+		if (!touchbuf) {
+			dev_err(dev, "Touchscreen not detected\n");
+			err = -ENODEV;
+			goto out;
+		}
+
+		dev_dbg(dev, "Got TS buffer 0x%x\n", touchbuf);
+
+		// mmap the physical memory
+		touchbuf &= ~0xc0000000;
+		ts->ts_base = ioremap(touchbuf, sizeof(struct ft5406_regs));
+		if (ts->ts_base == NULL)
+		{
+			dev_err(dev, "Failed to map physical address\n");
+			err = -ENOMEM;
+			goto out;
+		}
+	}
+	platform_set_drvdata(pdev, ts);
+	ts->pdev = pdev;
+	
+	ts->input_dev->name = "FT5406 memory based driver";
+	
+	__set_bit(EV_KEY, ts->input_dev->evbit);
+	__set_bit(EV_SYN, ts->input_dev->evbit);
+	__set_bit(EV_ABS, ts->input_dev->evbit);
+
+	input_set_abs_params(ts->input_dev, ABS_MT_POSITION_X, 0,
+			     SCREEN_WIDTH, 0, 0);
+	input_set_abs_params(ts->input_dev, ABS_MT_POSITION_Y, 0,
+			     SCREEN_HEIGHT, 0, 0);
+
+	input_mt_init_slots(ts->input_dev, MAXIMUM_SUPPORTED_POINTS, INPUT_MT_DIRECT);
+
+	input_set_drvdata(ts->input_dev, ts);
+	
+	err = input_register_device(ts->input_dev);
+	if (err) {
+		dev_err(dev, "could not register input device, %d\n",
+			err);
+		goto out;
+	}
+
+	// create thread to poll the touch events
+	ts->thread = kthread_run(ft5406_thread, ts, "ft5406");
+	if(ts->thread == NULL)
+	{
+		dev_err(dev, "Failed to create kernel thread");
+		err = -ENOMEM;
+		goto out;
+	}
+
+	return 0;
+
+out:
+	if (ts->bus_addr) {
+		dma_free_coherent(dev, PAGE_SIZE, ts->ts_base, ts->bus_addr);
+		ts->bus_addr = 0;
+		ts->ts_base = NULL;
+	} else if (ts->ts_base) {
+		iounmap(ts->ts_base);
+		ts->ts_base = NULL;
+	}
+	if (ts->input_dev) {
+		input_unregister_device(ts->input_dev);
+		ts->input_dev = NULL;
+	}
+	return err;
+}
+
+static int ft5406_remove(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct ft5406 *ts = (struct ft5406 *) platform_get_drvdata(pdev);
+	
+	dev_info(dev, "Removing rpi-ft5406\n");
+	
+	kthread_stop(ts->thread);
+
+	if (ts->bus_addr)
+		dma_free_coherent(dev, PAGE_SIZE, ts->ts_base, ts->bus_addr);
+	else if (ts->ts_base)
+		iounmap(ts->ts_base);
+	if (ts->input_dev)
+		input_unregister_device(ts->input_dev);
+	
+	return 0;
+}
+
+static const struct of_device_id ft5406_match[] = {
+	{ .compatible = "rpi,rpi-ft5406", },
+	{},
+};
+MODULE_DEVICE_TABLE(of, ft5406_match);
+
+static struct platform_driver ft5406_driver = {
+	.driver = {
+		.name   = "rpi-ft5406",
+		.owner  = THIS_MODULE,
+		.of_match_table = ft5406_match,
+	},
+	.probe          = ft5406_probe,
+	.remove         = ft5406_remove,
+};
+
+module_platform_driver(ft5406_driver);
+
+MODULE_AUTHOR("Gordon Hollingworth");
+MODULE_DESCRIPTION("Touchscreen driver for memory based FT5406");
+MODULE_LICENSE("GPL");
