--- /dev/null
+++ b/arch/arm/boot/dts/kirkwood-on100.dts
@@ -0,0 +1,160 @@
+/dts-v1/;
+
+#include "kirkwood.dtsi"
+#include "kirkwood-6282.dtsi"
+
+/ {
+	model = "Cisco Systems ON100";
+	compatible = "cisco,on100", "marvell,kirkwood-88f6282", "marvell,kirkwood";
+
+	memory {
+		device_type = "memory";
+		reg = <0x00000000 0x20000000>;
+	};
+
+	aliases {
+		serial0 = &uart0;
+	};
+
+	chosen {
+		bootargs = "console=ttyS0,115200n8 earlyprintk";
+		stdout-path = "serial0:115200n8";
+	};
+
+	gpio_keys {
+		compatible = "gpio-keys";
+		#address-cells = <1>;
+		#size-cells = <0>;
+		pinctrl-0 = <&pmx_btn_reset>;
+		pinctrl-names = "default";
+
+		button@1 {
+			label = "Reset Button";
+			linux,code = <KEY_RESTART>;
+			gpios = <&gpio1 9 GPIO_ACTIVE_LOW>;
+		};
+	};
+
+	gpio-leds {
+		compatible = "gpio-leds";
+		pinctrl-0 = < &pmx_led_health_r &pmx_led_health_g >;
+		pinctrl-names = "default";
+
+		health-g {
+			label = "on100:green:health";
+			gpios = <&gpio1 12 GPIO_ACTIVE_LOW>;
+		};
+
+		health-r {
+			label = "on100:red:health";
+			gpios = <&gpio1 13 GPIO_ACTIVE_LOW>;
+		};
+
+		health2-g {
+			label = "on100:green:health2";
+			gpios = <&gpio1 14 GPIO_ACTIVE_LOW>;
+		};
+
+		health2-r {
+			label = "on100:red:health2";
+			gpios = <&gpio1 15 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
+
+&eth0 {
+	status = "okay";
+
+	ethernet0-port@0 {
+		phy-handle = <&ethphy0>;
+		phy-connection-type = "rgmii-id";
+	};
+};
+
+&eth1 {
+	status = "okay";
+
+	ethernet1-port@0 {
+		phy-handle = <&ethphy1>;
+		phy-connection-type = "rgmii-id";
+	};
+};
+
+&mdio {
+	status = "okay";
+
+	ethphy0: ethernet-phy@0 {
+		/* Marvell 88E1121R */
+		compatible = "ethernet-phy-id0141.0cb0",
+			     "ethernet-phy-ieee802.3-c22";
+		reg = <0>;
+	};
+
+	ethphy1: ethernet-phy@1 {
+		/* Marvell 88E1121R */
+		compatible = "ethernet-phy-id0141.0cb0",
+			     "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
+
+&nand {
+	status = "okay";
+
+	partition@0 {
+		label = "u-boot";
+		reg = <0x00000000 0x000a0000>;
+		read-only;
+	};
+
+	partition@a0000 {
+		label = "u-boot environment";
+		reg = <0x000a0000 0x00020000>;
+		read-only;
+	};
+
+	partition@c0000 {
+		label = "kernel";
+		reg = <0x000c0000 0x00540000>;
+	};
+
+	partition@600000 {
+		label = "ubi";
+		reg = <0x00600000 0x1fa00000>;
+	};
+};
+
+&pinctrl {
+	pmx_led_health_r: pmx-led-health-r {
+		marvell,pins = "mpp45";
+		marvell,function = "gpio";
+	};
+
+	pmx_led_health_g: pmx-led-health-g {
+		marvell,pins = "mpp44";
+		marvell,function = "gpio";
+	};
+
+	pmx_led_health2_r: pmx-led-health2-r {
+		marvell,pins = "mpp47";
+		marvell,function = "gpio";
+	};
+
+	pmx_led_health2_g: pmx-led-health2-g {
+		marvell,pins = "mpp46";
+		marvell,function = "gpio";
+	};
+
+	pmx_btn_reset: pmx-led-reset {
+		marvell,pins = "mpp31";
+		marvell,function = "gpio";
+	};
+};
+
+&sdio {
+	status = "okay";
+};
+
+&uart0 {
+	status = "okay";
+};
--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -271,6 +271,7 @@ dtb-$(CONFIG_MACH_KIRKWOOD) += \
 	kirkwood-nsa310b.dtb \
 	kirkwood-nsa320.dtb \
 	kirkwood-nsa325.dtb \
+	kirkwood-on100.dtb \
 	kirkwood-openblocks_a6.dtb \
 	kirkwood-openblocks_a7.dtb \
 	kirkwood-openrd-base.dtb \
