From 717b9761b68bf9e63e9041079bfd77a090af4bdd Mon Sep 17 00:00:00 2001
From: Ben Wolsieffer <benwolsieffer@gmail.com>
Date: Sun, 9 Dec 2018 16:46:00 -0500
Subject: [PATCH 451/454] dtoverlays: fe-pi-audio: fix sgtl5000 compatible
 string

The compatible string was set to "fepi,sgtl5000", which worked for some
reason in 4.14, but does not work in 4.19, presumably due to some
change in the kernel matching logic. The correct string is
"fsl,sgtl5000".

Signed-off-by: Ben Wolsieffer <benwolsieffer@gmail.com>
---
 arch/arm/boot/dts/overlays/fe-pi-audio-overlay.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/overlays/fe-pi-audio-overlay.dts
+++ b/arch/arm/boot/dts/overlays/fe-pi-audio-overlay.dts
@@ -39,7 +39,7 @@
 
 			sgtl5000@0a {
 				#sound-dai-cells = <0>;
-				compatible = "fepi,sgtl5000";
+				compatible = "fsl,sgtl5000";
 				reg = <0x0a>;
 				clocks = <&sgtl5000_mclk>;
 				micbias-resistor-k-ohms = <2>;
