From e1a08730eeb0bad4d82c3bc40e74854872de618d Mon Sep 17 00:00:00 2001
From: Wright Feng <wright.feng@cypress.com>
Date: Wed, 21 Nov 2018 07:53:44 +0000
Subject: [PATCH] brcmfmac: set F2 watermark to 256 for 4373

We got SDIO_CRC_ERROR with 4373 on SDR104 when doing bi-directional
throughput test. Enable watermark to 256 to guarantee the operation
stability.

Reviewed-by: Arend van Spriel <arend.vanspriel@broadcom.com>
Signed-off-by: Wright Feng <wright.feng@cypress.com>
Signed-off-by: Chi-Hsien Lin <chi-hsien.lin@cypress.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 .../broadcom/brcm80211/brcmfmac/sdio.c        | 26 +++++++++++++++++--
 1 file changed, 24 insertions(+), 2 deletions(-)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
@@ -49,6 +49,10 @@
 #define DCMD_RESP_TIMEOUT	msecs_to_jiffies(2500)
 #define CTL_DONE_TIMEOUT	msecs_to_jiffies(2500)
 
+/* watermark expressed in number of words */
+#define DEFAULT_F2_WATERMARK    0x8
+#define CY_4373_F2_WATERMARK    0x40
+
 #ifdef DEBUG
 
 #define BRCMF_TRAP_INFO_SIZE	80
@@ -138,6 +142,8 @@ struct rte_console {
 /* 1: isolate internal sdio signals, put external pads in tri-state; requires
  * sdio bus power cycle to clear (rev 9) */
 #define SBSDIO_DEVCTL_PADS_ISO		0x08
+/* 1: enable F2 Watermark */
+#define SBSDIO_DEVCTL_F2WM_ENAB		0x10
 /* Force SD->SB reset mapping (rev 11) */
 #define SBSDIO_DEVCTL_SB_RST_CTL	0x30
 /*   Determined by CoreControl bit */
@@ -4057,6 +4063,7 @@ static void brcmf_sdio_firmware_callback
 	void *nvram;
 	u32 nvram_len;
 	u8 saveclk;
+	u8 devctl;
 
 	brcmf_dbg(TRACE, "Enter: dev=%s, err=%d\n", dev_name(dev), err);
 
@@ -4112,8 +4119,23 @@ static void brcmf_sdio_firmware_callback
 		brcmf_sdiod_writel(sdiod, core->base + SD_REG(hostintmask),
 				   bus->hostintmask, NULL);
 
-
-		brcmf_sdiod_writeb(sdiod, SBSDIO_WATERMARK, 8, &err);
+		switch (sdiod->func1->device) {
+		case SDIO_DEVICE_ID_CYPRESS_4373:
+			brcmf_dbg(INFO, "set F2 watermark to 0x%x*4 bytes\n",
+				  CY_4373_F2_WATERMARK);
+			brcmf_sdiod_writeb(sdiod, SBSDIO_WATERMARK,
+					   CY_4373_F2_WATERMARK, &err);
+			devctl = brcmf_sdiod_readb(sdiod, SBSDIO_DEVICE_CTL,
+						   &err);
+			devctl |= SBSDIO_DEVCTL_F2WM_ENAB;
+			brcmf_sdiod_writeb(sdiod, SBSDIO_DEVICE_CTL, devctl,
+					   &err);
+			break;
+		default:
+			brcmf_sdiod_writeb(sdiod, SBSDIO_WATERMARK,
+					   DEFAULT_F2_WATERMARK, &err);
+			break;
+		}
 	} else {
 		/* Disable F2 again */
 		sdio_disable_func(sdiod->func2);
