From 1e932b627e79aa2c70e2c7278e4ac930303faa3f Mon Sep 17 00:00:00 2001
From: Christian Lamparter <chunkeey@gmail.com>
Date: Thu, 21 Dec 2017 15:09:18 +0100
Subject: [PATCH 2/6] crypto: crypto4xx - support Revision B parts

This patch adds support for the crypto4xx RevB cores
found in the 460EX, 460SX and later cores (like the APM821xx).

Without this patch, the crypto4xx driver will not be
able to process any offloaded requests and simply hang
indefinitely.

Signed-off-by: Christian Lamparter <chunkeey@gmail.com>
---
 drivers/crypto/amcc/crypto4xx_core.c    | 48 +++++++++++++++++++++++++++++----
 drivers/crypto/amcc/crypto4xx_core.h    |  1 +
 drivers/crypto/amcc/crypto4xx_reg_def.h |  4 ++-
 3 files changed, 47 insertions(+), 6 deletions(-)

--- a/drivers/crypto/amcc/crypto4xx_core.c
+++ b/drivers/crypto/amcc/crypto4xx_core.c
@@ -128,7 +128,14 @@ static void crypto4xx_hw_init(struct cry
 	writel(PPC4XX_INT_DESCR_CNT, dev->ce_base + CRYPTO4XX_INT_DESCR_CNT);
 	writel(PPC4XX_INT_DESCR_CNT, dev->ce_base + CRYPTO4XX_INT_DESCR_CNT);
 	writel(PPC4XX_INT_CFG, dev->ce_base + CRYPTO4XX_INT_CFG);
-	writel(PPC4XX_PD_DONE_INT, dev->ce_base + CRYPTO4XX_INT_EN);
+	if (dev->is_revb) {
+		writel(PPC4XX_INT_TIMEOUT_CNT_REVB << 10,
+		       dev->ce_base + CRYPTO4XX_INT_TIMEOUT_CNT);
+		writel(PPC4XX_PD_DONE_INT | PPC4XX_TMO_ERR_INT,
+		       dev->ce_base + CRYPTO4XX_INT_EN);
+	} else {
+		writel(PPC4XX_PD_DONE_INT, dev->ce_base + CRYPTO4XX_INT_EN);
+	}
 }
 
 int crypto4xx_alloc_sa(struct crypto4xx_ctx *ctx, u32 size)
@@ -1079,18 +1086,29 @@ static void crypto4xx_bh_tasklet_cb(unsi
 /**
  * Top Half of isr.
  */
-static irqreturn_t crypto4xx_ce_interrupt_handler(int irq, void *data)
+static inline irqreturn_t crypto4xx_interrupt_handler(int irq, void *data,
+						      u32 clr_val)
 {
 	struct device *dev = (struct device *)data;
 	struct crypto4xx_core_device *core_dev = dev_get_drvdata(dev);
 
-	writel(PPC4XX_INTERRUPT_CLR,
-	       core_dev->dev->ce_base + CRYPTO4XX_INT_CLR);
+	writel(clr_val, core_dev->dev->ce_base + CRYPTO4XX_INT_CLR);
 	tasklet_schedule(&core_dev->tasklet);
 
 	return IRQ_HANDLED;
 }
 
+static irqreturn_t crypto4xx_ce_interrupt_handler(int irq, void *data)
+{
+	return crypto4xx_interrupt_handler(irq, data, PPC4XX_INTERRUPT_CLR);
+}
+
+static irqreturn_t crypto4xx_ce_interrupt_handler_revb(int irq, void *data)
+{
+	return crypto4xx_interrupt_handler(irq, data, PPC4XX_INTERRUPT_CLR |
+		PPC4XX_TMO_ERR_INT);
+}
+
 /**
  * Supported Crypto Algorithms
  */
@@ -1272,6 +1290,8 @@ static int crypto4xx_probe(struct platfo
 	struct resource res;
 	struct device *dev = &ofdev->dev;
 	struct crypto4xx_core_device *core_dev;
+	u32 pvr;
+	bool is_revb = true;
 
 	rc = of_address_to_resource(ofdev->dev.of_node, 0, &res);
 	if (rc)
@@ -1288,6 +1308,7 @@ static int crypto4xx_probe(struct platfo
 		       mfdcri(SDR0, PPC405EX_SDR0_SRST) | PPC405EX_CE_RESET);
 		mtdcri(SDR0, PPC405EX_SDR0_SRST,
 		       mfdcri(SDR0, PPC405EX_SDR0_SRST) & ~PPC405EX_CE_RESET);
+		is_revb = false;
 	} else if (of_find_compatible_node(NULL, NULL,
 			"amcc,ppc460sx-crypto")) {
 		mtdcri(SDR0, PPC460SX_SDR0_SRST,
@@ -1310,7 +1331,22 @@ static int crypto4xx_probe(struct platfo
 	if (!core_dev->dev)
 		goto err_alloc_dev;
 
+	/*
+	 * Older version of 460EX/GT have a hardware bug.
+	 * Hence they do not support H/W based security intr coalescing
+	 */
+	pvr = mfspr(SPRN_PVR);
+	if (is_revb && ((pvr >> 4) == 0x130218A)) {
+		u32 min = PVR_MIN(pvr);
+
+		if (min < 4) {
+			dev_info(dev, "RevA detected - disable interrupt coalescing\n");
+			is_revb = false;
+		}
+	}
+
 	core_dev->dev->core_dev = core_dev;
+	core_dev->dev->is_revb = is_revb;
 	core_dev->device = dev;
 	spin_lock_init(&core_dev->lock);
 	INIT_LIST_HEAD(&core_dev->dev->alg_list);
@@ -1340,7 +1376,9 @@ static int crypto4xx_probe(struct platfo
 
 	/* Register for Crypto isr, Crypto Engine IRQ */
 	core_dev->irq = irq_of_parse_and_map(ofdev->dev.of_node, 0);
-	rc = request_irq(core_dev->irq, crypto4xx_ce_interrupt_handler, 0,
+	rc = request_irq(core_dev->irq, is_revb ?
+			 crypto4xx_ce_interrupt_handler_revb :
+			 crypto4xx_ce_interrupt_handler, 0,
 			 core_dev->dev->name, dev);
 	if (rc)
 		goto err_request_irq;
--- a/drivers/crypto/amcc/crypto4xx_core.h
+++ b/drivers/crypto/amcc/crypto4xx_core.h
@@ -109,6 +109,7 @@ struct crypto4xx_device {
 	struct list_head alg_list;	/* List of algorithm supported
 					by this device */
 	struct ratelimit_state aead_ratelimit;
+	bool is_revb;
 };
 
 struct crypto4xx_core_device {
--- a/drivers/crypto/amcc/crypto4xx_reg_def.h
+++ b/drivers/crypto/amcc/crypto4xx_reg_def.h
@@ -121,13 +121,15 @@
 #define PPC4XX_PD_SIZE				6
 #define PPC4XX_CTX_DONE_INT			0x2000
 #define PPC4XX_PD_DONE_INT			0x8000
+#define PPC4XX_TMO_ERR_INT			0x40000
 #define PPC4XX_BYTE_ORDER			0x22222
 #define PPC4XX_INTERRUPT_CLR			0x3ffff
 #define PPC4XX_PRNG_CTRL_AUTO_EN		0x3
 #define PPC4XX_DC_3DES_EN			1
 #define PPC4XX_TRNG_EN				0x00020000
-#define PPC4XX_INT_DESCR_CNT			4
+#define PPC4XX_INT_DESCR_CNT			7
 #define PPC4XX_INT_TIMEOUT_CNT			0
+#define PPC4XX_INT_TIMEOUT_CNT_REVB		0x3FF
 #define PPC4XX_INT_CFG				1
 /**
  * all follow define are ad hoc
