From 861cb5eb467f5e38dce1aabe4e8db379255bd89b Mon Sep 17 00:00:00 2001
From: Stefan Wahren <stefan.wahren@i2se.com>
Date: Wed, 12 Dec 2018 20:20:06 +0100
Subject: [PATCH] brcmfmac: Fix access point mode

Since commit 1204aa17f3b4 ("brcmfmac: set WIPHY_FLAG_HAVE_AP_SME flag")
the Raspberry Pi 3 A+ (BCM43455) isn't able to operate in AP mode with
hostapd (device_ap_sme=1 use_monitor=0):

brcmfmac: brcmf_cfg80211_stop_ap: setting AP mode failed -52

So add the missing mgmt_stypes for AP mode to fix this.

Fixes: 1204aa17f3b4 ("brcmfmac: set WIPHY_FLAG_HAVE_AP_SME flag")
Suggested-by: Arend van Spriel <arend.vanspriel@broadcom.com>
Signed-off-by: Stefan Wahren <stefan.wahren@i2se.com>
Acked-by: Arend van Spriel <arend.vanspriel@broadcom.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 .../wireless/broadcom/brcm80211/brcmfmac/cfg80211.c    | 10 ++++++++++
 1 file changed, 10 insertions(+)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c
@@ -6314,6 +6314,16 @@ brcmf_txrx_stypes[NUM_NL80211_IFTYPES] =
 		.tx = 0xffff,
 		.rx = BIT(IEEE80211_STYPE_ACTION >> 4) |
 		      BIT(IEEE80211_STYPE_PROBE_REQ >> 4)
+	},
+	[NL80211_IFTYPE_AP] = {
+		.tx = 0xffff,
+		.rx = BIT(IEEE80211_STYPE_ASSOC_REQ >> 4) |
+		      BIT(IEEE80211_STYPE_REASSOC_REQ >> 4) |
+		      BIT(IEEE80211_STYPE_PROBE_REQ >> 4) |
+		      BIT(IEEE80211_STYPE_DISASSOC >> 4) |
+		      BIT(IEEE80211_STYPE_AUTH >> 4) |
+		      BIT(IEEE80211_STYPE_DEAUTH >> 4) |
+		      BIT(IEEE80211_STYPE_ACTION >> 4)
 	}
 };
 
