#!/bin/sh

. /lib/functions/uci-defaults.sh

set_wifi_led() {
	ucidef_set_led_netdev "wifi_led" "wifi" "${1}" "${2:-wlan0}"
}


board=$(board_name)
boardname="${board##*,}"

board_config_update

case $board in
3g-6200n|\
br-6475nd|\
mzk-w300nh2)
	set_wifi_led "$boardname:amber:wlan"
	;;
3g-6200nl|\
air3gii|\
hilink,hlk-7628n|\
mr-102n|\
skylab,skw92a|\
wnce2001|\
zbt-we2026)
	set_wifi_led "$boardname:green:wlan"
	;;
ai-br100)
	ucidef_set_led_netdev "wan" "wan" "$boardname:blue:wan" "eth0.2"
	set_wifi_led "$boardname:blue:wlan"
	;;
alfa-network,ac1200rm)
	set_wifi_led "$boardname:green:wlan2g" "wlan1"
	;;
alfa-network,awusfree1|\
edimax,br-6478ac-v2)
	set_wifi_led "$boardname:blue:wlan"
	;;
alfa-network,tube-e4g)
	ucidef_set_led_netdev "4g" "4g" "$boardname:green:4g" "wwan0"
	ucidef_set_led_netdev "lan" "lan" "$boardname:blue:lan" "eth0"
	;;
all0256n-4M|\
all0256n-8M)
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "all0256n:green:rssilow" "wlan0" "1" "40" "0" "6"
	ucidef_set_led_rssi "rssimedium" "RSSIMEDIUM" "all0256n:green:rssimed" "wlan0" "30" "80" "-29" "5"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "all0256n:green:rssihigh" "wlan0" "70" "100" "-69" "8"
	set_wifi_led "rt2800pci-phy0::radio"
	;;
ar670w|\
ar725w|\
awapn2403)
	set_wifi_led "rt2800soc-phy0::radio"
	;;
asl26555-8M|\
asl26555-16M)
	ucidef_set_led_netdev "eth" "ETH" "asl26555:green:eth" "eth0"
	set_wifi_led "asl26555:green:wlan"
	;;
bdcom,wap2100-sk|\
hiwifi,hc5861b)
	set_wifi_led "$boardname:green:wlan2g"
	;;
belkin,f9k1109v1)
	set_usb_led "$boardname:green:usb1"
	ucidef_set_led_netdev "lan" "lan" "$boardname:blue:wps" "eth0"
	;;
broadway)
	set_wifi_led "$boardname:red:wps_active"
	;;
c108)
	ucidef_set_led_netdev "lan" "lan" "$boardname:green:lan" "eth0"
	ucidef_set_led_netdev "modem" "modem" "$boardname:green:modem" "wwan0"
	;;
c20i)
	ucidef_set_led_switch "lan" "lan" "$boardname:blue:lan" "switch0" "0x1e"
	ucidef_set_led_switch "wan" "wan" "$boardname:blue:wan" "switch0" "0x01"
	ucidef_set_led_wlan "wlan" "wlan" "$boardname:blue:wlan" "phy0radio"
	;;
c50)
	ucidef_set_led_switch "lan" "lan" "$boardname:green:lan" "switch0" "0x1e"
	ucidef_set_led_switch "wan" "wan" "$boardname:green:wan" "switch0" "0x01"
	ucidef_set_led_netdev "wlan2g" "wlan2g" "$boardname:green:wlan2g" wlan1
	set_wifi_led "$boardname:green:wlan5g"
	;;
cf-wr800n)
	ucidef_set_led_netdev "lan" "lan" "$boardname:white:ethernet" eth0.1
	set_wifi_led "$boardname:white:wifi"
	;;
cudy,wr1000)
	ucidef_set_led_switch "wan" "wan" "$boardname:blue:wan" "switch0" "0x10"
	ucidef_set_led_switch "lan1" "lan1" "$boardname:blue:lan1" "switch0" "0x08"
	ucidef_set_led_switch "lan2" "lan2" "$boardname:blue:lan2" "switch0" "0x04"
	;;
d240|\
mlw221|\
mlwg2|\
rakwireless,rak633|\
rt-ac51u)
	set_wifi_led "$boardname:blue:wifi"
	;;
dcs-930l-b1)
	ucidef_set_led_netdev "wifi" "WiFi" "$boardname:blue:wps"
	;;
dir-300-b1|\
dir-300-b7|\
dir-320-b1|\
dir-600-b1|\
dir-610-a1|\
dir-615-d|\
dir-615-h1|\
dir-620-a1|\
esr-9753|\
hlk-rm04|\
kn|\
nbg-419n2|\
sl-r7205|\
v11st-fe|\
w306r-v20|\
w502u|\
wt1520-4M|\
wt1520-8M|\
zyxel,keenetic-start)
	set_wifi_led "rt2800pci-phy0::radio"
	;;
dir-620-d1|\
dlink,dwr-116-a1|\
head-weblink,hdrm200|\
kn_rc|\
kn_rf|\
kng_rc|\
mzk-ex300np|\
oy-0001|\
tew-714tru|\
zbt-wr8305rt)
	set_wifi_led "$boardname:green:wifi"
	;;
dlink,dwr-118-a1)
	ucidef_set_led_switch "lan" "lan" "$boardname:green:lan" "switch0" "0x1f"
	ucidef_set_led_switch "wan" "wan" "$boardname:green:wan" "switch0" "0x20"
	set_wifi_led "$boardname:green:wlan2g" "wlan1"
	;;
dlink,dwr-118-a2)
	ucidef_set_led_switch "lan" "lan" "$boardname:green:lan" "switch0" "0x0e"
	ucidef_set_led_switch "wan" "wan" "$boardname:green:wan" "switch0" "0x01"
	set_wifi_led "$boardname:green:wlan2g" "wlan1"
	;;
dlink,dwr-921-c1|\
dlink,dwr-922-e2)
	set_wifi_led "$boardname:green:wifi"
	ucidef_set_led_switch "lan" "lan" "$boardname:green:lan" "switch0" "0x0f"
	ucidef_set_led_netdev "signalstrength" "signalstrength" "$boardname:green:sigstrength" "wwan0" "link"
	ucidef_set_led_netdev "4g" "4g" "$boardname:green:4g" "wwan0" "tx rx"
	;;
dir-860l-b1)
	ucidef_set_led_netdev "wan" "wan" "$boardname:green:net" "eth0.2"
	;;
ex2700|\
wn3000rpv3)
	set_wifi_led "$boardname:green:router"
	;;
ex3700)
	ucidef_set_led_netdev "wlan5g" "ROUTER (green)" "$boardname:green:router" "wlan0"
	ucidef_set_led_netdev "wlan2g" "DEVICE (green)" "$boardname:green:device" "wlan1"
	;;
f5d8235-v1)
	set_wifi_led "$boardname:blue:wireless"
	;;
fonera20n|\
tiny-ac)
	set_wifi_led "$boardname:orange:wifi"
	;;
gnubee,gb-pc1|\
gnubee,gb-pc2)
	ucidef_set_led_switch "lan1" "lan1" "$boardname:green:lan1" "switch0" "0x01"
	ucidef_set_led_switch "lan2" "lan2" "$boardname:green:lan2" "switch0" "0x10"
	;;
gl-mt300a|\
gl-mt300n|\
gl-mt750)
	set_wifi_led "$boardname:wlan"
	;;
gl-mt300n-v2)
	set_wifi_led "$boardname:red:wlan"
	ucidef_set_led_switch "wan" "wan" "$boardname:green:wan" "switch0" "0x1"
	;;
hc5661|\
hc5661a)
	ucidef_set_led_netdev "internet" "internet" "$boardname:blue:internet" "eth0.2"
	set_wifi_led "$boardname:blue:wlan2g"
	;;
hc5761|\
hc5861)
	ucidef_set_led_netdev "internet" "internet" "$boardname:blue:internet" "eth0.2"
	ucidef_set_led_netdev "wifi5g" "wifi5g" "$boardname:blue:wlan5g" "wlan0"
	ucidef_set_led_netdev "wifi2g" "wifi2g" "$boardname:blue:wlan2g" "wlan1"
	;;
hg255d)
	set_wifi_led "$boardname:green:wlan"
	ucidef_set_led_netdev "internet" "internet" "$boardname:green:internet" "eth0.2"
	;;
hpm)
	ucidef_set_led_netdev "eth" "ETH" "$boardname:green:eth" "eth0"
	set_wifi_led "$boardname:green:wifi"
	;;
ht-tm02)
	ucidef_set_led_netdev "eth" "Ethernet" "$boardname:green:lan" "eth0"
	set_wifi_led "$boardname:blue:wlan"
	;;
iodata,wn-ac1167gr|\
iodata,wn-ac733gr3)
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "$boardname:green:wlan5g" "phy0radio"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "$boardname:green:wlan2g" "phy1radio"
	;;
kimax,u35wf)
	set_wifi_led "$boardname:blue:wifi"
	ucidef_set_led_netdev "eth" "ETH" "$boardname:green:eth" "eth0"
	;;
lava,lr-25g001)
	ucidef_set_led_netdev "wlan2g" "WiFi 2.4GHz" "$boardname:green:wlan2g" "wlan1"
	ucidef_set_led_netdev "wlan5g" "WiFi 5GHz" "$boardname:green:wlan5g" "wlan0"
	;;
linkits7688)
	ucidef_set_led_wlan "wifi" "wifi" "linkit-smart-7688:orange:wifi" "phy0tpt"
	;;
m2m)
	set_wifi_led "$boardname:blue:wifi"
	ucidef_set_led_netdev "eth" "Ethernet" "$boardname:green:wan" "eth0"
	;;
mikrotik,rbm11g)
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "$boardname:green:rssi0" "wlan0" "1" "100"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "$boardname:green:rssi1" "wlan0" "20" "100"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "$boardname:green:rssi2" "wlan0" "40" "100"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "$boardname:green:rssi3" "wlan0" "60" "100"
	ucidef_set_led_rssi "rssiveryhigh" "RSSIVERYHIGH" "$boardname:green:rssi4" "wlan0" "80" "100"
	;;
miniembplug)
	set_wifi_led "$boardname:red:wlan"
	;;
mr200)
	ucidef_set_led_netdev "lan" "lan" "$boardname:white:lan" "eth0.1"
	ucidef_set_led_netdev "wan" "wan" "$boardname:white:wan" "usb0"
	set_wifi_led "$boardname:white:wlan"
	;;
mtc,wr1201)
	ucidef_set_led_switch "eth_link" "LAN link" "$boardname:green:eth_link" "switch0" "0x0f"
	;;
mzk-ex750np|\
zbtlink,zbt-we826-e)
	set_wifi_led "$boardname:red:wifi"
	;;
netgear,r6120)
	ucidef_set_led_switch "lan" "lan" "$boardname:green:lan" "switch0" "0x0f"
	ucidef_set_led_switch "wan" "wan" "$boardname:green:wan" "switch0" "0x10"
	ucidef_set_led_wlan "wlan2g" "WiFi 2.4GHz" "$boardname:green:wlan2g" "phy0tpt"
	;;
gehua,ghl-r-001|\
pbr-m1)
	ucidef_set_led_netdev "internet" "internet" "$boardname:blue:internet" "eth0.2"
	;;
d-team,newifi-d2)
	ucidef_set_led_switch "internet" "internet" "$boardname:amber:internet" "switch0" "0x10"
	ucidef_set_led_netdev "wlan2g" "WiFi 2.4GHz" "$boardname:blue:wlan2g" "wlan0"
	ucidef_set_led_netdev "wlan5g" "WiFi 5GHz" "$boardname:blue:wlan5g" "wlan1"
	;;
psg1208)
	set_wifi_led "$boardname:white:wlan2g"
	;;
px-4885-4M|\
px-4885-8M)
	set_wifi_led "px-4885:orange:wifi"
	;;
r6220|\
netgear,r6350|\
wndr3700v5)
	ucidef_set_led_switch "wan" "wan" "$boardname:green:wan" "switch0" "0x10"
	set_wifi_led "$boardname:green:wifi"
	;;
re350-v1)
	ucidef_set_led_netdev "wifi2g" "Wifi 2.4G" "$boardname:blue:wifi2G" "wlan0"
	ucidef_set_led_netdev "wifi5g" "Wifi 5G" "$boardname:blue:wifi5G" "wlan1"
	ucidef_set_led_netdev "eth_act" "LAN act" "$boardname:green:eth_act" "eth0" "tx rx"
	ucidef_set_led_switch "eth_link" "LAN link" "$boardname:green:eth_link" "switch0" "0x01"
	;;
rp-n53)
	ucidef_set_led_netdev "eth" "Network" "$boardname:white:back" "eth0"
	set_wifi_led "$boardname:blue:wifi"
	;;
rt-n12p)
	ucidef_set_led_netdev "lan" "lan" "$boardname:green:lan" eth0.1
	ucidef_set_led_netdev "wan" "wan" "$boardname:green:wan" eth0.2
	set_wifi_led "$boardname:green:air"
	;;
rt-n14u)
	ucidef_set_led_netdev "lan" "lan" "$boardname:blue:lan" eth0.1
	ucidef_set_led_netdev "wan" "wan" "$boardname:blue:wan" eth0.2
	set_wifi_led "$boardname:blue:air"
	;;
tama,w06)
	ucidef_set_led_netdev "wan" "WAN" "$boardname:green:wan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "$boardname:green:wlan" "phy0tpt"
	;;
tl-wr840n-v4)
	ucidef_set_led_wlan "wlan2g" "wlan2g" "$boardname:green:wlan" "phy0tpt"
	ucidef_set_led_switch "lan" "lan" "$boardname:green:lan" "switch0" "0x1e"
	ucidef_set_led_switch "wan" "wan" "$boardname:green:wan" "switch0" "0x01"
	;;
tl-wr841n-v13)
	ucidef_set_led_wlan "wlan2g" "wlan2g" "$boardname:green:wlan" "phy0tpt"
	ucidef_set_led_switch "lan1" "lan1" "$boardname:green:lan1" "switch0" "0x2"
	ucidef_set_led_switch "lan2" "lan2" "$boardname:green:lan2" "switch0" "0x4"
	ucidef_set_led_switch "lan3" "lan3" "$boardname:green:lan3" "switch0" "0x8"
	ucidef_set_led_switch "lan4" "lan4" "$boardname:green:lan4" "switch0" "0x10"
	ucidef_set_led_switch "wan" "wan" "$boardname:green:wan" "switch0" "0x01"
	;;
tplink,c2-v1)
	ucidef_set_led_switch "lan" "lan" "$boardname:green:lan" "switch1" "0x1e"
	ucidef_set_led_switch "wan" "wan" "$boardname:green:wan" "switch1" "0x01"
	set_wifi_led "$boardname:green:wlan"
	;;
tplink,c20-v1)
	ucidef_set_led_switch "lan" "lan" "$boardname:blue:lan" "switch0" "0x1e"
	ucidef_set_led_switch "wan" "wan" "$boardname:blue:wan" "switch0" "0x01"
	ucidef_set_led_netdev "wlan2g" "wlan2g" "$boardname:blue:wlan2g" "wlan0"
	;;
tplink,c20-v4)
	ucidef_set_led_switch "lan" "lan" "$boardname:green:lan" "switch0" "0x1e"
	ucidef_set_led_switch "wan" "wan" "$boardname:green:wan" "switch0" "0x01"
	ucidef_set_led_netdev "wlan2g" "wlan2g" "$boardname:green:wlan2g" "wlan0"
	;;
tplink,c50-v3|\
tplink,c50-v4)
	ucidef_set_led_switch "lan" "lan" "$boardname:green:lan" "switch0" "0x1e"
	ucidef_set_led_switch "wan" "wan" "$boardname:green:wan" "switch0" "0x01"
	ucidef_set_led_wlan "wlan2g" "wlan2g" "$boardname:green:wlan2g" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "wlan5g" "$boardname:green:wlan5g" "phy1tpt"
	;;
tplink,tl-wa801nd-v5)
	ucidef_set_led_wlan "wlan" "wlan" "$boardname:green:wlan" "phy0tpt"
	ucidef_set_led_netdev "lan" "lan" "$boardname:green:lan" "eth0"
	;;
tplink,tl-mr3020-v3)
	set_wifi_led "$boardname:green:wlan"
	ucidef_set_led_netdev "lan" "LAN" "$boardname:green:lan" "eth0"
	;;
tplink,tl-mr3420-v5|\
tplink,tl-wr842n-v5)
	ucidef_set_led_wlan "wlan2g" "wlan2g" "$boardname:green:wlan" "phy0tpt"
	ucidef_set_led_switch "lan" "lan" "$boardname:green:lan" "switch0" "0x1e"
	ucidef_set_led_switch "wan" "wan" "$boardname:green:wan" "switch0" "0x01"
	;;
tplink,tl-wr902ac-v3)
	ucidef_set_led_wlan "wlan2g" "wlan2g" "$boardname:green:wlan" "phy0tpt"
	ucidef_set_led_switch "lan" "lan" "$boardname:green:lan" "switch0" "0x10"
	;;
u25awf-h1)
	set_wifi_led "u25awf:red:wifi"
	ucidef_set_led_netdev "eth" "eth" "u25awf:green:lan" "eth0"
	;;
u7628-01-128M-16M)
	ucidef_set_led_switch "lan1" "lan1" "u7628-01:green:lan1" "switch0" "0x2"
	ucidef_set_led_switch "lan2" "lan2" "u7628-01:green:lan2" "switch0" "0x4"
	ucidef_set_led_switch "lan3" "lan3" "u7628-01:green:lan3" "switch0" "0x8"
	ucidef_set_led_switch "lan4" "lan4" "u7628-01:green:lan4" "switch0" "0x10"
	ucidef_set_led_switch "wan" "wan" "u7628-01:green:wan" "switch0" "0x01"
	set_wifi_led "u7628-01:green:wlan"
	;;
vocore-8M|\
vocore-16M)
	ucidef_set_led_netdev "eth" "ETH" "vocore:orange:eth" "eth0"
	;;
wavlink,wl-wn570ha1)
	ucidef_set_led_switch "wan" "wan" "$boardname:green:wan" "switch0" "0x01"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "wifi-low" "wifi-low" "$boardname:green:wifi-low" "wlan0" "1" "49"
	ucidef_set_led_rssi "wifi-med" "wifi-med" "$boardname:green:wifi-med" "wlan0" "50" "84"
	ucidef_set_led_rssi "wifi-high" "wifi-high" "$boardname:green:wifi-high" "wlan0" "85" "100"
	set_wifi_led "$boardname:green:wifi"
	;;
wavlink,wl-wn575a3)
	ucidef_set_rssimon "wlan1" "200000" "1"
	ucidef_set_led_rssi "wifi-low" "wifi-low" "$boardname:green:wifi-low" "wlan1" "1" "49"
	ucidef_set_led_rssi "wifi-med" "wifi-med" "$boardname:green:wifi-med" "wlan1" "50" "84"
	ucidef_set_led_rssi "wifi-high" "wifi-high" "$boardname:green:wifi-high" "wlan1" "85" "100"
	;;
we1026-5g-16m)
	ucidef_set_led_netdev "lan" "LAN" "we1026-5g:green:lan" "eth0"
	set_wifi_led "we1026-5g:green:wifi"
	;;
wrh-300cr)
	set_wifi_led "$boardname:green:wlan"
	ucidef_set_led_netdev "lan" "lan" "$boardname:green:ethernet" "eth0"
	;;
xiaomi,mir3g)
	ucidef_set_led_switch "wan-amber"  "WAN (amber)"  "$boardname:amber:wan"  "switch0" "0x02" "0x08"
	ucidef_set_led_switch "lan1-amber" "LAN1 (amber)" "$boardname:amber:lan1" "switch0" "0x08" "0x08"
	ucidef_set_led_switch "lan2-amber" "LAN2 (amber)" "$boardname:amber:lan2" "switch0" "0x04" "0x08"
	;;
xiaomi,mir3p)
	ucidef_set_led_switch "wan-amber"  "WAN (amber)"  "$boardname:amber:wan"  "switch0" "0x10" "0x08"
	ucidef_set_led_switch "lan1-amber" "LAN1 (amber)" "$boardname:amber:lan1" "switch0" "0x02" "0x08"
	ucidef_set_led_switch "lan2-amber" "LAN2 (amber)" "$boardname:amber:lan2" "switch0" "0x04" "0x08"
	ucidef_set_led_switch "lan3-amber" "LAN3 (amber)" "$boardname:amber:lan3" "switch0" "0x08" "0x08"
	;;
xzwifi,creativebox-v1)
	ucidef_set_led_switch "internet" "internet" "$boardname:blue:internet" "switch0" "0x10"
	;;
y1)
	ucidef_set_led_netdev "wifi" "WIFI" "$boardname:blue:wifi" "wlan1"
	ucidef_set_led_netdev "wifi5g" "WIFI5G" "$boardname:blue:wifi5g" "wlan0"
	ucidef_set_led_switch "lan" "LAN" "$boardname:blue:lan" "switch0" "0x03"
	;;
y1s)
	ucidef_set_led_netdev "wifi" "WIFI" "$boardname:yellow:wifi" "wlan1"
	ucidef_set_led_netdev "wifi5g" "WIFI5G" "$boardname:blue:wifi" "wlan0"
	ucidef_set_led_netdev "wan" "WAN" "$boardname:blue:internet" "eth0.2" "tx rx"
	;;
youhua,wr1200js)
	ucidef_set_led_switch "internet" "INTERNET" "$boardname:green:wan" "switch0" "0x01"
	;;
zbt-ape522ii)
	ucidef_set_led_netdev "wlan2g4" "wlan1-link" "$boardname:green:wlan2g4" "wlan1"
	ucidef_set_led_netdev "sys1" "wlan1" "$boardname:green:sys1" "wlan1" "tx rx"
	ucidef_set_led_netdev "sys2" "wlan0" "$boardname:green:sys2" "wlan0" "tx rx"
	;;
zbt-wa05)
	set_wifi_led "$boardname:blue:air"
	;;
zbt-we826-16M|\
zbt-we826-32M)
	set_wifi_led "zbt-we826:green:wifi"
	;;
zbtlink,zbt-we1226)
	set_wifi_led "$boardname:green:wlan"
	ucidef_set_led_switch "lan1" "LAN1" "$boardname:green:lan1" "switch0" "0x01"
	ucidef_set_led_switch "lan2" "LAN2" "$boardname:green:lan2" "switch0" "0x02"
	ucidef_set_led_switch "wan" "WAN" "$boardname:green:wan" "switch0" "0x10"
	;;
zorlik,zl5900v2)
	ucidef_set_led_netdev "lan" "lan" "$boardname:green:lan" eth0
	;;
zyxel,keenetic-extra-ii)
	set_wifi_led "$boardname:green:wifi"
	ucidef_set_led_switch "internet" "internet" "$boardname:green:internet" "switch0" "0x01"
	;;
youku-yk1)
	set_wifi_led "$boardname:blue:air"
	ucidef_set_led_switch "wan" "wan" "$boardname:blue:wan" "switch0" "0x10"
	;;
esac

board_config_flush

exit 0
