From 43c0810969b4aee4e7a836212bc2eb8987f31d8a Mon Sep 17 00:00:00 2001
From: Matthias Reichl <hias@horus.com>
Date: Fri, 2 Feb 2018 20:30:42 +0100
Subject: [PATCH 211/454] ASoC: allo-piano-dac-plus: fix S24_LE format

Remove set_bclk_ratio call so 24-bit data is transmitted in
24 bclk cycles.

Signed-off-by: Matthias Reichl <hias@horus.com>
---
 sound/soc/bcm/allo-piano-dac-plus.c | 5 -----
 1 file changed, 5 deletions(-)

--- a/sound/soc/bcm/allo-piano-dac-plus.c
+++ b/sound/soc/bcm/allo-piano-dac-plus.c
@@ -795,9 +795,6 @@ static int snd_allo_piano_dac_hw_params(
 		struct snd_pcm_hw_params *params)
 {
 	struct snd_soc_pcm_runtime *rtd = substream->private_data;
-	struct snd_soc_dai *cpu_dai = rtd->cpu_dai;
-	unsigned int sample_bits =
-		snd_pcm_format_physical_width(params_format(params));
 	unsigned int rate = params_rate(params);
 	struct snd_soc_card *card = rtd->card;
 	struct glb_pool *glb_ptr = card->drvdata;
@@ -839,8 +836,6 @@ static int snd_allo_piano_dac_hw_params(
 	if (ret < 0)
 		return ret;
 
-	ret = snd_soc_dai_set_bclk_ratio(cpu_dai, sample_bits * 2);
-
 	return ret;
 }
 
