/dts-v1/;

#include "VR200.dtsi"

/ {
	compatible = "tplink,vr200v", "lantiq,xway", "lantiq,vr9";
	model = "TP-LINK Archer VR200v";

	chosen {
		bootargs = "console=ttyLTQ0,115200 mem=126M vpe1_load_addr=0x87e00000 vpe1_mem=2M maxvpes=1 maxtcs=1 nosmp";
	};

	aliases {
		led-boot = &power;
		led-failsafe = &power;
		led-running = &power;
		led-upgrade = &power;

		led-dsl = &dsl;
		led-internet = &internet;
		led-wifi = &wlan5g;

		led-usb = &led_usb;
		led-usb2 = &led_usb;
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <100>;
		reset {
			label = "reset";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wifi {
			label = "wifi";
			gpios = <&gpio 0 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_RFKILL>;
			linux,input-type = <EV_SW>;
		};

		wps {
			label = "wps";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		dect_paging {
			label = "dect_paging";
			gpios = <&gpio 39 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_PHONE>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";
		power: power {
			label = "vr200v:blue:power";
			gpios = <&gpio 46 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		dsl: dsl {
			label = "vr200v:blue:dsl";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};
		internet: internet {
			label = "vr200v:blue:internet";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};
		led_usb: usb {
			label = "vr200v:blue:usb";
			gpios = <&gpio 25 GPIO_ACTIVE_LOW>;
		};
		eth {
			label = "vr200v:blue:lan";
			gpios = <&gpio 40 GPIO_ACTIVE_LOW>;
		};
		wlan {
			label = "vr200v:blue:wlan";
			gpios = <&gpio 24 GPIO_ACTIVE_LOW>;
		};
		wlan5g: wifi {
			label = "vr200v:blue:wlan5g";
			gpios = <&gpio 20 GPIO_ACTIVE_LOW>;
		};
		phone {
			label = "vr200v:blue:phone";
			gpios = <&gpio 44 GPIO_ACTIVE_LOW>;
		};
	};	
};

&vmmc {
	status = "okay";
	gpios = <&gpio 30 GPIO_ACTIVE_HIGH  //fxs relay
			 &gpio 31 GPIO_ACTIVE_HIGH  //still unknown
			 &gpio 3  GPIO_ACTIVE_HIGH>; //reset_slic?
};
