From ab58c737bc723f52e787e1767bbbf0fcbe39a27b Mon Sep 17 00:00:00 2001
From: Biwen Li <biwen.li@nxp.com>
Date: Wed, 17 Apr 2019 18:58:43 +0800
Subject: [PATCH] mc-bus: support layerscape
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This is an integrated patch of mc-bus for layerscape

Signed-off-by: Bharat Bhushan <Bharat.Bhushan@nxp.com>
Signed-off-by: Biwen Li <biwen.li@nxp.com>
Signed-off-by: Bogdan Purcareata <bogdan.purcareata@nxp.com>
Signed-off-by: Cristian Sovaiala <cristian.sovaiala@freescale.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
Signed-off-by: Guanhua Gao <guanhua.gao@nxp.com>
Signed-off-by: Horia Geantă <horia.geanta@nxp.com>
Signed-off-by: Ioana Ciornei <ioana.ciornei@nxp.com>
Signed-off-by: Ioana Radulescu <ruxandra.radulescu@nxp.com>
Signed-off-by: J. German Rivera <German.Rivera@freescale.com>
Signed-off-by: Laurentiu Tudor <laurentiu.tudor@nxp.com>
Signed-off-by: Lijun Pan <Lijun.Pan@freescale.com>
Signed-off-by: Nipun Gupta <nipun.gupta@nxp.com>
Signed-off-by: Radu Alexe <radu.alexe@nxp.com>
Signed-off-by: Razvan Stefanescu <razvan.stefanescu@nxp.com>
Signed-off-by: Roy Pledge <roy.pledge@nxp.com>
Signed-off-by: Stuart Yoder <stuart.yoder@nxp.com>
---
 drivers/bus/Kconfig                           |    2 +
 drivers/bus/Makefile                          |    4 +
 drivers/bus/fsl-mc/Kconfig                    |   23 +
 drivers/bus/fsl-mc/Makefile                   |   21 +
 .../{staging/fsl-mc/bus => bus/fsl-mc}/dpbp.c |   97 +-
 .../fsl-mc/bus => bus/fsl-mc}/dpcon.c         |  103 +-
 drivers/bus/fsl-mc/dpmcp.c                    |   99 ++
 .../fsl-mc/bus => bus/fsl-mc}/dprc-driver.c   |   96 +-
 .../{staging/fsl-mc/bus => bus/fsl-mc}/dprc.c |  289 +----
 .../bus => bus/fsl-mc}/fsl-mc-allocator.c     |  123 +-
 .../fsl-mc/bus => bus/fsl-mc}/fsl-mc-bus.c    |  322 +++++-
 .../fsl-mc/bus => bus/fsl-mc}/fsl-mc-msi.c    |   16 +-
 drivers/bus/fsl-mc/fsl-mc-private.h           |  223 ++++
 drivers/bus/fsl-mc/fsl-mc-restool.c           |  219 ++++
 .../fsl-mc/bus => bus/fsl-mc}/mc-io.c         |   51 +-
 .../fsl-mc/bus => bus/fsl-mc}/mc-sys.c        |   33 +-
 drivers/irqchip/Kconfig                       |    6 +
 drivers/irqchip/Makefile                      |    1 +
 drivers/irqchip/irq-gic-v3-its-fsl-mc-msi.c   |   98 ++
 .../staging/fsl-dpaa2/ethernet/dpaa2-eth.c    |    2 +-
 .../staging/fsl-dpaa2/ethernet/dpaa2-eth.h    |    3 +-
 drivers/staging/fsl-dpaa2/ethernet/dpni.c     |    2 +-
 drivers/staging/fsl-mc/bus/Kconfig            |   15 +-
 drivers/staging/fsl-mc/bus/Makefile           |   13 -
 drivers/staging/fsl-mc/bus/dpio/dpio-driver.c |    2 +-
 .../staging/fsl-mc/bus/dpio/dpio-service.c    |    2 +-
 drivers/staging/fsl-mc/bus/dpio/dpio.c        |   14 +-
 drivers/staging/fsl-mc/bus/dpmcp-cmd.h        |   56 -
 drivers/staging/fsl-mc/bus/dpmcp.h            |   60 -
 drivers/staging/fsl-mc/bus/dpmng-cmd.h        |   58 -
 drivers/staging/fsl-mc/bus/dprc-cmd.h         |  451 --------
 drivers/staging/fsl-mc/bus/dprc.h             |  268 -----
 .../fsl-mc/bus/irq-gic-v3-its-fsl-mc-msi.c    |    1 +
 include/linux/fsl/mc.h                        | 1029 +++++++++++++++++
 include/uapi/linux/fsl_mc.h                   |   31 +
 35 files changed, 2302 insertions(+), 1531 deletions(-)
 create mode 100644 drivers/bus/fsl-mc/Kconfig
 create mode 100644 drivers/bus/fsl-mc/Makefile
 rename drivers/{staging/fsl-mc/bus => bus/fsl-mc}/dpbp.c (67%)
 rename drivers/{staging/fsl-mc/bus => bus/fsl-mc}/dpcon.c (70%)
 create mode 100644 drivers/bus/fsl-mc/dpmcp.c
 rename drivers/{staging/fsl-mc/bus => bus/fsl-mc}/dprc-driver.c (93%)
 rename drivers/{staging/fsl-mc/bus => bus/fsl-mc}/dprc.c (68%)
 rename drivers/{staging/fsl-mc/bus => bus/fsl-mc}/fsl-mc-allocator.c (84%)
 rename drivers/{staging/fsl-mc/bus => bus/fsl-mc}/fsl-mc-bus.c (75%)
 rename drivers/{staging/fsl-mc/bus => bus/fsl-mc}/fsl-mc-msi.c (96%)
 create mode 100644 drivers/bus/fsl-mc/fsl-mc-private.h
 create mode 100644 drivers/bus/fsl-mc/fsl-mc-restool.c
 rename drivers/{staging/fsl-mc/bus => bus/fsl-mc}/mc-io.c (89%)
 rename drivers/{staging/fsl-mc/bus => bus/fsl-mc}/mc-sys.c (90%)
 create mode 100644 drivers/irqchip/irq-gic-v3-its-fsl-mc-msi.c
 delete mode 100644 drivers/staging/fsl-mc/bus/dpmcp-cmd.h
 delete mode 100644 drivers/staging/fsl-mc/bus/dpmcp.h
 delete mode 100644 drivers/staging/fsl-mc/bus/dpmng-cmd.h
 delete mode 100644 drivers/staging/fsl-mc/bus/dprc-cmd.h
 delete mode 100644 drivers/staging/fsl-mc/bus/dprc.h
 create mode 100644 include/linux/fsl/mc.h
 create mode 100644 include/uapi/linux/fsl_mc.h

--- a/drivers/bus/Kconfig
+++ b/drivers/bus/Kconfig
@@ -184,4 +184,6 @@ config DA8XX_MSTPRI
 	  configuration. Allows to adjust the priorities of all master
 	  peripherals.
 
+source "drivers/bus/fsl-mc/Kconfig"
+
 endmenu
--- a/drivers/bus/Makefile
+++ b/drivers/bus/Makefile
@@ -8,6 +8,10 @@ obj-$(CONFIG_ARM_CCI)		+= arm-cci.o
 obj-$(CONFIG_ARM_CCN)		+= arm-ccn.o
 
 obj-$(CONFIG_BRCMSTB_GISB_ARB)	+= brcmstb_gisb.o
+
+# DPAA2 fsl-mc bus
+obj-$(CONFIG_FSL_MC_BUS)	+= fsl-mc/
+
 obj-$(CONFIG_IMX_WEIM)		+= imx-weim.o
 obj-$(CONFIG_MIPS_CDMM)		+= mips_cdmm.o
 obj-$(CONFIG_MVEBU_MBUS) 	+= mvebu-mbus.o
--- /dev/null
+++ b/drivers/bus/fsl-mc/Kconfig
@@ -0,0 +1,23 @@
+# SPDX-License-Identifier: GPL-2.0
+#
+# DPAA2 fsl-mc bus
+#
+# Copyright (C) 2014-2016 Freescale Semiconductor, Inc.
+#
+
+config FSL_MC_BUS
+	bool "QorIQ DPAA2 fsl-mc bus driver"
+	depends on OF && (ARCH_LAYERSCAPE || (COMPILE_TEST && (ARM || ARM64 || X86 || PPC)))
+	select GENERIC_MSI_IRQ_DOMAIN
+	help
+	  Driver to enable the bus infrastructure for the QorIQ DPAA2
+	  architecture.  The fsl-mc bus driver handles discovery of
+	  DPAA2 objects (which are represented as Linux devices) and
+	  binding objects to drivers.
+
+config FSL_MC_RESTOOL
+	bool "Management Complex (MC) restool support"
+	depends on FSL_MC_BUS
+	help
+	  Provides kernel support for the Management Complex resource
+	  manager user-space tool - restool.
--- /dev/null
+++ b/drivers/bus/fsl-mc/Makefile
@@ -0,0 +1,21 @@
+# SPDX-License-Identifier: GPL-2.0
+#
+# Freescale Management Complex (MC) bus drivers
+#
+# Copyright (C) 2014 Freescale Semiconductor, Inc.
+#
+obj-$(CONFIG_FSL_MC_BUS) += mc-bus-driver.o
+
+mc-bus-driver-objs := fsl-mc-bus.o \
+		      mc-sys.o \
+		      mc-io.o \
+		      dpbp.o \
+		      dpcon.o \
+		      dprc.o \
+		      dprc-driver.o \
+		      fsl-mc-allocator.o \
+		      fsl-mc-msi.o \
+		      dpmcp.o
+
+# MC restool kernel support
+obj-$(CONFIG_FSL_MC_RESTOOL) += fsl-mc-restool.o
--- a/drivers/staging/fsl-mc/bus/dpbp.c
+++ /dev/null
@@ -1,253 +0,0 @@
-// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
-/*
- * Copyright 2013-2016 Freescale Semiconductor Inc.
- *
- */
-#include <linux/kernel.h>
-#include "../include/mc.h"
-#include "../include/dpbp.h"
-
-#include "dpbp-cmd.h"
-
-/**
- * dpbp_open() - Open a control session for the specified object.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @dpbp_id:	DPBP unique ID
- * @token:	Returned token; use in subsequent API calls
- *
- * This function can be used to open a control session for an
- * already created object; an object may have been declared in
- * the DPL or by calling the dpbp_create function.
- * This function returns a unique authentication token,
- * associated with the specific object ID and the specific MC
- * portal; this token must be used in all subsequent commands for
- * this specific object
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dpbp_open(struct fsl_mc_io *mc_io,
-	      u32 cmd_flags,
-	      int dpbp_id,
-	      u16 *token)
-{
-	struct mc_command cmd = { 0 };
-	struct dpbp_cmd_open *cmd_params;
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPBP_CMDID_OPEN,
-					  cmd_flags, 0);
-	cmd_params = (struct dpbp_cmd_open *)cmd.params;
-	cmd_params->dpbp_id = cpu_to_le32(dpbp_id);
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	*token = mc_cmd_hdr_read_token(&cmd);
-
-	return err;
-}
-EXPORT_SYMBOL(dpbp_open);
-
-/**
- * dpbp_close() - Close the control session of the object
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPBP object
- *
- * After this function is called, no further operations are
- * allowed on the object without opening a new control session.
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dpbp_close(struct fsl_mc_io *mc_io,
-	       u32 cmd_flags,
-	       u16 token)
-{
-	struct mc_command cmd = { 0 };
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPBP_CMDID_CLOSE, cmd_flags,
-					  token);
-
-	/* send command to mc*/
-	return mc_send_command(mc_io, &cmd);
-}
-EXPORT_SYMBOL(dpbp_close);
-
-/**
- * dpbp_enable() - Enable the DPBP.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPBP object
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dpbp_enable(struct fsl_mc_io *mc_io,
-		u32 cmd_flags,
-		u16 token)
-{
-	struct mc_command cmd = { 0 };
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPBP_CMDID_ENABLE, cmd_flags,
-					  token);
-
-	/* send command to mc*/
-	return mc_send_command(mc_io, &cmd);
-}
-EXPORT_SYMBOL(dpbp_enable);
-
-/**
- * dpbp_disable() - Disable the DPBP.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPBP object
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dpbp_disable(struct fsl_mc_io *mc_io,
-		 u32 cmd_flags,
-		 u16 token)
-{
-	struct mc_command cmd = { 0 };
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPBP_CMDID_DISABLE,
-					  cmd_flags, token);
-
-	/* send command to mc*/
-	return mc_send_command(mc_io, &cmd);
-}
-EXPORT_SYMBOL(dpbp_disable);
-
-/**
- * dpbp_is_enabled() - Check if the DPBP is enabled.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPBP object
- * @en:		Returns '1' if object is enabled; '0' otherwise
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dpbp_is_enabled(struct fsl_mc_io *mc_io,
-		    u32 cmd_flags,
-		    u16 token,
-		    int *en)
-{
-	struct mc_command cmd = { 0 };
-	struct dpbp_rsp_is_enabled *rsp_params;
-	int err;
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPBP_CMDID_IS_ENABLED, cmd_flags,
-					  token);
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	rsp_params = (struct dpbp_rsp_is_enabled *)cmd.params;
-	*en = rsp_params->enabled & DPBP_ENABLE;
-
-	return 0;
-}
-EXPORT_SYMBOL(dpbp_is_enabled);
-
-/**
- * dpbp_reset() - Reset the DPBP, returns the object to initial state.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPBP object
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dpbp_reset(struct fsl_mc_io *mc_io,
-	       u32 cmd_flags,
-	       u16 token)
-{
-	struct mc_command cmd = { 0 };
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPBP_CMDID_RESET,
-					  cmd_flags, token);
-
-	/* send command to mc*/
-	return mc_send_command(mc_io, &cmd);
-}
-EXPORT_SYMBOL(dpbp_reset);
-
-/**
- * dpbp_get_attributes - Retrieve DPBP attributes.
- *
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPBP object
- * @attr:	Returned object's attributes
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dpbp_get_attributes(struct fsl_mc_io *mc_io,
-			u32 cmd_flags,
-			u16 token,
-			struct dpbp_attr *attr)
-{
-	struct mc_command cmd = { 0 };
-	struct dpbp_rsp_get_attributes *rsp_params;
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPBP_CMDID_GET_ATTR,
-					  cmd_flags, token);
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	rsp_params = (struct dpbp_rsp_get_attributes *)cmd.params;
-	attr->bpid = le16_to_cpu(rsp_params->bpid);
-	attr->id = le32_to_cpu(rsp_params->id);
-
-	return 0;
-}
-EXPORT_SYMBOL(dpbp_get_attributes);
-
-/**
- * dpbp_get_api_version - Get Data Path Buffer Pool API version
- * @mc_io:	Pointer to Mc portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @major_ver:	Major version of Buffer Pool API
- * @minor_ver:	Minor version of Buffer Pool API
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dpbp_get_api_version(struct fsl_mc_io *mc_io,
-			 u32 cmd_flags,
-			 u16 *major_ver,
-			 u16 *minor_ver)
-{
-	struct mc_command cmd = { 0 };
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPBP_CMDID_GET_API_VERSION,
-					  cmd_flags, 0);
-
-	/* send command to mc */
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	mc_cmd_read_api_version(&cmd, major_ver, minor_ver);
-
-	return 0;
-}
-EXPORT_SYMBOL(dpbp_get_api_version);
--- /dev/null
+++ b/drivers/bus/fsl-mc/dpbp.c
@@ -0,0 +1,186 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * Copyright 2013-2016 Freescale Semiconductor Inc.
+ *
+ */
+#include <linux/kernel.h>
+#include <linux/fsl/mc.h>
+#include <linux/fsl/mc.h>
+
+#include "fsl-mc-private.h"
+
+/**
+ * dpbp_open() - Open a control session for the specified object.
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @dpbp_id:	DPBP unique ID
+ * @token:	Returned token; use in subsequent API calls
+ *
+ * This function can be used to open a control session for an
+ * already created object; an object may have been declared in
+ * the DPL or by calling the dpbp_create function.
+ * This function returns a unique authentication token,
+ * associated with the specific object ID and the specific MC
+ * portal; this token must be used in all subsequent commands for
+ * this specific object
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dpbp_open(struct fsl_mc_io *mc_io,
+	      u32 cmd_flags,
+	      int dpbp_id,
+	      u16 *token)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dpbp_cmd_open *cmd_params;
+	int err;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPBP_CMDID_OPEN,
+					  cmd_flags, 0);
+	cmd_params = (struct dpbp_cmd_open *)cmd.params;
+	cmd_params->dpbp_id = cpu_to_le32(dpbp_id);
+
+	/* send command to mc*/
+	err = mc_send_command(mc_io, &cmd);
+	if (err)
+		return err;
+
+	/* retrieve response parameters */
+	*token = mc_cmd_hdr_read_token(&cmd);
+
+	return err;
+}
+EXPORT_SYMBOL_GPL(dpbp_open);
+
+/**
+ * dpbp_close() - Close the control session of the object
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPBP object
+ *
+ * After this function is called, no further operations are
+ * allowed on the object without opening a new control session.
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dpbp_close(struct fsl_mc_io *mc_io,
+	       u32 cmd_flags,
+	       u16 token)
+{
+	struct fsl_mc_command cmd = { 0 };
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPBP_CMDID_CLOSE, cmd_flags,
+					  token);
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
+EXPORT_SYMBOL_GPL(dpbp_close);
+
+/**
+ * dpbp_enable() - Enable the DPBP.
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPBP object
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dpbp_enable(struct fsl_mc_io *mc_io,
+		u32 cmd_flags,
+		u16 token)
+{
+	struct fsl_mc_command cmd = { 0 };
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPBP_CMDID_ENABLE, cmd_flags,
+					  token);
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
+EXPORT_SYMBOL_GPL(dpbp_enable);
+
+/**
+ * dpbp_disable() - Disable the DPBP.
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPBP object
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dpbp_disable(struct fsl_mc_io *mc_io,
+		 u32 cmd_flags,
+		 u16 token)
+{
+	struct fsl_mc_command cmd = { 0 };
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPBP_CMDID_DISABLE,
+					  cmd_flags, token);
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
+EXPORT_SYMBOL_GPL(dpbp_disable);
+
+/**
+ * dpbp_reset() - Reset the DPBP, returns the object to initial state.
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPBP object
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dpbp_reset(struct fsl_mc_io *mc_io,
+	       u32 cmd_flags,
+	       u16 token)
+{
+	struct fsl_mc_command cmd = { 0 };
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPBP_CMDID_RESET,
+					  cmd_flags, token);
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
+EXPORT_SYMBOL_GPL(dpbp_reset);
+
+/**
+ * dpbp_get_attributes - Retrieve DPBP attributes.
+ *
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPBP object
+ * @attr:	Returned object's attributes
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dpbp_get_attributes(struct fsl_mc_io *mc_io,
+			u32 cmd_flags,
+			u16 token,
+			struct dpbp_attr *attr)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dpbp_rsp_get_attributes *rsp_params;
+	int err;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPBP_CMDID_GET_ATTR,
+					  cmd_flags, token);
+
+	/* send command to mc*/
+	err = mc_send_command(mc_io, &cmd);
+	if (err)
+		return err;
+
+	/* retrieve response parameters */
+	rsp_params = (struct dpbp_rsp_get_attributes *)cmd.params;
+	attr->bpid = le16_to_cpu(rsp_params->bpid);
+	attr->id = le32_to_cpu(rsp_params->id);
+
+	return 0;
+}
+EXPORT_SYMBOL_GPL(dpbp_get_attributes);
--- a/drivers/staging/fsl-mc/bus/dpcon.c
+++ /dev/null
@@ -1,291 +0,0 @@
-// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
-/*
- * Copyright 2013-2016 Freescale Semiconductor Inc.
- *
- */
-#include <linux/kernel.h>
-#include "../include/mc.h"
-#include "../include/dpcon.h"
-
-#include "dpcon-cmd.h"
-
-/**
- * dpcon_open() - Open a control session for the specified object
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @dpcon_id:	DPCON unique ID
- * @token:	Returned token; use in subsequent API calls
- *
- * This function can be used to open a control session for an
- * already created object; an object may have been declared in
- * the DPL or by calling the dpcon_create() function.
- * This function returns a unique authentication token,
- * associated with the specific object ID and the specific MC
- * portal; this token must be used in all subsequent commands for
- * this specific object.
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dpcon_open(struct fsl_mc_io *mc_io,
-	       u32 cmd_flags,
-	       int dpcon_id,
-	       u16 *token)
-{
-	struct mc_command cmd = { 0 };
-	struct dpcon_cmd_open *dpcon_cmd;
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPCON_CMDID_OPEN,
-					  cmd_flags,
-					  0);
-	dpcon_cmd = (struct dpcon_cmd_open *)cmd.params;
-	dpcon_cmd->dpcon_id = cpu_to_le32(dpcon_id);
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	*token = mc_cmd_hdr_read_token(&cmd);
-
-	return 0;
-}
-EXPORT_SYMBOL(dpcon_open);
-
-/**
- * dpcon_close() - Close the control session of the object
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPCON object
- *
- * After this function is called, no further operations are
- * allowed on the object without opening a new control session.
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dpcon_close(struct fsl_mc_io *mc_io,
-		u32 cmd_flags,
-		u16 token)
-{
-	struct mc_command cmd = { 0 };
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPCON_CMDID_CLOSE,
-					  cmd_flags,
-					  token);
-
-	/* send command to mc*/
-	return mc_send_command(mc_io, &cmd);
-}
-EXPORT_SYMBOL(dpcon_close);
-
-/**
- * dpcon_enable() - Enable the DPCON
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPCON object
- *
- * Return:	'0' on Success; Error code otherwise
- */
-int dpcon_enable(struct fsl_mc_io *mc_io,
-		 u32 cmd_flags,
-		 u16 token)
-{
-	struct mc_command cmd = { 0 };
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPCON_CMDID_ENABLE,
-					  cmd_flags,
-					  token);
-
-	/* send command to mc*/
-	return mc_send_command(mc_io, &cmd);
-}
-EXPORT_SYMBOL(dpcon_enable);
-
-/**
- * dpcon_disable() - Disable the DPCON
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPCON object
- *
- * Return:	'0' on Success; Error code otherwise
- */
-int dpcon_disable(struct fsl_mc_io *mc_io,
-		  u32 cmd_flags,
-		  u16 token)
-{
-	struct mc_command cmd = { 0 };
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPCON_CMDID_DISABLE,
-					  cmd_flags,
-					  token);
-
-	/* send command to mc*/
-	return mc_send_command(mc_io, &cmd);
-}
-EXPORT_SYMBOL(dpcon_disable);
-
-/**
- * dpcon_is_enabled() -	Check if the DPCON is enabled.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPCON object
- * @en:		Returns '1' if object is enabled; '0' otherwise
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dpcon_is_enabled(struct fsl_mc_io *mc_io,
-		     u32 cmd_flags,
-		     u16 token,
-		     int *en)
-{
-	struct mc_command cmd = { 0 };
-	struct dpcon_rsp_is_enabled *dpcon_rsp;
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPCON_CMDID_IS_ENABLED,
-					  cmd_flags,
-					  token);
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	dpcon_rsp = (struct dpcon_rsp_is_enabled *)cmd.params;
-	*en = dpcon_rsp->enabled & DPCON_ENABLE;
-
-	return 0;
-}
-EXPORT_SYMBOL(dpcon_is_enabled);
-
-/**
- * dpcon_reset() - Reset the DPCON, returns the object to initial state.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPCON object
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dpcon_reset(struct fsl_mc_io *mc_io,
-		u32 cmd_flags,
-		u16 token)
-{
-	struct mc_command cmd = { 0 };
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPCON_CMDID_RESET,
-					  cmd_flags, token);
-
-	/* send command to mc*/
-	return mc_send_command(mc_io, &cmd);
-}
-EXPORT_SYMBOL(dpcon_reset);
-
-/**
- * dpcon_get_attributes() - Retrieve DPCON attributes.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPCON object
- * @attr:	Object's attributes
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dpcon_get_attributes(struct fsl_mc_io *mc_io,
-			 u32 cmd_flags,
-			 u16 token,
-			 struct dpcon_attr *attr)
-{
-	struct mc_command cmd = { 0 };
-	struct dpcon_rsp_get_attr *dpcon_rsp;
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPCON_CMDID_GET_ATTR,
-					  cmd_flags,
-					  token);
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	dpcon_rsp = (struct dpcon_rsp_get_attr *)cmd.params;
-	attr->id = le32_to_cpu(dpcon_rsp->id);
-	attr->qbman_ch_id = le16_to_cpu(dpcon_rsp->qbman_ch_id);
-	attr->num_priorities = dpcon_rsp->num_priorities;
-
-	return 0;
-}
-EXPORT_SYMBOL(dpcon_get_attributes);
-
-/**
- * dpcon_set_notification() - Set DPCON notification destination
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPCON object
- * @cfg:	Notification parameters
- *
- * Return:	'0' on Success; Error code otherwise
- */
-int dpcon_set_notification(struct fsl_mc_io *mc_io,
-			   u32 cmd_flags,
-			   u16 token,
-			   struct dpcon_notification_cfg *cfg)
-{
-	struct mc_command cmd = { 0 };
-	struct dpcon_cmd_set_notification *dpcon_cmd;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPCON_CMDID_SET_NOTIFICATION,
-					  cmd_flags,
-					  token);
-	dpcon_cmd = (struct dpcon_cmd_set_notification *)cmd.params;
-	dpcon_cmd->dpio_id = cpu_to_le32(cfg->dpio_id);
-	dpcon_cmd->priority = cfg->priority;
-	dpcon_cmd->user_ctx = cpu_to_le64(cfg->user_ctx);
-
-	/* send command to mc*/
-	return mc_send_command(mc_io, &cmd);
-}
-EXPORT_SYMBOL(dpcon_set_notification);
-
-/**
- * dpcon_get_api_version - Get Data Path Concentrator API version
- * @mc_io:	Pointer to MC portal's DPCON object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @major_ver:	Major version of DPCON API
- * @minor_ver:	Minor version of DPCON API
- *
- * Return:	'0' on Success; Error code otherwise
- */
-int dpcon_get_api_version(struct fsl_mc_io *mc_io,
-			  u32 cmd_flags,
-			  u16 *major_ver,
-			  u16 *minor_ver)
-{
-	struct mc_command cmd = { 0 };
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPCON_CMDID_GET_API_VERSION,
-					  cmd_flags, 0);
-
-	/* send command to mc */
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	mc_cmd_read_api_version(&cmd, major_ver, minor_ver);
-
-	return 0;
-}
-EXPORT_SYMBOL(dpcon_get_api_version);
--- /dev/null
+++ b/drivers/bus/fsl-mc/dpcon.c
@@ -0,0 +1,222 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * Copyright 2013-2016 Freescale Semiconductor Inc.
+ *
+ */
+#include <linux/kernel.h>
+#include <linux/fsl/mc.h>
+#include <linux/fsl/mc.h>
+
+#include "fsl-mc-private.h"
+
+/**
+ * dpcon_open() - Open a control session for the specified object
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @dpcon_id:	DPCON unique ID
+ * @token:	Returned token; use in subsequent API calls
+ *
+ * This function can be used to open a control session for an
+ * already created object; an object may have been declared in
+ * the DPL or by calling the dpcon_create() function.
+ * This function returns a unique authentication token,
+ * associated with the specific object ID and the specific MC
+ * portal; this token must be used in all subsequent commands for
+ * this specific object.
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dpcon_open(struct fsl_mc_io *mc_io,
+	       u32 cmd_flags,
+	       int dpcon_id,
+	       u16 *token)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dpcon_cmd_open *dpcon_cmd;
+	int err;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPCON_CMDID_OPEN,
+					  cmd_flags,
+					  0);
+	dpcon_cmd = (struct dpcon_cmd_open *)cmd.params;
+	dpcon_cmd->dpcon_id = cpu_to_le32(dpcon_id);
+
+	/* send command to mc*/
+	err = mc_send_command(mc_io, &cmd);
+	if (err)
+		return err;
+
+	/* retrieve response parameters */
+	*token = mc_cmd_hdr_read_token(&cmd);
+
+	return 0;
+}
+EXPORT_SYMBOL_GPL(dpcon_open);
+
+/**
+ * dpcon_close() - Close the control session of the object
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPCON object
+ *
+ * After this function is called, no further operations are
+ * allowed on the object without opening a new control session.
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dpcon_close(struct fsl_mc_io *mc_io,
+		u32 cmd_flags,
+		u16 token)
+{
+	struct fsl_mc_command cmd = { 0 };
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPCON_CMDID_CLOSE,
+					  cmd_flags,
+					  token);
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
+EXPORT_SYMBOL_GPL(dpcon_close);
+
+/**
+ * dpcon_enable() - Enable the DPCON
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPCON object
+ *
+ * Return:	'0' on Success; Error code otherwise
+ */
+int dpcon_enable(struct fsl_mc_io *mc_io,
+		 u32 cmd_flags,
+		 u16 token)
+{
+	struct fsl_mc_command cmd = { 0 };
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPCON_CMDID_ENABLE,
+					  cmd_flags,
+					  token);
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
+EXPORT_SYMBOL_GPL(dpcon_enable);
+
+/**
+ * dpcon_disable() - Disable the DPCON
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPCON object
+ *
+ * Return:	'0' on Success; Error code otherwise
+ */
+int dpcon_disable(struct fsl_mc_io *mc_io,
+		  u32 cmd_flags,
+		  u16 token)
+{
+	struct fsl_mc_command cmd = { 0 };
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPCON_CMDID_DISABLE,
+					  cmd_flags,
+					  token);
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
+EXPORT_SYMBOL_GPL(dpcon_disable);
+
+/**
+ * dpcon_reset() - Reset the DPCON, returns the object to initial state.
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPCON object
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dpcon_reset(struct fsl_mc_io *mc_io,
+		u32 cmd_flags,
+		u16 token)
+{
+	struct fsl_mc_command cmd = { 0 };
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPCON_CMDID_RESET,
+					  cmd_flags, token);
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
+EXPORT_SYMBOL_GPL(dpcon_reset);
+
+/**
+ * dpcon_get_attributes() - Retrieve DPCON attributes.
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPCON object
+ * @attr:	Object's attributes
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dpcon_get_attributes(struct fsl_mc_io *mc_io,
+			 u32 cmd_flags,
+			 u16 token,
+			 struct dpcon_attr *attr)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dpcon_rsp_get_attr *dpcon_rsp;
+	int err;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPCON_CMDID_GET_ATTR,
+					  cmd_flags,
+					  token);
+
+	/* send command to mc*/
+	err = mc_send_command(mc_io, &cmd);
+	if (err)
+		return err;
+
+	/* retrieve response parameters */
+	dpcon_rsp = (struct dpcon_rsp_get_attr *)cmd.params;
+	attr->id = le32_to_cpu(dpcon_rsp->id);
+	attr->qbman_ch_id = le16_to_cpu(dpcon_rsp->qbman_ch_id);
+	attr->num_priorities = dpcon_rsp->num_priorities;
+
+	return 0;
+}
+EXPORT_SYMBOL_GPL(dpcon_get_attributes);
+
+/**
+ * dpcon_set_notification() - Set DPCON notification destination
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPCON object
+ * @cfg:	Notification parameters
+ *
+ * Return:	'0' on Success; Error code otherwise
+ */
+int dpcon_set_notification(struct fsl_mc_io *mc_io,
+			   u32 cmd_flags,
+			   u16 token,
+			   struct dpcon_notification_cfg *cfg)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dpcon_cmd_set_notification *dpcon_cmd;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPCON_CMDID_SET_NOTIFICATION,
+					  cmd_flags,
+					  token);
+	dpcon_cmd = (struct dpcon_cmd_set_notification *)cmd.params;
+	dpcon_cmd->dpio_id = cpu_to_le32(cfg->dpio_id);
+	dpcon_cmd->priority = cfg->priority;
+	dpcon_cmd->user_ctx = cpu_to_le64(cfg->user_ctx);
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
+EXPORT_SYMBOL_GPL(dpcon_set_notification);
--- /dev/null
+++ b/drivers/bus/fsl-mc/dpmcp.c
@@ -0,0 +1,99 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * Copyright 2013-2016 Freescale Semiconductor Inc.
+ *
+ */
+#include <linux/kernel.h>
+#include <linux/fsl/mc.h>
+
+#include "fsl-mc-private.h"
+
+/**
+ * dpmcp_open() - Open a control session for the specified object.
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @dpmcp_id:	DPMCP unique ID
+ * @token:	Returned token; use in subsequent API calls
+ *
+ * This function can be used to open a control session for an
+ * already created object; an object may have been declared in
+ * the DPL or by calling the dpmcp_create function.
+ * This function returns a unique authentication token,
+ * associated with the specific object ID and the specific MC
+ * portal; this token must be used in all subsequent commands for
+ * this specific object
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dpmcp_open(struct fsl_mc_io *mc_io,
+	       u32 cmd_flags,
+	       int dpmcp_id,
+	       u16 *token)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dpmcp_cmd_open *cmd_params;
+	int err;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPMCP_CMDID_OPEN,
+					  cmd_flags, 0);
+	cmd_params = (struct dpmcp_cmd_open *)cmd.params;
+	cmd_params->dpmcp_id = cpu_to_le32(dpmcp_id);
+
+	/* send command to mc*/
+	err = mc_send_command(mc_io, &cmd);
+	if (err)
+		return err;
+
+	/* retrieve response parameters */
+	*token = mc_cmd_hdr_read_token(&cmd);
+
+	return err;
+}
+
+/**
+ * dpmcp_close() - Close the control session of the object
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPMCP object
+ *
+ * After this function is called, no further operations are
+ * allowed on the object without opening a new control session.
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dpmcp_close(struct fsl_mc_io *mc_io,
+		u32 cmd_flags,
+		u16 token)
+{
+	struct fsl_mc_command cmd = { 0 };
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPMCP_CMDID_CLOSE,
+					  cmd_flags, token);
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
+
+/**
+ * dpmcp_reset() - Reset the DPMCP, returns the object to initial state.
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPMCP object
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dpmcp_reset(struct fsl_mc_io *mc_io,
+		u32 cmd_flags,
+		u16 token)
+{
+	struct fsl_mc_command cmd = { 0 };
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPMCP_CMDID_RESET,
+					  cmd_flags, token);
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
--- a/drivers/staging/fsl-mc/bus/dprc-driver.c
+++ /dev/null
@@ -1,813 +0,0 @@
-// SPDX-License-Identifier: GPL-2.0
-/*
- * Freescale data path resource container (DPRC) driver
- *
- * Copyright (C) 2014-2016 Freescale Semiconductor, Inc.
- * Author: German Rivera <German.Rivera@freescale.com>
- *
- */
-
-#include <linux/module.h>
-#include <linux/slab.h>
-#include <linux/interrupt.h>
-#include <linux/msi.h>
-#include "../include/mc.h"
-
-#include "dprc-cmd.h"
-#include "fsl-mc-private.h"
-
-#define FSL_MC_DPRC_DRIVER_NAME    "fsl_mc_dprc"
-
-struct fsl_mc_child_objs {
-	int child_count;
-	struct fsl_mc_obj_desc *child_array;
-};
-
-static bool fsl_mc_device_match(struct fsl_mc_device *mc_dev,
-				struct fsl_mc_obj_desc *obj_desc)
-{
-	return mc_dev->obj_desc.id == obj_desc->id &&
-	       strcmp(mc_dev->obj_desc.type, obj_desc->type) == 0;
-
-}
-
-static int __fsl_mc_device_remove_if_not_in_mc(struct device *dev, void *data)
-{
-	int i;
-	struct fsl_mc_child_objs *objs;
-	struct fsl_mc_device *mc_dev;
-
-	WARN_ON(!dev);
-	WARN_ON(!data);
-	mc_dev = to_fsl_mc_device(dev);
-	objs = data;
-
-	for (i = 0; i < objs->child_count; i++) {
-		struct fsl_mc_obj_desc *obj_desc = &objs->child_array[i];
-
-		if (strlen(obj_desc->type) != 0 &&
-		    fsl_mc_device_match(mc_dev, obj_desc))
-			break;
-	}
-
-	if (i == objs->child_count)
-		fsl_mc_device_remove(mc_dev);
-
-	return 0;
-}
-
-static int __fsl_mc_device_remove(struct device *dev, void *data)
-{
-	WARN_ON(!dev);
-	WARN_ON(data);
-	fsl_mc_device_remove(to_fsl_mc_device(dev));
-	return 0;
-}
-
-/**
- * dprc_remove_devices - Removes devices for objects removed from a DPRC
- *
- * @mc_bus_dev: pointer to the fsl-mc device that represents a DPRC object
- * @obj_desc_array: array of object descriptors for child objects currently
- * present in the DPRC in the MC.
- * @num_child_objects_in_mc: number of entries in obj_desc_array
- *
- * Synchronizes the state of the Linux bus driver with the actual state of
- * the MC by removing devices that represent MC objects that have
- * been dynamically removed in the physical DPRC.
- */
-static void dprc_remove_devices(struct fsl_mc_device *mc_bus_dev,
-				struct fsl_mc_obj_desc *obj_desc_array,
-				int num_child_objects_in_mc)
-{
-	if (num_child_objects_in_mc != 0) {
-		/*
-		 * Remove child objects that are in the DPRC in Linux,
-		 * but not in the MC:
-		 */
-		struct fsl_mc_child_objs objs;
-
-		objs.child_count = num_child_objects_in_mc;
-		objs.child_array = obj_desc_array;
-		device_for_each_child(&mc_bus_dev->dev, &objs,
-				      __fsl_mc_device_remove_if_not_in_mc);
-	} else {
-		/*
-		 * There are no child objects for this DPRC in the MC.
-		 * So, remove all the child devices from Linux:
-		 */
-		device_for_each_child(&mc_bus_dev->dev, NULL,
-				      __fsl_mc_device_remove);
-	}
-}
-
-static int __fsl_mc_device_match(struct device *dev, void *data)
-{
-	struct fsl_mc_obj_desc *obj_desc = data;
-	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
-
-	return fsl_mc_device_match(mc_dev, obj_desc);
-}
-
-static struct fsl_mc_device *fsl_mc_device_lookup(struct fsl_mc_obj_desc
-								*obj_desc,
-						  struct fsl_mc_device
-								*mc_bus_dev)
-{
-	struct device *dev;
-
-	dev = device_find_child(&mc_bus_dev->dev, obj_desc,
-				__fsl_mc_device_match);
-
-	return dev ? to_fsl_mc_device(dev) : NULL;
-}
-
-/**
- * check_plugged_state_change - Check change in an MC object's plugged state
- *
- * @mc_dev: pointer to the fsl-mc device for a given MC object
- * @obj_desc: pointer to the MC object's descriptor in the MC
- *
- * If the plugged state has changed from unplugged to plugged, the fsl-mc
- * device is bound to the corresponding device driver.
- * If the plugged state has changed from plugged to unplugged, the fsl-mc
- * device is unbound from the corresponding device driver.
- */
-static void check_plugged_state_change(struct fsl_mc_device *mc_dev,
-				       struct fsl_mc_obj_desc *obj_desc)
-{
-	int error;
-	u32 plugged_flag_at_mc =
-			obj_desc->state & FSL_MC_OBJ_STATE_PLUGGED;
-
-	if (plugged_flag_at_mc !=
-	    (mc_dev->obj_desc.state & FSL_MC_OBJ_STATE_PLUGGED)) {
-		if (plugged_flag_at_mc) {
-			mc_dev->obj_desc.state |= FSL_MC_OBJ_STATE_PLUGGED;
-			error = device_attach(&mc_dev->dev);
-			if (error < 0) {
-				dev_err(&mc_dev->dev,
-					"device_attach() failed: %d\n",
-					error);
-			}
-		} else {
-			mc_dev->obj_desc.state &= ~FSL_MC_OBJ_STATE_PLUGGED;
-			device_release_driver(&mc_dev->dev);
-		}
-	}
-}
-
-/**
- * dprc_add_new_devices - Adds devices to the logical bus for a DPRC
- *
- * @mc_bus_dev: pointer to the fsl-mc device that represents a DPRC object
- * @obj_desc_array: array of device descriptors for child devices currently
- * present in the physical DPRC.
- * @num_child_objects_in_mc: number of entries in obj_desc_array
- *
- * Synchronizes the state of the Linux bus driver with the actual
- * state of the MC by adding objects that have been newly discovered
- * in the physical DPRC.
- */
-static void dprc_add_new_devices(struct fsl_mc_device *mc_bus_dev,
-				 struct fsl_mc_obj_desc *obj_desc_array,
-				 int num_child_objects_in_mc)
-{
-	int error;
-	int i;
-
-	for (i = 0; i < num_child_objects_in_mc; i++) {
-		struct fsl_mc_device *child_dev;
-		struct fsl_mc_obj_desc *obj_desc = &obj_desc_array[i];
-
-		if (strlen(obj_desc->type) == 0)
-			continue;
-
-		/*
-		 * Check if device is already known to Linux:
-		 */
-		child_dev = fsl_mc_device_lookup(obj_desc, mc_bus_dev);
-		if (child_dev) {
-			check_plugged_state_change(child_dev, obj_desc);
-			put_device(&child_dev->dev);
-			continue;
-		}
-
-		error = fsl_mc_device_add(obj_desc, NULL, &mc_bus_dev->dev,
-					  &child_dev);
-		if (error < 0)
-			continue;
-	}
-}
-
-/**
- * dprc_scan_objects - Discover objects in a DPRC
- *
- * @mc_bus_dev: pointer to the fsl-mc device that represents a DPRC object
- * @total_irq_count: total number of IRQs needed by objects in the DPRC.
- *
- * Detects objects added and removed from a DPRC and synchronizes the
- * state of the Linux bus driver, MC by adding and removing
- * devices accordingly.
- * Two types of devices can be found in a DPRC: allocatable objects (e.g.,
- * dpbp, dpmcp) and non-allocatable devices (e.g., dprc, dpni).
- * All allocatable devices needed to be probed before all non-allocatable
- * devices, to ensure that device drivers for non-allocatable
- * devices can allocate any type of allocatable devices.
- * That is, we need to ensure that the corresponding resource pools are
- * populated before they can get allocation requests from probe callbacks
- * of the device drivers for the non-allocatable devices.
- */
-static int dprc_scan_objects(struct fsl_mc_device *mc_bus_dev,
-			     unsigned int *total_irq_count)
-{
-	int num_child_objects;
-	int dprc_get_obj_failures;
-	int error;
-	unsigned int irq_count = mc_bus_dev->obj_desc.irq_count;
-	struct fsl_mc_obj_desc *child_obj_desc_array = NULL;
-
-	error = dprc_get_obj_count(mc_bus_dev->mc_io,
-				   0,
-				   mc_bus_dev->mc_handle,
-				   &num_child_objects);
-	if (error < 0) {
-		dev_err(&mc_bus_dev->dev, "dprc_get_obj_count() failed: %d\n",
-			error);
-		return error;
-	}
-
-	if (num_child_objects != 0) {
-		int i;
-
-		child_obj_desc_array =
-		    devm_kmalloc_array(&mc_bus_dev->dev, num_child_objects,
-				       sizeof(*child_obj_desc_array),
-				       GFP_KERNEL);
-		if (!child_obj_desc_array)
-			return -ENOMEM;
-
-		/*
-		 * Discover objects currently present in the physical DPRC:
-		 */
-		dprc_get_obj_failures = 0;
-		for (i = 0; i < num_child_objects; i++) {
-			struct fsl_mc_obj_desc *obj_desc =
-			    &child_obj_desc_array[i];
-
-			error = dprc_get_obj(mc_bus_dev->mc_io,
-					     0,
-					     mc_bus_dev->mc_handle,
-					     i, obj_desc);
-			if (error < 0) {
-				dev_err(&mc_bus_dev->dev,
-					"dprc_get_obj(i=%d) failed: %d\n",
-					i, error);
-				/*
-				 * Mark the obj entry as "invalid", by using the
-				 * empty string as obj type:
-				 */
-				obj_desc->type[0] = '\0';
-				obj_desc->id = error;
-				dprc_get_obj_failures++;
-				continue;
-			}
-
-			/*
-			 * add a quirk for all versions of dpsec < 4.0...none
-			 * are coherent regardless of what the MC reports.
-			 */
-			if ((strcmp(obj_desc->type, "dpseci") == 0) &&
-			    (obj_desc->ver_major < 4))
-				obj_desc->flags |=
-					FSL_MC_OBJ_FLAG_NO_MEM_SHAREABILITY;
-
-			irq_count += obj_desc->irq_count;
-			dev_dbg(&mc_bus_dev->dev,
-				"Discovered object: type %s, id %d\n",
-				obj_desc->type, obj_desc->id);
-		}
-
-		if (dprc_get_obj_failures != 0) {
-			dev_err(&mc_bus_dev->dev,
-				"%d out of %d devices could not be retrieved\n",
-				dprc_get_obj_failures, num_child_objects);
-		}
-	}
-
-	*total_irq_count = irq_count;
-	dprc_remove_devices(mc_bus_dev, child_obj_desc_array,
-			    num_child_objects);
-
-	dprc_add_new_devices(mc_bus_dev, child_obj_desc_array,
-			     num_child_objects);
-
-	if (child_obj_desc_array)
-		devm_kfree(&mc_bus_dev->dev, child_obj_desc_array);
-
-	return 0;
-}
-
-/**
- * dprc_scan_container - Scans a physical DPRC and synchronizes Linux bus state
- *
- * @mc_bus_dev: pointer to the fsl-mc device that represents a DPRC object
- *
- * Scans the physical DPRC and synchronizes the state of the Linux
- * bus driver with the actual state of the MC by adding and removing
- * devices as appropriate.
- */
-static int dprc_scan_container(struct fsl_mc_device *mc_bus_dev)
-{
-	int error;
-	unsigned int irq_count;
-	struct fsl_mc_bus *mc_bus = to_fsl_mc_bus(mc_bus_dev);
-
-	fsl_mc_init_all_resource_pools(mc_bus_dev);
-
-	/*
-	 * Discover objects in the DPRC:
-	 */
-	mutex_lock(&mc_bus->scan_mutex);
-	error = dprc_scan_objects(mc_bus_dev, &irq_count);
-	mutex_unlock(&mc_bus->scan_mutex);
-	if (error < 0)
-		goto error;
-
-	if (dev_get_msi_domain(&mc_bus_dev->dev) && !mc_bus->irq_resources) {
-		if (irq_count > FSL_MC_IRQ_POOL_MAX_TOTAL_IRQS) {
-			dev_warn(&mc_bus_dev->dev,
-				 "IRQs needed (%u) exceed IRQs preallocated (%u)\n",
-				 irq_count, FSL_MC_IRQ_POOL_MAX_TOTAL_IRQS);
-		}
-
-		error = fsl_mc_populate_irq_pool(
-				mc_bus,
-				FSL_MC_IRQ_POOL_MAX_TOTAL_IRQS);
-		if (error < 0)
-			goto error;
-	}
-
-	return 0;
-error:
-	fsl_mc_cleanup_all_resource_pools(mc_bus_dev);
-	return error;
-}
-
-/**
- * dprc_irq0_handler - Regular ISR for DPRC interrupt 0
- *
- * @irq: IRQ number of the interrupt being handled
- * @arg: Pointer to device structure
- */
-static irqreturn_t dprc_irq0_handler(int irq_num, void *arg)
-{
-	return IRQ_WAKE_THREAD;
-}
-
-/**
- * dprc_irq0_handler_thread - Handler thread function for DPRC interrupt 0
- *
- * @irq: IRQ number of the interrupt being handled
- * @arg: Pointer to device structure
- */
-static irqreturn_t dprc_irq0_handler_thread(int irq_num, void *arg)
-{
-	int error;
-	u32 status;
-	struct device *dev = arg;
-	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
-	struct fsl_mc_bus *mc_bus = to_fsl_mc_bus(mc_dev);
-	struct fsl_mc_io *mc_io = mc_dev->mc_io;
-	struct msi_desc *msi_desc = mc_dev->irqs[0]->msi_desc;
-
-	dev_dbg(dev, "DPRC IRQ %d triggered on CPU %u\n",
-		irq_num, smp_processor_id());
-
-	if (WARN_ON(!(mc_dev->flags & FSL_MC_IS_DPRC)))
-		return IRQ_HANDLED;
-
-	mutex_lock(&mc_bus->scan_mutex);
-	if (WARN_ON(!msi_desc || msi_desc->irq != (u32)irq_num))
-		goto out;
-
-	status = 0;
-	error = dprc_get_irq_status(mc_io, 0, mc_dev->mc_handle, 0,
-				    &status);
-	if (error < 0) {
-		dev_err(dev,
-			"dprc_get_irq_status() failed: %d\n", error);
-		goto out;
-	}
-
-	error = dprc_clear_irq_status(mc_io, 0, mc_dev->mc_handle, 0,
-				      status);
-	if (error < 0) {
-		dev_err(dev,
-			"dprc_clear_irq_status() failed: %d\n", error);
-		goto out;
-	}
-
-	if (status & (DPRC_IRQ_EVENT_OBJ_ADDED |
-		      DPRC_IRQ_EVENT_OBJ_REMOVED |
-		      DPRC_IRQ_EVENT_CONTAINER_DESTROYED |
-		      DPRC_IRQ_EVENT_OBJ_DESTROYED |
-		      DPRC_IRQ_EVENT_OBJ_CREATED)) {
-		unsigned int irq_count;
-
-		error = dprc_scan_objects(mc_dev, &irq_count);
-		if (error < 0) {
-			/*
-			 * If the error is -ENXIO, we ignore it, as it indicates
-			 * that the object scan was aborted, as we detected that
-			 * an object was removed from the DPRC in the MC, while
-			 * we were scanning the DPRC.
-			 */
-			if (error != -ENXIO) {
-				dev_err(dev, "dprc_scan_objects() failed: %d\n",
-					error);
-			}
-
-			goto out;
-		}
-
-		if (irq_count > FSL_MC_IRQ_POOL_MAX_TOTAL_IRQS) {
-			dev_warn(dev,
-				 "IRQs needed (%u) exceed IRQs preallocated (%u)\n",
-				 irq_count, FSL_MC_IRQ_POOL_MAX_TOTAL_IRQS);
-		}
-	}
-
-out:
-	mutex_unlock(&mc_bus->scan_mutex);
-	return IRQ_HANDLED;
-}
-
-/*
- * Disable and clear interrupt for a given DPRC object
- */
-static int disable_dprc_irq(struct fsl_mc_device *mc_dev)
-{
-	int error;
-	struct fsl_mc_io *mc_io = mc_dev->mc_io;
-
-	WARN_ON(mc_dev->obj_desc.irq_count != 1);
-
-	/*
-	 * Disable generation of interrupt, while we configure it:
-	 */
-	error = dprc_set_irq_enable(mc_io, 0, mc_dev->mc_handle, 0, 0);
-	if (error < 0) {
-		dev_err(&mc_dev->dev,
-			"Disabling DPRC IRQ failed: dprc_set_irq_enable() failed: %d\n",
-			error);
-		return error;
-	}
-
-	/*
-	 * Disable all interrupt causes for the interrupt:
-	 */
-	error = dprc_set_irq_mask(mc_io, 0, mc_dev->mc_handle, 0, 0x0);
-	if (error < 0) {
-		dev_err(&mc_dev->dev,
-			"Disabling DPRC IRQ failed: dprc_set_irq_mask() failed: %d\n",
-			error);
-		return error;
-	}
-
-	/*
-	 * Clear any leftover interrupts:
-	 */
-	error = dprc_clear_irq_status(mc_io, 0, mc_dev->mc_handle, 0, ~0x0U);
-	if (error < 0) {
-		dev_err(&mc_dev->dev,
-			"Disabling DPRC IRQ failed: dprc_clear_irq_status() failed: %d\n",
-			error);
-		return error;
-	}
-
-	return 0;
-}
-
-static int register_dprc_irq_handler(struct fsl_mc_device *mc_dev)
-{
-	int error;
-	struct fsl_mc_device_irq *irq = mc_dev->irqs[0];
-
-	WARN_ON(mc_dev->obj_desc.irq_count != 1);
-
-	/*
-	 * NOTE: devm_request_threaded_irq() invokes the device-specific
-	 * function that programs the MSI physically in the device
-	 */
-	error = devm_request_threaded_irq(&mc_dev->dev,
-					  irq->msi_desc->irq,
-					  dprc_irq0_handler,
-					  dprc_irq0_handler_thread,
-					  IRQF_NO_SUSPEND | IRQF_ONESHOT,
-					  dev_name(&mc_dev->dev),
-					  &mc_dev->dev);
-	if (error < 0) {
-		dev_err(&mc_dev->dev,
-			"devm_request_threaded_irq() failed: %d\n",
-			error);
-		return error;
-	}
-
-	return 0;
-}
-
-static int enable_dprc_irq(struct fsl_mc_device *mc_dev)
-{
-	int error;
-
-	/*
-	 * Enable all interrupt causes for the interrupt:
-	 */
-	error = dprc_set_irq_mask(mc_dev->mc_io, 0, mc_dev->mc_handle, 0,
-				  ~0x0u);
-	if (error < 0) {
-		dev_err(&mc_dev->dev,
-			"Enabling DPRC IRQ failed: dprc_set_irq_mask() failed: %d\n",
-			error);
-
-		return error;
-	}
-
-	/*
-	 * Enable generation of the interrupt:
-	 */
-	error = dprc_set_irq_enable(mc_dev->mc_io, 0, mc_dev->mc_handle, 0, 1);
-	if (error < 0) {
-		dev_err(&mc_dev->dev,
-			"Enabling DPRC IRQ failed: dprc_set_irq_enable() failed: %d\n",
-			error);
-
-		return error;
-	}
-
-	return 0;
-}
-
-/*
- * Setup interrupt for a given DPRC device
- */
-static int dprc_setup_irq(struct fsl_mc_device *mc_dev)
-{
-	int error;
-
-	error = fsl_mc_allocate_irqs(mc_dev);
-	if (error < 0)
-		return error;
-
-	error = disable_dprc_irq(mc_dev);
-	if (error < 0)
-		goto error_free_irqs;
-
-	error = register_dprc_irq_handler(mc_dev);
-	if (error < 0)
-		goto error_free_irqs;
-
-	error = enable_dprc_irq(mc_dev);
-	if (error < 0)
-		goto error_free_irqs;
-
-	return 0;
-
-error_free_irqs:
-	fsl_mc_free_irqs(mc_dev);
-	return error;
-}
-
-/**
- * dprc_probe - callback invoked when a DPRC is being bound to this driver
- *
- * @mc_dev: Pointer to fsl-mc device representing a DPRC
- *
- * It opens the physical DPRC in the MC.
- * It scans the DPRC to discover the MC objects contained in it.
- * It creates the interrupt pool for the MC bus associated with the DPRC.
- * It configures the interrupts for the DPRC device itself.
- */
-static int dprc_probe(struct fsl_mc_device *mc_dev)
-{
-	int error;
-	size_t region_size;
-	struct device *parent_dev = mc_dev->dev.parent;
-	struct fsl_mc_bus *mc_bus = to_fsl_mc_bus(mc_dev);
-	bool mc_io_created = false;
-	bool msi_domain_set = false;
-	u16 major_ver, minor_ver;
-
-	if (WARN_ON(strcmp(mc_dev->obj_desc.type, "dprc") != 0))
-		return -EINVAL;
-
-	if (WARN_ON(dev_get_msi_domain(&mc_dev->dev)))
-		return -EINVAL;
-
-	if (!mc_dev->mc_io) {
-		/*
-		 * This is a child DPRC:
-		 */
-		if (WARN_ON(!dev_is_fsl_mc(parent_dev)))
-			return -EINVAL;
-
-		if (WARN_ON(mc_dev->obj_desc.region_count == 0))
-			return -EINVAL;
-
-		region_size = resource_size(mc_dev->regions);
-
-		error = fsl_create_mc_io(&mc_dev->dev,
-					 mc_dev->regions[0].start,
-					 region_size,
-					 NULL,
-					 FSL_MC_IO_ATOMIC_CONTEXT_PORTAL,
-					 &mc_dev->mc_io);
-		if (error < 0)
-			return error;
-
-		mc_io_created = true;
-
-		/*
-		 * Inherit parent MSI domain:
-		 */
-		dev_set_msi_domain(&mc_dev->dev,
-				   dev_get_msi_domain(parent_dev));
-		msi_domain_set = true;
-	} else {
-		/*
-		 * This is a root DPRC
-		 */
-		struct irq_domain *mc_msi_domain;
-
-		if (WARN_ON(dev_is_fsl_mc(parent_dev)))
-			return -EINVAL;
-
-		error = fsl_mc_find_msi_domain(parent_dev,
-					       &mc_msi_domain);
-		if (error < 0) {
-			dev_warn(&mc_dev->dev,
-				 "WARNING: MC bus without interrupt support\n");
-		} else {
-			dev_set_msi_domain(&mc_dev->dev, mc_msi_domain);
-			msi_domain_set = true;
-		}
-	}
-
-	error = dprc_open(mc_dev->mc_io, 0, mc_dev->obj_desc.id,
-			  &mc_dev->mc_handle);
-	if (error < 0) {
-		dev_err(&mc_dev->dev, "dprc_open() failed: %d\n", error);
-		goto error_cleanup_msi_domain;
-	}
-
-	error = dprc_get_attributes(mc_dev->mc_io, 0, mc_dev->mc_handle,
-				    &mc_bus->dprc_attr);
-	if (error < 0) {
-		dev_err(&mc_dev->dev, "dprc_get_attributes() failed: %d\n",
-			error);
-		goto error_cleanup_open;
-	}
-
-	error = dprc_get_api_version(mc_dev->mc_io, 0,
-				     &major_ver,
-				     &minor_ver);
-	if (error < 0) {
-		dev_err(&mc_dev->dev, "dprc_get_api_version() failed: %d\n",
-			error);
-		goto error_cleanup_open;
-	}
-
-	if (major_ver < DPRC_MIN_VER_MAJOR ||
-	    (major_ver == DPRC_MIN_VER_MAJOR &&
-	     minor_ver < DPRC_MIN_VER_MINOR)) {
-		dev_err(&mc_dev->dev,
-			"ERROR: DPRC version %d.%d not supported\n",
-			major_ver, minor_ver);
-		error = -ENOTSUPP;
-		goto error_cleanup_open;
-	}
-
-	mutex_init(&mc_bus->scan_mutex);
-
-	/*
-	 * Discover MC objects in DPRC object:
-	 */
-	error = dprc_scan_container(mc_dev);
-	if (error < 0)
-		goto error_cleanup_open;
-
-	/*
-	 * Configure interrupt for the DPRC object associated with this MC bus:
-	 */
-	error = dprc_setup_irq(mc_dev);
-	if (error < 0)
-		goto error_cleanup_open;
-
-	dev_info(&mc_dev->dev, "DPRC device bound to driver");
-	return 0;
-
-error_cleanup_open:
-	(void)dprc_close(mc_dev->mc_io, 0, mc_dev->mc_handle);
-
-error_cleanup_msi_domain:
-	if (msi_domain_set)
-		dev_set_msi_domain(&mc_dev->dev, NULL);
-
-	if (mc_io_created) {
-		fsl_destroy_mc_io(mc_dev->mc_io);
-		mc_dev->mc_io = NULL;
-	}
-
-	return error;
-}
-
-/*
- * Tear down interrupt for a given DPRC object
- */
-static void dprc_teardown_irq(struct fsl_mc_device *mc_dev)
-{
-	struct fsl_mc_device_irq *irq = mc_dev->irqs[0];
-
-	(void)disable_dprc_irq(mc_dev);
-
-	devm_free_irq(&mc_dev->dev, irq->msi_desc->irq, &mc_dev->dev);
-
-	fsl_mc_free_irqs(mc_dev);
-}
-
-/**
- * dprc_remove - callback invoked when a DPRC is being unbound from this driver
- *
- * @mc_dev: Pointer to fsl-mc device representing the DPRC
- *
- * It removes the DPRC's child objects from Linux (not from the MC) and
- * closes the DPRC device in the MC.
- * It tears down the interrupts that were configured for the DPRC device.
- * It destroys the interrupt pool associated with this MC bus.
- */
-static int dprc_remove(struct fsl_mc_device *mc_dev)
-{
-	int error;
-	struct fsl_mc_bus *mc_bus = to_fsl_mc_bus(mc_dev);
-
-	if (WARN_ON(strcmp(mc_dev->obj_desc.type, "dprc") != 0))
-		return -EINVAL;
-	if (WARN_ON(!mc_dev->mc_io))
-		return -EINVAL;
-
-	if (WARN_ON(!mc_bus->irq_resources))
-		return -EINVAL;
-
-	if (dev_get_msi_domain(&mc_dev->dev))
-		dprc_teardown_irq(mc_dev);
-
-	device_for_each_child(&mc_dev->dev, NULL, __fsl_mc_device_remove);
-
-	if (dev_get_msi_domain(&mc_dev->dev)) {
-		fsl_mc_cleanup_irq_pool(mc_bus);
-		dev_set_msi_domain(&mc_dev->dev, NULL);
-	}
-
-	fsl_mc_cleanup_all_resource_pools(mc_dev);
-
-	error = dprc_close(mc_dev->mc_io, 0, mc_dev->mc_handle);
-	if (error < 0)
-		dev_err(&mc_dev->dev, "dprc_close() failed: %d\n", error);
-
-	if (!fsl_mc_is_root_dprc(&mc_dev->dev)) {
-		fsl_destroy_mc_io(mc_dev->mc_io);
-		mc_dev->mc_io = NULL;
-	}
-
-	dev_info(&mc_dev->dev, "DPRC device unbound from driver");
-	return 0;
-}
-
-static const struct fsl_mc_device_id match_id_table[] = {
-	{
-	 .vendor = FSL_MC_VENDOR_FREESCALE,
-	 .obj_type = "dprc"},
-	{.vendor = 0x0},
-};
-
-static struct fsl_mc_driver dprc_driver = {
-	.driver = {
-		   .name = FSL_MC_DPRC_DRIVER_NAME,
-		   .owner = THIS_MODULE,
-		   .pm = NULL,
-		   },
-	.match_id_table = match_id_table,
-	.probe = dprc_probe,
-	.remove = dprc_remove,
-};
-
-int __init dprc_driver_init(void)
-{
-	return fsl_mc_driver_register(&dprc_driver);
-}
-
-void dprc_driver_exit(void)
-{
-	fsl_mc_driver_unregister(&dprc_driver);
-}
--- /dev/null
+++ b/drivers/bus/fsl-mc/dprc-driver.c
@@ -0,0 +1,815 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Freescale data path resource container (DPRC) driver
+ *
+ * Copyright (C) 2014-2016 Freescale Semiconductor, Inc.
+ * Author: German Rivera <German.Rivera@freescale.com>
+ *
+ */
+
+#include <linux/module.h>
+#include <linux/slab.h>
+#include <linux/interrupt.h>
+#include <linux/msi.h>
+#include <linux/fsl/mc.h>
+
+#include "fsl-mc-private.h"
+
+#define FSL_MC_DPRC_DRIVER_NAME    "fsl_mc_dprc"
+
+struct fsl_mc_child_objs {
+	int child_count;
+	struct fsl_mc_obj_desc *child_array;
+};
+
+static bool fsl_mc_device_match(struct fsl_mc_device *mc_dev,
+				struct fsl_mc_obj_desc *obj_desc)
+{
+	return mc_dev->obj_desc.id == obj_desc->id &&
+	       strcmp(mc_dev->obj_desc.type, obj_desc->type) == 0;
+
+}
+
+static int __fsl_mc_device_remove_if_not_in_mc(struct device *dev, void *data)
+{
+	int i;
+	struct fsl_mc_child_objs *objs;
+	struct fsl_mc_device *mc_dev;
+
+	mc_dev = to_fsl_mc_device(dev);
+	objs = data;
+
+	for (i = 0; i < objs->child_count; i++) {
+		struct fsl_mc_obj_desc *obj_desc = &objs->child_array[i];
+
+		if (strlen(obj_desc->type) != 0 &&
+		    fsl_mc_device_match(mc_dev, obj_desc))
+			break;
+	}
+
+	if (i == objs->child_count)
+		fsl_mc_device_remove(mc_dev);
+
+	return 0;
+}
+
+static int __fsl_mc_device_remove(struct device *dev, void *data)
+{
+	fsl_mc_device_remove(to_fsl_mc_device(dev));
+	return 0;
+}
+
+/**
+ * dprc_remove_devices - Removes devices for objects removed from a DPRC
+ *
+ * @mc_bus_dev: pointer to the fsl-mc device that represents a DPRC object
+ * @obj_desc_array: array of object descriptors for child objects currently
+ * present in the DPRC in the MC.
+ * @num_child_objects_in_mc: number of entries in obj_desc_array
+ *
+ * Synchronizes the state of the Linux bus driver with the actual state of
+ * the MC by removing devices that represent MC objects that have
+ * been dynamically removed in the physical DPRC.
+ */
+static void dprc_remove_devices(struct fsl_mc_device *mc_bus_dev,
+				struct fsl_mc_obj_desc *obj_desc_array,
+				int num_child_objects_in_mc)
+{
+	if (num_child_objects_in_mc != 0) {
+		/*
+		 * Remove child objects that are in the DPRC in Linux,
+		 * but not in the MC:
+		 */
+		struct fsl_mc_child_objs objs;
+
+		objs.child_count = num_child_objects_in_mc;
+		objs.child_array = obj_desc_array;
+		device_for_each_child(&mc_bus_dev->dev, &objs,
+				      __fsl_mc_device_remove_if_not_in_mc);
+	} else {
+		/*
+		 * There are no child objects for this DPRC in the MC.
+		 * So, remove all the child devices from Linux:
+		 */
+		device_for_each_child(&mc_bus_dev->dev, NULL,
+				      __fsl_mc_device_remove);
+	}
+}
+
+static int __fsl_mc_device_match(struct device *dev, void *data)
+{
+	struct fsl_mc_obj_desc *obj_desc = data;
+	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
+
+	return fsl_mc_device_match(mc_dev, obj_desc);
+}
+
+static struct fsl_mc_device *fsl_mc_device_lookup(struct fsl_mc_obj_desc
+								*obj_desc,
+						  struct fsl_mc_device
+								*mc_bus_dev)
+{
+	struct device *dev;
+
+	dev = device_find_child(&mc_bus_dev->dev, obj_desc,
+				__fsl_mc_device_match);
+
+	return dev ? to_fsl_mc_device(dev) : NULL;
+}
+
+/**
+ * check_plugged_state_change - Check change in an MC object's plugged state
+ *
+ * @mc_dev: pointer to the fsl-mc device for a given MC object
+ * @obj_desc: pointer to the MC object's descriptor in the MC
+ *
+ * If the plugged state has changed from unplugged to plugged, the fsl-mc
+ * device is bound to the corresponding device driver.
+ * If the plugged state has changed from plugged to unplugged, the fsl-mc
+ * device is unbound from the corresponding device driver.
+ */
+static void check_plugged_state_change(struct fsl_mc_device *mc_dev,
+				       struct fsl_mc_obj_desc *obj_desc)
+{
+	int error;
+	u32 plugged_flag_at_mc =
+			obj_desc->state & FSL_MC_OBJ_STATE_PLUGGED;
+
+	if (plugged_flag_at_mc !=
+	    (mc_dev->obj_desc.state & FSL_MC_OBJ_STATE_PLUGGED)) {
+		if (plugged_flag_at_mc) {
+			mc_dev->obj_desc.state |= FSL_MC_OBJ_STATE_PLUGGED;
+			error = device_attach(&mc_dev->dev);
+			if (error < 0) {
+				dev_err(&mc_dev->dev,
+					"device_attach() failed: %d\n",
+					error);
+			}
+		} else {
+			mc_dev->obj_desc.state &= ~FSL_MC_OBJ_STATE_PLUGGED;
+			device_release_driver(&mc_dev->dev);
+		}
+	}
+}
+
+/**
+ * dprc_add_new_devices - Adds devices to the logical bus for a DPRC
+ *
+ * @mc_bus_dev: pointer to the fsl-mc device that represents a DPRC object
+ * @driver_override: driver override to apply to new objects found in the
+ * DPRC, or NULL, if none.
+ * @obj_desc_array: array of device descriptors for child devices currently
+ * present in the physical DPRC.
+ * @num_child_objects_in_mc: number of entries in obj_desc_array
+ *
+ * Synchronizes the state of the Linux bus driver with the actual
+ * state of the MC by adding objects that have been newly discovered
+ * in the physical DPRC.
+ */
+static void dprc_add_new_devices(struct fsl_mc_device *mc_bus_dev,
+				 const char *driver_override,
+				 struct fsl_mc_obj_desc *obj_desc_array,
+				 int num_child_objects_in_mc)
+{
+	int error;
+	int i;
+
+	for (i = 0; i < num_child_objects_in_mc; i++) {
+		struct fsl_mc_device *child_dev;
+		struct fsl_mc_obj_desc *obj_desc = &obj_desc_array[i];
+
+		if (strlen(obj_desc->type) == 0)
+			continue;
+
+		/*
+		 * Check if device is already known to Linux:
+		 */
+		child_dev = fsl_mc_device_lookup(obj_desc, mc_bus_dev);
+		if (child_dev) {
+			check_plugged_state_change(child_dev, obj_desc);
+			put_device(&child_dev->dev);
+			continue;
+		}
+
+		error = fsl_mc_device_add(obj_desc, NULL, &mc_bus_dev->dev,
+					  driver_override, &child_dev);
+		if (error < 0)
+			continue;
+	}
+}
+
+/**
+ * dprc_scan_objects - Discover objects in a DPRC
+ *
+ * @mc_bus_dev: pointer to the fsl-mc device that represents a DPRC object
+ * @driver_override: driver override to apply to new objects found in the
+ * DPRC, or NULL, if none.
+ * @total_irq_count: If argument is provided the function populates the
+ * total number of IRQs created by objects in the DPRC.
+ *
+ * Detects objects added and removed from a DPRC and synchronizes the
+ * state of the Linux bus driver, MC by adding and removing
+ * devices accordingly.
+ * Two types of devices can be found in a DPRC: allocatable objects (e.g.,
+ * dpbp, dpmcp) and non-allocatable devices (e.g., dprc, dpni).
+ * All allocatable devices needed to be probed before all non-allocatable
+ * devices, to ensure that device drivers for non-allocatable
+ * devices can allocate any type of allocatable devices.
+ * That is, we need to ensure that the corresponding resource pools are
+ * populated before they can get allocation requests from probe callbacks
+ * of the device drivers for the non-allocatable devices.
+ */
+int dprc_scan_objects(struct fsl_mc_device *mc_bus_dev,
+		      const char *driver_override,
+		      unsigned int *total_irq_count)
+{
+	int num_child_objects;
+	int dprc_get_obj_failures;
+	int error;
+	unsigned int irq_count = mc_bus_dev->obj_desc.irq_count;
+	struct fsl_mc_obj_desc *child_obj_desc_array = NULL;
+	struct fsl_mc_bus *mc_bus = to_fsl_mc_bus(mc_bus_dev);
+
+	error = dprc_get_obj_count(mc_bus_dev->mc_io,
+				   0,
+				   mc_bus_dev->mc_handle,
+				   &num_child_objects);
+	if (error < 0) {
+		dev_err(&mc_bus_dev->dev, "dprc_get_obj_count() failed: %d\n",
+			error);
+		return error;
+	}
+
+	if (num_child_objects != 0) {
+		int i;
+
+		child_obj_desc_array =
+		    devm_kmalloc_array(&mc_bus_dev->dev, num_child_objects,
+				       sizeof(*child_obj_desc_array),
+				       GFP_KERNEL);
+		if (!child_obj_desc_array)
+			return -ENOMEM;
+
+		/*
+		 * Discover objects currently present in the physical DPRC:
+		 */
+		dprc_get_obj_failures = 0;
+		for (i = 0; i < num_child_objects; i++) {
+			struct fsl_mc_obj_desc *obj_desc =
+			    &child_obj_desc_array[i];
+
+			error = dprc_get_obj(mc_bus_dev->mc_io,
+					     0,
+					     mc_bus_dev->mc_handle,
+					     i, obj_desc);
+			if (error < 0) {
+				dev_err(&mc_bus_dev->dev,
+					"dprc_get_obj(i=%d) failed: %d\n",
+					i, error);
+				/*
+				 * Mark the obj entry as "invalid", by using the
+				 * empty string as obj type:
+				 */
+				obj_desc->type[0] = '\0';
+				obj_desc->id = error;
+				dprc_get_obj_failures++;
+				continue;
+			}
+
+			/*
+			 * add a quirk for all versions of dpsec < 4.0...none
+			 * are coherent regardless of what the MC reports.
+			 */
+			if ((strcmp(obj_desc->type, "dpseci") == 0) &&
+			    (obj_desc->ver_major < 4))
+				obj_desc->flags |=
+					FSL_MC_OBJ_FLAG_NO_MEM_SHAREABILITY;
+
+			irq_count += obj_desc->irq_count;
+			dev_dbg(&mc_bus_dev->dev,
+				"Discovered object: type %s, id %d\n",
+				obj_desc->type, obj_desc->id);
+		}
+
+		if (dprc_get_obj_failures != 0) {
+			dev_err(&mc_bus_dev->dev,
+				"%d out of %d devices could not be retrieved\n",
+				dprc_get_obj_failures, num_child_objects);
+		}
+	}
+
+	/*
+	 * Allocate IRQ's before binding the scanned devices with their
+	 * respective drivers.
+	 */
+	if (dev_get_msi_domain(&mc_bus_dev->dev) && !mc_bus->irq_resources) {
+		if (irq_count > FSL_MC_IRQ_POOL_MAX_TOTAL_IRQS) {
+			dev_warn(&mc_bus_dev->dev,
+				 "IRQs needed (%u) exceed IRQs preallocated (%u)\n",
+				 irq_count, FSL_MC_IRQ_POOL_MAX_TOTAL_IRQS);
+		}
+
+		error = fsl_mc_populate_irq_pool(mc_bus,
+				FSL_MC_IRQ_POOL_MAX_TOTAL_IRQS);
+		if (error < 0)
+			return error;
+	}
+
+	if (total_irq_count)
+		*total_irq_count = irq_count;
+
+	dprc_remove_devices(mc_bus_dev, child_obj_desc_array,
+			    num_child_objects);
+
+	dprc_add_new_devices(mc_bus_dev, driver_override, child_obj_desc_array,
+			     num_child_objects);
+
+	if (child_obj_desc_array)
+		devm_kfree(&mc_bus_dev->dev, child_obj_desc_array);
+
+	return 0;
+}
+
+/**
+ * dprc_scan_container - Scans a physical DPRC and synchronizes Linux bus state
+ *
+ * @mc_bus_dev: pointer to the fsl-mc device that represents a DPRC object
+ *
+ * Scans the physical DPRC and synchronizes the state of the Linux
+ * bus driver with the actual state of the MC by adding and removing
+ * devices as appropriate.
+ */
+static int dprc_scan_container(struct fsl_mc_device *mc_bus_dev)
+{
+	int error;
+	struct fsl_mc_bus *mc_bus = to_fsl_mc_bus(mc_bus_dev);
+
+	fsl_mc_init_all_resource_pools(mc_bus_dev);
+
+	/*
+	 * Discover objects in the DPRC:
+	 */
+	mutex_lock(&mc_bus->scan_mutex);
+	error = dprc_scan_objects(mc_bus_dev, NULL, NULL);
+	mutex_unlock(&mc_bus->scan_mutex);
+	if (error < 0) {
+		fsl_mc_cleanup_all_resource_pools(mc_bus_dev);
+		return error;
+	}
+
+	return 0;
+}
+
+/**
+ * dprc_irq0_handler - Regular ISR for DPRC interrupt 0
+ *
+ * @irq: IRQ number of the interrupt being handled
+ * @arg: Pointer to device structure
+ */
+static irqreturn_t dprc_irq0_handler(int irq_num, void *arg)
+{
+	return IRQ_WAKE_THREAD;
+}
+
+/**
+ * dprc_irq0_handler_thread - Handler thread function for DPRC interrupt 0
+ *
+ * @irq: IRQ number of the interrupt being handled
+ * @arg: Pointer to device structure
+ */
+static irqreturn_t dprc_irq0_handler_thread(int irq_num, void *arg)
+{
+	int error;
+	u32 status;
+	struct device *dev = arg;
+	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
+	struct fsl_mc_bus *mc_bus = to_fsl_mc_bus(mc_dev);
+	struct fsl_mc_io *mc_io = mc_dev->mc_io;
+	struct msi_desc *msi_desc = mc_dev->irqs[0]->msi_desc;
+
+	dev_dbg(dev, "DPRC IRQ %d triggered on CPU %u\n",
+		irq_num, smp_processor_id());
+
+	if (!(mc_dev->flags & FSL_MC_IS_DPRC))
+		return IRQ_HANDLED;
+
+	mutex_lock(&mc_bus->scan_mutex);
+	if (!msi_desc || msi_desc->irq != (u32)irq_num)
+		goto out;
+
+	status = 0;
+	error = dprc_get_irq_status(mc_io, 0, mc_dev->mc_handle, 0,
+				    &status);
+	if (error < 0) {
+		dev_err(dev,
+			"dprc_get_irq_status() failed: %d\n", error);
+		goto out;
+	}
+
+	error = dprc_clear_irq_status(mc_io, 0, mc_dev->mc_handle, 0,
+				      status);
+	if (error < 0) {
+		dev_err(dev,
+			"dprc_clear_irq_status() failed: %d\n", error);
+		goto out;
+	}
+
+	if (status & (DPRC_IRQ_EVENT_OBJ_ADDED |
+		      DPRC_IRQ_EVENT_OBJ_REMOVED |
+		      DPRC_IRQ_EVENT_CONTAINER_DESTROYED |
+		      DPRC_IRQ_EVENT_OBJ_DESTROYED |
+		      DPRC_IRQ_EVENT_OBJ_CREATED)) {
+		unsigned int irq_count;
+
+		error = dprc_scan_objects(mc_dev, NULL, &irq_count);
+		if (error < 0) {
+			/*
+			 * If the error is -ENXIO, we ignore it, as it indicates
+			 * that the object scan was aborted, as we detected that
+			 * an object was removed from the DPRC in the MC, while
+			 * we were scanning the DPRC.
+			 */
+			if (error != -ENXIO) {
+				dev_err(dev, "dprc_scan_objects() failed: %d\n",
+					error);
+			}
+
+			goto out;
+		}
+
+		if (irq_count > FSL_MC_IRQ_POOL_MAX_TOTAL_IRQS) {
+			dev_warn(dev,
+				 "IRQs needed (%u) exceed IRQs preallocated (%u)\n",
+				 irq_count, FSL_MC_IRQ_POOL_MAX_TOTAL_IRQS);
+		}
+	}
+
+out:
+	mutex_unlock(&mc_bus->scan_mutex);
+	return IRQ_HANDLED;
+}
+
+/*
+ * Disable and clear interrupt for a given DPRC object
+ */
+static int disable_dprc_irq(struct fsl_mc_device *mc_dev)
+{
+	int error;
+	struct fsl_mc_io *mc_io = mc_dev->mc_io;
+
+	/*
+	 * Disable generation of interrupt, while we configure it:
+	 */
+	error = dprc_set_irq_enable(mc_io, 0, mc_dev->mc_handle, 0, 0);
+	if (error < 0) {
+		dev_err(&mc_dev->dev,
+			"Disabling DPRC IRQ failed: dprc_set_irq_enable() failed: %d\n",
+			error);
+		return error;
+	}
+
+	/*
+	 * Disable all interrupt causes for the interrupt:
+	 */
+	error = dprc_set_irq_mask(mc_io, 0, mc_dev->mc_handle, 0, 0x0);
+	if (error < 0) {
+		dev_err(&mc_dev->dev,
+			"Disabling DPRC IRQ failed: dprc_set_irq_mask() failed: %d\n",
+			error);
+		return error;
+	}
+
+	/*
+	 * Clear any leftover interrupts:
+	 */
+	error = dprc_clear_irq_status(mc_io, 0, mc_dev->mc_handle, 0, ~0x0U);
+	if (error < 0) {
+		dev_err(&mc_dev->dev,
+			"Disabling DPRC IRQ failed: dprc_clear_irq_status() failed: %d\n",
+			error);
+		return error;
+	}
+
+	return 0;
+}
+
+static int register_dprc_irq_handler(struct fsl_mc_device *mc_dev)
+{
+	int error;
+	struct fsl_mc_device_irq *irq = mc_dev->irqs[0];
+
+	/*
+	 * NOTE: devm_request_threaded_irq() invokes the device-specific
+	 * function that programs the MSI physically in the device
+	 */
+	error = devm_request_threaded_irq(&mc_dev->dev,
+					  irq->msi_desc->irq,
+					  dprc_irq0_handler,
+					  dprc_irq0_handler_thread,
+					  IRQF_NO_SUSPEND | IRQF_ONESHOT,
+					  dev_name(&mc_dev->dev),
+					  &mc_dev->dev);
+	if (error < 0) {
+		dev_err(&mc_dev->dev,
+			"devm_request_threaded_irq() failed: %d\n",
+			error);
+		return error;
+	}
+
+	return 0;
+}
+
+static int enable_dprc_irq(struct fsl_mc_device *mc_dev)
+{
+	int error;
+
+	/*
+	 * Enable all interrupt causes for the interrupt:
+	 */
+	error = dprc_set_irq_mask(mc_dev->mc_io, 0, mc_dev->mc_handle, 0,
+				  ~0x0u);
+	if (error < 0) {
+		dev_err(&mc_dev->dev,
+			"Enabling DPRC IRQ failed: dprc_set_irq_mask() failed: %d\n",
+			error);
+
+		return error;
+	}
+
+	/*
+	 * Enable generation of the interrupt:
+	 */
+	error = dprc_set_irq_enable(mc_dev->mc_io, 0, mc_dev->mc_handle, 0, 1);
+	if (error < 0) {
+		dev_err(&mc_dev->dev,
+			"Enabling DPRC IRQ failed: dprc_set_irq_enable() failed: %d\n",
+			error);
+
+		return error;
+	}
+
+	return 0;
+}
+
+/*
+ * Setup interrupt for a given DPRC device
+ */
+static int dprc_setup_irq(struct fsl_mc_device *mc_dev)
+{
+	int error;
+
+	error = fsl_mc_allocate_irqs(mc_dev);
+	if (error < 0)
+		return error;
+
+	error = disable_dprc_irq(mc_dev);
+	if (error < 0)
+		goto error_free_irqs;
+
+	error = register_dprc_irq_handler(mc_dev);
+	if (error < 0)
+		goto error_free_irqs;
+
+	error = enable_dprc_irq(mc_dev);
+	if (error < 0)
+		goto error_free_irqs;
+
+	return 0;
+
+error_free_irqs:
+	fsl_mc_free_irqs(mc_dev);
+	return error;
+}
+
+/**
+ * dprc_probe - callback invoked when a DPRC is being bound to this driver
+ *
+ * @mc_dev: Pointer to fsl-mc device representing a DPRC
+ *
+ * It opens the physical DPRC in the MC.
+ * It scans the DPRC to discover the MC objects contained in it.
+ * It creates the interrupt pool for the MC bus associated with the DPRC.
+ * It configures the interrupts for the DPRC device itself.
+ */
+static int dprc_probe(struct fsl_mc_device *mc_dev)
+{
+	int error;
+	size_t region_size;
+	struct device *parent_dev = mc_dev->dev.parent;
+	struct fsl_mc_bus *mc_bus = to_fsl_mc_bus(mc_dev);
+	bool mc_io_created = false;
+	bool msi_domain_set = false;
+	u16 major_ver, minor_ver;
+
+	if (!is_fsl_mc_bus_dprc(mc_dev))
+		return -EINVAL;
+
+	if (dev_get_msi_domain(&mc_dev->dev))
+		return -EINVAL;
+
+	if (!mc_dev->mc_io) {
+		/*
+		 * This is a child DPRC:
+		 */
+		if (!dev_is_fsl_mc(parent_dev))
+			return -EINVAL;
+
+		if (mc_dev->obj_desc.region_count == 0)
+			return -EINVAL;
+
+		region_size = resource_size(mc_dev->regions);
+
+		error = fsl_create_mc_io(&mc_dev->dev,
+					 mc_dev->regions[0].start,
+					 region_size,
+					 NULL,
+					 FSL_MC_IO_ATOMIC_CONTEXT_PORTAL,
+					 &mc_dev->mc_io);
+		if (error < 0)
+			return error;
+
+		mc_io_created = true;
+
+		/*
+		 * Inherit parent MSI domain:
+		 */
+		dev_set_msi_domain(&mc_dev->dev,
+				   dev_get_msi_domain(parent_dev));
+		msi_domain_set = true;
+	} else {
+		/*
+		 * This is a root DPRC
+		 */
+		struct irq_domain *mc_msi_domain;
+
+		if (dev_is_fsl_mc(parent_dev))
+			return -EINVAL;
+
+		error = fsl_mc_find_msi_domain(parent_dev,
+					       &mc_msi_domain);
+		if (error < 0) {
+			dev_warn(&mc_dev->dev,
+				 "WARNING: MC bus without interrupt support\n");
+		} else {
+			dev_set_msi_domain(&mc_dev->dev, mc_msi_domain);
+			msi_domain_set = true;
+		}
+	}
+
+	error = dprc_open(mc_dev->mc_io, 0, mc_dev->obj_desc.id,
+			  &mc_dev->mc_handle);
+	if (error < 0) {
+		dev_err(&mc_dev->dev, "dprc_open() failed: %d\n", error);
+		goto error_cleanup_msi_domain;
+	}
+
+	error = dprc_get_attributes(mc_dev->mc_io, 0, mc_dev->mc_handle,
+				    &mc_bus->dprc_attr);
+	if (error < 0) {
+		dev_err(&mc_dev->dev, "dprc_get_attributes() failed: %d\n",
+			error);
+		goto error_cleanup_open;
+	}
+
+	error = dprc_get_api_version(mc_dev->mc_io, 0,
+				     &major_ver,
+				     &minor_ver);
+	if (error < 0) {
+		dev_err(&mc_dev->dev, "dprc_get_api_version() failed: %d\n",
+			error);
+		goto error_cleanup_open;
+	}
+
+	if (major_ver < DPRC_MIN_VER_MAJOR ||
+	    (major_ver == DPRC_MIN_VER_MAJOR &&
+	     minor_ver < DPRC_MIN_VER_MINOR)) {
+		dev_err(&mc_dev->dev,
+			"ERROR: DPRC version %d.%d not supported\n",
+			major_ver, minor_ver);
+		error = -ENOTSUPP;
+		goto error_cleanup_open;
+	}
+
+	mutex_init(&mc_bus->scan_mutex);
+
+	/*
+	 * Discover MC objects in DPRC object:
+	 */
+	error = dprc_scan_container(mc_dev);
+	if (error < 0)
+		goto error_cleanup_open;
+
+	/*
+	 * Configure interrupt for the DPRC object associated with this MC bus:
+	 */
+	error = dprc_setup_irq(mc_dev);
+	if (error < 0)
+		goto error_cleanup_open;
+
+	dev_info(&mc_dev->dev, "DPRC device bound to driver");
+	return 0;
+
+error_cleanup_open:
+	(void)dprc_close(mc_dev->mc_io, 0, mc_dev->mc_handle);
+
+error_cleanup_msi_domain:
+	if (msi_domain_set)
+		dev_set_msi_domain(&mc_dev->dev, NULL);
+
+	if (mc_io_created) {
+		fsl_destroy_mc_io(mc_dev->mc_io);
+		mc_dev->mc_io = NULL;
+	}
+
+	return error;
+}
+
+/*
+ * Tear down interrupt for a given DPRC object
+ */
+static void dprc_teardown_irq(struct fsl_mc_device *mc_dev)
+{
+	struct fsl_mc_device_irq *irq = mc_dev->irqs[0];
+
+	(void)disable_dprc_irq(mc_dev);
+
+	devm_free_irq(&mc_dev->dev, irq->msi_desc->irq, &mc_dev->dev);
+
+	fsl_mc_free_irqs(mc_dev);
+}
+
+/**
+ * dprc_remove - callback invoked when a DPRC is being unbound from this driver
+ *
+ * @mc_dev: Pointer to fsl-mc device representing the DPRC
+ *
+ * It removes the DPRC's child objects from Linux (not from the MC) and
+ * closes the DPRC device in the MC.
+ * It tears down the interrupts that were configured for the DPRC device.
+ * It destroys the interrupt pool associated with this MC bus.
+ */
+static int dprc_remove(struct fsl_mc_device *mc_dev)
+{
+	int error;
+	struct fsl_mc_bus *mc_bus = to_fsl_mc_bus(mc_dev);
+
+	if (!is_fsl_mc_bus_dprc(mc_dev))
+		return -EINVAL;
+	if (!mc_dev->mc_io)
+		return -EINVAL;
+
+	if (!mc_bus->irq_resources)
+		return -EINVAL;
+
+	if (dev_get_msi_domain(&mc_dev->dev))
+		dprc_teardown_irq(mc_dev);
+
+	device_for_each_child(&mc_dev->dev, NULL, __fsl_mc_device_remove);
+
+	if (dev_get_msi_domain(&mc_dev->dev)) {
+		fsl_mc_cleanup_irq_pool(mc_bus);
+		dev_set_msi_domain(&mc_dev->dev, NULL);
+	}
+
+	fsl_mc_cleanup_all_resource_pools(mc_dev);
+
+	error = dprc_close(mc_dev->mc_io, 0, mc_dev->mc_handle);
+	if (error < 0)
+		dev_err(&mc_dev->dev, "dprc_close() failed: %d\n", error);
+
+	if (!fsl_mc_is_root_dprc(&mc_dev->dev)) {
+		fsl_destroy_mc_io(mc_dev->mc_io);
+		mc_dev->mc_io = NULL;
+	}
+
+	dev_info(&mc_dev->dev, "DPRC device unbound from driver");
+	return 0;
+}
+
+static const struct fsl_mc_device_id match_id_table[] = {
+	{
+	 .vendor = FSL_MC_VENDOR_FREESCALE,
+	 .obj_type = "dprc"},
+	{.vendor = 0x0},
+};
+
+static struct fsl_mc_driver dprc_driver = {
+	.driver = {
+		   .name = FSL_MC_DPRC_DRIVER_NAME,
+		   .owner = THIS_MODULE,
+		   .pm = NULL,
+		   },
+	.match_id_table = match_id_table,
+	.probe = dprc_probe,
+	.remove = dprc_remove,
+};
+
+int __init dprc_driver_init(void)
+{
+	return fsl_mc_driver_register(&dprc_driver);
+}
+
+void dprc_driver_exit(void)
+{
+	fsl_mc_driver_unregister(&dprc_driver);
+}
--- a/drivers/staging/fsl-mc/bus/dprc.c
+++ /dev/null
@@ -1,757 +0,0 @@
-// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
-/*
- * Copyright 2013-2016 Freescale Semiconductor Inc.
- *
- */
-#include <linux/kernel.h>
-#include "../include/mc.h"
-#include "dprc.h"
-
-#include "dprc-cmd.h"
-
-/**
- * dprc_open() - Open DPRC object for use
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @container_id: Container ID to open
- * @token:	Returned token of DPRC object
- *
- * Return:	'0' on Success; Error code otherwise.
- *
- * @warning	Required before any operation on the object.
- */
-int dprc_open(struct fsl_mc_io *mc_io,
-	      u32 cmd_flags,
-	      int container_id,
-	      u16 *token)
-{
-	struct mc_command cmd = { 0 };
-	struct dprc_cmd_open *cmd_params;
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_OPEN, cmd_flags,
-					  0);
-	cmd_params = (struct dprc_cmd_open *)cmd.params;
-	cmd_params->container_id = cpu_to_le32(container_id);
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	*token = mc_cmd_hdr_read_token(&cmd);
-
-	return 0;
-}
-EXPORT_SYMBOL(dprc_open);
-
-/**
- * dprc_close() - Close the control session of the object
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPRC object
- *
- * After this function is called, no further operations are
- * allowed on the object without opening a new control session.
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dprc_close(struct fsl_mc_io *mc_io,
-	       u32 cmd_flags,
-	       u16 token)
-{
-	struct mc_command cmd = { 0 };
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_CLOSE, cmd_flags,
-					  token);
-
-	/* send command to mc*/
-	return mc_send_command(mc_io, &cmd);
-}
-EXPORT_SYMBOL(dprc_close);
-
-/**
- * dprc_get_irq() - Get IRQ information from the DPRC.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPRC object
- * @irq_index:	The interrupt index to configure
- * @type:	Interrupt type: 0 represents message interrupt
- *		type (both irq_addr and irq_val are valid)
- * @irq_cfg:	IRQ attributes
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dprc_get_irq(struct fsl_mc_io *mc_io,
-		 u32 cmd_flags,
-		 u16 token,
-		 u8 irq_index,
-		 int *type,
-		 struct dprc_irq_cfg *irq_cfg)
-{
-	struct mc_command cmd = { 0 };
-	struct dprc_cmd_get_irq *cmd_params;
-	struct dprc_rsp_get_irq *rsp_params;
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_IRQ,
-					  cmd_flags,
-					  token);
-	cmd_params = (struct dprc_cmd_get_irq *)cmd.params;
-	cmd_params->irq_index = irq_index;
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	rsp_params = (struct dprc_rsp_get_irq *)cmd.params;
-	irq_cfg->val = le32_to_cpu(rsp_params->irq_val);
-	irq_cfg->paddr = le64_to_cpu(rsp_params->irq_addr);
-	irq_cfg->irq_num = le32_to_cpu(rsp_params->irq_num);
-	*type = le32_to_cpu(rsp_params->type);
-
-	return 0;
-}
-
-/**
- * dprc_set_irq() - Set IRQ information for the DPRC to trigger an interrupt.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPRC object
- * @irq_index:	Identifies the interrupt index to configure
- * @irq_cfg:	IRQ configuration
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dprc_set_irq(struct fsl_mc_io *mc_io,
-		 u32 cmd_flags,
-		 u16 token,
-		 u8 irq_index,
-		 struct dprc_irq_cfg *irq_cfg)
-{
-	struct mc_command cmd = { 0 };
-	struct dprc_cmd_set_irq *cmd_params;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_SET_IRQ,
-					  cmd_flags,
-					  token);
-	cmd_params = (struct dprc_cmd_set_irq *)cmd.params;
-	cmd_params->irq_val = cpu_to_le32(irq_cfg->val);
-	cmd_params->irq_index = irq_index;
-	cmd_params->irq_addr = cpu_to_le64(irq_cfg->paddr);
-	cmd_params->irq_num = cpu_to_le32(irq_cfg->irq_num);
-
-	/* send command to mc*/
-	return mc_send_command(mc_io, &cmd);
-}
-
-/**
- * dprc_get_irq_enable() - Get overall interrupt state.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPRC object
- * @irq_index:  The interrupt index to configure
- * @en:		Returned interrupt state - enable = 1, disable = 0
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dprc_get_irq_enable(struct fsl_mc_io *mc_io,
-			u32 cmd_flags,
-			u16 token,
-			u8 irq_index,
-			u8 *en)
-{
-	struct mc_command cmd = { 0 };
-	struct dprc_cmd_get_irq_enable *cmd_params;
-	struct dprc_rsp_get_irq_enable *rsp_params;
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_IRQ_ENABLE,
-					  cmd_flags, token);
-	cmd_params = (struct dprc_cmd_get_irq_enable *)cmd.params;
-	cmd_params->irq_index = irq_index;
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	rsp_params = (struct dprc_rsp_get_irq_enable *)cmd.params;
-	*en = rsp_params->enabled & DPRC_ENABLE;
-
-	return 0;
-}
-
-/**
- * dprc_set_irq_enable() - Set overall interrupt state.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPRC object
- * @irq_index:	The interrupt index to configure
- * @en:		Interrupt state - enable = 1, disable = 0
- *
- * Allows GPP software to control when interrupts are generated.
- * Each interrupt can have up to 32 causes.  The enable/disable control's the
- * overall interrupt state. if the interrupt is disabled no causes will cause
- * an interrupt.
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dprc_set_irq_enable(struct fsl_mc_io *mc_io,
-			u32 cmd_flags,
-			u16 token,
-			u8 irq_index,
-			u8 en)
-{
-	struct mc_command cmd = { 0 };
-	struct dprc_cmd_set_irq_enable *cmd_params;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_SET_IRQ_ENABLE,
-					  cmd_flags, token);
-	cmd_params = (struct dprc_cmd_set_irq_enable *)cmd.params;
-	cmd_params->enable = en & DPRC_ENABLE;
-	cmd_params->irq_index = irq_index;
-
-	/* send command to mc*/
-	return mc_send_command(mc_io, &cmd);
-}
-
-/**
- * dprc_get_irq_mask() - Get interrupt mask.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPRC object
- * @irq_index:	The interrupt index to configure
- * @mask:	Returned event mask to trigger interrupt
- *
- * Every interrupt can have up to 32 causes and the interrupt model supports
- * masking/unmasking each cause independently
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dprc_get_irq_mask(struct fsl_mc_io *mc_io,
-		      u32 cmd_flags,
-		      u16 token,
-		      u8 irq_index,
-		      u32 *mask)
-{
-	struct mc_command cmd = { 0 };
-	struct dprc_cmd_get_irq_mask *cmd_params;
-	struct dprc_rsp_get_irq_mask *rsp_params;
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_IRQ_MASK,
-					  cmd_flags, token);
-	cmd_params = (struct dprc_cmd_get_irq_mask *)cmd.params;
-	cmd_params->irq_index = irq_index;
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	rsp_params = (struct dprc_rsp_get_irq_mask *)cmd.params;
-	*mask = le32_to_cpu(rsp_params->mask);
-
-	return 0;
-}
-
-/**
- * dprc_set_irq_mask() - Set interrupt mask.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPRC object
- * @irq_index:	The interrupt index to configure
- * @mask:	event mask to trigger interrupt;
- *			each bit:
- *				0 = ignore event
- *				1 = consider event for asserting irq
- *
- * Every interrupt can have up to 32 causes and the interrupt model supports
- * masking/unmasking each cause independently
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dprc_set_irq_mask(struct fsl_mc_io *mc_io,
-		      u32 cmd_flags,
-		      u16 token,
-		      u8 irq_index,
-		      u32 mask)
-{
-	struct mc_command cmd = { 0 };
-	struct dprc_cmd_set_irq_mask *cmd_params;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_SET_IRQ_MASK,
-					  cmd_flags, token);
-	cmd_params = (struct dprc_cmd_set_irq_mask *)cmd.params;
-	cmd_params->mask = cpu_to_le32(mask);
-	cmd_params->irq_index = irq_index;
-
-	/* send command to mc*/
-	return mc_send_command(mc_io, &cmd);
-}
-
-/**
- * dprc_get_irq_status() - Get the current status of any pending interrupts.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPRC object
- * @irq_index:	The interrupt index to configure
- * @status:	Returned interrupts status - one bit per cause:
- *			0 = no interrupt pending
- *			1 = interrupt pending
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dprc_get_irq_status(struct fsl_mc_io *mc_io,
-			u32 cmd_flags,
-			u16 token,
-			u8 irq_index,
-			u32 *status)
-{
-	struct mc_command cmd = { 0 };
-	struct dprc_cmd_get_irq_status *cmd_params;
-	struct dprc_rsp_get_irq_status *rsp_params;
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_IRQ_STATUS,
-					  cmd_flags, token);
-	cmd_params = (struct dprc_cmd_get_irq_status *)cmd.params;
-	cmd_params->status = cpu_to_le32(*status);
-	cmd_params->irq_index = irq_index;
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	rsp_params = (struct dprc_rsp_get_irq_status *)cmd.params;
-	*status = le32_to_cpu(rsp_params->status);
-
-	return 0;
-}
-
-/**
- * dprc_clear_irq_status() - Clear a pending interrupt's status
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPRC object
- * @irq_index:	The interrupt index to configure
- * @status:	bits to clear (W1C) - one bit per cause:
- *					0 = don't change
- *					1 = clear status bit
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dprc_clear_irq_status(struct fsl_mc_io *mc_io,
-			  u32 cmd_flags,
-			  u16 token,
-			  u8 irq_index,
-			  u32 status)
-{
-	struct mc_command cmd = { 0 };
-	struct dprc_cmd_clear_irq_status *cmd_params;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_CLEAR_IRQ_STATUS,
-					  cmd_flags, token);
-	cmd_params = (struct dprc_cmd_clear_irq_status *)cmd.params;
-	cmd_params->status = cpu_to_le32(status);
-	cmd_params->irq_index = irq_index;
-
-	/* send command to mc*/
-	return mc_send_command(mc_io, &cmd);
-}
-
-/**
- * dprc_get_attributes() - Obtains container attributes
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPRC object
- * @attributes	Returned container attributes
- *
- * Return:     '0' on Success; Error code otherwise.
- */
-int dprc_get_attributes(struct fsl_mc_io *mc_io,
-			u32 cmd_flags,
-			u16 token,
-			struct dprc_attributes *attr)
-{
-	struct mc_command cmd = { 0 };
-	struct dprc_rsp_get_attributes *rsp_params;
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_ATTR,
-					  cmd_flags,
-					  token);
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	rsp_params = (struct dprc_rsp_get_attributes *)cmd.params;
-	attr->container_id = le32_to_cpu(rsp_params->container_id);
-	attr->icid = le16_to_cpu(rsp_params->icid);
-	attr->options = le32_to_cpu(rsp_params->options);
-	attr->portal_id = le32_to_cpu(rsp_params->portal_id);
-
-	return 0;
-}
-
-/**
- * dprc_get_obj_count() - Obtains the number of objects in the DPRC
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPRC object
- * @obj_count:	Number of objects assigned to the DPRC
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dprc_get_obj_count(struct fsl_mc_io *mc_io,
-		       u32 cmd_flags,
-		       u16 token,
-		       int *obj_count)
-{
-	struct mc_command cmd = { 0 };
-	struct dprc_rsp_get_obj_count *rsp_params;
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_OBJ_COUNT,
-					  cmd_flags, token);
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	rsp_params = (struct dprc_rsp_get_obj_count *)cmd.params;
-	*obj_count = le32_to_cpu(rsp_params->obj_count);
-
-	return 0;
-}
-EXPORT_SYMBOL(dprc_get_obj_count);
-
-/**
- * dprc_get_obj() - Get general information on an object
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPRC object
- * @obj_index:	Index of the object to be queried (< obj_count)
- * @obj_desc:	Returns the requested object descriptor
- *
- * The object descriptors are retrieved one by one by incrementing
- * obj_index up to (not including) the value of obj_count returned
- * from dprc_get_obj_count(). dprc_get_obj_count() must
- * be called prior to dprc_get_obj().
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dprc_get_obj(struct fsl_mc_io *mc_io,
-		 u32 cmd_flags,
-		 u16 token,
-		 int obj_index,
-		 struct fsl_mc_obj_desc *obj_desc)
-{
-	struct mc_command cmd = { 0 };
-	struct dprc_cmd_get_obj *cmd_params;
-	struct dprc_rsp_get_obj *rsp_params;
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_OBJ,
-					  cmd_flags,
-					  token);
-	cmd_params = (struct dprc_cmd_get_obj *)cmd.params;
-	cmd_params->obj_index = cpu_to_le32(obj_index);
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	rsp_params = (struct dprc_rsp_get_obj *)cmd.params;
-	obj_desc->id = le32_to_cpu(rsp_params->id);
-	obj_desc->vendor = le16_to_cpu(rsp_params->vendor);
-	obj_desc->irq_count = rsp_params->irq_count;
-	obj_desc->region_count = rsp_params->region_count;
-	obj_desc->state = le32_to_cpu(rsp_params->state);
-	obj_desc->ver_major = le16_to_cpu(rsp_params->version_major);
-	obj_desc->ver_minor = le16_to_cpu(rsp_params->version_minor);
-	obj_desc->flags = le16_to_cpu(rsp_params->flags);
-	strncpy(obj_desc->type, rsp_params->type, 16);
-	obj_desc->type[15] = '\0';
-	strncpy(obj_desc->label, rsp_params->label, 16);
-	obj_desc->label[15] = '\0';
-	return 0;
-}
-EXPORT_SYMBOL(dprc_get_obj);
-
-/**
- * dprc_set_obj_irq() - Set IRQ information for object to trigger an interrupt.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPRC object
- * @obj_type:	Type of the object to set its IRQ
- * @obj_id:	ID of the object to set its IRQ
- * @irq_index:	The interrupt index to configure
- * @irq_cfg:	IRQ configuration
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dprc_set_obj_irq(struct fsl_mc_io *mc_io,
-		     u32 cmd_flags,
-		     u16 token,
-		     char *obj_type,
-		     int obj_id,
-		     u8 irq_index,
-		     struct dprc_irq_cfg *irq_cfg)
-{
-	struct mc_command cmd = { 0 };
-	struct dprc_cmd_set_obj_irq *cmd_params;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_SET_OBJ_IRQ,
-					  cmd_flags,
-					  token);
-	cmd_params = (struct dprc_cmd_set_obj_irq *)cmd.params;
-	cmd_params->irq_val = cpu_to_le32(irq_cfg->val);
-	cmd_params->irq_index = irq_index;
-	cmd_params->irq_addr = cpu_to_le64(irq_cfg->paddr);
-	cmd_params->irq_num = cpu_to_le32(irq_cfg->irq_num);
-	cmd_params->obj_id = cpu_to_le32(obj_id);
-	strncpy(cmd_params->obj_type, obj_type, 16);
-	cmd_params->obj_type[15] = '\0';
-
-	/* send command to mc*/
-	return mc_send_command(mc_io, &cmd);
-}
-EXPORT_SYMBOL(dprc_set_obj_irq);
-
-/**
- * dprc_get_obj_irq() - Get IRQ information from object.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPRC object
- * @obj_type:	Type od the object to get its IRQ
- * @obj_id:	ID of the object to get its IRQ
- * @irq_index:	The interrupt index to configure
- * @type:	Interrupt type: 0 represents message interrupt
- *		type (both irq_addr and irq_val are valid)
- * @irq_cfg:	The returned IRQ attributes
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dprc_get_obj_irq(struct fsl_mc_io *mc_io,
-		     u32 cmd_flags,
-		     u16 token,
-		     char *obj_type,
-		     int obj_id,
-		     u8 irq_index,
-		     int *type,
-		     struct dprc_irq_cfg *irq_cfg)
-{
-	struct mc_command cmd = { 0 };
-	struct dprc_cmd_get_obj_irq *cmd_params;
-	struct dprc_rsp_get_obj_irq *rsp_params;
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_OBJ_IRQ,
-					  cmd_flags,
-					  token);
-	cmd_params = (struct dprc_cmd_get_obj_irq *)cmd.params;
-	cmd_params->obj_id = cpu_to_le32(obj_id);
-	cmd_params->irq_index = irq_index;
-	strncpy(cmd_params->obj_type, obj_type, 16);
-	cmd_params->obj_type[15] = '\0';
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	rsp_params = (struct dprc_rsp_get_obj_irq *)cmd.params;
-	irq_cfg->val = le32_to_cpu(rsp_params->irq_val);
-	irq_cfg->paddr = le64_to_cpu(rsp_params->irq_addr);
-	irq_cfg->irq_num = le32_to_cpu(rsp_params->irq_num);
-	*type = le32_to_cpu(rsp_params->type);
-
-	return 0;
-}
-EXPORT_SYMBOL(dprc_get_obj_irq);
-
-/**
- * dprc_get_res_count() - Obtains the number of free resources that are assigned
- *		to this container, by pool type
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPRC object
- * @type:	pool type
- * @res_count:	Returned number of free resources of the given
- *			resource type that are assigned to this DPRC
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dprc_get_res_count(struct fsl_mc_io *mc_io,
-		       u32 cmd_flags,
-		       u16 token,
-		       char *type,
-		       int *res_count)
-{
-	struct mc_command cmd = { 0 };
-	struct dprc_cmd_get_res_count *cmd_params;
-	struct dprc_rsp_get_res_count *rsp_params;
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_RES_COUNT,
-					  cmd_flags, token);
-	cmd_params = (struct dprc_cmd_get_res_count *)cmd.params;
-	strncpy(cmd_params->type, type, 16);
-	cmd_params->type[15] = '\0';
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	rsp_params = (struct dprc_rsp_get_res_count *)cmd.params;
-	*res_count = le32_to_cpu(rsp_params->res_count);
-
-	return 0;
-}
-EXPORT_SYMBOL(dprc_get_res_count);
-
-/**
- * dprc_get_obj_region() - Get region information for a specified object.
- * @mc_io:	Pointer to MC portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @token:	Token of DPRC object
- * @obj_type;	Object type as returned in dprc_get_obj()
- * @obj_id:	Unique object instance as returned in dprc_get_obj()
- * @region_index: The specific region to query
- * @region_desc:  Returns the requested region descriptor
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dprc_get_obj_region(struct fsl_mc_io *mc_io,
-			u32 cmd_flags,
-			u16 token,
-			char *obj_type,
-			int obj_id,
-			u8 region_index,
-			struct dprc_region_desc *region_desc)
-{
-	struct mc_command cmd = { 0 };
-	struct dprc_cmd_get_obj_region *cmd_params;
-	struct dprc_rsp_get_obj_region *rsp_params;
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_OBJ_REG,
-					  cmd_flags, token);
-	cmd_params = (struct dprc_cmd_get_obj_region *)cmd.params;
-	cmd_params->obj_id = cpu_to_le32(obj_id);
-	cmd_params->region_index = region_index;
-	strncpy(cmd_params->obj_type, obj_type, 16);
-	cmd_params->obj_type[15] = '\0';
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	rsp_params = (struct dprc_rsp_get_obj_region *)cmd.params;
-	region_desc->base_offset = le64_to_cpu(rsp_params->base_addr);
-	region_desc->size = le32_to_cpu(rsp_params->size);
-
-	return 0;
-}
-EXPORT_SYMBOL(dprc_get_obj_region);
-
-/**
- * dprc_get_api_version - Get Data Path Resource Container API version
- * @mc_io:	Pointer to Mc portal's I/O object
- * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
- * @major_ver:	Major version of Data Path Resource Container API
- * @minor_ver:	Minor version of Data Path Resource Container API
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dprc_get_api_version(struct fsl_mc_io *mc_io,
-			 u32 cmd_flags,
-			 u16 *major_ver,
-			 u16 *minor_ver)
-{
-	struct mc_command cmd = { 0 };
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_API_VERSION,
-					  cmd_flags, 0);
-
-	/* send command to mc */
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	mc_cmd_read_api_version(&cmd, major_ver, minor_ver);
-
-	return 0;
-}
-
-/**
- * dprc_get_container_id - Get container ID associated with a given portal.
- * @mc_io:		Pointer to Mc portal's I/O object
- * @cmd_flags:		Command flags; one or more of 'MC_CMD_FLAG_'
- * @container_id:	Requested container id
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-int dprc_get_container_id(struct fsl_mc_io *mc_io,
-			  u32 cmd_flags,
-			  int *container_id)
-{
-	struct mc_command cmd = { 0 };
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_CONT_ID,
-					  cmd_flags,
-					  0);
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	*container_id = (int)mc_cmd_read_object_id(&cmd);
-
-	return 0;
-}
--- /dev/null
+++ b/drivers/bus/fsl-mc/dprc.c
@@ -0,0 +1,576 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * Copyright 2013-2016 Freescale Semiconductor Inc.
+ *
+ */
+#include <linux/kernel.h>
+#include <linux/fsl/mc.h>
+
+#include "fsl-mc-private.h"
+
+/**
+ * dprc_open() - Open DPRC object for use
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @container_id: Container ID to open
+ * @token:	Returned token of DPRC object
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ *
+ * @warning	Required before any operation on the object.
+ */
+int dprc_open(struct fsl_mc_io *mc_io,
+	      u32 cmd_flags,
+	      int container_id,
+	      u16 *token)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dprc_cmd_open *cmd_params;
+	int err;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPRC_CMDID_OPEN, cmd_flags,
+					  0);
+	cmd_params = (struct dprc_cmd_open *)cmd.params;
+	cmd_params->container_id = cpu_to_le32(container_id);
+
+	/* send command to mc*/
+	err = mc_send_command(mc_io, &cmd);
+	if (err)
+		return err;
+
+	/* retrieve response parameters */
+	*token = mc_cmd_hdr_read_token(&cmd);
+
+	return 0;
+}
+EXPORT_SYMBOL_GPL(dprc_open);
+
+/**
+ * dprc_close() - Close the control session of the object
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPRC object
+ *
+ * After this function is called, no further operations are
+ * allowed on the object without opening a new control session.
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dprc_close(struct fsl_mc_io *mc_io,
+	       u32 cmd_flags,
+	       u16 token)
+{
+	struct fsl_mc_command cmd = { 0 };
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPRC_CMDID_CLOSE, cmd_flags,
+					  token);
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
+EXPORT_SYMBOL_GPL(dprc_close);
+
+/**
+ * dprc_reset_container - Reset child container.
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPRC object
+ * @child_container_id:	ID of the container to reset
+ *
+ * In case a software context crashes or becomes non-responsive, the parent
+ * may wish to reset its resources container before the software context is
+ * restarted.
+ *
+ * This routine informs all objects assigned to the child container that the
+ * container is being reset, so they may perform any cleanup operations that are
+ * needed. All objects handles that were owned by the child container shall be
+ * closed.
+ *
+ * Note that such request may be submitted even if the child software context
+ * has not crashed, but the resulting object cleanup operations will not be
+ * aware of that.
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dprc_reset_container(struct fsl_mc_io *mc_io,
+			 u32 cmd_flags,
+			 u16 token,
+			 int child_container_id)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dprc_cmd_reset_container *cmd_params;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPRC_CMDID_RESET_CONT,
+					  cmd_flags, token);
+	cmd_params = (struct dprc_cmd_reset_container *)cmd.params;
+	cmd_params->child_container_id = cpu_to_le32(child_container_id);
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
+EXPORT_SYMBOL_GPL(dprc_reset_container);
+
+/**
+ * dprc_set_irq() - Set IRQ information for the DPRC to trigger an interrupt.
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPRC object
+ * @irq_index:	Identifies the interrupt index to configure
+ * @irq_cfg:	IRQ configuration
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dprc_set_irq(struct fsl_mc_io *mc_io,
+		 u32 cmd_flags,
+		 u16 token,
+		 u8 irq_index,
+		 struct dprc_irq_cfg *irq_cfg)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dprc_cmd_set_irq *cmd_params;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPRC_CMDID_SET_IRQ,
+					  cmd_flags,
+					  token);
+	cmd_params = (struct dprc_cmd_set_irq *)cmd.params;
+	cmd_params->irq_val = cpu_to_le32(irq_cfg->val);
+	cmd_params->irq_index = irq_index;
+	cmd_params->irq_addr = cpu_to_le64(irq_cfg->paddr);
+	cmd_params->irq_num = cpu_to_le32(irq_cfg->irq_num);
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
+
+/**
+ * dprc_set_irq_enable() - Set overall interrupt state.
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPRC object
+ * @irq_index:	The interrupt index to configure
+ * @en:		Interrupt state - enable = 1, disable = 0
+ *
+ * Allows GPP software to control when interrupts are generated.
+ * Each interrupt can have up to 32 causes.  The enable/disable control's the
+ * overall interrupt state. if the interrupt is disabled no causes will cause
+ * an interrupt.
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dprc_set_irq_enable(struct fsl_mc_io *mc_io,
+			u32 cmd_flags,
+			u16 token,
+			u8 irq_index,
+			u8 en)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dprc_cmd_set_irq_enable *cmd_params;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPRC_CMDID_SET_IRQ_ENABLE,
+					  cmd_flags, token);
+	cmd_params = (struct dprc_cmd_set_irq_enable *)cmd.params;
+	cmd_params->enable = en & DPRC_ENABLE;
+	cmd_params->irq_index = irq_index;
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
+
+/**
+ * dprc_set_irq_mask() - Set interrupt mask.
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPRC object
+ * @irq_index:	The interrupt index to configure
+ * @mask:	event mask to trigger interrupt;
+ *			each bit:
+ *				0 = ignore event
+ *				1 = consider event for asserting irq
+ *
+ * Every interrupt can have up to 32 causes and the interrupt model supports
+ * masking/unmasking each cause independently
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dprc_set_irq_mask(struct fsl_mc_io *mc_io,
+		      u32 cmd_flags,
+		      u16 token,
+		      u8 irq_index,
+		      u32 mask)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dprc_cmd_set_irq_mask *cmd_params;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPRC_CMDID_SET_IRQ_MASK,
+					  cmd_flags, token);
+	cmd_params = (struct dprc_cmd_set_irq_mask *)cmd.params;
+	cmd_params->mask = cpu_to_le32(mask);
+	cmd_params->irq_index = irq_index;
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
+
+/**
+ * dprc_get_irq_status() - Get the current status of any pending interrupts.
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPRC object
+ * @irq_index:	The interrupt index to configure
+ * @status:	Returned interrupts status - one bit per cause:
+ *			0 = no interrupt pending
+ *			1 = interrupt pending
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dprc_get_irq_status(struct fsl_mc_io *mc_io,
+			u32 cmd_flags,
+			u16 token,
+			u8 irq_index,
+			u32 *status)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dprc_cmd_get_irq_status *cmd_params;
+	struct dprc_rsp_get_irq_status *rsp_params;
+	int err;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_IRQ_STATUS,
+					  cmd_flags, token);
+	cmd_params = (struct dprc_cmd_get_irq_status *)cmd.params;
+	cmd_params->status = cpu_to_le32(*status);
+	cmd_params->irq_index = irq_index;
+
+	/* send command to mc*/
+	err = mc_send_command(mc_io, &cmd);
+	if (err)
+		return err;
+
+	/* retrieve response parameters */
+	rsp_params = (struct dprc_rsp_get_irq_status *)cmd.params;
+	*status = le32_to_cpu(rsp_params->status);
+
+	return 0;
+}
+
+/**
+ * dprc_clear_irq_status() - Clear a pending interrupt's status
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPRC object
+ * @irq_index:	The interrupt index to configure
+ * @status:	bits to clear (W1C) - one bit per cause:
+ *					0 = don't change
+ *					1 = clear status bit
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dprc_clear_irq_status(struct fsl_mc_io *mc_io,
+			  u32 cmd_flags,
+			  u16 token,
+			  u8 irq_index,
+			  u32 status)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dprc_cmd_clear_irq_status *cmd_params;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPRC_CMDID_CLEAR_IRQ_STATUS,
+					  cmd_flags, token);
+	cmd_params = (struct dprc_cmd_clear_irq_status *)cmd.params;
+	cmd_params->status = cpu_to_le32(status);
+	cmd_params->irq_index = irq_index;
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
+
+/**
+ * dprc_get_attributes() - Obtains container attributes
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPRC object
+ * @attributes	Returned container attributes
+ *
+ * Return:     '0' on Success; Error code otherwise.
+ */
+int dprc_get_attributes(struct fsl_mc_io *mc_io,
+			u32 cmd_flags,
+			u16 token,
+			struct dprc_attributes *attr)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dprc_rsp_get_attributes *rsp_params;
+	int err;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_ATTR,
+					  cmd_flags,
+					  token);
+
+	/* send command to mc*/
+	err = mc_send_command(mc_io, &cmd);
+	if (err)
+		return err;
+
+	/* retrieve response parameters */
+	rsp_params = (struct dprc_rsp_get_attributes *)cmd.params;
+	attr->container_id = le32_to_cpu(rsp_params->container_id);
+	attr->icid = le32_to_cpu(rsp_params->icid);
+	attr->options = le32_to_cpu(rsp_params->options);
+	attr->portal_id = le32_to_cpu(rsp_params->portal_id);
+
+	return 0;
+}
+
+/**
+ * dprc_get_obj_count() - Obtains the number of objects in the DPRC
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPRC object
+ * @obj_count:	Number of objects assigned to the DPRC
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dprc_get_obj_count(struct fsl_mc_io *mc_io,
+		       u32 cmd_flags,
+		       u16 token,
+		       int *obj_count)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dprc_rsp_get_obj_count *rsp_params;
+	int err;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_OBJ_COUNT,
+					  cmd_flags, token);
+
+	/* send command to mc*/
+	err = mc_send_command(mc_io, &cmd);
+	if (err)
+		return err;
+
+	/* retrieve response parameters */
+	rsp_params = (struct dprc_rsp_get_obj_count *)cmd.params;
+	*obj_count = le32_to_cpu(rsp_params->obj_count);
+
+	return 0;
+}
+EXPORT_SYMBOL_GPL(dprc_get_obj_count);
+
+/**
+ * dprc_get_obj() - Get general information on an object
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPRC object
+ * @obj_index:	Index of the object to be queried (< obj_count)
+ * @obj_desc:	Returns the requested object descriptor
+ *
+ * The object descriptors are retrieved one by one by incrementing
+ * obj_index up to (not including) the value of obj_count returned
+ * from dprc_get_obj_count(). dprc_get_obj_count() must
+ * be called prior to dprc_get_obj().
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dprc_get_obj(struct fsl_mc_io *mc_io,
+		 u32 cmd_flags,
+		 u16 token,
+		 int obj_index,
+		 struct fsl_mc_obj_desc *obj_desc)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dprc_cmd_get_obj *cmd_params;
+	struct dprc_rsp_get_obj *rsp_params;
+	int err;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_OBJ,
+					  cmd_flags,
+					  token);
+	cmd_params = (struct dprc_cmd_get_obj *)cmd.params;
+	cmd_params->obj_index = cpu_to_le32(obj_index);
+
+	/* send command to mc*/
+	err = mc_send_command(mc_io, &cmd);
+	if (err)
+		return err;
+
+	/* retrieve response parameters */
+	rsp_params = (struct dprc_rsp_get_obj *)cmd.params;
+	obj_desc->id = le32_to_cpu(rsp_params->id);
+	obj_desc->vendor = le16_to_cpu(rsp_params->vendor);
+	obj_desc->irq_count = rsp_params->irq_count;
+	obj_desc->region_count = rsp_params->region_count;
+	obj_desc->state = le32_to_cpu(rsp_params->state);
+	obj_desc->ver_major = le16_to_cpu(rsp_params->version_major);
+	obj_desc->ver_minor = le16_to_cpu(rsp_params->version_minor);
+	obj_desc->flags = le16_to_cpu(rsp_params->flags);
+	strncpy(obj_desc->type, rsp_params->type, 16);
+	obj_desc->type[15] = '\0';
+	strncpy(obj_desc->label, rsp_params->label, 16);
+	obj_desc->label[15] = '\0';
+	return 0;
+}
+EXPORT_SYMBOL_GPL(dprc_get_obj);
+
+/**
+ * dprc_set_obj_irq() - Set IRQ information for object to trigger an interrupt.
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPRC object
+ * @obj_type:	Type of the object to set its IRQ
+ * @obj_id:	ID of the object to set its IRQ
+ * @irq_index:	The interrupt index to configure
+ * @irq_cfg:	IRQ configuration
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dprc_set_obj_irq(struct fsl_mc_io *mc_io,
+		     u32 cmd_flags,
+		     u16 token,
+		     char *obj_type,
+		     int obj_id,
+		     u8 irq_index,
+		     struct dprc_irq_cfg *irq_cfg)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dprc_cmd_set_obj_irq *cmd_params;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPRC_CMDID_SET_OBJ_IRQ,
+					  cmd_flags,
+					  token);
+	cmd_params = (struct dprc_cmd_set_obj_irq *)cmd.params;
+	cmd_params->irq_val = cpu_to_le32(irq_cfg->val);
+	cmd_params->irq_index = irq_index;
+	cmd_params->irq_addr = cpu_to_le64(irq_cfg->paddr);
+	cmd_params->irq_num = cpu_to_le32(irq_cfg->irq_num);
+	cmd_params->obj_id = cpu_to_le32(obj_id);
+	strncpy(cmd_params->obj_type, obj_type, 16);
+	cmd_params->obj_type[15] = '\0';
+
+	/* send command to mc*/
+	return mc_send_command(mc_io, &cmd);
+}
+EXPORT_SYMBOL_GPL(dprc_set_obj_irq);
+
+/**
+ * dprc_get_obj_region() - Get region information for a specified object.
+ * @mc_io:	Pointer to MC portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @token:	Token of DPRC object
+ * @obj_type;	Object type as returned in dprc_get_obj()
+ * @obj_id:	Unique object instance as returned in dprc_get_obj()
+ * @region_index: The specific region to query
+ * @region_desc:  Returns the requested region descriptor
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dprc_get_obj_region(struct fsl_mc_io *mc_io,
+			u32 cmd_flags,
+			u16 token,
+			char *obj_type,
+			int obj_id,
+			u8 region_index,
+			struct dprc_region_desc *region_desc)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dprc_cmd_get_obj_region *cmd_params;
+	struct dprc_rsp_get_obj_region *rsp_params;
+	int err;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_OBJ_REG,
+					  cmd_flags, token);
+	cmd_params = (struct dprc_cmd_get_obj_region *)cmd.params;
+	cmd_params->obj_id = cpu_to_le32(obj_id);
+	cmd_params->region_index = region_index;
+	strncpy(cmd_params->obj_type, obj_type, 16);
+	cmd_params->obj_type[15] = '\0';
+
+	/* send command to mc*/
+	err = mc_send_command(mc_io, &cmd);
+	if (err)
+		return err;
+
+	/* retrieve response parameters */
+	rsp_params = (struct dprc_rsp_get_obj_region *)cmd.params;
+	region_desc->base_offset = le32_to_cpu(rsp_params->base_offset);
+	region_desc->size = le32_to_cpu(rsp_params->size);
+	region_desc->type = rsp_params->type;
+	region_desc->flags = le32_to_cpu(rsp_params->flags);
+	region_desc->base_address = le64_to_cpu(rsp_params->base_addr);
+
+	return 0;
+}
+EXPORT_SYMBOL_GPL(dprc_get_obj_region);
+
+/**
+ * dprc_get_api_version - Get Data Path Resource Container API version
+ * @mc_io:	Pointer to Mc portal's I/O object
+ * @cmd_flags:	Command flags; one or more of 'MC_CMD_FLAG_'
+ * @major_ver:	Major version of Data Path Resource Container API
+ * @minor_ver:	Minor version of Data Path Resource Container API
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dprc_get_api_version(struct fsl_mc_io *mc_io,
+			 u32 cmd_flags,
+			 u16 *major_ver,
+			 u16 *minor_ver)
+{
+	struct fsl_mc_command cmd = { 0 };
+	int err;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_API_VERSION,
+					  cmd_flags, 0);
+
+	/* send command to mc */
+	err = mc_send_command(mc_io, &cmd);
+	if (err)
+		return err;
+
+	/* retrieve response parameters */
+	mc_cmd_read_api_version(&cmd, major_ver, minor_ver);
+
+	return 0;
+}
+
+/**
+ * dprc_get_container_id - Get container ID associated with a given portal.
+ * @mc_io:		Pointer to Mc portal's I/O object
+ * @cmd_flags:		Command flags; one or more of 'MC_CMD_FLAG_'
+ * @container_id:	Requested container id
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+int dprc_get_container_id(struct fsl_mc_io *mc_io,
+			  u32 cmd_flags,
+			  int *container_id)
+{
+	struct fsl_mc_command cmd = { 0 };
+	int err;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPRC_CMDID_GET_CONT_ID,
+					  cmd_flags,
+					  0);
+
+	/* send command to mc*/
+	err = mc_send_command(mc_io, &cmd);
+	if (err)
+		return err;
+
+	/* retrieve response parameters */
+	*container_id = (int)mc_cmd_read_object_id(&cmd);
+
+	return 0;
+}
--- a/drivers/staging/fsl-mc/bus/fsl-mc-allocator.c
+++ /dev/null
@@ -1,663 +0,0 @@
-// SPDX-License-Identifier: GPL-2.0
-/*
- * fsl-mc object allocator driver
- *
- * Copyright (C) 2013-2016 Freescale Semiconductor, Inc.
- *
- */
-
-#include <linux/module.h>
-#include <linux/msi.h>
-#include "../include/mc.h"
-
-#include "fsl-mc-private.h"
-
-static bool __must_check fsl_mc_is_allocatable(const char *obj_type)
-{
-	return strcmp(obj_type, "dpbp") == 0 ||
-	       strcmp(obj_type, "dpmcp") == 0 ||
-	       strcmp(obj_type, "dpcon") == 0;
-}
-
-/**
- * fsl_mc_resource_pool_add_device - add allocatable object to a resource
- * pool of a given fsl-mc bus
- *
- * @mc_bus: pointer to the fsl-mc bus
- * @pool_type: pool type
- * @mc_dev: pointer to allocatable fsl-mc device
- */
-static int __must_check fsl_mc_resource_pool_add_device(struct fsl_mc_bus
-								*mc_bus,
-							enum fsl_mc_pool_type
-								pool_type,
-							struct fsl_mc_device
-								*mc_dev)
-{
-	struct fsl_mc_resource_pool *res_pool;
-	struct fsl_mc_resource *resource;
-	struct fsl_mc_device *mc_bus_dev = &mc_bus->mc_dev;
-	int error = -EINVAL;
-
-	if (WARN_ON(pool_type < 0 || pool_type >= FSL_MC_NUM_POOL_TYPES))
-		goto out;
-	if (WARN_ON(!fsl_mc_is_allocatable(mc_dev->obj_desc.type)))
-		goto out;
-	if (WARN_ON(mc_dev->resource))
-		goto out;
-
-	res_pool = &mc_bus->resource_pools[pool_type];
-	if (WARN_ON(res_pool->type != pool_type))
-		goto out;
-	if (WARN_ON(res_pool->mc_bus != mc_bus))
-		goto out;
-
-	mutex_lock(&res_pool->mutex);
-
-	if (WARN_ON(res_pool->max_count < 0))
-		goto out_unlock;
-	if (WARN_ON(res_pool->free_count < 0 ||
-		    res_pool->free_count > res_pool->max_count))
-		goto out_unlock;
-
-	resource = devm_kzalloc(&mc_bus_dev->dev, sizeof(*resource),
-				GFP_KERNEL);
-	if (!resource) {
-		error = -ENOMEM;
-		dev_err(&mc_bus_dev->dev,
-			"Failed to allocate memory for fsl_mc_resource\n");
-		goto out_unlock;
-	}
-
-	resource->type = pool_type;
-	resource->id = mc_dev->obj_desc.id;
-	resource->data = mc_dev;
-	resource->parent_pool = res_pool;
-	INIT_LIST_HEAD(&resource->node);
-	list_add_tail(&resource->node, &res_pool->free_list);
-	mc_dev->resource = resource;
-	res_pool->free_count++;
-	res_pool->max_count++;
-	error = 0;
-out_unlock:
-	mutex_unlock(&res_pool->mutex);
-out:
-	return error;
-}
-
-/**
- * fsl_mc_resource_pool_remove_device - remove an allocatable device from a
- * resource pool
- *
- * @mc_dev: pointer to allocatable fsl-mc device
- *
- * It permanently removes an allocatable fsl-mc device from the resource
- * pool. It's an error if the device is in use.
- */
-static int __must_check fsl_mc_resource_pool_remove_device(struct fsl_mc_device
-								   *mc_dev)
-{
-	struct fsl_mc_device *mc_bus_dev;
-	struct fsl_mc_bus *mc_bus;
-	struct fsl_mc_resource_pool *res_pool;
-	struct fsl_mc_resource *resource;
-	int error = -EINVAL;
-
-	if (WARN_ON(!fsl_mc_is_allocatable(mc_dev->obj_desc.type)))
-		goto out;
-
-	resource = mc_dev->resource;
-	if (WARN_ON(!resource || resource->data != mc_dev))
-		goto out;
-
-	mc_bus_dev = to_fsl_mc_device(mc_dev->dev.parent);
-	mc_bus = to_fsl_mc_bus(mc_bus_dev);
-	res_pool = resource->parent_pool;
-	if (WARN_ON(res_pool != &mc_bus->resource_pools[resource->type]))
-		goto out;
-
-	mutex_lock(&res_pool->mutex);
-
-	if (WARN_ON(res_pool->max_count <= 0))
-		goto out_unlock;
-	if (WARN_ON(res_pool->free_count <= 0 ||
-		    res_pool->free_count > res_pool->max_count))
-		goto out_unlock;
-
-	/*
-	 * If the device is currently allocated, its resource is not
-	 * in the free list and thus, the device cannot be removed.
-	 */
-	if (list_empty(&resource->node)) {
-		error = -EBUSY;
-		dev_err(&mc_bus_dev->dev,
-			"Device %s cannot be removed from resource pool\n",
-			dev_name(&mc_dev->dev));
-		goto out_unlock;
-	}
-
-	list_del_init(&resource->node);
-	res_pool->free_count--;
-	res_pool->max_count--;
-
-	devm_kfree(&mc_bus_dev->dev, resource);
-	mc_dev->resource = NULL;
-	error = 0;
-out_unlock:
-	mutex_unlock(&res_pool->mutex);
-out:
-	return error;
-}
-
-static const char *const fsl_mc_pool_type_strings[] = {
-	[FSL_MC_POOL_DPMCP] = "dpmcp",
-	[FSL_MC_POOL_DPBP] = "dpbp",
-	[FSL_MC_POOL_DPCON] = "dpcon",
-	[FSL_MC_POOL_IRQ] = "irq",
-};
-
-static int __must_check object_type_to_pool_type(const char *object_type,
-						 enum fsl_mc_pool_type
-								*pool_type)
-{
-	unsigned int i;
-
-	for (i = 0; i < ARRAY_SIZE(fsl_mc_pool_type_strings); i++) {
-		if (strcmp(object_type, fsl_mc_pool_type_strings[i]) == 0) {
-			*pool_type = i;
-			return 0;
-		}
-	}
-
-	return -EINVAL;
-}
-
-int __must_check fsl_mc_resource_allocate(struct fsl_mc_bus *mc_bus,
-					  enum fsl_mc_pool_type pool_type,
-					  struct fsl_mc_resource **new_resource)
-{
-	struct fsl_mc_resource_pool *res_pool;
-	struct fsl_mc_resource *resource;
-	struct fsl_mc_device *mc_bus_dev = &mc_bus->mc_dev;
-	int error = -EINVAL;
-
-	BUILD_BUG_ON(ARRAY_SIZE(fsl_mc_pool_type_strings) !=
-		     FSL_MC_NUM_POOL_TYPES);
-
-	*new_resource = NULL;
-	if (WARN_ON(pool_type < 0 || pool_type >= FSL_MC_NUM_POOL_TYPES))
-		goto out;
-
-	res_pool = &mc_bus->resource_pools[pool_type];
-	if (WARN_ON(res_pool->mc_bus != mc_bus))
-		goto out;
-
-	mutex_lock(&res_pool->mutex);
-	resource = list_first_entry_or_null(&res_pool->free_list,
-					    struct fsl_mc_resource, node);
-
-	if (!resource) {
-		WARN_ON(res_pool->free_count != 0);
-		error = -ENXIO;
-		dev_err(&mc_bus_dev->dev,
-			"No more resources of type %s left\n",
-			fsl_mc_pool_type_strings[pool_type]);
-		goto out_unlock;
-	}
-
-	if (WARN_ON(resource->type != pool_type))
-		goto out_unlock;
-	if (WARN_ON(resource->parent_pool != res_pool))
-		goto out_unlock;
-	if (WARN_ON(res_pool->free_count <= 0 ||
-		    res_pool->free_count > res_pool->max_count))
-		goto out_unlock;
-
-	list_del_init(&resource->node);
-
-	res_pool->free_count--;
-	error = 0;
-out_unlock:
-	mutex_unlock(&res_pool->mutex);
-	*new_resource = resource;
-out:
-	return error;
-}
-EXPORT_SYMBOL_GPL(fsl_mc_resource_allocate);
-
-void fsl_mc_resource_free(struct fsl_mc_resource *resource)
-{
-	struct fsl_mc_resource_pool *res_pool;
-
-	res_pool = resource->parent_pool;
-	if (WARN_ON(resource->type != res_pool->type))
-		return;
-
-	mutex_lock(&res_pool->mutex);
-	if (WARN_ON(res_pool->free_count < 0 ||
-		    res_pool->free_count >= res_pool->max_count))
-		goto out_unlock;
-
-	if (WARN_ON(!list_empty(&resource->node)))
-		goto out_unlock;
-
-	list_add_tail(&resource->node, &res_pool->free_list);
-	res_pool->free_count++;
-out_unlock:
-	mutex_unlock(&res_pool->mutex);
-}
-EXPORT_SYMBOL_GPL(fsl_mc_resource_free);
-
-/**
- * fsl_mc_object_allocate - Allocates an fsl-mc object of the given
- * pool type from a given fsl-mc bus instance
- *
- * @mc_dev: fsl-mc device which is used in conjunction with the
- * allocated object
- * @pool_type: pool type
- * @new_mc_dev: pointer to area where the pointer to the allocated device
- * is to be returned
- *
- * Allocatable objects are always used in conjunction with some functional
- * device.  This function allocates an object of the specified type from
- * the DPRC containing the functional device.
- *
- * NOTE: pool_type must be different from FSL_MC_POOL_MCP, since MC
- * portals are allocated using fsl_mc_portal_allocate(), instead of
- * this function.
- */
-int __must_check fsl_mc_object_allocate(struct fsl_mc_device *mc_dev,
-					enum fsl_mc_pool_type pool_type,
-					struct fsl_mc_device **new_mc_adev)
-{
-	struct fsl_mc_device *mc_bus_dev;
-	struct fsl_mc_bus *mc_bus;
-	struct fsl_mc_device *mc_adev;
-	int error = -EINVAL;
-	struct fsl_mc_resource *resource = NULL;
-
-	*new_mc_adev = NULL;
-	if (WARN_ON(mc_dev->flags & FSL_MC_IS_DPRC))
-		goto error;
-
-	if (WARN_ON(!dev_is_fsl_mc(mc_dev->dev.parent)))
-		goto error;
-
-	if (WARN_ON(pool_type == FSL_MC_POOL_DPMCP))
-		goto error;
-
-	mc_bus_dev = to_fsl_mc_device(mc_dev->dev.parent);
-	mc_bus = to_fsl_mc_bus(mc_bus_dev);
-	error = fsl_mc_resource_allocate(mc_bus, pool_type, &resource);
-	if (error < 0)
-		goto error;
-
-	mc_adev = resource->data;
-	if (WARN_ON(!mc_adev))
-		goto error;
-
-	*new_mc_adev = mc_adev;
-	return 0;
-error:
-	if (resource)
-		fsl_mc_resource_free(resource);
-
-	return error;
-}
-EXPORT_SYMBOL_GPL(fsl_mc_object_allocate);
-
-/**
- * fsl_mc_object_free - Returns an fsl-mc object to the resource
- * pool where it came from.
- * @mc_adev: Pointer to the fsl-mc device
- */
-void fsl_mc_object_free(struct fsl_mc_device *mc_adev)
-{
-	struct fsl_mc_resource *resource;
-
-	resource = mc_adev->resource;
-	if (WARN_ON(resource->type == FSL_MC_POOL_DPMCP))
-		return;
-	if (WARN_ON(resource->data != mc_adev))
-		return;
-
-	fsl_mc_resource_free(resource);
-}
-EXPORT_SYMBOL_GPL(fsl_mc_object_free);
-
-/*
- * A DPRC and the devices in the DPRC all share the same GIC-ITS device
- * ID.  A block of IRQs is pre-allocated and maintained in a pool
- * from which devices can allocate them when needed.
- */
-
-/*
- * Initialize the interrupt pool associated with an fsl-mc bus.
- * It allocates a block of IRQs from the GIC-ITS.
- */
-int fsl_mc_populate_irq_pool(struct fsl_mc_bus *mc_bus,
-			     unsigned int irq_count)
-{
-	unsigned int i;
-	struct msi_desc *msi_desc;
-	struct fsl_mc_device_irq *irq_resources;
-	struct fsl_mc_device_irq *mc_dev_irq;
-	int error;
-	struct fsl_mc_device *mc_bus_dev = &mc_bus->mc_dev;
-	struct fsl_mc_resource_pool *res_pool =
-			&mc_bus->resource_pools[FSL_MC_POOL_IRQ];
-
-	if (WARN_ON(irq_count == 0 ||
-		    irq_count > FSL_MC_IRQ_POOL_MAX_TOTAL_IRQS))
-		return -EINVAL;
-
-	error = fsl_mc_msi_domain_alloc_irqs(&mc_bus_dev->dev, irq_count);
-	if (error < 0)
-		return error;
-
-	irq_resources = devm_kzalloc(&mc_bus_dev->dev,
-				     sizeof(*irq_resources) * irq_count,
-				     GFP_KERNEL);
-	if (!irq_resources) {
-		error = -ENOMEM;
-		goto cleanup_msi_irqs;
-	}
-
-	for (i = 0; i < irq_count; i++) {
-		mc_dev_irq = &irq_resources[i];
-
-		/*
-		 * NOTE: This mc_dev_irq's MSI addr/value pair will be set
-		 * by the fsl_mc_msi_write_msg() callback
-		 */
-		mc_dev_irq->resource.type = res_pool->type;
-		mc_dev_irq->resource.data = mc_dev_irq;
-		mc_dev_irq->resource.parent_pool = res_pool;
-		INIT_LIST_HEAD(&mc_dev_irq->resource.node);
-		list_add_tail(&mc_dev_irq->resource.node, &res_pool->free_list);
-	}
-
-	for_each_msi_entry(msi_desc, &mc_bus_dev->dev) {
-		mc_dev_irq = &irq_resources[msi_desc->fsl_mc.msi_index];
-		mc_dev_irq->msi_desc = msi_desc;
-		mc_dev_irq->resource.id = msi_desc->irq;
-	}
-
-	res_pool->max_count = irq_count;
-	res_pool->free_count = irq_count;
-	mc_bus->irq_resources = irq_resources;
-	return 0;
-
-cleanup_msi_irqs:
-	fsl_mc_msi_domain_free_irqs(&mc_bus_dev->dev);
-	return error;
-}
-EXPORT_SYMBOL_GPL(fsl_mc_populate_irq_pool);
-
-/**
- * Teardown the interrupt pool associated with an fsl-mc bus.
- * It frees the IRQs that were allocated to the pool, back to the GIC-ITS.
- */
-void fsl_mc_cleanup_irq_pool(struct fsl_mc_bus *mc_bus)
-{
-	struct fsl_mc_device *mc_bus_dev = &mc_bus->mc_dev;
-	struct fsl_mc_resource_pool *res_pool =
-			&mc_bus->resource_pools[FSL_MC_POOL_IRQ];
-
-	if (WARN_ON(!mc_bus->irq_resources))
-		return;
-
-	if (WARN_ON(res_pool->max_count == 0))
-		return;
-
-	if (WARN_ON(res_pool->free_count != res_pool->max_count))
-		return;
-
-	INIT_LIST_HEAD(&res_pool->free_list);
-	res_pool->max_count = 0;
-	res_pool->free_count = 0;
-	mc_bus->irq_resources = NULL;
-	fsl_mc_msi_domain_free_irqs(&mc_bus_dev->dev);
-}
-EXPORT_SYMBOL_GPL(fsl_mc_cleanup_irq_pool);
-
-/**
- * Allocate the IRQs required by a given fsl-mc device.
- */
-int __must_check fsl_mc_allocate_irqs(struct fsl_mc_device *mc_dev)
-{
-	int i;
-	int irq_count;
-	int res_allocated_count = 0;
-	int error = -EINVAL;
-	struct fsl_mc_device_irq **irqs = NULL;
-	struct fsl_mc_bus *mc_bus;
-	struct fsl_mc_resource_pool *res_pool;
-
-	if (WARN_ON(mc_dev->irqs))
-		return -EINVAL;
-
-	irq_count = mc_dev->obj_desc.irq_count;
-	if (WARN_ON(irq_count == 0))
-		return -EINVAL;
-
-	if (strcmp(mc_dev->obj_desc.type, "dprc") == 0)
-		mc_bus = to_fsl_mc_bus(mc_dev);
-	else
-		mc_bus = to_fsl_mc_bus(to_fsl_mc_device(mc_dev->dev.parent));
-
-	if (WARN_ON(!mc_bus->irq_resources))
-		return -EINVAL;
-
-	res_pool = &mc_bus->resource_pools[FSL_MC_POOL_IRQ];
-	if (res_pool->free_count < irq_count) {
-		dev_err(&mc_dev->dev,
-			"Not able to allocate %u irqs for device\n", irq_count);
-		return -ENOSPC;
-	}
-
-	irqs = devm_kzalloc(&mc_dev->dev, irq_count * sizeof(irqs[0]),
-			    GFP_KERNEL);
-	if (!irqs)
-		return -ENOMEM;
-
-	for (i = 0; i < irq_count; i++) {
-		struct fsl_mc_resource *resource;
-
-		error = fsl_mc_resource_allocate(mc_bus, FSL_MC_POOL_IRQ,
-						 &resource);
-		if (error < 0)
-			goto error_resource_alloc;
-
-		irqs[i] = to_fsl_mc_irq(resource);
-		res_allocated_count++;
-
-		WARN_ON(irqs[i]->mc_dev);
-		irqs[i]->mc_dev = mc_dev;
-		irqs[i]->dev_irq_index = i;
-	}
-
-	mc_dev->irqs = irqs;
-	return 0;
-
-error_resource_alloc:
-	for (i = 0; i < res_allocated_count; i++) {
-		irqs[i]->mc_dev = NULL;
-		fsl_mc_resource_free(&irqs[i]->resource);
-	}
-
-	return error;
-}
-EXPORT_SYMBOL_GPL(fsl_mc_allocate_irqs);
-
-/*
- * Frees the IRQs that were allocated for an fsl-mc device.
- */
-void fsl_mc_free_irqs(struct fsl_mc_device *mc_dev)
-{
-	int i;
-	int irq_count;
-	struct fsl_mc_bus *mc_bus;
-	struct fsl_mc_device_irq **irqs = mc_dev->irqs;
-
-	if (WARN_ON(!irqs))
-		return;
-
-	irq_count = mc_dev->obj_desc.irq_count;
-
-	if (strcmp(mc_dev->obj_desc.type, "dprc") == 0)
-		mc_bus = to_fsl_mc_bus(mc_dev);
-	else
-		mc_bus = to_fsl_mc_bus(to_fsl_mc_device(mc_dev->dev.parent));
-
-	if (WARN_ON(!mc_bus->irq_resources))
-		return;
-
-	for (i = 0; i < irq_count; i++) {
-		WARN_ON(!irqs[i]->mc_dev);
-		irqs[i]->mc_dev = NULL;
-		fsl_mc_resource_free(&irqs[i]->resource);
-	}
-
-	mc_dev->irqs = NULL;
-}
-EXPORT_SYMBOL_GPL(fsl_mc_free_irqs);
-
-void fsl_mc_init_all_resource_pools(struct fsl_mc_device *mc_bus_dev)
-{
-	int pool_type;
-	struct fsl_mc_bus *mc_bus = to_fsl_mc_bus(mc_bus_dev);
-
-	for (pool_type = 0; pool_type < FSL_MC_NUM_POOL_TYPES; pool_type++) {
-		struct fsl_mc_resource_pool *res_pool =
-		    &mc_bus->resource_pools[pool_type];
-
-		res_pool->type = pool_type;
-		res_pool->max_count = 0;
-		res_pool->free_count = 0;
-		res_pool->mc_bus = mc_bus;
-		INIT_LIST_HEAD(&res_pool->free_list);
-		mutex_init(&res_pool->mutex);
-	}
-}
-
-static void fsl_mc_cleanup_resource_pool(struct fsl_mc_device *mc_bus_dev,
-					 enum fsl_mc_pool_type pool_type)
-{
-	struct fsl_mc_resource *resource;
-	struct fsl_mc_resource *next;
-	struct fsl_mc_bus *mc_bus = to_fsl_mc_bus(mc_bus_dev);
-	struct fsl_mc_resource_pool *res_pool =
-					&mc_bus->resource_pools[pool_type];
-	int free_count = 0;
-
-	WARN_ON(res_pool->type != pool_type);
-	WARN_ON(res_pool->free_count != res_pool->max_count);
-
-	list_for_each_entry_safe(resource, next, &res_pool->free_list, node) {
-		free_count++;
-		WARN_ON(resource->type != res_pool->type);
-		WARN_ON(resource->parent_pool != res_pool);
-		devm_kfree(&mc_bus_dev->dev, resource);
-	}
-
-	WARN_ON(free_count != res_pool->free_count);
-}
-
-void fsl_mc_cleanup_all_resource_pools(struct fsl_mc_device *mc_bus_dev)
-{
-	int pool_type;
-
-	for (pool_type = 0; pool_type < FSL_MC_NUM_POOL_TYPES; pool_type++)
-		fsl_mc_cleanup_resource_pool(mc_bus_dev, pool_type);
-}
-
-/**
- * fsl_mc_allocator_probe - callback invoked when an allocatable device is
- * being added to the system
- */
-static int fsl_mc_allocator_probe(struct fsl_mc_device *mc_dev)
-{
-	enum fsl_mc_pool_type pool_type;
-	struct fsl_mc_device *mc_bus_dev;
-	struct fsl_mc_bus *mc_bus;
-	int error;
-
-	if (WARN_ON(!fsl_mc_is_allocatable(mc_dev->obj_desc.type)))
-		return -EINVAL;
-
-	mc_bus_dev = to_fsl_mc_device(mc_dev->dev.parent);
-	if (WARN_ON(!dev_is_fsl_mc(&mc_bus_dev->dev)))
-		return -EINVAL;
-
-	mc_bus = to_fsl_mc_bus(mc_bus_dev);
-	error = object_type_to_pool_type(mc_dev->obj_desc.type, &pool_type);
-	if (error < 0)
-		return error;
-
-	error = fsl_mc_resource_pool_add_device(mc_bus, pool_type, mc_dev);
-	if (error < 0)
-		return error;
-
-	dev_dbg(&mc_dev->dev,
-		"Allocatable fsl-mc device bound to fsl_mc_allocator driver");
-	return 0;
-}
-
-/**
- * fsl_mc_allocator_remove - callback invoked when an allocatable device is
- * being removed from the system
- */
-static int fsl_mc_allocator_remove(struct fsl_mc_device *mc_dev)
-{
-	int error;
-
-	if (WARN_ON(!fsl_mc_is_allocatable(mc_dev->obj_desc.type)))
-		return -EINVAL;
-
-	if (mc_dev->resource) {
-		error = fsl_mc_resource_pool_remove_device(mc_dev);
-		if (error < 0)
-			return error;
-	}
-
-	dev_dbg(&mc_dev->dev,
-		"Allocatable fsl-mc device unbound from fsl_mc_allocator driver");
-	return 0;
-}
-
-static const struct fsl_mc_device_id match_id_table[] = {
-	{
-	 .vendor = FSL_MC_VENDOR_FREESCALE,
-	 .obj_type = "dpbp",
-	},
-	{
-	 .vendor = FSL_MC_VENDOR_FREESCALE,
-	 .obj_type = "dpmcp",
-	},
-	{
-	 .vendor = FSL_MC_VENDOR_FREESCALE,
-	 .obj_type = "dpcon",
-	},
-	{.vendor = 0x0},
-};
-
-static struct fsl_mc_driver fsl_mc_allocator_driver = {
-	.driver = {
-		   .name = "fsl_mc_allocator",
-		   .pm = NULL,
-		   },
-	.match_id_table = match_id_table,
-	.probe = fsl_mc_allocator_probe,
-	.remove = fsl_mc_allocator_remove,
-};
-
-int __init fsl_mc_allocator_driver_init(void)
-{
-	return fsl_mc_driver_register(&fsl_mc_allocator_driver);
-}
-
-void fsl_mc_allocator_driver_exit(void)
-{
-	fsl_mc_driver_unregister(&fsl_mc_allocator_driver);
-}
--- /dev/null
+++ b/drivers/bus/fsl-mc/fsl-mc-allocator.c
@@ -0,0 +1,666 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * fsl-mc object allocator driver
+ *
+ * Copyright (C) 2013-2016 Freescale Semiconductor, Inc.
+ *
+ */
+
+#include <linux/module.h>
+#include <linux/msi.h>
+#include <linux/fsl/mc.h>
+
+#include "fsl-mc-private.h"
+
+static bool __must_check fsl_mc_is_allocatable(struct fsl_mc_device *mc_dev)
+{
+	return is_fsl_mc_bus_dpbp(mc_dev) ||
+	       is_fsl_mc_bus_dpmcp(mc_dev) ||
+	       is_fsl_mc_bus_dpcon(mc_dev);
+}
+
+/**
+ * fsl_mc_resource_pool_add_device - add allocatable object to a resource
+ * pool of a given fsl-mc bus
+ *
+ * @mc_bus: pointer to the fsl-mc bus
+ * @pool_type: pool type
+ * @mc_dev: pointer to allocatable fsl-mc device
+ */
+static int __must_check fsl_mc_resource_pool_add_device(struct fsl_mc_bus
+								*mc_bus,
+							enum fsl_mc_pool_type
+								pool_type,
+							struct fsl_mc_device
+								*mc_dev)
+{
+	struct fsl_mc_resource_pool *res_pool;
+	struct fsl_mc_resource *resource;
+	struct fsl_mc_device *mc_bus_dev = &mc_bus->mc_dev;
+	int error = -EINVAL;
+
+	if (pool_type < 0 || pool_type >= FSL_MC_NUM_POOL_TYPES)
+		goto out;
+	if (!fsl_mc_is_allocatable(mc_dev))
+		goto out;
+	if (mc_dev->resource)
+		goto out;
+
+	res_pool = &mc_bus->resource_pools[pool_type];
+	if (res_pool->type != pool_type)
+		goto out;
+	if (res_pool->mc_bus != mc_bus)
+		goto out;
+
+	mutex_lock(&res_pool->mutex);
+
+	if (res_pool->max_count < 0)
+		goto out_unlock;
+	if (res_pool->free_count < 0 ||
+	    res_pool->free_count > res_pool->max_count)
+		goto out_unlock;
+
+	resource = devm_kzalloc(&mc_bus_dev->dev, sizeof(*resource),
+				GFP_KERNEL);
+	if (!resource) {
+		error = -ENOMEM;
+		dev_err(&mc_bus_dev->dev,
+			"Failed to allocate memory for fsl_mc_resource\n");
+		goto out_unlock;
+	}
+
+	resource->type = pool_type;
+	resource->id = mc_dev->obj_desc.id;
+	resource->data = mc_dev;
+	resource->parent_pool = res_pool;
+	INIT_LIST_HEAD(&resource->node);
+	list_add_tail(&resource->node, &res_pool->free_list);
+	mc_dev->resource = resource;
+	res_pool->free_count++;
+	res_pool->max_count++;
+	error = 0;
+out_unlock:
+	mutex_unlock(&res_pool->mutex);
+out:
+	return error;
+}
+
+/**
+ * fsl_mc_resource_pool_remove_device - remove an allocatable device from a
+ * resource pool
+ *
+ * @mc_dev: pointer to allocatable fsl-mc device
+ *
+ * It permanently removes an allocatable fsl-mc device from the resource
+ * pool. It's an error if the device is in use.
+ */
+static int __must_check fsl_mc_resource_pool_remove_device(struct fsl_mc_device
+								   *mc_dev)
+{
+	struct fsl_mc_device *mc_bus_dev;
+	struct fsl_mc_bus *mc_bus;
+	struct fsl_mc_resource_pool *res_pool;
+	struct fsl_mc_resource *resource;
+	int error = -EINVAL;
+
+	if (!fsl_mc_is_allocatable(mc_dev))
+		goto out;
+
+	resource = mc_dev->resource;
+	if (!resource || resource->data != mc_dev)
+		goto out;
+
+	mc_bus_dev = to_fsl_mc_device(mc_dev->dev.parent);
+	mc_bus = to_fsl_mc_bus(mc_bus_dev);
+	res_pool = resource->parent_pool;
+	if (res_pool != &mc_bus->resource_pools[resource->type])
+		goto out;
+
+	mutex_lock(&res_pool->mutex);
+
+	if (res_pool->max_count <= 0)
+		goto out_unlock;
+	if (res_pool->free_count <= 0 ||
+	    res_pool->free_count > res_pool->max_count)
+		goto out_unlock;
+
+	/*
+	 * If the device is currently allocated, its resource is not
+	 * in the free list and thus, the device cannot be removed.
+	 */
+	if (list_empty(&resource->node)) {
+		error = -EBUSY;
+		dev_err(&mc_bus_dev->dev,
+			"Device %s cannot be removed from resource pool\n",
+			dev_name(&mc_dev->dev));
+		goto out_unlock;
+	}
+
+	list_del_init(&resource->node);
+	res_pool->free_count--;
+	res_pool->max_count--;
+
+	devm_kfree(&mc_bus_dev->dev, resource);
+	mc_dev->resource = NULL;
+	error = 0;
+out_unlock:
+	mutex_unlock(&res_pool->mutex);
+out:
+	return error;
+}
+
+static const char *const fsl_mc_pool_type_strings[] = {
+	[FSL_MC_POOL_DPMCP] = "dpmcp",
+	[FSL_MC_POOL_DPBP] = "dpbp",
+	[FSL_MC_POOL_DPCON] = "dpcon",
+	[FSL_MC_POOL_IRQ] = "irq",
+};
+
+static int __must_check object_type_to_pool_type(const char *object_type,
+						 enum fsl_mc_pool_type
+								*pool_type)
+{
+	unsigned int i;
+
+	for (i = 0; i < ARRAY_SIZE(fsl_mc_pool_type_strings); i++) {
+		if (strcmp(object_type, fsl_mc_pool_type_strings[i]) == 0) {
+			*pool_type = i;
+			return 0;
+		}
+	}
+
+	return -EINVAL;
+}
+
+int __must_check fsl_mc_resource_allocate(struct fsl_mc_bus *mc_bus,
+					  enum fsl_mc_pool_type pool_type,
+					  struct fsl_mc_resource **new_resource)
+{
+	struct fsl_mc_resource_pool *res_pool;
+	struct fsl_mc_resource *resource;
+	struct fsl_mc_device *mc_bus_dev = &mc_bus->mc_dev;
+	int error = -EINVAL;
+
+	BUILD_BUG_ON(ARRAY_SIZE(fsl_mc_pool_type_strings) !=
+		     FSL_MC_NUM_POOL_TYPES);
+
+	*new_resource = NULL;
+	if (pool_type < 0 || pool_type >= FSL_MC_NUM_POOL_TYPES)
+		goto out;
+
+	res_pool = &mc_bus->resource_pools[pool_type];
+	if (res_pool->mc_bus != mc_bus)
+		goto out;
+
+	mutex_lock(&res_pool->mutex);
+	resource = list_first_entry_or_null(&res_pool->free_list,
+					    struct fsl_mc_resource, node);
+
+	if (!resource) {
+		error = -ENXIO;
+		dev_err(&mc_bus_dev->dev,
+			"No more resources of type %s left\n",
+			fsl_mc_pool_type_strings[pool_type]);
+		goto out_unlock;
+	}
+
+	if (resource->type != pool_type)
+		goto out_unlock;
+	if (resource->parent_pool != res_pool)
+		goto out_unlock;
+	if (res_pool->free_count <= 0 ||
+	    res_pool->free_count > res_pool->max_count)
+		goto out_unlock;
+
+	list_del_init(&resource->node);
+
+	res_pool->free_count--;
+	error = 0;
+out_unlock:
+	mutex_unlock(&res_pool->mutex);
+	*new_resource = resource;
+out:
+	return error;
+}
+EXPORT_SYMBOL_GPL(fsl_mc_resource_allocate);
+
+void fsl_mc_resource_free(struct fsl_mc_resource *resource)
+{
+	struct fsl_mc_resource_pool *res_pool;
+
+	res_pool = resource->parent_pool;
+	if (resource->type != res_pool->type)
+		return;
+
+	mutex_lock(&res_pool->mutex);
+	if (res_pool->free_count < 0 ||
+	    res_pool->free_count >= res_pool->max_count)
+		goto out_unlock;
+
+	if (!list_empty(&resource->node))
+		goto out_unlock;
+
+	list_add_tail(&resource->node, &res_pool->free_list);
+	res_pool->free_count++;
+out_unlock:
+	mutex_unlock(&res_pool->mutex);
+}
+EXPORT_SYMBOL_GPL(fsl_mc_resource_free);
+
+/**
+ * fsl_mc_object_allocate - Allocates an fsl-mc object of the given
+ * pool type from a given fsl-mc bus instance
+ *
+ * @mc_dev: fsl-mc device which is used in conjunction with the
+ * allocated object
+ * @pool_type: pool type
+ * @new_mc_dev: pointer to area where the pointer to the allocated device
+ * is to be returned
+ *
+ * Allocatable objects are always used in conjunction with some functional
+ * device.  This function allocates an object of the specified type from
+ * the DPRC containing the functional device.
+ *
+ * NOTE: pool_type must be different from FSL_MC_POOL_MCP, since MC
+ * portals are allocated using fsl_mc_portal_allocate(), instead of
+ * this function.
+ */
+int __must_check fsl_mc_object_allocate(struct fsl_mc_device *mc_dev,
+					enum fsl_mc_pool_type pool_type,
+					struct fsl_mc_device **new_mc_adev)
+{
+	struct fsl_mc_device *mc_bus_dev;
+	struct fsl_mc_bus *mc_bus;
+	struct fsl_mc_device *mc_adev;
+	int error = -EINVAL;
+	struct fsl_mc_resource *resource = NULL;
+
+	*new_mc_adev = NULL;
+	if (mc_dev->flags & FSL_MC_IS_DPRC)
+		goto error;
+
+	if (!dev_is_fsl_mc(mc_dev->dev.parent))
+		goto error;
+
+	if (pool_type == FSL_MC_POOL_DPMCP)
+		goto error;
+
+	mc_bus_dev = to_fsl_mc_device(mc_dev->dev.parent);
+	mc_bus = to_fsl_mc_bus(mc_bus_dev);
+	error = fsl_mc_resource_allocate(mc_bus, pool_type, &resource);
+	if (error < 0)
+		goto error;
+
+	mc_adev = resource->data;
+	if (!mc_adev)
+		goto error;
+
+	mc_adev->consumer_link = device_link_add(&mc_dev->dev,
+						 &mc_adev->dev,
+						 DL_FLAG_AUTOREMOVE_CONSUMER);
+	if (!mc_adev->consumer_link) {
+		error = -EINVAL;
+		goto error;
+	}
+
+	*new_mc_adev = mc_adev;
+	return 0;
+error:
+	if (resource)
+		fsl_mc_resource_free(resource);
+
+	return error;
+}
+EXPORT_SYMBOL_GPL(fsl_mc_object_allocate);
+
+/**
+ * fsl_mc_object_free - Returns an fsl-mc object to the resource
+ * pool where it came from.
+ * @mc_adev: Pointer to the fsl-mc device
+ */
+void fsl_mc_object_free(struct fsl_mc_device *mc_adev)
+{
+	struct fsl_mc_resource *resource;
+
+	resource = mc_adev->resource;
+	if (resource->type == FSL_MC_POOL_DPMCP)
+		return;
+	if (resource->data != mc_adev)
+		return;
+
+	fsl_mc_resource_free(resource);
+
+	device_link_del(mc_adev->consumer_link);
+	mc_adev->consumer_link = NULL;
+}
+EXPORT_SYMBOL_GPL(fsl_mc_object_free);
+
+/*
+ * A DPRC and the devices in the DPRC all share the same GIC-ITS device
+ * ID.  A block of IRQs is pre-allocated and maintained in a pool
+ * from which devices can allocate them when needed.
+ */
+
+/*
+ * Initialize the interrupt pool associated with an fsl-mc bus.
+ * It allocates a block of IRQs from the GIC-ITS.
+ */
+int fsl_mc_populate_irq_pool(struct fsl_mc_bus *mc_bus,
+			     unsigned int irq_count)
+{
+	unsigned int i;
+	struct msi_desc *msi_desc;
+	struct fsl_mc_device_irq *irq_resources;
+	struct fsl_mc_device_irq *mc_dev_irq;
+	int error;
+	struct fsl_mc_device *mc_bus_dev = &mc_bus->mc_dev;
+	struct fsl_mc_resource_pool *res_pool =
+			&mc_bus->resource_pools[FSL_MC_POOL_IRQ];
+
+	if (irq_count == 0 ||
+	    irq_count > FSL_MC_IRQ_POOL_MAX_TOTAL_IRQS)
+		return -EINVAL;
+
+	error = fsl_mc_msi_domain_alloc_irqs(&mc_bus_dev->dev, irq_count);
+	if (error < 0)
+		return error;
+
+	irq_resources = devm_kzalloc(&mc_bus_dev->dev,
+				     sizeof(*irq_resources) * irq_count,
+				     GFP_KERNEL);
+	if (!irq_resources) {
+		error = -ENOMEM;
+		goto cleanup_msi_irqs;
+	}
+
+	for (i = 0; i < irq_count; i++) {
+		mc_dev_irq = &irq_resources[i];
+
+		/*
+		 * NOTE: This mc_dev_irq's MSI addr/value pair will be set
+		 * by the fsl_mc_msi_write_msg() callback
+		 */
+		mc_dev_irq->resource.type = res_pool->type;
+		mc_dev_irq->resource.data = mc_dev_irq;
+		mc_dev_irq->resource.parent_pool = res_pool;
+		INIT_LIST_HEAD(&mc_dev_irq->resource.node);
+		list_add_tail(&mc_dev_irq->resource.node, &res_pool->free_list);
+	}
+
+	for_each_msi_entry(msi_desc, &mc_bus_dev->dev) {
+		mc_dev_irq = &irq_resources[msi_desc->fsl_mc.msi_index];
+		mc_dev_irq->msi_desc = msi_desc;
+		mc_dev_irq->resource.id = msi_desc->irq;
+	}
+
+	res_pool->max_count = irq_count;
+	res_pool->free_count = irq_count;
+	mc_bus->irq_resources = irq_resources;
+	return 0;
+
+cleanup_msi_irqs:
+	fsl_mc_msi_domain_free_irqs(&mc_bus_dev->dev);
+	return error;
+}
+EXPORT_SYMBOL_GPL(fsl_mc_populate_irq_pool);
+
+/**
+ * Teardown the interrupt pool associated with an fsl-mc bus.
+ * It frees the IRQs that were allocated to the pool, back to the GIC-ITS.
+ */
+void fsl_mc_cleanup_irq_pool(struct fsl_mc_bus *mc_bus)
+{
+	struct fsl_mc_device *mc_bus_dev = &mc_bus->mc_dev;
+	struct fsl_mc_resource_pool *res_pool =
+			&mc_bus->resource_pools[FSL_MC_POOL_IRQ];
+
+	if (!mc_bus->irq_resources)
+		return;
+
+	if (res_pool->max_count == 0)
+		return;
+
+	if (res_pool->free_count != res_pool->max_count)
+		return;
+
+	INIT_LIST_HEAD(&res_pool->free_list);
+	res_pool->max_count = 0;
+	res_pool->free_count = 0;
+	mc_bus->irq_resources = NULL;
+	fsl_mc_msi_domain_free_irqs(&mc_bus_dev->dev);
+}
+EXPORT_SYMBOL_GPL(fsl_mc_cleanup_irq_pool);
+
+/**
+ * Allocate the IRQs required by a given fsl-mc device.
+ */
+int __must_check fsl_mc_allocate_irqs(struct fsl_mc_device *mc_dev)
+{
+	int i;
+	int irq_count;
+	int res_allocated_count = 0;
+	int error = -EINVAL;
+	struct fsl_mc_device_irq **irqs = NULL;
+	struct fsl_mc_bus *mc_bus;
+	struct fsl_mc_resource_pool *res_pool;
+
+	if (mc_dev->irqs)
+		return -EINVAL;
+
+	irq_count = mc_dev->obj_desc.irq_count;
+	if (irq_count == 0)
+		return -EINVAL;
+
+	if (is_fsl_mc_bus_dprc(mc_dev))
+		mc_bus = to_fsl_mc_bus(mc_dev);
+	else
+		mc_bus = to_fsl_mc_bus(to_fsl_mc_device(mc_dev->dev.parent));
+
+	if (!mc_bus->irq_resources)
+		return -EINVAL;
+
+	res_pool = &mc_bus->resource_pools[FSL_MC_POOL_IRQ];
+	if (res_pool->free_count < irq_count) {
+		dev_err(&mc_dev->dev,
+			"Not able to allocate %u irqs for device\n", irq_count);
+		return -ENOSPC;
+	}
+
+	irqs = devm_kzalloc(&mc_dev->dev, irq_count * sizeof(irqs[0]),
+			    GFP_KERNEL);
+	if (!irqs)
+		return -ENOMEM;
+
+	for (i = 0; i < irq_count; i++) {
+		struct fsl_mc_resource *resource;
+
+		error = fsl_mc_resource_allocate(mc_bus, FSL_MC_POOL_IRQ,
+						 &resource);
+		if (error < 0)
+			goto error_resource_alloc;
+
+		irqs[i] = to_fsl_mc_irq(resource);
+		res_allocated_count++;
+
+		irqs[i]->mc_dev = mc_dev;
+		irqs[i]->dev_irq_index = i;
+	}
+
+	mc_dev->irqs = irqs;
+	return 0;
+
+error_resource_alloc:
+	for (i = 0; i < res_allocated_count; i++) {
+		irqs[i]->mc_dev = NULL;
+		fsl_mc_resource_free(&irqs[i]->resource);
+	}
+
+	return error;
+}
+EXPORT_SYMBOL_GPL(fsl_mc_allocate_irqs);
+
+/*
+ * Frees the IRQs that were allocated for an fsl-mc device.
+ */
+void fsl_mc_free_irqs(struct fsl_mc_device *mc_dev)
+{
+	int i;
+	int irq_count;
+	struct fsl_mc_bus *mc_bus;
+	struct fsl_mc_device_irq **irqs = mc_dev->irqs;
+
+	if (!irqs)
+		return;
+
+	irq_count = mc_dev->obj_desc.irq_count;
+
+	if (is_fsl_mc_bus_dprc(mc_dev))
+		mc_bus = to_fsl_mc_bus(mc_dev);
+	else
+		mc_bus = to_fsl_mc_bus(to_fsl_mc_device(mc_dev->dev.parent));
+
+	if (!mc_bus->irq_resources)
+		return;
+
+	for (i = 0; i < irq_count; i++) {
+		irqs[i]->mc_dev = NULL;
+		fsl_mc_resource_free(&irqs[i]->resource);
+	}
+
+	mc_dev->irqs = NULL;
+}
+EXPORT_SYMBOL_GPL(fsl_mc_free_irqs);
+
+void fsl_mc_init_all_resource_pools(struct fsl_mc_device *mc_bus_dev)
+{
+	int pool_type;
+	struct fsl_mc_bus *mc_bus = to_fsl_mc_bus(mc_bus_dev);
+
+	for (pool_type = 0; pool_type < FSL_MC_NUM_POOL_TYPES; pool_type++) {
+		struct fsl_mc_resource_pool *res_pool =
+		    &mc_bus->resource_pools[pool_type];
+
+		res_pool->type = pool_type;
+		res_pool->max_count = 0;
+		res_pool->free_count = 0;
+		res_pool->mc_bus = mc_bus;
+		INIT_LIST_HEAD(&res_pool->free_list);
+		mutex_init(&res_pool->mutex);
+	}
+}
+EXPORT_SYMBOL_GPL(fsl_mc_init_all_resource_pools);
+
+static void fsl_mc_cleanup_resource_pool(struct fsl_mc_device *mc_bus_dev,
+					 enum fsl_mc_pool_type pool_type)
+{
+	struct fsl_mc_resource *resource;
+	struct fsl_mc_resource *next;
+	struct fsl_mc_bus *mc_bus = to_fsl_mc_bus(mc_bus_dev);
+	struct fsl_mc_resource_pool *res_pool =
+					&mc_bus->resource_pools[pool_type];
+	int free_count = 0;
+
+	list_for_each_entry_safe(resource, next, &res_pool->free_list, node) {
+		free_count++;
+		devm_kfree(&mc_bus_dev->dev, resource);
+	}
+}
+
+void fsl_mc_cleanup_all_resource_pools(struct fsl_mc_device *mc_bus_dev)
+{
+	int pool_type;
+
+	for (pool_type = 0; pool_type < FSL_MC_NUM_POOL_TYPES; pool_type++)
+		fsl_mc_cleanup_resource_pool(mc_bus_dev, pool_type);
+}
+EXPORT_SYMBOL_GPL(fsl_mc_cleanup_all_resource_pools);
+
+/**
+ * fsl_mc_allocator_probe - callback invoked when an allocatable device is
+ * being added to the system
+ */
+static int fsl_mc_allocator_probe(struct fsl_mc_device *mc_dev)
+{
+	enum fsl_mc_pool_type pool_type;
+	struct fsl_mc_device *mc_bus_dev;
+	struct fsl_mc_bus *mc_bus;
+	int error;
+
+	if (!fsl_mc_is_allocatable(mc_dev))
+		return -EINVAL;
+
+	mc_bus_dev = to_fsl_mc_device(mc_dev->dev.parent);
+	if (!dev_is_fsl_mc(&mc_bus_dev->dev))
+		return -EINVAL;
+
+	mc_bus = to_fsl_mc_bus(mc_bus_dev);
+	error = object_type_to_pool_type(mc_dev->obj_desc.type, &pool_type);
+	if (error < 0)
+		return error;
+
+	error = fsl_mc_resource_pool_add_device(mc_bus, pool_type, mc_dev);
+	if (error < 0)
+		return error;
+
+	dev_dbg(&mc_dev->dev,
+		"Allocatable fsl-mc device bound to fsl_mc_allocator driver");
+	return 0;
+}
+
+/**
+ * fsl_mc_allocator_remove - callback invoked when an allocatable device is
+ * being removed from the system
+ */
+static int fsl_mc_allocator_remove(struct fsl_mc_device *mc_dev)
+{
+	int error;
+
+	if (!fsl_mc_is_allocatable(mc_dev))
+		return -EINVAL;
+
+	if (mc_dev->resource) {
+		error = fsl_mc_resource_pool_remove_device(mc_dev);
+		if (error < 0)
+			return error;
+	}
+
+	dev_dbg(&mc_dev->dev,
+		"Allocatable fsl-mc device unbound from fsl_mc_allocator driver");
+	return 0;
+}
+
+static const struct fsl_mc_device_id match_id_table[] = {
+	{
+	 .vendor = FSL_MC_VENDOR_FREESCALE,
+	 .obj_type = "dpbp",
+	},
+	{
+	 .vendor = FSL_MC_VENDOR_FREESCALE,
+	 .obj_type = "dpmcp",
+	},
+	{
+	 .vendor = FSL_MC_VENDOR_FREESCALE,
+	 .obj_type = "dpcon",
+	},
+	{.vendor = 0x0},
+};
+
+static struct fsl_mc_driver fsl_mc_allocator_driver = {
+	.driver = {
+		   .name = "fsl_mc_allocator",
+		   .pm = NULL,
+		   },
+	.match_id_table = match_id_table,
+	.probe = fsl_mc_allocator_probe,
+	.remove = fsl_mc_allocator_remove,
+};
+
+int __init fsl_mc_allocator_driver_init(void)
+{
+	return fsl_mc_driver_register(&fsl_mc_allocator_driver);
+}
+
+void fsl_mc_allocator_driver_exit(void)
+{
+	fsl_mc_driver_unregister(&fsl_mc_allocator_driver);
+}
--- a/drivers/staging/fsl-mc/bus/fsl-mc-bus.c
+++ /dev/null
@@ -1,900 +0,0 @@
-// SPDX-License-Identifier: GPL-2.0
-/*
- * Freescale Management Complex (MC) bus driver
- *
- * Copyright (C) 2014-2016 Freescale Semiconductor, Inc.
- * Author: German Rivera <German.Rivera@freescale.com>
- *
- */
-
-#define pr_fmt(fmt) "fsl-mc: " fmt
-
-#include <linux/module.h>
-#include <linux/of_device.h>
-#include <linux/of_address.h>
-#include <linux/ioport.h>
-#include <linux/slab.h>
-#include <linux/limits.h>
-#include <linux/bitops.h>
-#include <linux/msi.h>
-#include <linux/dma-mapping.h>
-
-#include "fsl-mc-private.h"
-#include "dprc-cmd.h"
-#include "dpmng-cmd.h"
-
-/**
- * Default DMA mask for devices on a fsl-mc bus
- */
-#define FSL_MC_DEFAULT_DMA_MASK	(~0ULL)
-
-/**
- * struct fsl_mc - Private data of a "fsl,qoriq-mc" platform device
- * @root_mc_bus_dev: fsl-mc device representing the root DPRC
- * @num_translation_ranges: number of entries in addr_translation_ranges
- * @translation_ranges: array of bus to system address translation ranges
- */
-struct fsl_mc {
-	struct fsl_mc_device *root_mc_bus_dev;
-	u8 num_translation_ranges;
-	struct fsl_mc_addr_translation_range *translation_ranges;
-};
-
-/**
- * struct fsl_mc_addr_translation_range - bus to system address translation
- * range
- * @mc_region_type: Type of MC region for the range being translated
- * @start_mc_offset: Start MC offset of the range being translated
- * @end_mc_offset: MC offset of the first byte after the range (last MC
- * offset of the range is end_mc_offset - 1)
- * @start_phys_addr: system physical address corresponding to start_mc_addr
- */
-struct fsl_mc_addr_translation_range {
-	enum dprc_region_type mc_region_type;
-	u64 start_mc_offset;
-	u64 end_mc_offset;
-	phys_addr_t start_phys_addr;
-};
-
-/**
- * struct mc_version
- * @major: Major version number: incremented on API compatibility changes
- * @minor: Minor version number: incremented on API additions (that are
- *		backward compatible); reset when major version is incremented
- * @revision: Internal revision number: incremented on implementation changes
- *		and/or bug fixes that have no impact on API
- */
-struct mc_version {
-	u32 major;
-	u32 minor;
-	u32 revision;
-};
-
-/**
- * fsl_mc_bus_match - device to driver matching callback
- * @dev: the fsl-mc device to match against
- * @drv: the device driver to search for matching fsl-mc object type
- * structures
- *
- * Returns 1 on success, 0 otherwise.
- */
-static int fsl_mc_bus_match(struct device *dev, struct device_driver *drv)
-{
-	const struct fsl_mc_device_id *id;
-	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
-	struct fsl_mc_driver *mc_drv = to_fsl_mc_driver(drv);
-	bool found = false;
-
-	if (!mc_drv->match_id_table)
-		goto out;
-
-	/*
-	 * If the object is not 'plugged' don't match.
-	 * Only exception is the root DPRC, which is a special case.
-	 */
-	if ((mc_dev->obj_desc.state & FSL_MC_OBJ_STATE_PLUGGED) == 0 &&
-	    !fsl_mc_is_root_dprc(&mc_dev->dev))
-		goto out;
-
-	/*
-	 * Traverse the match_id table of the given driver, trying to find
-	 * a matching for the given device.
-	 */
-	for (id = mc_drv->match_id_table; id->vendor != 0x0; id++) {
-		if (id->vendor == mc_dev->obj_desc.vendor &&
-		    strcmp(id->obj_type, mc_dev->obj_desc.type) == 0) {
-			found = true;
-
-			break;
-		}
-	}
-
-out:
-	dev_dbg(dev, "%smatched\n", found ? "" : "not ");
-	return found;
-}
-
-/**
- * fsl_mc_bus_uevent - callback invoked when a device is added
- */
-static int fsl_mc_bus_uevent(struct device *dev, struct kobj_uevent_env *env)
-{
-	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
-
-	if (add_uevent_var(env, "MODALIAS=fsl-mc:v%08Xd%s",
-			   mc_dev->obj_desc.vendor,
-			   mc_dev->obj_desc.type))
-		return -ENOMEM;
-
-	return 0;
-}
-
-static ssize_t modalias_show(struct device *dev, struct device_attribute *attr,
-			     char *buf)
-{
-	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
-
-	return sprintf(buf, "fsl-mc:v%08Xd%s\n", mc_dev->obj_desc.vendor,
-		       mc_dev->obj_desc.type);
-}
-static DEVICE_ATTR_RO(modalias);
-
-static struct attribute *fsl_mc_dev_attrs[] = {
-	&dev_attr_modalias.attr,
-	NULL,
-};
-
-ATTRIBUTE_GROUPS(fsl_mc_dev);
-
-struct bus_type fsl_mc_bus_type = {
-	.name = "fsl-mc",
-	.match = fsl_mc_bus_match,
-	.uevent = fsl_mc_bus_uevent,
-	.dev_groups = fsl_mc_dev_groups,
-};
-EXPORT_SYMBOL_GPL(fsl_mc_bus_type);
-
-static int fsl_mc_driver_probe(struct device *dev)
-{
-	struct fsl_mc_driver *mc_drv;
-	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
-	int error;
-
-	if (WARN_ON(!dev->driver))
-		return -EINVAL;
-
-	mc_drv = to_fsl_mc_driver(dev->driver);
-	if (WARN_ON(!mc_drv->probe))
-		return -EINVAL;
-
-	error = mc_drv->probe(mc_dev);
-	if (error < 0) {
-		dev_err(dev, "%s failed: %d\n", __func__, error);
-		return error;
-	}
-
-	return 0;
-}
-
-static int fsl_mc_driver_remove(struct device *dev)
-{
-	struct fsl_mc_driver *mc_drv = to_fsl_mc_driver(dev->driver);
-	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
-	int error;
-
-	if (WARN_ON(!dev->driver))
-		return -EINVAL;
-
-	error = mc_drv->remove(mc_dev);
-	if (error < 0) {
-		dev_err(dev, "%s failed: %d\n", __func__, error);
-		return error;
-	}
-
-	return 0;
-}
-
-static void fsl_mc_driver_shutdown(struct device *dev)
-{
-	struct fsl_mc_driver *mc_drv = to_fsl_mc_driver(dev->driver);
-	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
-
-	mc_drv->shutdown(mc_dev);
-}
-
-/**
- * __fsl_mc_driver_register - registers a child device driver with the
- * MC bus
- *
- * This function is implicitly invoked from the registration function of
- * fsl_mc device drivers, which is generated by the
- * module_fsl_mc_driver() macro.
- */
-int __fsl_mc_driver_register(struct fsl_mc_driver *mc_driver,
-			     struct module *owner)
-{
-	int error;
-
-	mc_driver->driver.owner = owner;
-	mc_driver->driver.bus = &fsl_mc_bus_type;
-
-	if (mc_driver->probe)
-		mc_driver->driver.probe = fsl_mc_driver_probe;
-
-	if (mc_driver->remove)
-		mc_driver->driver.remove = fsl_mc_driver_remove;
-
-	if (mc_driver->shutdown)
-		mc_driver->driver.shutdown = fsl_mc_driver_shutdown;
-
-	error = driver_register(&mc_driver->driver);
-	if (error < 0) {
-		pr_err("driver_register() failed for %s: %d\n",
-		       mc_driver->driver.name, error);
-		return error;
-	}
-
-	return 0;
-}
-EXPORT_SYMBOL_GPL(__fsl_mc_driver_register);
-
-/**
- * fsl_mc_driver_unregister - unregisters a device driver from the
- * MC bus
- */
-void fsl_mc_driver_unregister(struct fsl_mc_driver *mc_driver)
-{
-	driver_unregister(&mc_driver->driver);
-}
-EXPORT_SYMBOL_GPL(fsl_mc_driver_unregister);
-
-/**
- * mc_get_version() - Retrieves the Management Complex firmware
- *			version information
- * @mc_io:		Pointer to opaque I/O object
- * @cmd_flags:		Command flags; one or more of 'MC_CMD_FLAG_'
- * @mc_ver_info:	Returned version information structure
- *
- * Return:	'0' on Success; Error code otherwise.
- */
-static int mc_get_version(struct fsl_mc_io *mc_io,
-			  u32 cmd_flags,
-			  struct mc_version *mc_ver_info)
-{
-	struct mc_command cmd = { 0 };
-	struct dpmng_rsp_get_version *rsp_params;
-	int err;
-
-	/* prepare command */
-	cmd.header = mc_encode_cmd_header(DPMNG_CMDID_GET_VERSION,
-					  cmd_flags,
-					  0);
-
-	/* send command to mc*/
-	err = mc_send_command(mc_io, &cmd);
-	if (err)
-		return err;
-
-	/* retrieve response parameters */
-	rsp_params = (struct dpmng_rsp_get_version *)cmd.params;
-	mc_ver_info->revision = le32_to_cpu(rsp_params->revision);
-	mc_ver_info->major = le32_to_cpu(rsp_params->version_major);
-	mc_ver_info->minor = le32_to_cpu(rsp_params->version_minor);
-
-	return 0;
-}
-
-/**
- * fsl_mc_get_root_dprc - function to traverse to the root dprc
- */
-static void fsl_mc_get_root_dprc(struct device *dev,
-				 struct device **root_dprc_dev)
-{
-	if (WARN_ON(!dev)) {
-		*root_dprc_dev = NULL;
-	} else if (WARN_ON(!dev_is_fsl_mc(dev))) {
-		*root_dprc_dev = NULL;
-	} else {
-		*root_dprc_dev = dev;
-		while (dev_is_fsl_mc((*root_dprc_dev)->parent))
-			*root_dprc_dev = (*root_dprc_dev)->parent;
-	}
-}
-
-static int get_dprc_attr(struct fsl_mc_io *mc_io,
-			 int container_id, struct dprc_attributes *attr)
-{
-	u16 dprc_handle;
-	int error;
-
-	error = dprc_open(mc_io, 0, container_id, &dprc_handle);
-	if (error < 0) {
-		dev_err(mc_io->dev, "dprc_open() failed: %d\n", error);
-		return error;
-	}
-
-	memset(attr, 0, sizeof(struct dprc_attributes));
-	error = dprc_get_attributes(mc_io, 0, dprc_handle, attr);
-	if (error < 0) {
-		dev_err(mc_io->dev, "dprc_get_attributes() failed: %d\n",
-			error);
-		goto common_cleanup;
-	}
-
-	error = 0;
-
-common_cleanup:
-	(void)dprc_close(mc_io, 0, dprc_handle);
-	return error;
-}
-
-static int get_dprc_icid(struct fsl_mc_io *mc_io,
-			 int container_id, u16 *icid)
-{
-	struct dprc_attributes attr;
-	int error;
-
-	error = get_dprc_attr(mc_io, container_id, &attr);
-	if (error == 0)
-		*icid = attr.icid;
-
-	return error;
-}
-
-static int translate_mc_addr(struct fsl_mc_device *mc_dev,
-			     enum dprc_region_type mc_region_type,
-			     u64 mc_offset, phys_addr_t *phys_addr)
-{
-	int i;
-	struct device *root_dprc_dev;
-	struct fsl_mc *mc;
-
-	fsl_mc_get_root_dprc(&mc_dev->dev, &root_dprc_dev);
-	if (WARN_ON(!root_dprc_dev))
-		return -EINVAL;
-	mc = dev_get_drvdata(root_dprc_dev->parent);
-
-	if (mc->num_translation_ranges == 0) {
-		/*
-		 * Do identity mapping:
-		 */
-		*phys_addr = mc_offset;
-		return 0;
-	}
-
-	for (i = 0; i < mc->num_translation_ranges; i++) {
-		struct fsl_mc_addr_translation_range *range =
-			&mc->translation_ranges[i];
-
-		if (mc_region_type == range->mc_region_type &&
-		    mc_offset >= range->start_mc_offset &&
-		    mc_offset < range->end_mc_offset) {
-			*phys_addr = range->start_phys_addr +
-				     (mc_offset - range->start_mc_offset);
-			return 0;
-		}
-	}
-
-	return -EFAULT;
-}
-
-static int fsl_mc_device_get_mmio_regions(struct fsl_mc_device *mc_dev,
-					  struct fsl_mc_device *mc_bus_dev)
-{
-	int i;
-	int error;
-	struct resource *regions;
-	struct fsl_mc_obj_desc *obj_desc = &mc_dev->obj_desc;
-	struct device *parent_dev = mc_dev->dev.parent;
-	enum dprc_region_type mc_region_type;
-
-	if (strcmp(obj_desc->type, "dprc") == 0 ||
-	    strcmp(obj_desc->type, "dpmcp") == 0) {
-		mc_region_type = DPRC_REGION_TYPE_MC_PORTAL;
-	} else if (strcmp(obj_desc->type, "dpio") == 0) {
-		mc_region_type = DPRC_REGION_TYPE_QBMAN_PORTAL;
-	} else {
-		/*
-		 * This function should not have been called for this MC object
-		 * type, as this object type is not supposed to have MMIO
-		 * regions
-		 */
-		WARN_ON(true);
-		return -EINVAL;
-	}
-
-	regions = kmalloc_array(obj_desc->region_count,
-				sizeof(regions[0]), GFP_KERNEL);
-	if (!regions)
-		return -ENOMEM;
-
-	for (i = 0; i < obj_desc->region_count; i++) {
-		struct dprc_region_desc region_desc;
-
-		error = dprc_get_obj_region(mc_bus_dev->mc_io,
-					    0,
-					    mc_bus_dev->mc_handle,
-					    obj_desc->type,
-					    obj_desc->id, i, &region_desc);
-		if (error < 0) {
-			dev_err(parent_dev,
-				"dprc_get_obj_region() failed: %d\n", error);
-			goto error_cleanup_regions;
-		}
-
-		WARN_ON(region_desc.size == 0);
-		error = translate_mc_addr(mc_dev, mc_region_type,
-					  region_desc.base_offset,
-					  &regions[i].start);
-		if (error < 0) {
-			dev_err(parent_dev,
-				"Invalid MC offset: %#x (for %s.%d\'s region %d)\n",
-				region_desc.base_offset,
-				obj_desc->type, obj_desc->id, i);
-			goto error_cleanup_regions;
-		}
-
-		regions[i].end = regions[i].start + region_desc.size - 1;
-		regions[i].name = "fsl-mc object MMIO region";
-		regions[i].flags = IORESOURCE_IO;
-		if (region_desc.flags & DPRC_REGION_CACHEABLE)
-			regions[i].flags |= IORESOURCE_CACHEABLE;
-	}
-
-	mc_dev->regions = regions;
-	return 0;
-
-error_cleanup_regions:
-	kfree(regions);
-	return error;
-}
-
-/**
- * fsl_mc_is_root_dprc - function to check if a given device is a root dprc
- */
-bool fsl_mc_is_root_dprc(struct device *dev)
-{
-	struct device *root_dprc_dev;
-
-	fsl_mc_get_root_dprc(dev, &root_dprc_dev);
-	if (!root_dprc_dev)
-		return false;
-	return dev == root_dprc_dev;
-}
-
-static void fsl_mc_device_release(struct device *dev)
-{
-	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
-
-	kfree(mc_dev->regions);
-
-	if (strcmp(mc_dev->obj_desc.type, "dprc") == 0)
-		kfree(to_fsl_mc_bus(mc_dev));
-	else
-		kfree(mc_dev);
-}
-
-/**
- * Add a newly discovered fsl-mc device to be visible in Linux
- */
-int fsl_mc_device_add(struct fsl_mc_obj_desc *obj_desc,
-		      struct fsl_mc_io *mc_io,
-		      struct device *parent_dev,
-		      struct fsl_mc_device **new_mc_dev)
-{
-	int error;
-	struct fsl_mc_device *mc_dev = NULL;
-	struct fsl_mc_bus *mc_bus = NULL;
-	struct fsl_mc_device *parent_mc_dev;
-
-	if (dev_is_fsl_mc(parent_dev))
-		parent_mc_dev = to_fsl_mc_device(parent_dev);
-	else
-		parent_mc_dev = NULL;
-
-	if (strcmp(obj_desc->type, "dprc") == 0) {
-		/*
-		 * Allocate an MC bus device object:
-		 */
-		mc_bus = kzalloc(sizeof(*mc_bus), GFP_KERNEL);
-		if (!mc_bus)
-			return -ENOMEM;
-
-		mc_dev = &mc_bus->mc_dev;
-	} else {
-		/*
-		 * Allocate a regular fsl_mc_device object:
-		 */
-		mc_dev = kzalloc(sizeof(*mc_dev), GFP_KERNEL);
-		if (!mc_dev)
-			return -ENOMEM;
-	}
-
-	mc_dev->obj_desc = *obj_desc;
-	mc_dev->mc_io = mc_io;
-	device_initialize(&mc_dev->dev);
-	mc_dev->dev.parent = parent_dev;
-	mc_dev->dev.bus = &fsl_mc_bus_type;
-	mc_dev->dev.release = fsl_mc_device_release;
-	dev_set_name(&mc_dev->dev, "%s.%d", obj_desc->type, obj_desc->id);
-
-	if (strcmp(obj_desc->type, "dprc") == 0) {
-		struct fsl_mc_io *mc_io2;
-
-		mc_dev->flags |= FSL_MC_IS_DPRC;
-
-		/*
-		 * To get the DPRC's ICID, we need to open the DPRC
-		 * in get_dprc_icid(). For child DPRCs, we do so using the
-		 * parent DPRC's MC portal instead of the child DPRC's MC
-		 * portal, in case the child DPRC is already opened with
-		 * its own portal (e.g., the DPRC used by AIOP).
-		 *
-		 * NOTE: There cannot be more than one active open for a
-		 * given MC object, using the same MC portal.
-		 */
-		if (parent_mc_dev) {
-			/*
-			 * device being added is a child DPRC device
-			 */
-			mc_io2 = parent_mc_dev->mc_io;
-		} else {
-			/*
-			 * device being added is the root DPRC device
-			 */
-			if (WARN_ON(!mc_io)) {
-				error = -EINVAL;
-				goto error_cleanup_dev;
-			}
-
-			mc_io2 = mc_io;
-		}
-
-		error = get_dprc_icid(mc_io2, obj_desc->id, &mc_dev->icid);
-		if (error < 0)
-			goto error_cleanup_dev;
-	} else {
-		/*
-		 * A non-DPRC object has to be a child of a DPRC, use the
-		 * parent's ICID and interrupt domain.
-		 */
-		mc_dev->icid = parent_mc_dev->icid;
-		mc_dev->dma_mask = FSL_MC_DEFAULT_DMA_MASK;
-		mc_dev->dev.dma_mask = &mc_dev->dma_mask;
-		dev_set_msi_domain(&mc_dev->dev,
-				   dev_get_msi_domain(&parent_mc_dev->dev));
-	}
-
-	/*
-	 * Get MMIO regions for the device from the MC:
-	 *
-	 * NOTE: the root DPRC is a special case as its MMIO region is
-	 * obtained from the device tree
-	 */
-	if (parent_mc_dev && obj_desc->region_count != 0) {
-		error = fsl_mc_device_get_mmio_regions(mc_dev,
-						       parent_mc_dev);
-		if (error < 0)
-			goto error_cleanup_dev;
-	}
-
-	/* Objects are coherent, unless 'no shareability' flag set. */
-	if (!(obj_desc->flags & FSL_MC_OBJ_FLAG_NO_MEM_SHAREABILITY))
-		arch_setup_dma_ops(&mc_dev->dev, 0, 0, NULL, true);
-
-	/*
-	 * The device-specific probe callback will get invoked by device_add()
-	 */
-	error = device_add(&mc_dev->dev);
-	if (error < 0) {
-		dev_err(parent_dev,
-			"device_add() failed for device %s: %d\n",
-			dev_name(&mc_dev->dev), error);
-		goto error_cleanup_dev;
-	}
-
-	dev_dbg(parent_dev, "added %s\n", dev_name(&mc_dev->dev));
-
-	*new_mc_dev = mc_dev;
-	return 0;
-
-error_cleanup_dev:
-	kfree(mc_dev->regions);
-	kfree(mc_bus);
-	kfree(mc_dev);
-
-	return error;
-}
-EXPORT_SYMBOL_GPL(fsl_mc_device_add);
-
-/**
- * fsl_mc_device_remove - Remove an fsl-mc device from being visible to
- * Linux
- *
- * @mc_dev: Pointer to an fsl-mc device
- */
-void fsl_mc_device_remove(struct fsl_mc_device *mc_dev)
-{
-	/*
-	 * The device-specific remove callback will get invoked by device_del()
-	 */
-	device_del(&mc_dev->dev);
-	put_device(&mc_dev->dev);
-}
-EXPORT_SYMBOL_GPL(fsl_mc_device_remove);
-
-static int parse_mc_ranges(struct device *dev,
-			   int *paddr_cells,
-			   int *mc_addr_cells,
-			   int *mc_size_cells,
-			   const __be32 **ranges_start)
-{
-	const __be32 *prop;
-	int range_tuple_cell_count;
-	int ranges_len;
-	int tuple_len;
-	struct device_node *mc_node = dev->of_node;
-
-	*ranges_start = of_get_property(mc_node, "ranges", &ranges_len);
-	if (!(*ranges_start) || !ranges_len) {
-		dev_warn(dev,
-			 "missing or empty ranges property for device tree node '%s'\n",
-			 mc_node->name);
-		return 0;
-	}
-
-	*paddr_cells = of_n_addr_cells(mc_node);
-
-	prop = of_get_property(mc_node, "#address-cells", NULL);
-	if (prop)
-		*mc_addr_cells = be32_to_cpup(prop);
-	else
-		*mc_addr_cells = *paddr_cells;
-
-	prop = of_get_property(mc_node, "#size-cells", NULL);
-	if (prop)
-		*mc_size_cells = be32_to_cpup(prop);
-	else
-		*mc_size_cells = of_n_size_cells(mc_node);
-
-	range_tuple_cell_count = *paddr_cells + *mc_addr_cells +
-				 *mc_size_cells;
-
-	tuple_len = range_tuple_cell_count * sizeof(__be32);
-	if (ranges_len % tuple_len != 0) {
-		dev_err(dev, "malformed ranges property '%s'\n", mc_node->name);
-		return -EINVAL;
-	}
-
-	return ranges_len / tuple_len;
-}
-
-static int get_mc_addr_translation_ranges(struct device *dev,
-					  struct fsl_mc_addr_translation_range
-						**ranges,
-					  u8 *num_ranges)
-{
-	int ret;
-	int paddr_cells;
-	int mc_addr_cells;
-	int mc_size_cells;
-	int i;
-	const __be32 *ranges_start;
-	const __be32 *cell;
-
-	ret = parse_mc_ranges(dev,
-			      &paddr_cells,
-			      &mc_addr_cells,
-			      &mc_size_cells,
-			      &ranges_start);
-	if (ret < 0)
-		return ret;
-
-	*num_ranges = ret;
-	if (!ret) {
-		/*
-		 * Missing or empty ranges property ("ranges;") for the
-		 * 'fsl,qoriq-mc' node. In this case, identity mapping
-		 * will be used.
-		 */
-		*ranges = NULL;
-		return 0;
-	}
-
-	*ranges = devm_kcalloc(dev, *num_ranges,
-			       sizeof(struct fsl_mc_addr_translation_range),
-			       GFP_KERNEL);
-	if (!(*ranges))
-		return -ENOMEM;
-
-	cell = ranges_start;
-	for (i = 0; i < *num_ranges; ++i) {
-		struct fsl_mc_addr_translation_range *range = &(*ranges)[i];
-
-		range->mc_region_type = of_read_number(cell, 1);
-		range->start_mc_offset = of_read_number(cell + 1,
-							mc_addr_cells - 1);
-		cell += mc_addr_cells;
-		range->start_phys_addr = of_read_number(cell, paddr_cells);
-		cell += paddr_cells;
-		range->end_mc_offset = range->start_mc_offset +
-				     of_read_number(cell, mc_size_cells);
-
-		cell += mc_size_cells;
-	}
-
-	return 0;
-}
-
-/**
- * fsl_mc_bus_probe - callback invoked when the root MC bus is being
- * added
- */
-static int fsl_mc_bus_probe(struct platform_device *pdev)
-{
-	struct fsl_mc_obj_desc obj_desc;
-	int error;
-	struct fsl_mc *mc;
-	struct fsl_mc_device *mc_bus_dev = NULL;
-	struct fsl_mc_io *mc_io = NULL;
-	int container_id;
-	phys_addr_t mc_portal_phys_addr;
-	u32 mc_portal_size;
-	struct mc_version mc_version;
-	struct resource res;
-
-	mc = devm_kzalloc(&pdev->dev, sizeof(*mc), GFP_KERNEL);
-	if (!mc)
-		return -ENOMEM;
-
-	platform_set_drvdata(pdev, mc);
-
-	/*
-	 * Get physical address of MC portal for the root DPRC:
-	 */
-	error = of_address_to_resource(pdev->dev.of_node, 0, &res);
-	if (error < 0) {
-		dev_err(&pdev->dev,
-			"of_address_to_resource() failed for %pOF\n",
-			pdev->dev.of_node);
-		return error;
-	}
-
-	mc_portal_phys_addr = res.start;
-	mc_portal_size = resource_size(&res);
-	error = fsl_create_mc_io(&pdev->dev, mc_portal_phys_addr,
-				 mc_portal_size, NULL,
-				 FSL_MC_IO_ATOMIC_CONTEXT_PORTAL, &mc_io);
-	if (error < 0)
-		return error;
-
-	error = mc_get_version(mc_io, 0, &mc_version);
-	if (error != 0) {
-		dev_err(&pdev->dev,
-			"mc_get_version() failed with error %d\n", error);
-		goto error_cleanup_mc_io;
-	}
-
-	dev_info(&pdev->dev, "MC firmware version: %u.%u.%u\n",
-		 mc_version.major, mc_version.minor, mc_version.revision);
-
-	error = get_mc_addr_translation_ranges(&pdev->dev,
-					       &mc->translation_ranges,
-					       &mc->num_translation_ranges);
-	if (error < 0)
-		goto error_cleanup_mc_io;
-
-	error = dprc_get_container_id(mc_io, 0, &container_id);
-	if (error < 0) {
-		dev_err(&pdev->dev,
-			"dprc_get_container_id() failed: %d\n", error);
-		goto error_cleanup_mc_io;
-	}
-
-	memset(&obj_desc, 0, sizeof(struct fsl_mc_obj_desc));
-	error = dprc_get_api_version(mc_io, 0,
-				     &obj_desc.ver_major,
-				     &obj_desc.ver_minor);
-	if (error < 0)
-		goto error_cleanup_mc_io;
-
-	obj_desc.vendor = FSL_MC_VENDOR_FREESCALE;
-	strcpy(obj_desc.type, "dprc");
-	obj_desc.id = container_id;
-	obj_desc.irq_count = 1;
-	obj_desc.region_count = 0;
-
-	error = fsl_mc_device_add(&obj_desc, mc_io, &pdev->dev, &mc_bus_dev);
-	if (error < 0)
-		goto error_cleanup_mc_io;
-
-	mc->root_mc_bus_dev = mc_bus_dev;
-	return 0;
-
-error_cleanup_mc_io:
-	fsl_destroy_mc_io(mc_io);
-	return error;
-}
-
-/**
- * fsl_mc_bus_remove - callback invoked when the root MC bus is being
- * removed
- */
-static int fsl_mc_bus_remove(struct platform_device *pdev)
-{
-	struct fsl_mc *mc = platform_get_drvdata(pdev);
-
-	if (WARN_ON(!fsl_mc_is_root_dprc(&mc->root_mc_bus_dev->dev)))
-		return -EINVAL;
-
-	fsl_mc_device_remove(mc->root_mc_bus_dev);
-
-	fsl_destroy_mc_io(mc->root_mc_bus_dev->mc_io);
-	mc->root_mc_bus_dev->mc_io = NULL;
-
-	return 0;
-}
-
-static const struct of_device_id fsl_mc_bus_match_table[] = {
-	{.compatible = "fsl,qoriq-mc",},
-	{},
-};
-
-MODULE_DEVICE_TABLE(of, fsl_mc_bus_match_table);
-
-static struct platform_driver fsl_mc_bus_driver = {
-	.driver = {
-		   .name = "fsl_mc_bus",
-		   .pm = NULL,
-		   .of_match_table = fsl_mc_bus_match_table,
-		   },
-	.probe = fsl_mc_bus_probe,
-	.remove = fsl_mc_bus_remove,
-};
-
-static int __init fsl_mc_bus_driver_init(void)
-{
-	int error;
-
-	error = bus_register(&fsl_mc_bus_type);
-	if (error < 0) {
-		pr_err("bus type registration failed: %d\n", error);
-		goto error_cleanup_cache;
-	}
-
-	error = platform_driver_register(&fsl_mc_bus_driver);
-	if (error < 0) {
-		pr_err("platform_driver_register() failed: %d\n", error);
-		goto error_cleanup_bus;
-	}
-
-	error = dprc_driver_init();
-	if (error < 0)
-		goto error_cleanup_driver;
-
-	error = fsl_mc_allocator_driver_init();
-	if (error < 0)
-		goto error_cleanup_dprc_driver;
-
-	error = its_fsl_mc_msi_init();
-	if (error < 0)
-		goto error_cleanup_mc_allocator;
-
-	return 0;
-
-error_cleanup_mc_allocator:
-	fsl_mc_allocator_driver_exit();
-
-error_cleanup_dprc_driver:
-	dprc_driver_exit();
-
-error_cleanup_driver:
-	platform_driver_unregister(&fsl_mc_bus_driver);
-
-error_cleanup_bus:
-	bus_unregister(&fsl_mc_bus_type);
-
-error_cleanup_cache:
-	return error;
-}
-postcore_initcall(fsl_mc_bus_driver_init);
--- /dev/null
+++ b/drivers/bus/fsl-mc/fsl-mc-bus.c
@@ -0,0 +1,1148 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Freescale Management Complex (MC) bus driver
+ *
+ * Copyright (C) 2014-2016 Freescale Semiconductor, Inc.
+ * Author: German Rivera <German.Rivera@freescale.com>
+ *
+ */
+
+#define pr_fmt(fmt) "fsl-mc: " fmt
+
+#include <linux/module.h>
+#include <linux/of_device.h>
+#include <linux/of_address.h>
+#include <linux/ioport.h>
+#include <linux/slab.h>
+#include <linux/limits.h>
+#include <linux/bitops.h>
+#include <linux/msi.h>
+#include <linux/dma-mapping.h>
+
+#include "fsl-mc-private.h"
+
+/**
+ * Default DMA mask for devices on a fsl-mc bus
+ */
+#define FSL_MC_DEFAULT_DMA_MASK	(~0ULL)
+
+/**
+ * struct fsl_mc - Private data of a "fsl,qoriq-mc" platform device
+ * @root_mc_bus_dev: fsl-mc device representing the root DPRC
+ * @num_translation_ranges: number of entries in addr_translation_ranges
+ * @translation_ranges: array of bus to system address translation ranges
+ */
+struct fsl_mc {
+	struct fsl_mc_device *root_mc_bus_dev;
+	u8 num_translation_ranges;
+	struct fsl_mc_addr_translation_range *translation_ranges;
+};
+
+/**
+ * struct fsl_mc_addr_translation_range - bus to system address translation
+ * range
+ * @mc_region_type: Type of MC region for the range being translated
+ * @start_mc_offset: Start MC offset of the range being translated
+ * @end_mc_offset: MC offset of the first byte after the range (last MC
+ * offset of the range is end_mc_offset - 1)
+ * @start_phys_addr: system physical address corresponding to start_mc_addr
+ */
+struct fsl_mc_addr_translation_range {
+	enum dprc_region_type mc_region_type;
+	u64 start_mc_offset;
+	u64 end_mc_offset;
+	phys_addr_t start_phys_addr;
+};
+
+/**
+ * struct mc_version
+ * @major: Major version number: incremented on API compatibility changes
+ * @minor: Minor version number: incremented on API additions (that are
+ *		backward compatible); reset when major version is incremented
+ * @revision: Internal revision number: incremented on implementation changes
+ *		and/or bug fixes that have no impact on API
+ */
+struct mc_version {
+	u32 major;
+	u32 minor;
+	u32 revision;
+};
+
+/**
+ * fsl_mc_bus_match - device to driver matching callback
+ * @dev: the fsl-mc device to match against
+ * @drv: the device driver to search for matching fsl-mc object type
+ * structures
+ *
+ * Returns 1 on success, 0 otherwise.
+ */
+static int fsl_mc_bus_match(struct device *dev, struct device_driver *drv)
+{
+	const struct fsl_mc_device_id *id;
+	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
+	struct fsl_mc_driver *mc_drv = to_fsl_mc_driver(drv);
+	bool found = false;
+
+	/* When driver_override is set, only bind to the matching driver */
+	if (mc_dev->driver_override) {
+		found = !strcmp(mc_dev->driver_override, mc_drv->driver.name);
+		goto out;
+	}
+
+	if (!mc_drv->match_id_table)
+		goto out;
+
+	/*
+	 * If the object is not 'plugged' don't match.
+	 * Only exception is the root DPRC, which is a special case.
+	 */
+	if ((mc_dev->obj_desc.state & FSL_MC_OBJ_STATE_PLUGGED) == 0 &&
+	    !fsl_mc_is_root_dprc(&mc_dev->dev))
+		goto out;
+
+	/*
+	 * Traverse the match_id table of the given driver, trying to find
+	 * a matching for the given device.
+	 */
+	for (id = mc_drv->match_id_table; id->vendor != 0x0; id++) {
+		if (id->vendor == mc_dev->obj_desc.vendor &&
+		    strcmp(id->obj_type, mc_dev->obj_desc.type) == 0) {
+			found = true;
+
+			break;
+		}
+	}
+
+out:
+	dev_dbg(dev, "%smatched\n", found ? "" : "not ");
+	return found;
+}
+
+/**
+ * fsl_mc_bus_uevent - callback invoked when a device is added
+ */
+static int fsl_mc_bus_uevent(struct device *dev, struct kobj_uevent_env *env)
+{
+	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
+
+	if (add_uevent_var(env, "MODALIAS=fsl-mc:v%08Xd%s",
+			   mc_dev->obj_desc.vendor,
+			   mc_dev->obj_desc.type))
+		return -ENOMEM;
+
+	return 0;
+}
+
+static ssize_t modalias_show(struct device *dev, struct device_attribute *attr,
+			     char *buf)
+{
+	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
+
+	return sprintf(buf, "fsl-mc:v%08Xd%s\n", mc_dev->obj_desc.vendor,
+		       mc_dev->obj_desc.type);
+}
+static DEVICE_ATTR_RO(modalias);
+
+static ssize_t rescan_store(struct device *dev,
+			    struct device_attribute *attr,
+			    const char *buf, size_t count)
+{
+	struct fsl_mc_device *root_mc_dev;
+	struct fsl_mc_bus *root_mc_bus;
+	unsigned long val;
+
+	if (!fsl_mc_is_root_dprc(dev))
+		return -EINVAL;
+
+	root_mc_dev = to_fsl_mc_device(dev);
+	root_mc_bus = to_fsl_mc_bus(root_mc_dev);
+
+	if (kstrtoul(buf, 0, &val) < 0)
+		return -EINVAL;
+
+	if (val) {
+		mutex_lock(&root_mc_bus->scan_mutex);
+		dprc_scan_objects(root_mc_dev, NULL, NULL);
+		mutex_unlock(&root_mc_bus->scan_mutex);
+	}
+
+	return count;
+}
+static DEVICE_ATTR_WO(rescan);
+
+static ssize_t driver_override_store(struct device *dev,
+				     struct device_attribute *attr,
+				     const char *buf, size_t count)
+{
+	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
+	const char *driver_override, *old = mc_dev->driver_override;
+	char *cp;
+
+	if (WARN_ON(dev->bus != &fsl_mc_bus_type))
+		return -EINVAL;
+
+	if (count >= (PAGE_SIZE - 1))
+		return -EINVAL;
+
+	driver_override = kstrndup(buf, count, GFP_KERNEL);
+	if (!driver_override)
+		return -ENOMEM;
+
+	cp = strchr(driver_override, '\n');
+	if (cp)
+		*cp = '\0';
+
+	if (strlen(driver_override)) {
+		mc_dev->driver_override = driver_override;
+	} else {
+		kfree(driver_override);
+		mc_dev->driver_override = NULL;
+	}
+
+	kfree(old);
+
+	return count;
+}
+
+static ssize_t driver_override_show(struct device *dev,
+				    struct device_attribute *attr, char *buf)
+{
+	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
+
+	return snprintf(buf, PAGE_SIZE, "%s\n", mc_dev->driver_override);
+}
+static DEVICE_ATTR_RW(driver_override);
+
+static struct attribute *fsl_mc_dev_attrs[] = {
+	&dev_attr_modalias.attr,
+	&dev_attr_rescan.attr,
+	&dev_attr_driver_override.attr,
+	NULL,
+};
+
+ATTRIBUTE_GROUPS(fsl_mc_dev);
+
+static int scan_fsl_mc_bus(struct device *dev, void *data)
+{
+	struct fsl_mc_device *root_mc_dev;
+	struct fsl_mc_bus *root_mc_bus;
+
+	if (!fsl_mc_is_root_dprc(dev))
+		goto exit;
+
+	root_mc_dev = to_fsl_mc_device(dev);
+	root_mc_bus = to_fsl_mc_bus(root_mc_dev);
+	mutex_lock(&root_mc_bus->scan_mutex);
+	dprc_scan_objects(root_mc_dev, NULL, NULL);
+	mutex_unlock(&root_mc_bus->scan_mutex);
+
+exit:
+	return 0;
+}
+
+static ssize_t bus_rescan_store(struct bus_type *bus,
+				const char *buf, size_t count)
+{
+	unsigned long val;
+
+	if (kstrtoul(buf, 0, &val) < 0)
+		return -EINVAL;
+
+	if (val)
+		bus_for_each_dev(bus, NULL, NULL, scan_fsl_mc_bus);
+
+	return count;
+}
+static BUS_ATTR(rescan, 0220, NULL, bus_rescan_store);
+
+static struct attribute *fsl_mc_bus_attrs[] = {
+	&bus_attr_rescan.attr,
+	NULL,
+};
+
+static const struct attribute_group fsl_mc_bus_group = {
+	.attrs = fsl_mc_bus_attrs,
+};
+
+static const struct attribute_group *fsl_mc_bus_groups[] = {
+	&fsl_mc_bus_group,
+	NULL,
+};
+
+struct bus_type fsl_mc_bus_type = {
+	.name = "fsl-mc",
+	.match = fsl_mc_bus_match,
+	.uevent = fsl_mc_bus_uevent,
+	.dev_groups = fsl_mc_dev_groups,
+	.bus_groups = fsl_mc_bus_groups,
+};
+EXPORT_SYMBOL_GPL(fsl_mc_bus_type);
+
+struct device_type fsl_mc_bus_dprc_type = {
+	.name = "fsl_mc_bus_dprc"
+};
+
+struct device_type fsl_mc_bus_dpni_type = {
+	.name = "fsl_mc_bus_dpni"
+};
+
+struct device_type fsl_mc_bus_dpio_type = {
+	.name = "fsl_mc_bus_dpio"
+};
+
+struct device_type fsl_mc_bus_dpsw_type = {
+	.name = "fsl_mc_bus_dpsw"
+};
+
+struct device_type fsl_mc_bus_dpdmux_type = {
+	.name = "fsl_mc_bus_dpdmux"
+};
+
+struct device_type fsl_mc_bus_dpbp_type = {
+	.name = "fsl_mc_bus_dpbp"
+};
+
+struct device_type fsl_mc_bus_dpcon_type = {
+	.name = "fsl_mc_bus_dpcon"
+};
+
+struct device_type fsl_mc_bus_dpmcp_type = {
+	.name = "fsl_mc_bus_dpmcp"
+};
+
+struct device_type fsl_mc_bus_dpmac_type = {
+	.name = "fsl_mc_bus_dpmac"
+};
+
+struct device_type fsl_mc_bus_dprtc_type = {
+	.name = "fsl_mc_bus_dprtc"
+};
+
+struct device_type fsl_mc_bus_dpseci_type = {
+	.name = "fsl_mc_bus_dpseci"
+};
+
+struct device_type fsl_mc_bus_dpdcei_type = {
+	.name = "fsl_mc_bus_dpdcei"
+};
+
+struct device_type fsl_mc_bus_dpaiop_type = {
+	.name = "fsl_mc_bus_dpaiop"
+};
+
+struct device_type fsl_mc_bus_dpci_type = {
+	.name = "fsl_mc_bus_dpci"
+};
+
+struct device_type fsl_mc_bus_dpdmai_type = {
+	.name = "fsl_mc_bus_dpdmai"
+};
+
+static struct device_type *fsl_mc_get_device_type(const char *type)
+{
+	static const struct {
+		struct device_type *dev_type;
+		const char *type;
+	} dev_types[] = {
+		{ &fsl_mc_bus_dprc_type, "dprc" },
+		{ &fsl_mc_bus_dpni_type, "dpni" },
+		{ &fsl_mc_bus_dpio_type, "dpio" },
+		{ &fsl_mc_bus_dpsw_type, "dpsw" },
+		{ &fsl_mc_bus_dpdmux_type, "dpdmux" },
+		{ &fsl_mc_bus_dpbp_type, "dpbp" },
+		{ &fsl_mc_bus_dpcon_type, "dpcon" },
+		{ &fsl_mc_bus_dpmcp_type, "dpmcp" },
+		{ &fsl_mc_bus_dpmac_type, "dpmac" },
+		{ &fsl_mc_bus_dprtc_type, "dprtc" },
+		{ &fsl_mc_bus_dpseci_type, "dpseci" },
+		{ &fsl_mc_bus_dpdcei_type, "dpdcei" },
+		{ &fsl_mc_bus_dpaiop_type, "dpaiop" },
+		{ &fsl_mc_bus_dpci_type, "dpci" },
+		{ &fsl_mc_bus_dpdmai_type, "dpdmai" },
+		{ NULL, NULL }
+	};
+	int i;
+
+	for (i = 0; dev_types[i].dev_type; i++)
+		if (!strcmp(dev_types[i].type, type))
+			return dev_types[i].dev_type;
+
+	return NULL;
+}
+
+static int fsl_mc_driver_probe(struct device *dev)
+{
+	struct fsl_mc_driver *mc_drv;
+	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
+	int error;
+
+	mc_drv = to_fsl_mc_driver(dev->driver);
+
+	error = mc_drv->probe(mc_dev);
+	if (error < 0) {
+		if (error != -EPROBE_DEFER)
+			dev_err(dev, "%s failed: %d\n", __func__, error);
+		return error;
+	}
+
+	return 0;
+}
+
+static int fsl_mc_driver_remove(struct device *dev)
+{
+	struct fsl_mc_driver *mc_drv = to_fsl_mc_driver(dev->driver);
+	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
+	int error;
+
+	error = mc_drv->remove(mc_dev);
+	if (error < 0) {
+		dev_err(dev, "%s failed: %d\n", __func__, error);
+		return error;
+	}
+
+	return 0;
+}
+
+static void fsl_mc_driver_shutdown(struct device *dev)
+{
+	struct fsl_mc_driver *mc_drv = to_fsl_mc_driver(dev->driver);
+	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
+
+	mc_drv->shutdown(mc_dev);
+}
+
+/**
+ * __fsl_mc_driver_register - registers a child device driver with the
+ * MC bus
+ *
+ * This function is implicitly invoked from the registration function of
+ * fsl_mc device drivers, which is generated by the
+ * module_fsl_mc_driver() macro.
+ */
+int __fsl_mc_driver_register(struct fsl_mc_driver *mc_driver,
+			     struct module *owner)
+{
+	int error;
+
+	mc_driver->driver.owner = owner;
+	mc_driver->driver.bus = &fsl_mc_bus_type;
+
+	if (mc_driver->probe)
+		mc_driver->driver.probe = fsl_mc_driver_probe;
+
+	if (mc_driver->remove)
+		mc_driver->driver.remove = fsl_mc_driver_remove;
+
+	if (mc_driver->shutdown)
+		mc_driver->driver.shutdown = fsl_mc_driver_shutdown;
+
+	error = driver_register(&mc_driver->driver);
+	if (error < 0) {
+		pr_err("driver_register() failed for %s: %d\n",
+		       mc_driver->driver.name, error);
+		return error;
+	}
+
+	return 0;
+}
+EXPORT_SYMBOL_GPL(__fsl_mc_driver_register);
+
+/**
+ * fsl_mc_driver_unregister - unregisters a device driver from the
+ * MC bus
+ */
+void fsl_mc_driver_unregister(struct fsl_mc_driver *mc_driver)
+{
+	driver_unregister(&mc_driver->driver);
+}
+EXPORT_SYMBOL_GPL(fsl_mc_driver_unregister);
+
+/**
+ * mc_get_version() - Retrieves the Management Complex firmware
+ *			version information
+ * @mc_io:		Pointer to opaque I/O object
+ * @cmd_flags:		Command flags; one or more of 'MC_CMD_FLAG_'
+ * @mc_ver_info:	Returned version information structure
+ *
+ * Return:	'0' on Success; Error code otherwise.
+ */
+static int mc_get_version(struct fsl_mc_io *mc_io,
+			  u32 cmd_flags,
+			  struct mc_version *mc_ver_info)
+{
+	struct fsl_mc_command cmd = { 0 };
+	struct dpmng_rsp_get_version *rsp_params;
+	int err;
+
+	/* prepare command */
+	cmd.header = mc_encode_cmd_header(DPMNG_CMDID_GET_VERSION,
+					  cmd_flags,
+					  0);
+
+	/* send command to mc*/
+	err = mc_send_command(mc_io, &cmd);
+	if (err)
+		return err;
+
+	/* retrieve response parameters */
+	rsp_params = (struct dpmng_rsp_get_version *)cmd.params;
+	mc_ver_info->revision = le32_to_cpu(rsp_params->revision);
+	mc_ver_info->major = le32_to_cpu(rsp_params->version_major);
+	mc_ver_info->minor = le32_to_cpu(rsp_params->version_minor);
+
+	return 0;
+}
+
+/**
+ * fsl_mc_get_root_dprc - function to traverse to the root dprc
+ */
+void fsl_mc_get_root_dprc(struct device *dev,
+			  struct device **root_dprc_dev)
+{
+	if (!dev) {
+		*root_dprc_dev = NULL;
+	} else if (!dev_is_fsl_mc(dev)) {
+		*root_dprc_dev = NULL;
+	} else {
+		*root_dprc_dev = dev;
+		while (dev_is_fsl_mc((*root_dprc_dev)->parent))
+			*root_dprc_dev = (*root_dprc_dev)->parent;
+	}
+}
+EXPORT_SYMBOL_GPL(fsl_mc_get_root_dprc);
+
+static int get_dprc_attr(struct fsl_mc_io *mc_io,
+			 int container_id, struct dprc_attributes *attr)
+{
+	u16 dprc_handle;
+	int error;
+
+	error = dprc_open(mc_io, 0, container_id, &dprc_handle);
+	if (error < 0) {
+		dev_err(mc_io->dev, "dprc_open() failed: %d\n", error);
+		return error;
+	}
+
+	memset(attr, 0, sizeof(struct dprc_attributes));
+	error = dprc_get_attributes(mc_io, 0, dprc_handle, attr);
+	if (error < 0) {
+		dev_err(mc_io->dev, "dprc_get_attributes() failed: %d\n",
+			error);
+		goto common_cleanup;
+	}
+
+	error = 0;
+
+common_cleanup:
+	(void)dprc_close(mc_io, 0, dprc_handle);
+	return error;
+}
+
+static int get_dprc_icid(struct fsl_mc_io *mc_io,
+			 int container_id, u32 *icid)
+{
+	struct dprc_attributes attr;
+	int error;
+
+	error = get_dprc_attr(mc_io, container_id, &attr);
+	if (error == 0)
+		*icid = attr.icid;
+
+	return error;
+}
+
+static int translate_mc_addr(struct fsl_mc_device *mc_dev,
+			     enum dprc_region_type mc_region_type,
+			     u64 mc_offset, phys_addr_t *phys_addr)
+{
+	int i;
+	struct device *root_dprc_dev;
+	struct fsl_mc *mc;
+
+	fsl_mc_get_root_dprc(&mc_dev->dev, &root_dprc_dev);
+	mc = dev_get_drvdata(root_dprc_dev->parent);
+
+	if (mc->num_translation_ranges == 0) {
+		/*
+		 * Do identity mapping:
+		 */
+		*phys_addr = mc_offset;
+		return 0;
+	}
+
+	for (i = 0; i < mc->num_translation_ranges; i++) {
+		struct fsl_mc_addr_translation_range *range =
+			&mc->translation_ranges[i];
+
+		if (mc_region_type == range->mc_region_type &&
+		    mc_offset >= range->start_mc_offset &&
+		    mc_offset < range->end_mc_offset) {
+			*phys_addr = range->start_phys_addr +
+				     (mc_offset - range->start_mc_offset);
+			return 0;
+		}
+	}
+
+	return -EFAULT;
+}
+
+static int fsl_mc_device_get_mmio_regions(struct fsl_mc_device *mc_dev,
+					  struct fsl_mc_device *mc_bus_dev)
+{
+	int i;
+	int error;
+	struct resource *regions;
+	struct fsl_mc_obj_desc *obj_desc = &mc_dev->obj_desc;
+	struct device *parent_dev = mc_dev->dev.parent;
+	enum dprc_region_type mc_region_type;
+
+	if (is_fsl_mc_bus_dprc(mc_dev) ||
+	    is_fsl_mc_bus_dpmcp(mc_dev)) {
+		mc_region_type = DPRC_REGION_TYPE_MC_PORTAL;
+	} else if (is_fsl_mc_bus_dpio(mc_dev)) {
+		mc_region_type = DPRC_REGION_TYPE_QBMAN_PORTAL;
+	} else {
+		/*
+		 * This function should not have been called for this MC object
+		 * type, as this object type is not supposed to have MMIO
+		 * regions
+		 */
+		return -EINVAL;
+	}
+
+	regions = kmalloc_array(obj_desc->region_count,
+				sizeof(regions[0]), GFP_KERNEL);
+	if (!regions)
+		return -ENOMEM;
+
+	for (i = 0; i < obj_desc->region_count; i++) {
+		struct dprc_region_desc region_desc;
+
+		error = dprc_get_obj_region(mc_bus_dev->mc_io,
+					    0,
+					    mc_bus_dev->mc_handle,
+					    obj_desc->type,
+					    obj_desc->id, i, &region_desc);
+		if (error < 0) {
+			dev_err(parent_dev,
+				"dprc_get_obj_region() failed: %d\n", error);
+			goto error_cleanup_regions;
+		}
+		/* Older MC only returned region offset and no base address
+		 * If base address is in the region_desc use it otherwise
+		 * revert to old mechanism
+		 */
+		if (region_desc.base_address)
+			regions[i].start = region_desc.base_address +
+					   region_desc.base_offset;
+		else
+			error = translate_mc_addr(mc_dev, mc_region_type,
+						  region_desc.base_offset,
+						  &regions[i].start);
+		if (error < 0) {
+			dev_err(parent_dev,
+				"Invalid MC offset: %#x (for %s.%d\'s region %d)\n",
+				region_desc.base_offset,
+				obj_desc->type, obj_desc->id, i);
+			goto error_cleanup_regions;
+		}
+
+		regions[i].end = regions[i].start + region_desc.size - 1;
+		regions[i].name = "fsl-mc object MMIO region";
+		regions[i].flags = IORESOURCE_IO;
+		if (region_desc.flags & DPRC_REGION_CACHEABLE)
+			regions[i].flags |= IORESOURCE_CACHEABLE;
+		if (region_desc.flags & DPRC_REGION_SHAREABLE)
+			regions[i].flags |= IORESOURCE_MEM;
+	}
+
+	mc_dev->regions = regions;
+	return 0;
+
+error_cleanup_regions:
+	kfree(regions);
+	return error;
+}
+
+/**
+ * fsl_mc_is_root_dprc - function to check if a given device is a root dprc
+ */
+bool fsl_mc_is_root_dprc(struct device *dev)
+{
+	struct device *root_dprc_dev;
+
+	fsl_mc_get_root_dprc(dev, &root_dprc_dev);
+	if (!root_dprc_dev)
+		return false;
+	return dev == root_dprc_dev;
+}
+
+static void fsl_mc_device_release(struct device *dev)
+{
+	struct fsl_mc_device *mc_dev = to_fsl_mc_device(dev);
+
+	kfree(mc_dev->regions);
+
+	if (is_fsl_mc_bus_dprc(mc_dev))
+		kfree(to_fsl_mc_bus(mc_dev));
+	else
+		kfree(mc_dev);
+}
+
+/**
+ * Add a newly discovered fsl-mc device to be visible in Linux
+ */
+int fsl_mc_device_add(struct fsl_mc_obj_desc *obj_desc,
+		      struct fsl_mc_io *mc_io,
+		      struct device *parent_dev,
+		      const char *driver_override,
+		      struct fsl_mc_device **new_mc_dev)
+{
+	int error;
+	struct fsl_mc_device *mc_dev = NULL;
+	struct fsl_mc_bus *mc_bus = NULL;
+	struct fsl_mc_device *parent_mc_dev;
+
+	if (dev_is_fsl_mc(parent_dev))
+		parent_mc_dev = to_fsl_mc_device(parent_dev);
+	else
+		parent_mc_dev = NULL;
+
+	if (strcmp(obj_desc->type, "dprc") == 0) {
+		/*
+		 * Allocate an MC bus device object:
+		 */
+		mc_bus = kzalloc(sizeof(*mc_bus), GFP_KERNEL);
+		if (!mc_bus)
+			return -ENOMEM;
+
+		mc_dev = &mc_bus->mc_dev;
+	} else {
+		/*
+		 * Allocate a regular fsl_mc_device object:
+		 */
+		mc_dev = kzalloc(sizeof(*mc_dev), GFP_KERNEL);
+		if (!mc_dev)
+			return -ENOMEM;
+	}
+
+	mc_dev->obj_desc = *obj_desc;
+	mc_dev->mc_io = mc_io;
+
+	if (driver_override) {
+		/*
+		 * We trust driver_override, so we don't need to use
+		 * kstrndup() here
+		 */
+		mc_dev->driver_override = kstrdup(driver_override, GFP_KERNEL);
+		if (!mc_dev->driver_override) {
+			error = -ENOMEM;
+			goto error_cleanup_dev;
+		}
+	}
+
+	device_initialize(&mc_dev->dev);
+	mc_dev->dev.parent = parent_dev;
+	mc_dev->dev.bus = &fsl_mc_bus_type;
+	mc_dev->dev.release = fsl_mc_device_release;
+	mc_dev->dev.type = fsl_mc_get_device_type(obj_desc->type);
+	if (!mc_dev->dev.type) {
+		error = -ENODEV;
+		dev_err(parent_dev, "unknown device type %s\n", obj_desc->type);
+		goto error_cleanup_dev;
+	}
+	dev_set_name(&mc_dev->dev, "%s.%d", obj_desc->type, obj_desc->id);
+
+	if (strcmp(obj_desc->type, "dprc") == 0) {
+		struct fsl_mc_io *mc_io2;
+
+		mc_dev->flags |= FSL_MC_IS_DPRC;
+
+		/*
+		 * To get the DPRC's ICID, we need to open the DPRC
+		 * in get_dprc_icid(). For child DPRCs, we do so using the
+		 * parent DPRC's MC portal instead of the child DPRC's MC
+		 * portal, in case the child DPRC is already opened with
+		 * its own portal (e.g., the DPRC used by AIOP).
+		 *
+		 * NOTE: There cannot be more than one active open for a
+		 * given MC object, using the same MC portal.
+		 */
+		if (parent_mc_dev) {
+			/*
+			 * device being added is a child DPRC device
+			 */
+			mc_io2 = parent_mc_dev->mc_io;
+		} else {
+			/*
+			 * device being added is the root DPRC device
+			 */
+			if (!mc_io) {
+				error = -EINVAL;
+				goto error_cleanup_dev;
+			}
+
+			mc_io2 = mc_io;
+		}
+
+		error = get_dprc_icid(mc_io2, obj_desc->id, &mc_dev->icid);
+		if (error < 0)
+			goto error_cleanup_dev;
+	} else {
+		/*
+		 * A non-DPRC object has to be a child of a DPRC, use the
+		 * parent's ICID and interrupt domain.
+		 */
+		mc_dev->icid = parent_mc_dev->icid;
+		mc_dev->dma_mask = FSL_MC_DEFAULT_DMA_MASK;
+		mc_dev->dev.dma_mask = &mc_dev->dma_mask;
+		mc_dev->dev.coherent_dma_mask = mc_dev->dma_mask;
+		dev_set_msi_domain(&mc_dev->dev,
+				   dev_get_msi_domain(&parent_mc_dev->dev));
+	}
+
+	/*
+	 * Get MMIO regions for the device from the MC:
+	 *
+	 * NOTE: the root DPRC is a special case as its MMIO region is
+	 * obtained from the device tree
+	 */
+	if (parent_mc_dev && obj_desc->region_count != 0) {
+		error = fsl_mc_device_get_mmio_regions(mc_dev,
+						       parent_mc_dev);
+		if (error < 0)
+			goto error_cleanup_dev;
+	}
+
+	/*
+	 * The device-specific probe callback will get invoked by device_add()
+	 */
+	error = device_add(&mc_dev->dev);
+	if (error < 0) {
+		dev_err(parent_dev,
+			"device_add() failed for device %s: %d\n",
+			dev_name(&mc_dev->dev), error);
+		goto error_cleanup_dev;
+	}
+
+	dev_dbg(parent_dev, "added %s\n", dev_name(&mc_dev->dev));
+
+	*new_mc_dev = mc_dev;
+	return 0;
+
+error_cleanup_dev:
+	kfree(mc_dev->regions);
+	kfree(mc_bus);
+	kfree(mc_dev);
+
+	return error;
+}
+EXPORT_SYMBOL_GPL(fsl_mc_device_add);
+
+/**
+ * fsl_mc_device_remove - Remove an fsl-mc device from being visible to
+ * Linux
+ *
+ * @mc_dev: Pointer to an fsl-mc device
+ */
+void fsl_mc_device_remove(struct fsl_mc_device *mc_dev)
+{
+	kfree(mc_dev->driver_override);
+	mc_dev->driver_override = NULL;
+
+	/*
+	 * The device-specific remove callback will get invoked by device_del()
+	 */
+	device_del(&mc_dev->dev);
+	put_device(&mc_dev->dev);
+}
+EXPORT_SYMBOL_GPL(fsl_mc_device_remove);
+
+static int parse_mc_ranges(struct device *dev,
+			   int *paddr_cells,
+			   int *mc_addr_cells,
+			   int *mc_size_cells,
+			   const __be32 **ranges_start)
+{
+	const __be32 *prop;
+	int range_tuple_cell_count;
+	int ranges_len;
+	int tuple_len;
+	struct device_node *mc_node = dev->of_node;
+
+	*ranges_start = of_get_property(mc_node, "ranges", &ranges_len);
+	if (!(*ranges_start) || !ranges_len) {
+		dev_warn(dev,
+			 "missing or empty ranges property for device tree node '%s'\n",
+			 mc_node->name);
+		return 0;
+	}
+
+	*paddr_cells = of_n_addr_cells(mc_node);
+
+	prop = of_get_property(mc_node, "#address-cells", NULL);
+	if (prop)
+		*mc_addr_cells = be32_to_cpup(prop);
+	else
+		*mc_addr_cells = *paddr_cells;
+
+	prop = of_get_property(mc_node, "#size-cells", NULL);
+	if (prop)
+		*mc_size_cells = be32_to_cpup(prop);
+	else
+		*mc_size_cells = of_n_size_cells(mc_node);
+
+	range_tuple_cell_count = *paddr_cells + *mc_addr_cells +
+				 *mc_size_cells;
+
+	tuple_len = range_tuple_cell_count * sizeof(__be32);
+	if (ranges_len % tuple_len != 0) {
+		dev_err(dev, "malformed ranges property '%s'\n", mc_node->name);
+		return -EINVAL;
+	}
+
+	return ranges_len / tuple_len;
+}
+
+static int get_mc_addr_translation_ranges(struct device *dev,
+					  struct fsl_mc_addr_translation_range
+						**ranges,
+					  u8 *num_ranges)
+{
+	int ret;
+	int paddr_cells;
+	int mc_addr_cells;
+	int mc_size_cells;
+	int i;
+	const __be32 *ranges_start;
+	const __be32 *cell;
+
+	ret = parse_mc_ranges(dev,
+			      &paddr_cells,
+			      &mc_addr_cells,
+			      &mc_size_cells,
+			      &ranges_start);
+	if (ret < 0)
+		return ret;
+
+	*num_ranges = ret;
+	if (!ret) {
+		/*
+		 * Missing or empty ranges property ("ranges;") for the
+		 * 'fsl,qoriq-mc' node. In this case, identity mapping
+		 * will be used.
+		 */
+		*ranges = NULL;
+		return 0;
+	}
+
+	*ranges = devm_kcalloc(dev, *num_ranges,
+			       sizeof(struct fsl_mc_addr_translation_range),
+			       GFP_KERNEL);
+	if (!(*ranges))
+		return -ENOMEM;
+
+	cell = ranges_start;
+	for (i = 0; i < *num_ranges; ++i) {
+		struct fsl_mc_addr_translation_range *range = &(*ranges)[i];
+
+		range->mc_region_type = of_read_number(cell, 1);
+		range->start_mc_offset = of_read_number(cell + 1,
+							mc_addr_cells - 1);
+		cell += mc_addr_cells;
+		range->start_phys_addr = of_read_number(cell, paddr_cells);
+		cell += paddr_cells;
+		range->end_mc_offset = range->start_mc_offset +
+				     of_read_number(cell, mc_size_cells);
+
+		cell += mc_size_cells;
+	}
+
+	return 0;
+}
+
+/**
+ * fsl_mc_bus_probe - callback invoked when the root MC bus is being
+ * added
+ */
+static int fsl_mc_bus_probe(struct platform_device *pdev)
+{
+	struct fsl_mc_obj_desc obj_desc;
+	int error;
+	struct fsl_mc *mc;
+	struct fsl_mc_device *mc_bus_dev = NULL;
+	struct fsl_mc_io *mc_io = NULL;
+	struct fsl_mc_bus *mc_bus = NULL;
+	int container_id;
+	phys_addr_t mc_portal_phys_addr;
+	u32 mc_portal_size;
+	struct mc_version mc_version;
+	struct resource res;
+
+	mc = devm_kzalloc(&pdev->dev, sizeof(*mc), GFP_KERNEL);
+	if (!mc)
+		return -ENOMEM;
+
+	platform_set_drvdata(pdev, mc);
+
+	/*
+	 * Get physical address of MC portal for the root DPRC:
+	 */
+	error = of_address_to_resource(pdev->dev.of_node, 0, &res);
+	if (error < 0) {
+		dev_err(&pdev->dev,
+			"of_address_to_resource() failed for %pOF\n",
+			pdev->dev.of_node);
+		return error;
+	}
+
+	mc_portal_phys_addr = res.start;
+	mc_portal_size = resource_size(&res);
+	error = fsl_create_mc_io(&pdev->dev, mc_portal_phys_addr,
+				 mc_portal_size, NULL,
+				 FSL_MC_IO_ATOMIC_CONTEXT_PORTAL, &mc_io);
+	if (error < 0)
+		return error;
+
+	error = mc_get_version(mc_io, 0, &mc_version);
+	if (error != 0) {
+		dev_err(&pdev->dev,
+			"mc_get_version() failed with error %d\n", error);
+		goto error_cleanup_mc_io;
+	}
+
+	dev_info(&pdev->dev, "MC firmware version: %u.%u.%u\n",
+		 mc_version.major, mc_version.minor, mc_version.revision);
+
+	error = get_mc_addr_translation_ranges(&pdev->dev,
+					       &mc->translation_ranges,
+					       &mc->num_translation_ranges);
+	if (error < 0)
+		goto error_cleanup_mc_io;
+
+	error = dprc_get_container_id(mc_io, 0, &container_id);
+	if (error < 0) {
+		dev_err(&pdev->dev,
+			"dprc_get_container_id() failed: %d\n", error);
+		goto error_cleanup_mc_io;
+	}
+
+	memset(&obj_desc, 0, sizeof(struct fsl_mc_obj_desc));
+	error = dprc_get_api_version(mc_io, 0,
+				     &obj_desc.ver_major,
+				     &obj_desc.ver_minor);
+	if (error < 0)
+		goto error_cleanup_mc_io;
+
+	obj_desc.vendor = FSL_MC_VENDOR_FREESCALE;
+	strcpy(obj_desc.type, "dprc");
+	obj_desc.id = container_id;
+	obj_desc.irq_count = 1;
+	obj_desc.region_count = 0;
+
+	error = fsl_mc_device_add(&obj_desc, mc_io, &pdev->dev, NULL,
+				 &mc_bus_dev);
+	if (error < 0)
+		goto error_cleanup_mc_io;
+
+	mc_bus = to_fsl_mc_bus(mc_bus_dev);
+	error = fsl_mc_restool_create_device_file(mc_bus);
+	if (error < 0)
+		goto error_cleanup_device;
+
+	mc->root_mc_bus_dev = mc_bus_dev;
+
+	return 0;
+
+error_cleanup_device:
+	fsl_mc_device_remove(mc_bus_dev);
+
+error_cleanup_mc_io:
+	fsl_destroy_mc_io(mc_io);
+	return error;
+}
+
+/**
+ * fsl_mc_bus_remove - callback invoked when the root MC bus is being
+ * removed
+ */
+static int fsl_mc_bus_remove(struct platform_device *pdev)
+{
+	struct fsl_mc *mc = platform_get_drvdata(pdev);
+	struct fsl_mc_bus *mc_bus = to_fsl_mc_bus(mc->root_mc_bus_dev);
+
+	if (!fsl_mc_is_root_dprc(&mc->root_mc_bus_dev->dev))
+		return -EINVAL;
+
+	fsl_mc_restool_remove_device_file(mc_bus);
+	fsl_mc_device_remove(mc->root_mc_bus_dev);
+
+	fsl_destroy_mc_io(mc->root_mc_bus_dev->mc_io);
+	mc->root_mc_bus_dev->mc_io = NULL;
+
+	return 0;
+}
+
+static const struct of_device_id fsl_mc_bus_match_table[] = {
+	{.compatible = "fsl,qoriq-mc",},
+	{},
+};
+
+MODULE_DEVICE_TABLE(of, fsl_mc_bus_match_table);
+
+static struct platform_driver fsl_mc_bus_driver = {
+	.driver = {
+		   .name = "fsl_mc_bus",
+		   .pm = NULL,
+		   .of_match_table = fsl_mc_bus_match_table,
+		   },
+	.probe = fsl_mc_bus_probe,
+	.remove = fsl_mc_bus_remove,
+};
+
+static int __init fsl_mc_bus_driver_init(void)
+{
+	int error;
+
+	error = bus_register(&fsl_mc_bus_type);
+	if (error < 0) {
+		pr_err("bus type registration failed: %d\n", error);
+		goto error_cleanup_cache;
+	}
+
+	error = platform_driver_register(&fsl_mc_bus_driver);
+	if (error < 0) {
+		pr_err("platform_driver_register() failed: %d\n", error);
+		goto error_cleanup_bus;
+	}
+
+	error = dprc_driver_init();
+	if (error < 0)
+		goto error_cleanup_driver;
+
+	error = fsl_mc_allocator_driver_init();
+	if (error < 0)
+		goto error_cleanup_dprc_driver;
+
+	error = fsl_mc_restool_init();
+	if (error < 0)
+		goto error_cleanup_mc_allocator;
+
+	return 0;
+
+error_cleanup_mc_allocator:
+	fsl_mc_allocator_driver_exit();
+
+error_cleanup_dprc_driver:
+	dprc_driver_exit();
+
+error_cleanup_driver:
+	platform_driver_unregister(&fsl_mc_bus_driver);
+
+error_cleanup_bus:
+	bus_unregister(&fsl_mc_bus_type);
+
+error_cleanup_cache:
+	return error;
+}
+postcore_initcall(fsl_mc_bus_driver_init);
--- a/drivers/staging/fsl-mc/bus/fsl-mc-msi.c
+++ /dev/null
@@ -1,285 +0,0 @@
-// SPDX-License-Identifier: GPL-2.0
-/*
- * Freescale Management Complex (MC) bus driver MSI support
- *
- * Copyright (C) 2015-2016 Freescale Semiconductor, Inc.
- * Author: German Rivera <German.Rivera@freescale.com>
- *
- */
-
-#include <linux/of_device.h>
-#include <linux/of_address.h>
-#include <linux/of_irq.h>
-#include <linux/irq.h>
-#include <linux/irqdomain.h>
-#include <linux/msi.h>
-#include "fsl-mc-private.h"
-
-#ifdef GENERIC_MSI_DOMAIN_OPS
-/*
- * Generate a unique ID identifying the interrupt (only used within the MSI
- * irqdomain.  Combine the icid with the interrupt index.
- */
-static irq_hw_number_t fsl_mc_domain_calc_hwirq(struct fsl_mc_device *dev,
-						struct msi_desc *desc)
-{
-	/*
-	 * Make the base hwirq value for ICID*10000 so it is readable
-	 * as a decimal value in /proc/interrupts.
-	 */
-	return (irq_hw_number_t)(desc->fsl_mc.msi_index + (dev->icid * 10000));
-}
-
-static void fsl_mc_msi_set_desc(msi_alloc_info_t *arg,
-				struct msi_desc *desc)
-{
-	arg->desc = desc;
-	arg->hwirq = fsl_mc_domain_calc_hwirq(to_fsl_mc_device(desc->dev),
-					      desc);
-}
-#else
-#define fsl_mc_msi_set_desc NULL
-#endif
-
-static void fsl_mc_msi_update_dom_ops(struct msi_domain_info *info)
-{
-	struct msi_domain_ops *ops = info->ops;
-
-	if (WARN_ON(!ops))
-		return;
-
-	/*
-	 * set_desc should not be set by the caller
-	 */
-	if (!ops->set_desc)
-		ops->set_desc = fsl_mc_msi_set_desc;
-}
-
-static void __fsl_mc_msi_write_msg(struct fsl_mc_device *mc_bus_dev,
-				   struct fsl_mc_device_irq *mc_dev_irq)
-{
-	int error;
-	struct fsl_mc_device *owner_mc_dev = mc_dev_irq->mc_dev;
-	struct msi_desc *msi_desc = mc_dev_irq->msi_desc;
-	struct dprc_irq_cfg irq_cfg;
-
-	/*
-	 * msi_desc->msg.address is 0x0 when this function is invoked in
-	 * the free_irq() code path. In this case, for the MC, we don't
-	 * really need to "unprogram" the MSI, so we just return.
-	 */
-	if (msi_desc->msg.address_lo == 0x0 && msi_desc->msg.address_hi == 0x0)
-		return;
-
-	if (WARN_ON(!owner_mc_dev))
-		return;
-
-	irq_cfg.paddr = ((u64)msi_desc->msg.address_hi << 32) |
-			msi_desc->msg.address_lo;
-	irq_cfg.val = msi_desc->msg.data;
-	irq_cfg.irq_num = msi_desc->irq;
-
-	if (owner_mc_dev == mc_bus_dev) {
-		/*
-		 * IRQ is for the mc_bus_dev's DPRC itself
-		 */
-		error = dprc_set_irq(mc_bus_dev->mc_io,
-				     MC_CMD_FLAG_INTR_DIS | MC_CMD_FLAG_PRI,
-				     mc_bus_dev->mc_handle,
-				     mc_dev_irq->dev_irq_index,
-				     &irq_cfg);
-		if (error < 0) {
-			dev_err(&owner_mc_dev->dev,
-				"dprc_set_irq() failed: %d\n", error);
-		}
-	} else {
-		/*
-		 * IRQ is for for a child device of mc_bus_dev
-		 */
-		error = dprc_set_obj_irq(mc_bus_dev->mc_io,
-					 MC_CMD_FLAG_INTR_DIS | MC_CMD_FLAG_PRI,
-					 mc_bus_dev->mc_handle,
-					 owner_mc_dev->obj_desc.type,
-					 owner_mc_dev->obj_desc.id,
-					 mc_dev_irq->dev_irq_index,
-					 &irq_cfg);
-		if (error < 0) {
-			dev_err(&owner_mc_dev->dev,
-				"dprc_obj_set_irq() failed: %d\n", error);
-		}
-	}
-}
-
-/*
- * NOTE: This function is invoked with interrupts disabled
- */
-static void fsl_mc_msi_write_msg(struct irq_data *irq_data,
-				 struct msi_msg *msg)
-{
-	struct msi_desc *msi_desc = irq_data_get_msi_desc(irq_data);
-	struct fsl_mc_device *mc_bus_dev = to_fsl_mc_device(msi_desc->dev);
-	struct fsl_mc_bus *mc_bus = to_fsl_mc_bus(mc_bus_dev);
-	struct fsl_mc_device_irq *mc_dev_irq =
-		&mc_bus->irq_resources[msi_desc->fsl_mc.msi_index];
-
-	WARN_ON(mc_dev_irq->msi_desc != msi_desc);
-	msi_desc->msg = *msg;
-
-	/*
-	 * Program the MSI (paddr, value) pair in the device:
-	 */
-	__fsl_mc_msi_write_msg(mc_bus_dev, mc_dev_irq);
-}
-
-static void fsl_mc_msi_update_chip_ops(struct msi_domain_info *info)
-{
-	struct irq_chip *chip = info->chip;
-
-	if (WARN_ON((!chip)))
-		return;
-
-	/*
-	 * irq_write_msi_msg should not be set by the caller
-	 */
-	if (!chip->irq_write_msi_msg)
-		chip->irq_write_msi_msg = fsl_mc_msi_write_msg;
-}
-
-/**
- * fsl_mc_msi_create_irq_domain - Create a fsl-mc MSI interrupt domain
- * @np:		Optional device-tree node of the interrupt controller
- * @info:	MSI domain info
- * @parent:	Parent irq domain
- *
- * Updates the domain and chip ops and creates a fsl-mc MSI
- * interrupt domain.
- *
- * Returns:
- * A domain pointer or NULL in case of failure.
- */
-struct irq_domain *fsl_mc_msi_create_irq_domain(struct fwnode_handle *fwnode,
-						struct msi_domain_info *info,
-						struct irq_domain *parent)
-{
-	struct irq_domain *domain;
-
-	if (info->flags & MSI_FLAG_USE_DEF_DOM_OPS)
-		fsl_mc_msi_update_dom_ops(info);
-	if (info->flags & MSI_FLAG_USE_DEF_CHIP_OPS)
-		fsl_mc_msi_update_chip_ops(info);
-
-	domain = msi_create_irq_domain(fwnode, info, parent);
-	if (domain)
-		irq_domain_update_bus_token(domain, DOMAIN_BUS_FSL_MC_MSI);
-
-	return domain;
-}
-
-int fsl_mc_find_msi_domain(struct device *mc_platform_dev,
-			   struct irq_domain **mc_msi_domain)
-{
-	struct irq_domain *msi_domain;
-	struct device_node *mc_of_node = mc_platform_dev->of_node;
-
-	msi_domain = of_msi_get_domain(mc_platform_dev, mc_of_node,
-				       DOMAIN_BUS_FSL_MC_MSI);
-	if (!msi_domain) {
-		pr_err("Unable to find fsl-mc MSI domain for %pOF\n",
-		       mc_of_node);
-
-		return -ENOENT;
-	}
-
-	*mc_msi_domain = msi_domain;
-	return 0;
-}
-
-static void fsl_mc_msi_free_descs(struct device *dev)
-{
-	struct msi_desc *desc, *tmp;
-
-	list_for_each_entry_safe(desc, tmp, dev_to_msi_list(dev), list) {
-		list_del(&desc->list);
-		free_msi_entry(desc);
-	}
-}
-
-static int fsl_mc_msi_alloc_descs(struct device *dev, unsigned int irq_count)
-
-{
-	unsigned int i;
-	int error;
-	struct msi_desc *msi_desc;
-
-	for (i = 0; i < irq_count; i++) {
-		msi_desc = alloc_msi_entry(dev, 1, NULL);
-		if (!msi_desc) {
-			dev_err(dev, "Failed to allocate msi entry\n");
-			error = -ENOMEM;
-			goto cleanup_msi_descs;
-		}
-
-		msi_desc->fsl_mc.msi_index = i;
-		INIT_LIST_HEAD(&msi_desc->list);
-		list_add_tail(&msi_desc->list, dev_to_msi_list(dev));
-	}
-
-	return 0;
-
-cleanup_msi_descs:
-	fsl_mc_msi_free_descs(dev);
-	return error;
-}
-
-int fsl_mc_msi_domain_alloc_irqs(struct device *dev,
-				 unsigned int irq_count)
-{
-	struct irq_domain *msi_domain;
-	int error;
-
-	if (WARN_ON(!list_empty(dev_to_msi_list(dev))))
-		return -EINVAL;
-
-	error = fsl_mc_msi_alloc_descs(dev, irq_count);
-	if (error < 0)
-		return error;
-
-	msi_domain = dev_get_msi_domain(dev);
-	if (WARN_ON(!msi_domain)) {
-		error = -EINVAL;
-		goto cleanup_msi_descs;
-	}
-
-	/*
-	 * NOTE: Calling this function will trigger the invocation of the
-	 * its_fsl_mc_msi_prepare() callback
-	 */
-	error = msi_domain_alloc_irqs(msi_domain, dev, irq_count);
-
-	if (error) {
-		dev_err(dev, "Failed to allocate IRQs\n");
-		goto cleanup_msi_descs;
-	}
-
-	return 0;
-
-cleanup_msi_descs:
-	fsl_mc_msi_free_descs(dev);
-	return error;
-}
-
-void fsl_mc_msi_domain_free_irqs(struct device *dev)
-{
-	struct irq_domain *msi_domain;
-
-	msi_domain = dev_get_msi_domain(dev);
-	if (WARN_ON(!msi_domain))
-		return;
-
-	msi_domain_free_irqs(msi_domain, dev);
-
-	if (WARN_ON(list_empty(dev_to_msi_list(dev))))
-		return;
-
-	fsl_mc_msi_free_descs(dev);
-}
--- /dev/null
+++ b/drivers/bus/fsl-mc/fsl-mc-msi.c
@@ -0,0 +1,285 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Freescale Management Complex (MC) bus driver MSI support
+ *
+ * Copyright (C) 2015-2016 Freescale Semiconductor, Inc.
+ * Author: German Rivera <German.Rivera@freescale.com>
+ *
+ */
+
+#include <linux/of_device.h>
+#include <linux/of_address.h>
+#include <linux/of_irq.h>
+#include <linux/irq.h>
+#include <linux/irqdomain.h>
+#include <linux/msi.h>
+
+#include "fsl-mc-private.h"
+
+#ifdef GENERIC_MSI_DOMAIN_OPS
+/*
+ * Generate a unique ID identifying the interrupt (only used within the MSI
+ * irqdomain.  Combine the icid with the interrupt index.
+ */
+static irq_hw_number_t fsl_mc_domain_calc_hwirq(struct fsl_mc_device *dev,
+						struct msi_desc *desc)
+{
+	/*
+	 * Make the base hwirq value for ICID*10000 so it is readable
+	 * as a decimal value in /proc/interrupts.
+	 */
+	return (irq_hw_number_t)(desc->fsl_mc.msi_index + (dev->icid * 10000));
+}
+
+static void fsl_mc_msi_set_desc(msi_alloc_info_t *arg,
+				struct msi_desc *desc)
+{
+	arg->desc = desc;
+	arg->hwirq = fsl_mc_domain_calc_hwirq(to_fsl_mc_device(desc->dev),
+					      desc);
+}
+#else
+#define fsl_mc_msi_set_desc NULL
+#endif
+
+static void fsl_mc_msi_update_dom_ops(struct msi_domain_info *info)
+{
+	struct msi_domain_ops *ops = info->ops;
+
+	if (!ops)
+		return;
+
+	/*
+	 * set_desc should not be set by the caller
+	 */
+	if (!ops->set_desc)
+		ops->set_desc = fsl_mc_msi_set_desc;
+}
+
+static void __fsl_mc_msi_write_msg(struct fsl_mc_device *mc_bus_dev,
+				   struct fsl_mc_device_irq *mc_dev_irq)
+{
+	int error;
+	struct fsl_mc_device *owner_mc_dev = mc_dev_irq->mc_dev;
+	struct msi_desc *msi_desc = mc_dev_irq->msi_desc;
+	struct dprc_irq_cfg irq_cfg;
+
+	/*
+	 * msi_desc->msg.address is 0x0 when this function is invoked in
+	 * the free_irq() code path. In this case, for the MC, we don't
+	 * really need to "unprogram" the MSI, so we just return.
+	 */
+	if (msi_desc->msg.address_lo == 0x0 && msi_desc->msg.address_hi == 0x0)
+		return;
+
+	if (!owner_mc_dev)
+		return;
+
+	irq_cfg.paddr = ((u64)msi_desc->msg.address_hi << 32) |
+			msi_desc->msg.address_lo;
+	irq_cfg.val = msi_desc->msg.data;
+	irq_cfg.irq_num = msi_desc->irq;
+
+	if (owner_mc_dev == mc_bus_dev) {
+		/*
+		 * IRQ is for the mc_bus_dev's DPRC itself
+		 */
+		error = dprc_set_irq(mc_bus_dev->mc_io,
+				     MC_CMD_FLAG_INTR_DIS | MC_CMD_FLAG_PRI,
+				     mc_bus_dev->mc_handle,
+				     mc_dev_irq->dev_irq_index,
+				     &irq_cfg);
+		if (error < 0) {
+			dev_err(&owner_mc_dev->dev,
+				"dprc_set_irq() failed: %d\n", error);
+		}
+	} else {
+		/*
+		 * IRQ is for for a child device of mc_bus_dev
+		 */
+		error = dprc_set_obj_irq(mc_bus_dev->mc_io,
+					 MC_CMD_FLAG_INTR_DIS | MC_CMD_FLAG_PRI,
+					 mc_bus_dev->mc_handle,
+					 owner_mc_dev->obj_desc.type,
+					 owner_mc_dev->obj_desc.id,
+					 mc_dev_irq->dev_irq_index,
+					 &irq_cfg);
+		if (error < 0) {
+			dev_err(&owner_mc_dev->dev,
+				"dprc_obj_set_irq() failed: %d\n", error);
+		}
+	}
+}
+
+/*
+ * NOTE: This function is invoked with interrupts disabled
+ */
+static void fsl_mc_msi_write_msg(struct irq_data *irq_data,
+				 struct msi_msg *msg)
+{
+	struct msi_desc *msi_desc = irq_data_get_msi_desc(irq_data);
+	struct fsl_mc_device *mc_bus_dev = to_fsl_mc_device(msi_desc->dev);
+	struct fsl_mc_bus *mc_bus = to_fsl_mc_bus(mc_bus_dev);
+	struct fsl_mc_device_irq *mc_dev_irq =
+		&mc_bus->irq_resources[msi_desc->fsl_mc.msi_index];
+
+	msi_desc->msg = *msg;
+
+	/*
+	 * Program the MSI (paddr, value) pair in the device:
+	 */
+	__fsl_mc_msi_write_msg(mc_bus_dev, mc_dev_irq);
+}
+
+static void fsl_mc_msi_update_chip_ops(struct msi_domain_info *info)
+{
+	struct irq_chip *chip = info->chip;
+
+	if (!chip)
+		return;
+
+	/*
+	 * irq_write_msi_msg should not be set by the caller
+	 */
+	if (!chip->irq_write_msi_msg)
+		chip->irq_write_msi_msg = fsl_mc_msi_write_msg;
+}
+
+/**
+ * fsl_mc_msi_create_irq_domain - Create a fsl-mc MSI interrupt domain
+ * @np:		Optional device-tree node of the interrupt controller
+ * @info:	MSI domain info
+ * @parent:	Parent irq domain
+ *
+ * Updates the domain and chip ops and creates a fsl-mc MSI
+ * interrupt domain.
+ *
+ * Returns:
+ * A domain pointer or NULL in case of failure.
+ */
+struct irq_domain *fsl_mc_msi_create_irq_domain(struct fwnode_handle *fwnode,
+						struct msi_domain_info *info,
+						struct irq_domain *parent)
+{
+	struct irq_domain *domain;
+
+	if (info->flags & MSI_FLAG_USE_DEF_DOM_OPS)
+		fsl_mc_msi_update_dom_ops(info);
+	if (info->flags & MSI_FLAG_USE_DEF_CHIP_OPS)
+		fsl_mc_msi_update_chip_ops(info);
+
+	domain = msi_create_irq_domain(fwnode, info, parent);
+	if (domain)
+		irq_domain_update_bus_token(domain, DOMAIN_BUS_FSL_MC_MSI);
+
+	return domain;
+}
+
+int fsl_mc_find_msi_domain(struct device *mc_platform_dev,
+			   struct irq_domain **mc_msi_domain)
+{
+	struct irq_domain *msi_domain;
+	struct device_node *mc_of_node = mc_platform_dev->of_node;
+
+	msi_domain = of_msi_get_domain(mc_platform_dev, mc_of_node,
+				       DOMAIN_BUS_FSL_MC_MSI);
+	if (!msi_domain) {
+		pr_err("Unable to find fsl-mc MSI domain for %pOF\n",
+		       mc_of_node);
+
+		return -ENOENT;
+	}
+
+	*mc_msi_domain = msi_domain;
+	return 0;
+}
+
+static void fsl_mc_msi_free_descs(struct device *dev)
+{
+	struct msi_desc *desc, *tmp;
+
+	list_for_each_entry_safe(desc, tmp, dev_to_msi_list(dev), list) {
+		list_del(&desc->list);
+		free_msi_entry(desc);
+	}
+}
+
+static int fsl_mc_msi_alloc_descs(struct device *dev, unsigned int irq_count)
+
+{
+	unsigned int i;
+	int error;
+	struct msi_desc *msi_desc;
+
+	for (i = 0; i < irq_count; i++) {
+		msi_desc = alloc_msi_entry(dev, 1, NULL);
+		if (!msi_desc) {
+			dev_err(dev, "Failed to allocate msi entry\n");
+			error = -ENOMEM;
+			goto cleanup_msi_descs;
+		}
+
+		msi_desc->fsl_mc.msi_index = i;
+		INIT_LIST_HEAD(&msi_desc->list);
+		list_add_tail(&msi_desc->list, dev_to_msi_list(dev));
+	}
+
+	return 0;
+
+cleanup_msi_descs:
+	fsl_mc_msi_free_descs(dev);
+	return error;
+}
+
+int fsl_mc_msi_domain_alloc_irqs(struct device *dev,
+				 unsigned int irq_count)
+{
+	struct irq_domain *msi_domain;
+	int error;
+
+	if (!list_empty(dev_to_msi_list(dev)))
+		return -EINVAL;
+
+	error = fsl_mc_msi_alloc_descs(dev, irq_count);
+	if (error < 0)
+		return error;
+
+	msi_domain = dev_get_msi_domain(dev);
+	if (!msi_domain) {
+		error = -EINVAL;
+		goto cleanup_msi_descs;
+	}
+
+	/*
+	 * NOTE: Calling this function will trigger the invocation of the
+	 * its_fsl_mc_msi_prepare() callback
+	 */
+	error = msi_domain_alloc_irqs(msi_domain, dev, irq_count);
+
+	if (error) {
+		dev_err(dev, "Failed to allocate IRQs\n");
+		goto cleanup_msi_descs;
+	}
+
+	return 0;
+
+cleanup_msi_descs:
+	fsl_mc_msi_free_descs(dev);
+	return error;
+}
+
+void fsl_mc_msi_domain_free_irqs(struct device *dev)
+{
+	struct irq_domain *msi_domain;
+
+	msi_domain = dev_get_msi_domain(dev);
+	if (!msi_domain)
+		return;
+
+	msi_domain_free_irqs(msi_domain, dev);
+
+	if (list_empty(dev_to_msi_list(dev)))
+		return;
+
+	fsl_mc_msi_free_descs(dev);
+}
--- /dev/null
+++ b/drivers/bus/fsl-mc/fsl-mc-private.h
@@ -0,0 +1,223 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Freescale Management Complex (MC) bus private declarations
+ *
+ * Copyright (C) 2016 Freescale Semiconductor, Inc.
+ *
+ */
+#ifndef _FSL_MC_PRIVATE_H_
+#define _FSL_MC_PRIVATE_H_
+
+#include <linux/fsl/mc.h>
+#include <linux/mutex.h>
+#include <linux/cdev.h>
+#include <linux/ioctl.h>
+
+/*
+ * Data Path Management Complex (DPMNG) General API
+ */
+
+/* DPMNG command versioning */
+#define DPMNG_CMD_BASE_VERSION		1
+#define DPMNG_CMD_ID_OFFSET		4
+
+#define DPMNG_CMD(id)	(((id) << DPMNG_CMD_ID_OFFSET) | DPMNG_CMD_BASE_VERSION)
+
+/* DPMNG command IDs */
+#define DPMNG_CMDID_GET_VERSION		DPMNG_CMD(0x831)
+
+struct dpmng_rsp_get_version {
+	__le32 revision;
+	__le32 version_major;
+	__le32 version_minor;
+};
+
+/*
+ * Data Path Management Command Portal (DPMCP) API
+ */
+
+/* Minimal supported DPMCP Version */
+#define DPMCP_MIN_VER_MAJOR		3
+#define DPMCP_MIN_VER_MINOR		0
+
+/* DPMCP command versioning */
+#define DPMCP_CMD_BASE_VERSION		1
+#define DPMCP_CMD_ID_OFFSET		4
+
+#define DPMCP_CMD(id)	(((id) << DPMCP_CMD_ID_OFFSET) | DPMCP_CMD_BASE_VERSION)
+
+/* DPMCP command IDs */
+#define DPMCP_CMDID_CLOSE		DPMCP_CMD(0x800)
+#define DPMCP_CMDID_OPEN		DPMCP_CMD(0x80b)
+#define DPMCP_CMDID_RESET		DPMCP_CMD(0x005)
+
+struct dpmcp_cmd_open {
+	__le32 dpmcp_id;
+};
+
+/*
+ * Initialization and runtime control APIs for DPMCP
+ */
+int dpmcp_open(struct fsl_mc_io *mc_io,
+	       u32 cmd_flags,
+	       int dpmcp_id,
+	       u16 *token);
+
+int dpmcp_close(struct fsl_mc_io *mc_io,
+		u32 cmd_flags,
+		u16 token);
+
+int dpmcp_reset(struct fsl_mc_io *mc_io,
+		u32 cmd_flags,
+		u16 token);
+
+/*
+ * Data Path Buffer Pool (DPBP) API
+ */
+
+/* DPBP Version */
+#define DPBP_VER_MAJOR				3
+#define DPBP_VER_MINOR				2
+
+/* Command versioning */
+#define DPBP_CMD_BASE_VERSION			1
+#define DPBP_CMD_ID_OFFSET			4
+
+#define DPBP_CMD(id)	(((id) << DPBP_CMD_ID_OFFSET) | DPBP_CMD_BASE_VERSION)
+
+/* Command IDs */
+#define DPBP_CMDID_CLOSE		DPBP_CMD(0x800)
+#define DPBP_CMDID_OPEN			DPBP_CMD(0x804)
+
+#define DPBP_CMDID_ENABLE		DPBP_CMD(0x002)
+#define DPBP_CMDID_DISABLE		DPBP_CMD(0x003)
+#define DPBP_CMDID_GET_ATTR		DPBP_CMD(0x004)
+#define DPBP_CMDID_RESET		DPBP_CMD(0x005)
+
+struct dpbp_cmd_open {
+	__le32 dpbp_id;
+};
+
+#define DPBP_ENABLE			0x1
+
+struct dpbp_rsp_get_attributes {
+	/* response word 0 */
+	__le16 pad;
+	__le16 bpid;
+	__le32 id;
+	/* response word 1 */
+	__le16 version_major;
+	__le16 version_minor;
+};
+
+/*
+ * Data Path Concentrator (DPCON) API
+ */
+
+/* DPCON Version */
+#define DPCON_VER_MAJOR				3
+#define DPCON_VER_MINOR				2
+
+/* Command versioning */
+#define DPCON_CMD_BASE_VERSION			1
+#define DPCON_CMD_ID_OFFSET			4
+
+#define DPCON_CMD(id)	(((id) << DPCON_CMD_ID_OFFSET) | DPCON_CMD_BASE_VERSION)
+
+/* Command IDs */
+#define DPCON_CMDID_CLOSE			DPCON_CMD(0x800)
+#define DPCON_CMDID_OPEN			DPCON_CMD(0x808)
+
+#define DPCON_CMDID_ENABLE			DPCON_CMD(0x002)
+#define DPCON_CMDID_DISABLE			DPCON_CMD(0x003)
+#define DPCON_CMDID_GET_ATTR			DPCON_CMD(0x004)
+#define DPCON_CMDID_RESET			DPCON_CMD(0x005)
+
+#define DPCON_CMDID_SET_NOTIFICATION		DPCON_CMD(0x100)
+
+struct dpcon_cmd_open {
+	__le32 dpcon_id;
+};
+
+#define DPCON_ENABLE			1
+
+struct dpcon_rsp_get_attr {
+	/* response word 0 */
+	__le32 id;
+	__le16 qbman_ch_id;
+	u8 num_priorities;
+	u8 pad;
+};
+
+struct dpcon_cmd_set_notification {
+	/* cmd word 0 */
+	__le32 dpio_id;
+	u8 priority;
+	u8 pad[3];
+	/* cmd word 1 */
+	__le64 user_ctx;
+};
+
+int __must_check fsl_mc_device_add(struct fsl_mc_obj_desc *obj_desc,
+				   struct fsl_mc_io *mc_io,
+				   struct device *parent_dev,
+				   const char *driver_override,
+				   struct fsl_mc_device **new_mc_dev);
+
+int __init dprc_driver_init(void);
+
+void dprc_driver_exit(void);
+
+int __init fsl_mc_allocator_driver_init(void);
+
+void fsl_mc_allocator_driver_exit(void);
+
+int __must_check fsl_mc_resource_allocate(struct fsl_mc_bus *mc_bus,
+					  enum fsl_mc_pool_type pool_type,
+					  struct fsl_mc_resource
+							  **new_resource);
+
+void fsl_mc_resource_free(struct fsl_mc_resource *resource);
+
+int fsl_mc_msi_domain_alloc_irqs(struct device *dev,
+				 unsigned int irq_count);
+
+void fsl_mc_msi_domain_free_irqs(struct device *dev);
+
+int __must_check fsl_create_mc_io(struct device *dev,
+				  phys_addr_t mc_portal_phys_addr,
+				  u32 mc_portal_size,
+				  struct fsl_mc_device *dpmcp_dev,
+				  u32 flags, struct fsl_mc_io **new_mc_io);
+
+void fsl_destroy_mc_io(struct fsl_mc_io *mc_io);
+
+bool fsl_mc_is_root_dprc(struct device *dev);
+
+#ifdef CONFIG_FSL_MC_RESTOOL
+
+int fsl_mc_restool_create_device_file(struct fsl_mc_bus *mc_bus);
+
+void fsl_mc_restool_remove_device_file(struct fsl_mc_bus *mc_bus);
+
+int fsl_mc_restool_init(void);
+
+#else
+
+static inline int fsl_mc_restool_create_device_file(struct fsl_mc_bus *mc_bus)
+{
+	return 0;
+}
+
+static inline void fsl_mc_restool_remove_device_file(struct fsl_mc_bus *mc_bus)
+{
+}
+
+static inline int fsl_mc_restool_init(void)
+{
+	return 0;
+}
+
+#endif
+
+#endif /* _FSL_MC_PRIVATE_H_ */
--- /dev/null
+++ b/drivers/bus/fsl-mc/fsl-mc-restool.c
@@ -0,0 +1,219 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Management Complex (MC) restool support
+ *
+ * Copyright 2018 NXP
+ *
+ */
+
+#include <linux/slab.h>
+#include <linux/cdev.h>
+#include <linux/fs.h>
+#include <linux/uaccess.h>
+
+#include "fsl-mc-private.h"
+
+#define FSL_MC_BUS_MAX_MINORS	1
+
+static struct class *fsl_mc_bus_class;
+static int fsl_mc_bus_major;
+
+static int fsl_mc_restool_send_command(unsigned long arg,
+				       struct fsl_mc_io *mc_io)
+{
+	struct fsl_mc_command mc_cmd;
+	int error;
+
+	error = copy_from_user(&mc_cmd, (void __user *)arg, sizeof(mc_cmd));
+	if (error)
+		return -EFAULT;
+
+	error = mc_send_command(mc_io, &mc_cmd);
+	if (error)
+		return error;
+
+	error = copy_to_user((void __user *)arg, &mc_cmd, sizeof(mc_cmd));
+	if (error)
+		return -EFAULT;
+
+	return 0;
+}
+
+int fsl_mc_restool_init(void)
+{
+	dev_t dev;
+	int error;
+
+	fsl_mc_bus_class = class_create(THIS_MODULE, "fsl_mc_bus");
+	if (IS_ERR(fsl_mc_bus_class)) {
+		error = PTR_ERR(fsl_mc_bus_class);
+		return error;
+	}
+
+	error = alloc_chrdev_region(&dev, 0,
+				    FSL_MC_BUS_MAX_MINORS,
+				    "fsl_mc_bus");
+	if (error < 0)
+		return error;
+
+	fsl_mc_bus_major = MAJOR(dev);
+
+	return 0;
+}
+
+static int fsl_mc_restool_dev_open(struct inode *inode, struct file *filep)
+{
+	struct fsl_mc_device *root_mc_device;
+	struct fsl_mc_restool *mc_restool;
+	struct fsl_mc_bus *mc_bus;
+	struct fsl_mc_io *dynamic_mc_io;
+	int error;
+
+	mc_restool = container_of(inode->i_cdev, struct fsl_mc_restool, cdev);
+	mc_bus = container_of(mc_restool, struct fsl_mc_bus, restool_misc);
+	root_mc_device = &mc_bus->mc_dev;
+
+	mutex_lock(&mc_restool->mutex);
+
+	if (!mc_restool->local_instance_in_use) {
+		filep->private_data = root_mc_device->mc_io;
+		mc_restool->local_instance_in_use = true;
+	} else {
+		dynamic_mc_io = kzalloc(sizeof(*dynamic_mc_io), GFP_KERNEL);
+		if (!dynamic_mc_io) {
+			error = -ENOMEM;
+			goto error_alloc_mc_io;
+		}
+
+		error = fsl_mc_portal_allocate(root_mc_device, 0,
+					       &dynamic_mc_io);
+		if (error) {
+			pr_err("Could not allocate MC portal\n");
+			goto error_portal_allocate;
+		}
+
+		mc_restool->dynamic_instance_count++;
+		filep->private_data = dynamic_mc_io;
+	}
+
+	mutex_unlock(&mc_restool->mutex);
+
+	return 0;
+
+error_portal_allocate:
+	kfree(dynamic_mc_io);
+
+error_alloc_mc_io:
+	mutex_unlock(&mc_restool->mutex);
+
+	return error;
+}
+
+static int fsl_mc_restool_dev_release(struct inode *inode, struct file *filep)
+{
+	struct fsl_mc_device *root_mc_device;
+	struct fsl_mc_restool *mc_restool;
+	struct fsl_mc_bus *mc_bus;
+	struct fsl_mc_io *mc_io;
+
+	mc_restool = container_of(inode->i_cdev, struct fsl_mc_restool, cdev);
+	mc_bus = container_of(mc_restool, struct fsl_mc_bus, restool_misc);
+	root_mc_device = &mc_bus->mc_dev;
+	mc_io = filep->private_data;
+
+	mutex_lock(&mc_restool->mutex);
+
+	if (WARN_ON(!mc_restool->local_instance_in_use &&
+		    mc_restool->dynamic_instance_count == 0)) {
+		mutex_unlock(&mc_restool->mutex);
+		return -EINVAL;
+	}
+
+	if (filep->private_data == root_mc_device->mc_io) {
+		mc_restool->local_instance_in_use = false;
+	} else {
+		fsl_mc_portal_free(mc_io);
+		kfree(mc_io);
+		mc_restool->dynamic_instance_count--;
+	}
+
+	filep->private_data = NULL;
+	mutex_unlock(&mc_restool->mutex);
+
+	return 0;
+}
+
+static long fsl_mc_restool_dev_ioctl(struct file *file,
+				     unsigned int cmd,
+				     unsigned long arg)
+{
+	int error;
+
+	switch (cmd) {
+	case RESTOOL_SEND_MC_COMMAND:
+		error = fsl_mc_restool_send_command(arg, file->private_data);
+		break;
+	default:
+		pr_err("%s: unexpected ioctl call number\n", __func__);
+		error = -EINVAL;
+	}
+
+	return error;
+}
+
+static const struct file_operations fsl_mc_restool_dev_fops = {
+	.owner = THIS_MODULE,
+	.open = fsl_mc_restool_dev_open,
+	.release = fsl_mc_restool_dev_release,
+	.unlocked_ioctl = fsl_mc_restool_dev_ioctl,
+};
+
+int fsl_mc_restool_create_device_file(struct fsl_mc_bus *mc_bus)
+{
+	struct fsl_mc_device *mc_dev = &mc_bus->mc_dev;
+	struct fsl_mc_restool *mc_restool = &mc_bus->restool_misc;
+	int error;
+
+	mc_restool = &mc_bus->restool_misc;
+	mc_restool->dev = MKDEV(fsl_mc_bus_major, 0);
+	cdev_init(&mc_restool->cdev, &fsl_mc_restool_dev_fops);
+
+	error = cdev_add(&mc_restool->cdev,
+			 mc_restool->dev,
+			 FSL_MC_BUS_MAX_MINORS);
+	if (error)
+		return error;
+
+	mc_restool->device = device_create(fsl_mc_bus_class,
+					   NULL,
+					   mc_restool->dev,
+					   NULL,
+					   "%s",
+					   dev_name(&mc_dev->dev));
+	if (IS_ERR(mc_restool->device)) {
+		error = PTR_ERR(mc_restool->device);
+		goto error_device_create;
+	}
+
+	mutex_init(&mc_restool->mutex);
+
+	return 0;
+
+error_device_create:
+	cdev_del(&mc_restool->cdev);
+
+	return error;
+}
+
+void fsl_mc_restool_remove_device_file(struct fsl_mc_bus *mc_bus)
+{
+	struct fsl_mc_restool *mc_restool = &mc_bus->restool_misc;
+
+	if (WARN_ON(mc_restool->local_instance_in_use))
+		return;
+
+	if (WARN_ON(mc_restool->dynamic_instance_count != 0))
+		return;
+
+	cdev_del(&mc_restool->cdev);
+}
--- a/drivers/staging/fsl-mc/bus/mc-io.c
+++ /dev/null
@@ -1,292 +0,0 @@
-// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
-/*
- * Copyright 2013-2016 Freescale Semiconductor Inc.
- *
- */
-
-#include <linux/io.h>
-#include "../include/mc.h"
-
-#include "fsl-mc-private.h"
-#include "dpmcp.h"
-#include "dpmcp-cmd.h"
-
-static int fsl_mc_io_set_dpmcp(struct fsl_mc_io *mc_io,
-			       struct fsl_mc_device *dpmcp_dev)
-{
-	int error;
-
-	if (WARN_ON(!dpmcp_dev))
-		return -EINVAL;
-
-	if (WARN_ON(mc_io->dpmcp_dev))
-		return -EINVAL;
-
-	if (WARN_ON(dpmcp_dev->mc_io))
-		return -EINVAL;
-
-	error = dpmcp_open(mc_io,
-			   0,
-			   dpmcp_dev->obj_desc.id,
-			   &dpmcp_dev->mc_handle);
-	if (error < 0)
-		return error;
-
-	mc_io->dpmcp_dev = dpmcp_dev;
-	dpmcp_dev->mc_io = mc_io;
-	return 0;
-}
-
-static void fsl_mc_io_unset_dpmcp(struct fsl_mc_io *mc_io)
-{
-	int error;
-	struct fsl_mc_device *dpmcp_dev = mc_io->dpmcp_dev;
-
-	if (WARN_ON(!dpmcp_dev))
-		return;
-
-	if (WARN_ON(dpmcp_dev->mc_io != mc_io))
-		return;
-
-	error = dpmcp_close(mc_io,
-			    0,
-			    dpmcp_dev->mc_handle);
-	if (error < 0) {
-		dev_err(&dpmcp_dev->dev, "dpmcp_close() failed: %d\n",
-			error);
-	}
-
-	mc_io->dpmcp_dev = NULL;
-	dpmcp_dev->mc_io = NULL;
-}
-
-/**
- * Creates an MC I/O object
- *
- * @dev: device to be associated with the MC I/O object
- * @mc_portal_phys_addr: physical address of the MC portal to use
- * @mc_portal_size: size in bytes of the MC portal
- * @dpmcp-dev: Pointer to the DPMCP object associated with this MC I/O
- * object or NULL if none.
- * @flags: flags for the new MC I/O object
- * @new_mc_io: Area to return pointer to newly created MC I/O object
- *
- * Returns '0' on Success; Error code otherwise.
- */
-int __must_check fsl_create_mc_io(struct device *dev,
-				  phys_addr_t mc_portal_phys_addr,
-				  u32 mc_portal_size,
-				  struct fsl_mc_device *dpmcp_dev,
-				  u32 flags, struct fsl_mc_io **new_mc_io)
-{
-	int error;
-	struct fsl_mc_io *mc_io;
-	void __iomem *mc_portal_virt_addr;
-	struct resource *res;
-
-	mc_io = devm_kzalloc(dev, sizeof(*mc_io), GFP_KERNEL);
-	if (!mc_io)
-		return -ENOMEM;
-
-	mc_io->dev = dev;
-	mc_io->flags = flags;
-	mc_io->portal_phys_addr = mc_portal_phys_addr;
-	mc_io->portal_size = mc_portal_size;
-	if (flags & FSL_MC_IO_ATOMIC_CONTEXT_PORTAL)
-		spin_lock_init(&mc_io->spinlock);
-	else
-		mutex_init(&mc_io->mutex);
-
-	res = devm_request_mem_region(dev,
-				      mc_portal_phys_addr,
-				      mc_portal_size,
-				      "mc_portal");
-	if (!res) {
-		dev_err(dev,
-			"devm_request_mem_region failed for MC portal %pa\n",
-			&mc_portal_phys_addr);
-		return -EBUSY;
-	}
-
-	mc_portal_virt_addr = devm_ioremap_nocache(dev,
-						   mc_portal_phys_addr,
-						   mc_portal_size);
-	if (!mc_portal_virt_addr) {
-		dev_err(dev,
-			"devm_ioremap_nocache failed for MC portal %pa\n",
-			&mc_portal_phys_addr);
-		return -ENXIO;
-	}
-
-	mc_io->portal_virt_addr = mc_portal_virt_addr;
-	if (dpmcp_dev) {
-		error = fsl_mc_io_set_dpmcp(mc_io, dpmcp_dev);
-		if (error < 0)
-			goto error_destroy_mc_io;
-	}
-
-	*new_mc_io = mc_io;
-	return 0;
-
-error_destroy_mc_io:
-	fsl_destroy_mc_io(mc_io);
-	return error;
-}
-
-/**
- * Destroys an MC I/O object
- *
- * @mc_io: MC I/O object to destroy
- */
-void fsl_destroy_mc_io(struct fsl_mc_io *mc_io)
-{
-	struct fsl_mc_device *dpmcp_dev = mc_io->dpmcp_dev;
-
-	if (dpmcp_dev)
-		fsl_mc_io_unset_dpmcp(mc_io);
-
-	devm_iounmap(mc_io->dev, mc_io->portal_virt_addr);
-	devm_release_mem_region(mc_io->dev,
-				mc_io->portal_phys_addr,
-				mc_io->portal_size);
-
-	mc_io->portal_virt_addr = NULL;
-	devm_kfree(mc_io->dev, mc_io);
-}
-
-/**
- * fsl_mc_portal_allocate - Allocates an MC portal
- *
- * @mc_dev: MC device for which the MC portal is to be allocated
- * @mc_io_flags: Flags for the fsl_mc_io object that wraps the allocated
- * MC portal.
- * @new_mc_io: Pointer to area where the pointer to the fsl_mc_io object
- * that wraps the allocated MC portal is to be returned
- *
- * This function allocates an MC portal from the device's parent DPRC,
- * from the corresponding MC bus' pool of MC portals and wraps
- * it in a new fsl_mc_io object. If 'mc_dev' is a DPRC itself, the
- * portal is allocated from its own MC bus.
- */
-int __must_check fsl_mc_portal_allocate(struct fsl_mc_device *mc_dev,
-					u16 mc_io_flags,
-					struct fsl_mc_io **new_mc_io)
-{
-	struct fsl_mc_device *mc_bus_dev;
-	struct fsl_mc_bus *mc_bus;
-	phys_addr_t mc_portal_phys_addr;
-	size_t mc_portal_size;
-	struct fsl_mc_device *dpmcp_dev;
-	int error = -EINVAL;
-	struct fsl_mc_resource *resource = NULL;
-	struct fsl_mc_io *mc_io = NULL;
-
-	if (mc_dev->flags & FSL_MC_IS_DPRC) {
-		mc_bus_dev = mc_dev;
-	} else {
-		if (WARN_ON(!dev_is_fsl_mc(mc_dev->dev.parent)))
-			return error;
-
-		mc_bus_dev = to_fsl_mc_device(mc_dev->dev.parent);
-	}
-
-	mc_bus = to_fsl_mc_bus(mc_bus_dev);
-	*new_mc_io = NULL;
-	error = fsl_mc_resource_allocate(mc_bus, FSL_MC_POOL_DPMCP, &resource);
-	if (error < 0)
-		return error;
-
-	error = -EINVAL;
-	dpmcp_dev = resource->data;
-	if (WARN_ON(!dpmcp_dev))
-		goto error_cleanup_resource;
-
-	if (dpmcp_dev->obj_desc.ver_major < DPMCP_MIN_VER_MAJOR ||
-	    (dpmcp_dev->obj_desc.ver_major == DPMCP_MIN_VER_MAJOR &&
-	     dpmcp_dev->obj_desc.ver_minor < DPMCP_MIN_VER_MINOR)) {
-		dev_err(&dpmcp_dev->dev,
-			"ERROR: Version %d.%d of DPMCP not supported.\n",
-			dpmcp_dev->obj_desc.ver_major,
-			dpmcp_dev->obj_desc.ver_minor);
-		error = -ENOTSUPP;
-		goto error_cleanup_resource;
-	}
-
-	if (WARN_ON(dpmcp_dev->obj_desc.region_count == 0))
-		goto error_cleanup_resource;
-
-	mc_portal_phys_addr = dpmcp_dev->regions[0].start;
-	mc_portal_size = resource_size(dpmcp_dev->regions);
-
-	if (WARN_ON(mc_portal_size != mc_bus_dev->mc_io->portal_size))
-		goto error_cleanup_resource;
-
-	error = fsl_create_mc_io(&mc_bus_dev->dev,
-				 mc_portal_phys_addr,
-				 mc_portal_size, dpmcp_dev,
-				 mc_io_flags, &mc_io);
-	if (error < 0)
-		goto error_cleanup_resource;
-
-	*new_mc_io = mc_io;
-	return 0;
-
-error_cleanup_resource:
-	fsl_mc_resource_free(resource);
-	return error;
-}
-EXPORT_SYMBOL_GPL(fsl_mc_portal_allocate);
-
-/**
- * fsl_mc_portal_free - Returns an MC portal to the pool of free MC portals
- * of a given MC bus
- *
- * @mc_io: Pointer to the fsl_mc_io object that wraps the MC portal to free
- */
-void fsl_mc_portal_free(struct fsl_mc_io *mc_io)
-{
-	struct fsl_mc_device *dpmcp_dev;
-	struct fsl_mc_resource *resource;
-
-	/*
-	 * Every mc_io obtained by calling fsl_mc_portal_allocate() is supposed
-	 * to have a DPMCP object associated with.
-	 */
-	dpmcp_dev = mc_io->dpmcp_dev;
-	if (WARN_ON(!dpmcp_dev))
-		return;
-
-	resource = dpmcp_dev->resource;
-	if (WARN_ON(!resource || resource->type != FSL_MC_POOL_DPMCP))
-		return;
-
-	if (WARN_ON(resource->data != dpmcp_dev))
-		return;
-
-	fsl_destroy_mc_io(mc_io);
-	fsl_mc_resource_free(resource);
-}
-EXPORT_SYMBOL_GPL(fsl_mc_portal_free);
-
-/**
- * fsl_mc_portal_reset - Resets the dpmcp object for a given fsl_mc_io object
- *
- * @mc_io: Pointer to the fsl_mc_io object that wraps the MC portal to free
- */
-int fsl_mc_portal_reset(struct fsl_mc_io *mc_io)
-{
-	int error;
-	struct fsl_mc_device *dpmcp_dev = mc_io->dpmcp_dev;
-
-	if (WARN_ON(!dpmcp_dev))
-		return -EINVAL;
-
-	error = dpmcp_reset(mc_io, 0, dpmcp_dev->mc_handle);
-	if (error < 0) {
-		dev_err(&dpmcp_dev->dev, "dpmcp_reset() failed: %d\n", error);
-		return error;
-	}
-
-	return 0;
-}
-EXPORT_SYMBOL_GPL(fsl_mc_portal_reset);
--- /dev/null
+++ b/drivers/bus/fsl-mc/mc-io.c
@@ -0,0 +1,281 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * Copyright 2013-2016 Freescale Semiconductor Inc.
+ *
+ */
+
+#include <linux/io.h>
+#include <linux/fsl/mc.h>
+
+#include "fsl-mc-private.h"
+
+static int fsl_mc_io_set_dpmcp(struct fsl_mc_io *mc_io,
+			       struct fsl_mc_device *dpmcp_dev)
+{
+	int error;
+
+	if (mc_io->dpmcp_dev)
+		return -EINVAL;
+
+	if (dpmcp_dev->mc_io)
+		return -EINVAL;
+
+	error = dpmcp_open(mc_io,
+			   0,
+			   dpmcp_dev->obj_desc.id,
+			   &dpmcp_dev->mc_handle);
+	if (error < 0)
+		return error;
+
+	mc_io->dpmcp_dev = dpmcp_dev;
+	dpmcp_dev->mc_io = mc_io;
+	return 0;
+}
+
+static void fsl_mc_io_unset_dpmcp(struct fsl_mc_io *mc_io)
+{
+	int error;
+	struct fsl_mc_device *dpmcp_dev = mc_io->dpmcp_dev;
+
+	error = dpmcp_close(mc_io,
+			    0,
+			    dpmcp_dev->mc_handle);
+	if (error < 0) {
+		dev_err(&dpmcp_dev->dev, "dpmcp_close() failed: %d\n",
+			error);
+	}
+
+	mc_io->dpmcp_dev = NULL;
+	dpmcp_dev->mc_io = NULL;
+}
+
+/**
+ * Creates an MC I/O object
+ *
+ * @dev: device to be associated with the MC I/O object
+ * @mc_portal_phys_addr: physical address of the MC portal to use
+ * @mc_portal_size: size in bytes of the MC portal
+ * @dpmcp-dev: Pointer to the DPMCP object associated with this MC I/O
+ * object or NULL if none.
+ * @flags: flags for the new MC I/O object
+ * @new_mc_io: Area to return pointer to newly created MC I/O object
+ *
+ * Returns '0' on Success; Error code otherwise.
+ */
+int __must_check fsl_create_mc_io(struct device *dev,
+				  phys_addr_t mc_portal_phys_addr,
+				  u32 mc_portal_size,
+				  struct fsl_mc_device *dpmcp_dev,
+				  u32 flags, struct fsl_mc_io **new_mc_io)
+{
+	int error;
+	struct fsl_mc_io *mc_io;
+	void __iomem *mc_portal_virt_addr;
+	struct resource *res;
+
+	mc_io = devm_kzalloc(dev, sizeof(*mc_io), GFP_KERNEL);
+	if (!mc_io)
+		return -ENOMEM;
+
+	mc_io->dev = dev;
+	mc_io->flags = flags;
+	mc_io->portal_phys_addr = mc_portal_phys_addr;
+	mc_io->portal_size = mc_portal_size;
+	if (flags & FSL_MC_IO_ATOMIC_CONTEXT_PORTAL)
+		spin_lock_init(&mc_io->spinlock);
+	else
+		mutex_init(&mc_io->mutex);
+
+	res = devm_request_mem_region(dev,
+				      mc_portal_phys_addr,
+				      mc_portal_size,
+				      "mc_portal");
+	if (!res) {
+		dev_err(dev,
+			"devm_request_mem_region failed for MC portal %pa\n",
+			&mc_portal_phys_addr);
+		return -EBUSY;
+	}
+
+	mc_portal_virt_addr = devm_ioremap_nocache(dev,
+						   mc_portal_phys_addr,
+						   mc_portal_size);
+	if (!mc_portal_virt_addr) {
+		dev_err(dev,
+			"devm_ioremap_nocache failed for MC portal %pa\n",
+			&mc_portal_phys_addr);
+		return -ENXIO;
+	}
+
+	mc_io->portal_virt_addr = mc_portal_virt_addr;
+	if (dpmcp_dev) {
+		error = fsl_mc_io_set_dpmcp(mc_io, dpmcp_dev);
+		if (error < 0)
+			goto error_destroy_mc_io;
+	}
+
+	*new_mc_io = mc_io;
+	return 0;
+
+error_destroy_mc_io:
+	fsl_destroy_mc_io(mc_io);
+	return error;
+}
+
+/**
+ * Destroys an MC I/O object
+ *
+ * @mc_io: MC I/O object to destroy
+ */
+void fsl_destroy_mc_io(struct fsl_mc_io *mc_io)
+{
+	struct fsl_mc_device *dpmcp_dev = mc_io->dpmcp_dev;
+
+	if (dpmcp_dev)
+		fsl_mc_io_unset_dpmcp(mc_io);
+
+	devm_iounmap(mc_io->dev, mc_io->portal_virt_addr);
+	devm_release_mem_region(mc_io->dev,
+				mc_io->portal_phys_addr,
+				mc_io->portal_size);
+
+	mc_io->portal_virt_addr = NULL;
+	devm_kfree(mc_io->dev, mc_io);
+}
+
+/**
+ * fsl_mc_portal_allocate - Allocates an MC portal
+ *
+ * @mc_dev: MC device for which the MC portal is to be allocated
+ * @mc_io_flags: Flags for the fsl_mc_io object that wraps the allocated
+ * MC portal.
+ * @new_mc_io: Pointer to area where the pointer to the fsl_mc_io object
+ * that wraps the allocated MC portal is to be returned
+ *
+ * This function allocates an MC portal from the device's parent DPRC,
+ * from the corresponding MC bus' pool of MC portals and wraps
+ * it in a new fsl_mc_io object. If 'mc_dev' is a DPRC itself, the
+ * portal is allocated from its own MC bus.
+ */
+int __must_check fsl_mc_portal_allocate(struct fsl_mc_device *mc_dev,
+					u16 mc_io_flags,
+					struct fsl_mc_io **new_mc_io)
+{
+	struct fsl_mc_device *mc_bus_dev;
+	struct fsl_mc_bus *mc_bus;
+	phys_addr_t mc_portal_phys_addr;
+	size_t mc_portal_size;
+	struct fsl_mc_device *dpmcp_dev;
+	int error = -EINVAL;
+	struct fsl_mc_resource *resource = NULL;
+	struct fsl_mc_io *mc_io = NULL;
+
+	if (fsl_mc_is_root_dprc(&mc_dev->dev)) {
+		mc_bus_dev = mc_dev;
+	} else {
+		if (!dev_is_fsl_mc(mc_dev->dev.parent))
+			return error;
+
+		mc_bus_dev = to_fsl_mc_device(mc_dev->dev.parent);
+	}
+
+	mc_bus = to_fsl_mc_bus(mc_bus_dev);
+	*new_mc_io = NULL;
+	error = fsl_mc_resource_allocate(mc_bus, FSL_MC_POOL_DPMCP, &resource);
+	if (error < 0)
+		return error;
+
+	error = -EINVAL;
+	dpmcp_dev = resource->data;
+
+	if (dpmcp_dev->obj_desc.ver_major < DPMCP_MIN_VER_MAJOR ||
+	    (dpmcp_dev->obj_desc.ver_major == DPMCP_MIN_VER_MAJOR &&
+	     dpmcp_dev->obj_desc.ver_minor < DPMCP_MIN_VER_MINOR)) {
+		dev_err(&dpmcp_dev->dev,
+			"ERROR: Version %d.%d of DPMCP not supported.\n",
+			dpmcp_dev->obj_desc.ver_major,
+			dpmcp_dev->obj_desc.ver_minor);
+		error = -ENOTSUPP;
+		goto error_cleanup_resource;
+	}
+
+	mc_portal_phys_addr = dpmcp_dev->regions[0].start;
+	mc_portal_size = resource_size(dpmcp_dev->regions);
+
+	error = fsl_create_mc_io(&mc_bus_dev->dev,
+				 mc_portal_phys_addr,
+				 mc_portal_size, dpmcp_dev,
+				 mc_io_flags, &mc_io);
+	if (error < 0)
+		goto error_cleanup_resource;
+
+	dpmcp_dev->consumer_link = device_link_add(&mc_dev->dev,
+						   &dpmcp_dev->dev,
+						   DL_FLAG_AUTOREMOVE_CONSUMER);
+	if (!dpmcp_dev->consumer_link) {
+		error = -EINVAL;
+		goto error_cleanup_mc_io;
+	}
+
+	*new_mc_io = mc_io;
+	return 0;
+
+error_cleanup_mc_io:
+	fsl_destroy_mc_io(mc_io);
+error_cleanup_resource:
+	fsl_mc_resource_free(resource);
+	return error;
+}
+EXPORT_SYMBOL_GPL(fsl_mc_portal_allocate);
+
+/**
+ * fsl_mc_portal_free - Returns an MC portal to the pool of free MC portals
+ * of a given MC bus
+ *
+ * @mc_io: Pointer to the fsl_mc_io object that wraps the MC portal to free
+ */
+void fsl_mc_portal_free(struct fsl_mc_io *mc_io)
+{
+	struct fsl_mc_device *dpmcp_dev;
+	struct fsl_mc_resource *resource;
+
+	/*
+	 * Every mc_io obtained by calling fsl_mc_portal_allocate() is supposed
+	 * to have a DPMCP object associated with.
+	 */
+	dpmcp_dev = mc_io->dpmcp_dev;
+
+	resource = dpmcp_dev->resource;
+	if (!resource || resource->type != FSL_MC_POOL_DPMCP)
+		return;
+
+	if (resource->data != dpmcp_dev)
+		return;
+
+	fsl_destroy_mc_io(mc_io);
+	fsl_mc_resource_free(resource);
+
+	device_link_del(dpmcp_dev->consumer_link);
+	dpmcp_dev->consumer_link = NULL;
+}
+EXPORT_SYMBOL_GPL(fsl_mc_portal_free);
+
+/**
+ * fsl_mc_portal_reset - Resets the dpmcp object for a given fsl_mc_io object
+ *
+ * @mc_io: Pointer to the fsl_mc_io object that wraps the MC portal to free
+ */
+int fsl_mc_portal_reset(struct fsl_mc_io *mc_io)
+{
+	int error;
+	struct fsl_mc_device *dpmcp_dev = mc_io->dpmcp_dev;
+
+	error = dpmcp_reset(mc_io, 0, dpmcp_dev->mc_handle);
+	if (error < 0) {
+		dev_err(&dpmcp_dev->dev, "dpmcp_reset() failed: %d\n", error);
+		return error;
+	}
+
+	return 0;
+}
+EXPORT_SYMBOL_GPL(fsl_mc_portal_reset);
--- a/drivers/staging/fsl-mc/bus/mc-sys.c
+++ /dev/null
@@ -1,297 +0,0 @@
-// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
-/*
- * Copyright 2013-2016 Freescale Semiconductor Inc.
- *
- * I/O services to send MC commands to the MC hardware
- *
- */
-
-#include <linux/delay.h>
-#include <linux/slab.h>
-#include <linux/ioport.h>
-#include <linux/device.h>
-#include <linux/io.h>
-#include <linux/io-64-nonatomic-hi-lo.h>
-#include "../include/mc.h"
-
-#include "dpmcp.h"
-
-/**
- * Timeout in milliseconds to wait for the completion of an MC command
- */
-#define MC_CMD_COMPLETION_TIMEOUT_MS	500
-
-/*
- * usleep_range() min and max values used to throttle down polling
- * iterations while waiting for MC command completion
- */
-#define MC_CMD_COMPLETION_POLLING_MIN_SLEEP_USECS    10
-#define MC_CMD_COMPLETION_POLLING_MAX_SLEEP_USECS    500
-
-static enum mc_cmd_status mc_cmd_hdr_read_status(struct mc_command *cmd)
-{
-	struct mc_cmd_header *hdr = (struct mc_cmd_header *)&cmd->header;
-
-	return (enum mc_cmd_status)hdr->status;
-}
-
-static u16 mc_cmd_hdr_read_cmdid(struct mc_command *cmd)
-{
-	struct mc_cmd_header *hdr = (struct mc_cmd_header *)&cmd->header;
-	u16 cmd_id = le16_to_cpu(hdr->cmd_id);
-
-	return cmd_id;
-}
-
-static int mc_status_to_error(enum mc_cmd_status status)
-{
-	static const int mc_status_to_error_map[] = {
-		[MC_CMD_STATUS_OK] = 0,
-		[MC_CMD_STATUS_AUTH_ERR] = -EACCES,
-		[MC_CMD_STATUS_NO_PRIVILEGE] = -EPERM,
-		[MC_CMD_STATUS_DMA_ERR] = -EIO,
-		[MC_CMD_STATUS_CONFIG_ERR] = -ENXIO,
-		[MC_CMD_STATUS_TIMEOUT] = -ETIMEDOUT,
-		[MC_CMD_STATUS_NO_RESOURCE] = -ENAVAIL,
-		[MC_CMD_STATUS_NO_MEMORY] = -ENOMEM,
-		[MC_CMD_STATUS_BUSY] = -EBUSY,
-		[MC_CMD_STATUS_UNSUPPORTED_OP] = -ENOTSUPP,
-		[MC_CMD_STATUS_INVALID_STATE] = -ENODEV,
-	};
-
-	if (WARN_ON((u32)status >= ARRAY_SIZE(mc_status_to_error_map)))
-		return -EINVAL;
-
-	return mc_status_to_error_map[status];
-}
-
-static const char *mc_status_to_string(enum mc_cmd_status status)
-{
-	static const char *const status_strings[] = {
-		[MC_CMD_STATUS_OK] = "Command completed successfully",
-		[MC_CMD_STATUS_READY] = "Command ready to be processed",
-		[MC_CMD_STATUS_AUTH_ERR] = "Authentication error",
-		[MC_CMD_STATUS_NO_PRIVILEGE] = "No privilege",
-		[MC_CMD_STATUS_DMA_ERR] = "DMA or I/O error",
-		[MC_CMD_STATUS_CONFIG_ERR] = "Configuration error",
-		[MC_CMD_STATUS_TIMEOUT] = "Operation timed out",
-		[MC_CMD_STATUS_NO_RESOURCE] = "No resources",
-		[MC_CMD_STATUS_NO_MEMORY] = "No memory available",
-		[MC_CMD_STATUS_BUSY] = "Device is busy",
-		[MC_CMD_STATUS_UNSUPPORTED_OP] = "Unsupported operation",
-		[MC_CMD_STATUS_INVALID_STATE] = "Invalid state"
-	};
-
-	if ((unsigned int)status >= ARRAY_SIZE(status_strings))
-		return "Unknown MC error";
-
-	return status_strings[status];
-}
-
-/**
- * mc_write_command - writes a command to a Management Complex (MC) portal
- *
- * @portal: pointer to an MC portal
- * @cmd: pointer to a filled command
- */
-static inline void mc_write_command(struct mc_command __iomem *portal,
-				    struct mc_command *cmd)
-{
-	int i;
-
-	/* copy command parameters into the portal */
-	for (i = 0; i < MC_CMD_NUM_OF_PARAMS; i++)
-		/*
-		 * Data is already in the expected LE byte-order. Do an
-		 * extra LE -> CPU conversion so that the CPU -> LE done in
-		 * the device io write api puts it back in the right order.
-		 */
-		writeq_relaxed(le64_to_cpu(cmd->params[i]), &portal->params[i]);
-
-	/* submit the command by writing the header */
-	writeq(le64_to_cpu(cmd->header), &portal->header);
-}
-
-/**
- * mc_read_response - reads the response for the last MC command from a
- * Management Complex (MC) portal
- *
- * @portal: pointer to an MC portal
- * @resp: pointer to command response buffer
- *
- * Returns MC_CMD_STATUS_OK on Success; Error code otherwise.
- */
-static inline enum mc_cmd_status mc_read_response(struct mc_command __iomem *
-						  portal,
-						  struct mc_command *resp)
-{
-	int i;
-	enum mc_cmd_status status;
-
-	/* Copy command response header from MC portal: */
-	resp->header = cpu_to_le64(readq_relaxed(&portal->header));
-	status = mc_cmd_hdr_read_status(resp);
-	if (status != MC_CMD_STATUS_OK)
-		return status;
-
-	/* Copy command response data from MC portal: */
-	for (i = 0; i < MC_CMD_NUM_OF_PARAMS; i++)
-		/*
-		 * Data is expected to be in LE byte-order. Do an
-		 * extra CPU -> LE to revert the LE -> CPU done in
-		 * the device io read api.
-		 */
-		resp->params[i] =
-			cpu_to_le64(readq_relaxed(&portal->params[i]));
-
-	return status;
-}
-
-/**
- * Waits for the completion of an MC command doing preemptible polling.
- * uslepp_range() is called between polling iterations.
- *
- * @mc_io: MC I/O object to be used
- * @cmd: command buffer to receive MC response
- * @mc_status: MC command completion status
- */
-static int mc_polling_wait_preemptible(struct fsl_mc_io *mc_io,
-				       struct mc_command *cmd,
-				       enum mc_cmd_status *mc_status)
-{
-	enum mc_cmd_status status;
-	unsigned long jiffies_until_timeout =
-		jiffies + msecs_to_jiffies(MC_CMD_COMPLETION_TIMEOUT_MS);
-
-	/*
-	 * Wait for response from the MC hardware:
-	 */
-	for (;;) {
-		status = mc_read_response(mc_io->portal_virt_addr, cmd);
-		if (status != MC_CMD_STATUS_READY)
-			break;
-
-		/*
-		 * TODO: When MC command completion interrupts are supported
-		 * call wait function here instead of usleep_range()
-		 */
-		usleep_range(MC_CMD_COMPLETION_POLLING_MIN_SLEEP_USECS,
-			     MC_CMD_COMPLETION_POLLING_MAX_SLEEP_USECS);
-
-		if (time_after_eq(jiffies, jiffies_until_timeout)) {
-			dev_dbg(mc_io->dev,
-				"MC command timed out (portal: %pa, dprc handle: %#x, command: %#x)\n",
-				 &mc_io->portal_phys_addr,
-				 (unsigned int)mc_cmd_hdr_read_token(cmd),
-				 (unsigned int)mc_cmd_hdr_read_cmdid(cmd));
-
-			return -ETIMEDOUT;
-		}
-	}
-
-	*mc_status = status;
-	return 0;
-}
-
-/**
- * Waits for the completion of an MC command doing atomic polling.
- * udelay() is called between polling iterations.
- *
- * @mc_io: MC I/O object to be used
- * @cmd: command buffer to receive MC response
- * @mc_status: MC command completion status
- */
-static int mc_polling_wait_atomic(struct fsl_mc_io *mc_io,
-				  struct mc_command *cmd,
-				  enum mc_cmd_status *mc_status)
-{
-	enum mc_cmd_status status;
-	unsigned long timeout_usecs = MC_CMD_COMPLETION_TIMEOUT_MS * 1000;
-
-	BUILD_BUG_ON((MC_CMD_COMPLETION_TIMEOUT_MS * 1000) %
-		     MC_CMD_COMPLETION_POLLING_MAX_SLEEP_USECS != 0);
-
-	for (;;) {
-		status = mc_read_response(mc_io->portal_virt_addr, cmd);
-		if (status != MC_CMD_STATUS_READY)
-			break;
-
-		udelay(MC_CMD_COMPLETION_POLLING_MAX_SLEEP_USECS);
-		timeout_usecs -= MC_CMD_COMPLETION_POLLING_MAX_SLEEP_USECS;
-		if (timeout_usecs == 0) {
-			dev_dbg(mc_io->dev,
-				"MC command timed out (portal: %pa, dprc handle: %#x, command: %#x)\n",
-				 &mc_io->portal_phys_addr,
-				 (unsigned int)mc_cmd_hdr_read_token(cmd),
-				 (unsigned int)mc_cmd_hdr_read_cmdid(cmd));
-
-			return -ETIMEDOUT;
-		}
-	}
-
-	*mc_status = status;
-	return 0;
-}
-
-/**
- * Sends a command to the MC device using the given MC I/O object
- *
- * @mc_io: MC I/O object to be used
- * @cmd: command to be sent
- *
- * Returns '0' on Success; Error code otherwise.
- */
-int mc_send_command(struct fsl_mc_io *mc_io, struct mc_command *cmd)
-{
-	int error;
-	enum mc_cmd_status status;
-	unsigned long irq_flags = 0;
-
-	if (WARN_ON(in_irq() &&
-		    !(mc_io->flags & FSL_MC_IO_ATOMIC_CONTEXT_PORTAL)))
-		return -EINVAL;
-
-	if (mc_io->flags & FSL_MC_IO_ATOMIC_CONTEXT_PORTAL)
-		spin_lock_irqsave(&mc_io->spinlock, irq_flags);
-	else
-		mutex_lock(&mc_io->mutex);
-
-	/*
-	 * Send command to the MC hardware:
-	 */
-	mc_write_command(mc_io->portal_virt_addr, cmd);
-
-	/*
-	 * Wait for response from the MC hardware:
-	 */
-	if (!(mc_io->flags & FSL_MC_IO_ATOMIC_CONTEXT_PORTAL))
-		error = mc_polling_wait_preemptible(mc_io, cmd, &status);
-	else
-		error = mc_polling_wait_atomic(mc_io, cmd, &status);
-
-	if (error < 0)
-		goto common_exit;
-
-	if (status != MC_CMD_STATUS_OK) {
-		dev_dbg(mc_io->dev,
-			"MC command failed: portal: %pa, dprc handle: %#x, command: %#x, status: %s (%#x)\n",
-			 &mc_io->portal_phys_addr,
-			 (unsigned int)mc_cmd_hdr_read_token(cmd),
-			 (unsigned int)mc_cmd_hdr_read_cmdid(cmd),
-			 mc_status_to_string(status),
-			 (unsigned int)status);
-
-		error = mc_status_to_error(status);
-		goto common_exit;
-	}
-
-	error = 0;
-common_exit:
-	if (mc_io->flags & FSL_MC_IO_ATOMIC_CONTEXT_PORTAL)
-		spin_unlock_irqrestore(&mc_io->spinlock, irq_flags);
-	else
-		mutex_unlock(&mc_io->mutex);
-
-	return error;
-}
-EXPORT_SYMBOL(mc_send_command);
--- /dev/null
+++ b/drivers/bus/fsl-mc/mc-sys.c
@@ -0,0 +1,296 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
+/*
+ * Copyright 2013-2016 Freescale Semiconductor Inc.
+ *
+ * I/O services to send MC commands to the MC hardware
+ *
+ */
+
+#include <linux/delay.h>
+#include <linux/slab.h>
+#include <linux/ioport.h>
+#include <linux/device.h>
+#include <linux/io.h>
+#include <linux/io-64-nonatomic-hi-lo.h>
+#include <linux/fsl/mc.h>
+
+#include "fsl-mc-private.h"
+
+/**
+ * Timeout in milliseconds to wait for the completion of an MC command
+ */
+#define MC_CMD_COMPLETION_TIMEOUT_MS	15000
+
+/*
+ * usleep_range() min and max values used to throttle down polling
+ * iterations while waiting for MC command completion
+ */
+#define MC_CMD_COMPLETION_POLLING_MIN_SLEEP_USECS    10
+#define MC_CMD_COMPLETION_POLLING_MAX_SLEEP_USECS    500
+
+static enum mc_cmd_status mc_cmd_hdr_read_status(struct fsl_mc_command *cmd)
+{
+	struct mc_cmd_header *hdr = (struct mc_cmd_header *)&cmd->header;
+
+	return (enum mc_cmd_status)hdr->status;
+}
+
+static u16 mc_cmd_hdr_read_cmdid(struct fsl_mc_command *cmd)
+{
+	struct mc_cmd_header *hdr = (struct mc_cmd_header *)&cmd->header;
+	u16 cmd_id = le16_to_cpu(hdr->cmd_id);
+
+	return cmd_id;
+}
+
+static int mc_status_to_error(enum mc_cmd_status status)
+{
+	static const int mc_status_to_error_map[] = {
+		[MC_CMD_STATUS_OK] = 0,
+		[MC_CMD_STATUS_AUTH_ERR] = -EACCES,
+		[MC_CMD_STATUS_NO_PRIVILEGE] = -EPERM,
+		[MC_CMD_STATUS_DMA_ERR] = -EIO,
+		[MC_CMD_STATUS_CONFIG_ERR] = -ENXIO,
+		[MC_CMD_STATUS_TIMEOUT] = -ETIMEDOUT,
+		[MC_CMD_STATUS_NO_RESOURCE] = -ENAVAIL,
+		[MC_CMD_STATUS_NO_MEMORY] = -ENOMEM,
+		[MC_CMD_STATUS_BUSY] = -EBUSY,
+		[MC_CMD_STATUS_UNSUPPORTED_OP] = -ENOTSUPP,
+		[MC_CMD_STATUS_INVALID_STATE] = -ENODEV,
+	};
+
+	if ((u32)status >= ARRAY_SIZE(mc_status_to_error_map))
+		return -EINVAL;
+
+	return mc_status_to_error_map[status];
+}
+
+static const char *mc_status_to_string(enum mc_cmd_status status)
+{
+	static const char *const status_strings[] = {
+		[MC_CMD_STATUS_OK] = "Command completed successfully",
+		[MC_CMD_STATUS_READY] = "Command ready to be processed",
+		[MC_CMD_STATUS_AUTH_ERR] = "Authentication error",
+		[MC_CMD_STATUS_NO_PRIVILEGE] = "No privilege",
+		[MC_CMD_STATUS_DMA_ERR] = "DMA or I/O error",
+		[MC_CMD_STATUS_CONFIG_ERR] = "Configuration error",
+		[MC_CMD_STATUS_TIMEOUT] = "Operation timed out",
+		[MC_CMD_STATUS_NO_RESOURCE] = "No resources",
+		[MC_CMD_STATUS_NO_MEMORY] = "No memory available",
+		[MC_CMD_STATUS_BUSY] = "Device is busy",
+		[MC_CMD_STATUS_UNSUPPORTED_OP] = "Unsupported operation",
+		[MC_CMD_STATUS_INVALID_STATE] = "Invalid state"
+	};
+
+	if ((unsigned int)status >= ARRAY_SIZE(status_strings))
+		return "Unknown MC error";
+
+	return status_strings[status];
+}
+
+/**
+ * mc_write_command - writes a command to a Management Complex (MC) portal
+ *
+ * @portal: pointer to an MC portal
+ * @cmd: pointer to a filled command
+ */
+static inline void mc_write_command(struct fsl_mc_command __iomem *portal,
+				    struct fsl_mc_command *cmd)
+{
+	int i;
+
+	/* copy command parameters into the portal */
+	for (i = 0; i < MC_CMD_NUM_OF_PARAMS; i++)
+		/*
+		 * Data is already in the expected LE byte-order. Do an
+		 * extra LE -> CPU conversion so that the CPU -> LE done in
+		 * the device io write api puts it back in the right order.
+		 */
+		writeq_relaxed(le64_to_cpu(cmd->params[i]), &portal->params[i]);
+
+	/* submit the command by writing the header */
+	writeq(le64_to_cpu(cmd->header), &portal->header);
+}
+
+/**
+ * mc_read_response - reads the response for the last MC command from a
+ * Management Complex (MC) portal
+ *
+ * @portal: pointer to an MC portal
+ * @resp: pointer to command response buffer
+ *
+ * Returns MC_CMD_STATUS_OK on Success; Error code otherwise.
+ */
+static inline enum mc_cmd_status mc_read_response(struct fsl_mc_command __iomem
+						  *portal,
+						  struct fsl_mc_command *resp)
+{
+	int i;
+	enum mc_cmd_status status;
+
+	/* Copy command response header from MC portal: */
+	resp->header = cpu_to_le64(readq_relaxed(&portal->header));
+	status = mc_cmd_hdr_read_status(resp);
+	if (status != MC_CMD_STATUS_OK)
+		return status;
+
+	/* Copy command response data from MC portal: */
+	for (i = 0; i < MC_CMD_NUM_OF_PARAMS; i++)
+		/*
+		 * Data is expected to be in LE byte-order. Do an
+		 * extra CPU -> LE to revert the LE -> CPU done in
+		 * the device io read api.
+		 */
+		resp->params[i] =
+			cpu_to_le64(readq_relaxed(&portal->params[i]));
+
+	return status;
+}
+
+/**
+ * Waits for the completion of an MC command doing preemptible polling.
+ * uslepp_range() is called between polling iterations.
+ *
+ * @mc_io: MC I/O object to be used
+ * @cmd: command buffer to receive MC response
+ * @mc_status: MC command completion status
+ */
+static int mc_polling_wait_preemptible(struct fsl_mc_io *mc_io,
+				       struct fsl_mc_command *cmd,
+				       enum mc_cmd_status *mc_status)
+{
+	enum mc_cmd_status status;
+	unsigned long jiffies_until_timeout =
+		jiffies + msecs_to_jiffies(MC_CMD_COMPLETION_TIMEOUT_MS);
+
+	/*
+	 * Wait for response from the MC hardware:
+	 */
+	for (;;) {
+		status = mc_read_response(mc_io->portal_virt_addr, cmd);
+		if (status != MC_CMD_STATUS_READY)
+			break;
+
+		/*
+		 * TODO: When MC command completion interrupts are supported
+		 * call wait function here instead of usleep_range()
+		 */
+		usleep_range(MC_CMD_COMPLETION_POLLING_MIN_SLEEP_USECS,
+			     MC_CMD_COMPLETION_POLLING_MAX_SLEEP_USECS);
+
+		if (time_after_eq(jiffies, jiffies_until_timeout)) {
+			dev_dbg(mc_io->dev,
+				"MC command timed out (portal: %pa, dprc handle: %#x, command: %#x)\n",
+				 &mc_io->portal_phys_addr,
+				 (unsigned int)mc_cmd_hdr_read_token(cmd),
+				 (unsigned int)mc_cmd_hdr_read_cmdid(cmd));
+
+			return -ETIMEDOUT;
+		}
+	}
+
+	*mc_status = status;
+	return 0;
+}
+
+/**
+ * Waits for the completion of an MC command doing atomic polling.
+ * udelay() is called between polling iterations.
+ *
+ * @mc_io: MC I/O object to be used
+ * @cmd: command buffer to receive MC response
+ * @mc_status: MC command completion status
+ */
+static int mc_polling_wait_atomic(struct fsl_mc_io *mc_io,
+				  struct fsl_mc_command *cmd,
+				  enum mc_cmd_status *mc_status)
+{
+	enum mc_cmd_status status;
+	unsigned long timeout_usecs = MC_CMD_COMPLETION_TIMEOUT_MS * 1000;
+
+	BUILD_BUG_ON((MC_CMD_COMPLETION_TIMEOUT_MS * 1000) %
+		     MC_CMD_COMPLETION_POLLING_MAX_SLEEP_USECS != 0);
+
+	for (;;) {
+		status = mc_read_response(mc_io->portal_virt_addr, cmd);
+		if (status != MC_CMD_STATUS_READY)
+			break;
+
+		udelay(MC_CMD_COMPLETION_POLLING_MAX_SLEEP_USECS);
+		timeout_usecs -= MC_CMD_COMPLETION_POLLING_MAX_SLEEP_USECS;
+		if (timeout_usecs == 0) {
+			dev_dbg(mc_io->dev,
+				"MC command timed out (portal: %pa, dprc handle: %#x, command: %#x)\n",
+				 &mc_io->portal_phys_addr,
+				 (unsigned int)mc_cmd_hdr_read_token(cmd),
+				 (unsigned int)mc_cmd_hdr_read_cmdid(cmd));
+
+			return -ETIMEDOUT;
+		}
+	}
+
+	*mc_status = status;
+	return 0;
+}
+
+/**
+ * Sends a command to the MC device using the given MC I/O object
+ *
+ * @mc_io: MC I/O object to be used
+ * @cmd: command to be sent
+ *
+ * Returns '0' on Success; Error code otherwise.
+ */
+int mc_send_command(struct fsl_mc_io *mc_io, struct fsl_mc_command *cmd)
+{
+	int error;
+	enum mc_cmd_status status;
+	unsigned long irq_flags = 0;
+
+	if (in_irq() && !(mc_io->flags & FSL_MC_IO_ATOMIC_CONTEXT_PORTAL))
+		return -EINVAL;
+
+	if (mc_io->flags & FSL_MC_IO_ATOMIC_CONTEXT_PORTAL)
+		spin_lock_irqsave(&mc_io->spinlock, irq_flags);
+	else
+		mutex_lock(&mc_io->mutex);
+
+	/*
+	 * Send command to the MC hardware:
+	 */
+	mc_write_command(mc_io->portal_virt_addr, cmd);
+
+	/*
+	 * Wait for response from the MC hardware:
+	 */
+	if (!(mc_io->flags & FSL_MC_IO_ATOMIC_CONTEXT_PORTAL))
+		error = mc_polling_wait_preemptible(mc_io, cmd, &status);
+	else
+		error = mc_polling_wait_atomic(mc_io, cmd, &status);
+
+	if (error < 0)
+		goto common_exit;
+
+	if (status != MC_CMD_STATUS_OK) {
+		dev_dbg(mc_io->dev,
+			"MC command failed: portal: %pa, dprc handle: %#x, command: %#x, status: %s (%#x)\n",
+			 &mc_io->portal_phys_addr,
+			 (unsigned int)mc_cmd_hdr_read_token(cmd),
+			 (unsigned int)mc_cmd_hdr_read_cmdid(cmd),
+			 mc_status_to_string(status),
+			 (unsigned int)status);
+
+		error = mc_status_to_error(status);
+		goto common_exit;
+	}
+
+	error = 0;
+common_exit:
+	if (mc_io->flags & FSL_MC_IO_ATOMIC_CONTEXT_PORTAL)
+		spin_unlock_irqrestore(&mc_io->spinlock, irq_flags);
+	else
+		mutex_unlock(&mc_io->mutex);
+
+	return error;
+}
+EXPORT_SYMBOL_GPL(mc_send_command);
--- a/drivers/irqchip/Kconfig
+++ b/drivers/irqchip/Kconfig
@@ -42,6 +42,12 @@ config ARM_GIC_V3_ITS
 	depends on PCI
 	depends on PCI_MSI
 
+config ARM_GIC_V3_ITS_FSL_MC
+	bool
+	depends on ARM_GIC_V3_ITS
+	depends on FSL_MC_BUS
+	default ARM_GIC_V3_ITS
+
 config ARM_NVIC
 	bool
 	select IRQ_DOMAIN
--- a/drivers/irqchip/Makefile
+++ b/drivers/irqchip/Makefile
@@ -30,6 +30,7 @@ obj-$(CONFIG_ARCH_REALVIEW)		+= irq-gic-
 obj-$(CONFIG_ARM_GIC_V2M)		+= irq-gic-v2m.o
 obj-$(CONFIG_ARM_GIC_V3)		+= irq-gic-v3.o irq-gic-common.o
 obj-$(CONFIG_ARM_GIC_V3_ITS)		+= irq-gic-v3-its.o irq-gic-v3-its-pci-msi.o irq-gic-v3-its-platform-msi.o irq-gic-v4.o
+obj-$(CONFIG_ARM_GIC_V3_ITS_FSL_MC)	+= irq-gic-v3-its-fsl-mc-msi.o
 obj-$(CONFIG_PARTITION_PERCPU)		+= irq-partition-percpu.o
 obj-$(CONFIG_HISILICON_IRQ_MBIGEN)	+= irq-mbigen.o
 obj-$(CONFIG_ARM_NVIC)			+= irq-nvic.o
--- /dev/null
+++ b/drivers/irqchip/irq-gic-v3-its-fsl-mc-msi.c
@@ -0,0 +1,98 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Freescale Management Complex (MC) bus driver MSI support
+ *
+ * Copyright (C) 2015-2016 Freescale Semiconductor, Inc.
+ * Author: German Rivera <German.Rivera@freescale.com>
+ *
+ */
+
+#include <linux/of_device.h>
+#include <linux/of_address.h>
+#include <linux/irq.h>
+#include <linux/msi.h>
+#include <linux/of.h>
+#include <linux/of_irq.h>
+#include <linux/fsl/mc.h>
+
+static struct irq_chip its_msi_irq_chip = {
+	.name = "ITS-fMSI",
+	.irq_mask = irq_chip_mask_parent,
+	.irq_unmask = irq_chip_unmask_parent,
+	.irq_eoi = irq_chip_eoi_parent,
+	.irq_set_affinity = msi_domain_set_affinity
+};
+
+static int its_fsl_mc_msi_prepare(struct irq_domain *msi_domain,
+				  struct device *dev,
+				  int nvec, msi_alloc_info_t *info)
+{
+	struct fsl_mc_device *mc_bus_dev;
+	struct msi_domain_info *msi_info;
+
+	if (!dev_is_fsl_mc(dev))
+		return -EINVAL;
+
+	mc_bus_dev = to_fsl_mc_device(dev);
+	if (!(mc_bus_dev->flags & FSL_MC_IS_DPRC))
+		return -EINVAL;
+
+	/*
+	 * Set the device Id to be passed to the GIC-ITS:
+	 *
+	 * NOTE: This device id corresponds to the IOMMU stream ID
+	 * associated with the DPRC object (ICID).
+	 */
+	info->scratchpad[0].ul = mc_bus_dev->icid;
+	msi_info = msi_get_domain_info(msi_domain->parent);
+	return msi_info->ops->msi_prepare(msi_domain->parent, dev, nvec, info);
+}
+
+static struct msi_domain_ops its_fsl_mc_msi_ops __ro_after_init = {
+	.msi_prepare = its_fsl_mc_msi_prepare,
+};
+
+static struct msi_domain_info its_fsl_mc_msi_domain_info = {
+	.flags	= (MSI_FLAG_USE_DEF_DOM_OPS | MSI_FLAG_USE_DEF_CHIP_OPS),
+	.ops	= &its_fsl_mc_msi_ops,
+	.chip	= &its_msi_irq_chip,
+};
+
+static const struct of_device_id its_device_id[] = {
+	{	.compatible	= "arm,gic-v3-its",	},
+	{},
+};
+
+static int __init its_fsl_mc_msi_init(void)
+{
+	struct device_node *np;
+	struct irq_domain *parent;
+	struct irq_domain *mc_msi_domain;
+
+	for (np = of_find_matching_node(NULL, its_device_id); np;
+	     np = of_find_matching_node(np, its_device_id)) {
+		if (!of_property_read_bool(np, "msi-controller"))
+			continue;
+
+		parent = irq_find_matching_host(np, DOMAIN_BUS_NEXUS);
+		if (!parent || !msi_get_domain_info(parent)) {
+			pr_err("%pOF: unable to locate ITS domain\n", np);
+			continue;
+		}
+
+		mc_msi_domain = fsl_mc_msi_create_irq_domain(
+						 of_node_to_fwnode(np),
+						 &its_fsl_mc_msi_domain_info,
+						 parent);
+		if (!mc_msi_domain) {
+			pr_err("%pOF: unable to create fsl-mc domain\n", np);
+			continue;
+		}
+
+		pr_info("fsl-mc MSI: %pOF domain created\n", np);
+	}
+
+	return 0;
+}
+
+early_initcall(its_fsl_mc_msi_init);
--- a/drivers/staging/fsl-dpaa2/ethernet/dpaa2-eth.c
+++ b/drivers/staging/fsl-dpaa2/ethernet/dpaa2-eth.c
@@ -16,7 +16,7 @@
 #include <linux/filter.h>
 #include <linux/atomic.h>
 #include <net/sock.h>
-#include "../../fsl-mc/include/mc.h"
+#include <linux/fsl/mc.h>
 #include "dpaa2-eth.h"
 #include "dpaa2-eth-ceetm.h"
 
--- a/drivers/staging/fsl-dpaa2/ethernet/dpaa2-eth.h
+++ b/drivers/staging/fsl-dpaa2/ethernet/dpaa2-eth.h
@@ -9,12 +9,11 @@
 #include <linux/dcbnl.h>
 #include <linux/netdevice.h>
 #include <linux/if_vlan.h>
+#include <linux/fsl/mc.h>
 #include <linux/filter.h>
 
 #include "../../fsl-mc/include/dpaa2-io.h"
 #include "../../fsl-mc/include/dpaa2-fd.h"
-#include "../../fsl-mc/include/dpbp.h"
-#include "../../fsl-mc/include/dpcon.h"
 #include "dpni.h"
 #include "dpni-cmd.h"
 
--- a/drivers/staging/fsl-dpaa2/ethernet/dpni.c
+++ b/drivers/staging/fsl-dpaa2/ethernet/dpni.c
@@ -4,7 +4,7 @@
  */
 #include <linux/kernel.h>
 #include <linux/errno.h>
-#include "../../fsl-mc/include/mc.h"
+#include <linux/fsl/mc.h>
 #include "dpni.h"
 #include "dpni-cmd.h"
 
--- a/drivers/staging/fsl-mc/bus/Kconfig
+++ b/drivers/staging/fsl-mc/bus/Kconfig
@@ -5,15 +5,6 @@
 # Copyright (C) 2014-2016 Freescale Semiconductor, Inc.
 #
 
-config FSL_MC_BUS
-	bool "QorIQ DPAA2 fsl-mc bus driver"
-	depends on OF && (ARCH_LAYERSCAPE || (COMPILE_TEST && (ARM || ARM64 || X86_LOCAL_APIC || PPC)))
-	select GENERIC_MSI_IRQ_DOMAIN
-	help
-	  Driver to enable the bus infrastructure for the QorIQ DPAA2
-	  architecture.  The fsl-mc bus driver handles discovery of
-	  DPAA2 objects (which are represented as Linux devices) and
-	  binding objects to drivers.
 
 config FSL_MC_DPIO
         tristate "QorIQ DPAA2 DPIO driver"
@@ -24,3 +15,9 @@ config FSL_MC_DPIO
 	  other DPAA2 objects. This driver does not expose the DPIO
 	  objects individually, but groups them under a service layer
 	  API.
+
+config FSL_QBMAN_DEBUG
+	tristate "Freescale QBMAN Debug APIs"
+	depends on FSL_MC_DPIO
+	help
+	  QBMan debug assistant APIs.
--- a/drivers/staging/fsl-mc/bus/Makefile
+++ b/drivers/staging/fsl-mc/bus/Makefile
@@ -4,19 +4,6 @@
 #
 # Copyright (C) 2014 Freescale Semiconductor, Inc.
 #
-obj-$(CONFIG_FSL_MC_BUS) += mc-bus-driver.o
-
-mc-bus-driver-objs := fsl-mc-bus.o \
-		      mc-sys.o \
-		      mc-io.o \
-		      dprc.o \
-		      dprc-driver.o \
-		      fsl-mc-allocator.o \
-		      fsl-mc-msi.o \
-		      irq-gic-v3-its-fsl-mc-msi.o \
-		      dpmcp.o \
-		      dpbp.o \
-		      dpcon.o
 
 # MC DPIO driver
 obj-$(CONFIG_FSL_MC_DPIO) += dpio/
--- a/drivers/staging/fsl-mc/bus/dpio/dpio-driver.c
+++ b/drivers/staging/fsl-mc/bus/dpio/dpio-driver.c
@@ -15,7 +15,7 @@
 #include <linux/delay.h>
 #include <linux/io.h>
 
-#include "../../include/mc.h"
+#include <linux/fsl/mc.h>
 #include "../../include/dpaa2-io.h"
 
 #include "qbman-portal.h"
--- a/drivers/staging/fsl-mc/bus/dpio/dpio-service.c
+++ b/drivers/staging/fsl-mc/bus/dpio/dpio-service.c
@@ -5,7 +5,7 @@
  *
  */
 #include <linux/types.h>
-#include "../../include/mc.h"
+#include <linux/fsl/mc.h>
 #include "../../include/dpaa2-io.h"
 #include <linux/init.h>
 #include <linux/module.h>
--- a/drivers/staging/fsl-mc/bus/dpio/dpio.c
+++ b/drivers/staging/fsl-mc/bus/dpio/dpio.c
@@ -5,7 +5,7 @@
  *
  */
 #include <linux/kernel.h>
-#include "../../include/mc.h"
+#include <linux/fsl/mc.h>
 
 #include "dpio.h"
 #include "dpio-cmd.h"
@@ -37,7 +37,7 @@ int dpio_open(struct fsl_mc_io *mc_io,
 	      int dpio_id,
 	      u16 *token)
 {
-	struct mc_command cmd = { 0 };
+	struct fsl_mc_command cmd = { 0 };
 	struct dpio_cmd_open *dpio_cmd;
 	int err;
 
@@ -70,7 +70,7 @@ int dpio_close(struct fsl_mc_io *mc_io,
 	       u32 cmd_flags,
 	       u16 token)
 {
-	struct mc_command cmd = { 0 };
+	struct fsl_mc_command cmd = { 0 };
 
 	/* prepare command */
 	cmd.header = mc_encode_cmd_header(DPIO_CMDID_CLOSE,
@@ -92,7 +92,7 @@ int dpio_enable(struct fsl_mc_io *mc_io,
 		u32 cmd_flags,
 		u16 token)
 {
-	struct mc_command cmd = { 0 };
+	struct fsl_mc_command cmd = { 0 };
 
 	/* prepare command */
 	cmd.header = mc_encode_cmd_header(DPIO_CMDID_ENABLE,
@@ -114,7 +114,7 @@ int dpio_disable(struct fsl_mc_io *mc_io
 		 u32 cmd_flags,
 		 u16 token)
 {
-	struct mc_command cmd = { 0 };
+	struct fsl_mc_command cmd = { 0 };
 
 	/* prepare command */
 	cmd.header = mc_encode_cmd_header(DPIO_CMDID_DISABLE,
@@ -138,7 +138,7 @@ int dpio_get_attributes(struct fsl_mc_io
 			u16 token,
 			struct dpio_attr *attr)
 {
-	struct mc_command cmd = { 0 };
+	struct fsl_mc_command cmd = { 0 };
 	struct dpio_rsp_get_attr *dpio_rsp;
 	int err;
 
@@ -180,7 +180,7 @@ int dpio_get_api_version(struct fsl_mc_i
 			 u16 *major_ver,
 			 u16 *minor_ver)
 {
-	struct mc_command cmd = { 0 };
+	struct fsl_mc_command cmd = { 0 };
 	int err;
 
 	/* prepare command */
--- a/drivers/staging/fsl-mc/bus/dpmcp-cmd.h
+++ /dev/null
@@ -1,56 +0,0 @@
-/*
- * Copyright 2013-2016 Freescale Semiconductor Inc.
- *
- * Redistribution and use in source and binary forms, with or without
- * modification, are permitted provided that the following conditions are met:
- * * Redistributions of source code must retain the above copyright
- * notice, this list of conditions and the following disclaimer.
- * * Redistributions in binary form must reproduce the above copyright
- * notice, this list of conditions and the following disclaimer in the
- * documentation and/or other materials provided with the distribution.
- * * Neither the name of the above-listed copyright holders nor the
- * names of any contributors may be used to endorse or promote products
- * derived from this software without specific prior written permission.
- *
- * ALTERNATIVELY, this software may be distributed under the terms of the
- * GNU General Public License ("GPL") as published by the Free Software
- * Foundation, either version 2 of that License or (at your option) any
- * later version.
- *
- * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
- * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
- * IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
- * ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDERS OR CONTRIBUTORS BE
- * LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
- * CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
- * SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
- * INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
- * CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
- * ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
- * POSSIBILITY OF SUCH DAMAGE.
- */
-#ifndef _FSL_DPMCP_CMD_H
-#define _FSL_DPMCP_CMD_H
-
-/* Minimal supported DPMCP Version */
-#define DPMCP_MIN_VER_MAJOR		3
-#define DPMCP_MIN_VER_MINOR		0
-
-/* Command versioning */
-#define DPMCP_CMD_BASE_VERSION		1
-#define DPMCP_CMD_ID_OFFSET		4
-
-#define DPMCP_CMD(id)	(((id) << DPMCP_CMD_ID_OFFSET) | DPMCP_CMD_BASE_VERSION)
-
-/* Command IDs */
-#define DPMCP_CMDID_CLOSE		DPMCP_CMD(0x800)
-#define DPMCP_CMDID_OPEN		DPMCP_CMD(0x80b)
-#define DPMCP_CMDID_GET_API_VERSION	DPMCP_CMD(0xa0b)
-
-#define DPMCP_CMDID_RESET		DPMCP_CMD(0x005)
-
-struct dpmcp_cmd_open {
-	__le32 dpmcp_id;
-};
-
-#endif /* _FSL_DPMCP_CMD_H */
--- a/drivers/staging/fsl-mc/bus/dpmcp.h
+++ /dev/null
@@ -1,60 +0,0 @@
-/*
- * Copyright 2013-2016 Freescale Semiconductor Inc.
- *
- * Redistribution and use in source and binary forms, with or without
- * modification, are permitted provided that the following conditions are met:
- * * Redistributions of source code must retain the above copyright
- * notice, this list of conditions and the following disclaimer.
- * * Redistributions in binary form must reproduce the above copyright
- * notice, this list of conditions and the following disclaimer in the
- * documentation and/or other materials provided with the distribution.
- * * Neither the name of the above-listed copyright holders nor the
- * names of any contributors may be used to endorse or promote products
- * derived from this software without specific prior written permission.
- *
- * ALTERNATIVELY, this software may be distributed under the terms of the
- * GNU General Public License ("GPL") as published by the Free Software
- * Foundation, either version 2 of that License or (at your option) any
- * later version.
- *
- * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
- * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
- * IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
- * ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDERS OR CONTRIBUTORS BE
- * LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
- * CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
- * SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
- * INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
- * CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
- * ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
- * POSSIBILITY OF SUCH DAMAGE.
- */
-#ifndef __FSL_DPMCP_H
-#define __FSL_DPMCP_H
-
-/*
- * Data Path Management Command Portal API
- * Contains initialization APIs and runtime control APIs for DPMCP
- */
-
-struct fsl_mc_io;
-
-int dpmcp_open(struct fsl_mc_io *mc_io,
-	       u32 cmd_flags,
-	       int dpmcp_id,
-	       u16 *token);
-
-int dpmcp_close(struct fsl_mc_io *mc_io,
-		u32 cmd_flags,
-		u16 token);
-
-int dpmcp_get_api_version(struct fsl_mc_io *mc_io,
-			  u32 cmd_flags,
-			  u16 *major_ver,
-			  u16 *minor_ver);
-
-int dpmcp_reset(struct fsl_mc_io *mc_io,
-		u32 cmd_flags,
-		u16 token);
-
-#endif /* __FSL_DPMCP_H */
--- a/drivers/staging/fsl-mc/bus/dpmng-cmd.h
+++ /dev/null
@@ -1,58 +0,0 @@
-/*
- * Copyright 2013-2016 Freescale Semiconductor Inc.
- *
- * Redistribution and use in source and binary forms, with or without
- * modification, are permitted provided that the following conditions are met:
- *     * Redistributions of source code must retain the above copyright
- *       notice, this list of conditions and the following disclaimer.
- *     * Redistributions in binary form must reproduce the above copyright
- *       notice, this list of conditions and the following disclaimer in the
- *       documentation and/or other materials provided with the distribution.
- *     * Neither the name of the above-listed copyright holders nor the
- *       names of any contributors may be used to endorse or promote products
- *       derived from this software without specific prior written permission.
- *
- * ALTERNATIVELY, this software may be distributed under the terms of the
- * GNU General Public License ("GPL") as published by the Free Software
- * Foundation, either version 2 of that License or (at your option) any
- * later version.
- *
- * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
- * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
- * IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
- * ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDERS OR CONTRIBUTORS BE
- * LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
- * CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
- * SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
- * INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
- * CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
- * ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
- * POSSIBILITY OF SUCH DAMAGE.
- */
-
-/*
- * dpmng-cmd.h
- *
- * defines portal commands
- *
- */
-
-#ifndef __FSL_DPMNG_CMD_H
-#define __FSL_DPMNG_CMD_H
-
-/* Command versioning */
-#define DPMNG_CMD_BASE_VERSION		1
-#define DPMNG_CMD_ID_OFFSET		4
-
-#define DPMNG_CMD(id)	(((id) << DPMNG_CMD_ID_OFFSET) | DPMNG_CMD_BASE_VERSION)
-
-/* Command IDs */
-#define DPMNG_CMDID_GET_VERSION		DPMNG_CMD(0x831)
-
-struct dpmng_rsp_get_version {
-	__le32 revision;
-	__le32 version_major;
-	__le32 version_minor;
-};
-
-#endif /* __FSL_DPMNG_CMD_H */
--- a/drivers/staging/fsl-mc/bus/dprc-cmd.h
+++ /dev/null
@@ -1,451 +0,0 @@
-/*
- * Copyright 2013-2016 Freescale Semiconductor Inc.
- *
- * Redistribution and use in source and binary forms, with or without
- * modification, are permitted provided that the following conditions are met:
- *     * Redistributions of source code must retain the above copyright
- *       notice, this list of conditions and the following disclaimer.
- *     * Redistributions in binary form must reproduce the above copyright
- *       notice, this list of conditions and the following disclaimer in the
- *       documentation and/or other materials provided with the distribution.
- *     * Neither the name of the above-listed copyright holders nor the
- *       names of any contributors may be used to endorse or promote products
- *       derived from this software without specific prior written permission.
- *
- * ALTERNATIVELY, this software may be distributed under the terms of the
- * GNU General Public License ("GPL") as published by the Free Software
- * Foundation, either version 2 of that License or (at your option) any
- * later version.
- *
- * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
- * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
- * IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
- * ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDERS OR CONTRIBUTORS BE
- * LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
- * CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
- * SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
- * INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
- * CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
- * ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
- * POSSIBILITY OF SUCH DAMAGE.
- */
-
-/*
- * dprc-cmd.h
- *
- * defines dprc portal commands
- *
- */
-
-#ifndef _FSL_DPRC_CMD_H
-#define _FSL_DPRC_CMD_H
-
-/* Minimal supported DPRC Version */
-#define DPRC_MIN_VER_MAJOR			6
-#define DPRC_MIN_VER_MINOR			0
-
-/* Command versioning */
-#define DPRC_CMD_BASE_VERSION			1
-#define DPRC_CMD_ID_OFFSET			4
-
-#define DPRC_CMD(id)	(((id) << DPRC_CMD_ID_OFFSET) | DPRC_CMD_BASE_VERSION)
-
-/* Command IDs */
-#define DPRC_CMDID_CLOSE                        DPRC_CMD(0x800)
-#define DPRC_CMDID_OPEN                         DPRC_CMD(0x805)
-#define DPRC_CMDID_GET_API_VERSION              DPRC_CMD(0xa05)
-
-#define DPRC_CMDID_GET_ATTR                     DPRC_CMD(0x004)
-
-#define DPRC_CMDID_SET_IRQ                      DPRC_CMD(0x010)
-#define DPRC_CMDID_GET_IRQ                      DPRC_CMD(0x011)
-#define DPRC_CMDID_SET_IRQ_ENABLE               DPRC_CMD(0x012)
-#define DPRC_CMDID_GET_IRQ_ENABLE               DPRC_CMD(0x013)
-#define DPRC_CMDID_SET_IRQ_MASK                 DPRC_CMD(0x014)
-#define DPRC_CMDID_GET_IRQ_MASK                 DPRC_CMD(0x015)
-#define DPRC_CMDID_GET_IRQ_STATUS               DPRC_CMD(0x016)
-#define DPRC_CMDID_CLEAR_IRQ_STATUS             DPRC_CMD(0x017)
-
-#define DPRC_CMDID_GET_CONT_ID                  DPRC_CMD(0x830)
-#define DPRC_CMDID_GET_OBJ_COUNT                DPRC_CMD(0x159)
-#define DPRC_CMDID_GET_OBJ                      DPRC_CMD(0x15A)
-#define DPRC_CMDID_GET_RES_COUNT                DPRC_CMD(0x15B)
-#define DPRC_CMDID_GET_OBJ_REG                  DPRC_CMD(0x15E)
-#define DPRC_CMDID_SET_OBJ_IRQ                  DPRC_CMD(0x15F)
-#define DPRC_CMDID_GET_OBJ_IRQ                  DPRC_CMD(0x160)
-
-struct dprc_cmd_open {
-	__le32 container_id;
-};
-
-struct dprc_cmd_create_container {
-	/* cmd word 0 */
-	__le32 options;
-	__le16 icid;
-	__le16 pad0;
-	/* cmd word 1 */
-	__le32 pad1;
-	__le32 portal_id;
-	/* cmd words 2-3 */
-	u8 label[16];
-};
-
-struct dprc_rsp_create_container {
-	/* response word 0 */
-	__le64 pad0;
-	/* response word 1 */
-	__le32 child_container_id;
-	__le32 pad1;
-	/* response word 2 */
-	__le64 child_portal_addr;
-};
-
-struct dprc_cmd_destroy_container {
-	__le32 child_container_id;
-};
-
-struct dprc_cmd_reset_container {
-	__le32 child_container_id;
-};
-
-struct dprc_cmd_set_irq {
-	/* cmd word 0 */
-	__le32 irq_val;
-	u8 irq_index;
-	u8 pad[3];
-	/* cmd word 1 */
-	__le64 irq_addr;
-	/* cmd word 2 */
-	__le32 irq_num;
-};
-
-struct dprc_cmd_get_irq {
-	__le32 pad;
-	u8 irq_index;
-};
-
-struct dprc_rsp_get_irq {
-	/* response word 0 */
-	__le32 irq_val;
-	__le32 pad;
-	/* response word 1 */
-	__le64 irq_addr;
-	/* response word 2 */
-	__le32 irq_num;
-	__le32 type;
-};
-
-#define DPRC_ENABLE		0x1
-
-struct dprc_cmd_set_irq_enable {
-	u8 enable;
-	u8 pad[3];
-	u8 irq_index;
-};
-
-struct dprc_cmd_get_irq_enable {
-	__le32 pad;
-	u8 irq_index;
-};
-
-struct dprc_rsp_get_irq_enable {
-	u8 enabled;
-};
-
-struct dprc_cmd_set_irq_mask {
-	__le32 mask;
-	u8 irq_index;
-};
-
-struct dprc_cmd_get_irq_mask {
-	__le32 pad;
-	u8 irq_index;
-};
-
-struct dprc_rsp_get_irq_mask {
-	__le32 mask;
-};
-
-struct dprc_cmd_get_irq_status {
-	__le32 status;
-	u8 irq_index;
-};
-
-struct dprc_rsp_get_irq_status {
-	__le32 status;
-};
-
-struct dprc_cmd_clear_irq_status {
-	__le32 status;
-	u8 irq_index;
-};
-
-struct dprc_rsp_get_attributes {
-	/* response word 0 */
-	__le32 container_id;
-	__le16 icid;
-	__le16 pad;
-	/* response word 1 */
-	__le32 options;
-	__le32 portal_id;
-};
-
-struct dprc_cmd_set_res_quota {
-	/* cmd word 0 */
-	__le32 child_container_id;
-	__le16 quota;
-	__le16 pad;
-	/* cmd words 1-2 */
-	u8 type[16];
-};
-
-struct dprc_cmd_get_res_quota {
-	/* cmd word 0 */
-	__le32 child_container_id;
-	__le32 pad;
-	/* cmd word 1-2 */
-	u8 type[16];
-};
-
-struct dprc_rsp_get_res_quota {
-	__le32 pad;
-	__le16 quota;
-};
-
-struct dprc_cmd_assign {
-	/* cmd word 0 */
-	__le32 container_id;
-	__le32 options;
-	/* cmd word 1 */
-	__le32 num;
-	__le32 id_base_align;
-	/* cmd word 2-3 */
-	u8 type[16];
-};
-
-struct dprc_cmd_unassign {
-	/* cmd word 0 */
-	__le32 child_container_id;
-	__le32 options;
-	/* cmd word 1 */
-	__le32 num;
-	__le32 id_base_align;
-	/* cmd word 2-3 */
-	u8 type[16];
-};
-
-struct dprc_rsp_get_pool_count {
-	__le32 pool_count;
-};
-
-struct dprc_cmd_get_pool {
-	__le32 pool_index;
-};
-
-struct dprc_rsp_get_pool {
-	/* response word 0 */
-	__le64 pad;
-	/* response word 1-2 */
-	u8 type[16];
-};
-
-struct dprc_rsp_get_obj_count {
-	__le32 pad;
-	__le32 obj_count;
-};
-
-struct dprc_cmd_get_obj {
-	__le32 obj_index;
-};
-
-struct dprc_rsp_get_obj {
-	/* response word 0 */
-	__le32 pad0;
-	__le32 id;
-	/* response word 1 */
-	__le16 vendor;
-	u8 irq_count;
-	u8 region_count;
-	__le32 state;
-	/* response word 2 */
-	__le16 version_major;
-	__le16 version_minor;
-	__le16 flags;
-	__le16 pad1;
-	/* response word 3-4 */
-	u8 type[16];
-	/* response word 5-6 */
-	u8 label[16];
-};
-
-struct dprc_cmd_get_obj_desc {
-	/* cmd word 0 */
-	__le32 obj_id;
-	__le32 pad;
-	/* cmd word 1-2 */
-	u8 type[16];
-};
-
-struct dprc_rsp_get_obj_desc {
-	/* response word 0 */
-	__le32 pad0;
-	__le32 id;
-	/* response word 1 */
-	__le16 vendor;
-	u8 irq_count;
-	u8 region_count;
-	__le32 state;
-	/* response word 2 */
-	__le16 version_major;
-	__le16 version_minor;
-	__le16 flags;
-	__le16 pad1;
-	/* response word 3-4 */
-	u8 type[16];
-	/* response word 5-6 */
-	u8 label[16];
-};
-
-struct dprc_cmd_get_res_count {
-	/* cmd word 0 */
-	__le64 pad;
-	/* cmd word 1-2 */
-	u8 type[16];
-};
-
-struct dprc_rsp_get_res_count {
-	__le32 res_count;
-};
-
-struct dprc_cmd_get_res_ids {
-	/* cmd word 0 */
-	u8 pad0[5];
-	u8 iter_status;
-	__le16 pad1;
-	/* cmd word 1 */
-	__le32 base_id;
-	__le32 last_id;
-	/* cmd word 2-3 */
-	u8 type[16];
-};
-
-struct dprc_rsp_get_res_ids {
-	/* response word 0 */
-	u8 pad0[5];
-	u8 iter_status;
-	__le16 pad1;
-	/* response word 1 */
-	__le32 base_id;
-	__le32 last_id;
-};
-
-struct dprc_cmd_get_obj_region {
-	/* cmd word 0 */
-	__le32 obj_id;
-	__le16 pad0;
-	u8 region_index;
-	u8 pad1;
-	/* cmd word 1-2 */
-	__le64 pad2[2];
-	/* cmd word 3-4 */
-	u8 obj_type[16];
-};
-
-struct dprc_rsp_get_obj_region {
-	/* response word 0 */
-	__le64 pad;
-	/* response word 1 */
-	__le64 base_addr;
-	/* response word 2 */
-	__le32 size;
-};
-
-struct dprc_cmd_set_obj_label {
-	/* cmd word 0 */
-	__le32 obj_id;
-	__le32 pad;
-	/* cmd word 1-2 */
-	u8 label[16];
-	/* cmd word 3-4 */
-	u8 obj_type[16];
-};
-
-struct dprc_cmd_set_obj_irq {
-	/* cmd word 0 */
-	__le32 irq_val;
-	u8 irq_index;
-	u8 pad[3];
-	/* cmd word 1 */
-	__le64 irq_addr;
-	/* cmd word 2 */
-	__le32 irq_num;
-	__le32 obj_id;
-	/* cmd word 3-4 */
-	u8 obj_type[16];
-};
-
-struct dprc_cmd_get_obj_irq {
-	/* cmd word 0 */
-	__le32 obj_id;
-	u8 irq_index;
-	u8 pad[3];
-	/* cmd word 1-2 */
-	u8 obj_type[16];
-};
-
-struct dprc_rsp_get_obj_irq {
-	/* response word 0 */
-	__le32 irq_val;
-	__le32 pad;
-	/* response word 1 */
-	__le64 irq_addr;
-	/* response word 2 */
-	__le32 irq_num;
-	__le32 type;
-};
-
-struct dprc_cmd_connect {
-	/* cmd word 0 */
-	__le32 ep1_id;
-	__le32 ep1_interface_id;
-	/* cmd word 1 */
-	__le32 ep2_id;
-	__le32 ep2_interface_id;
-	/* cmd word 2-3 */
-	u8 ep1_type[16];
-	/* cmd word 4 */
-	__le32 max_rate;
-	__le32 committed_rate;
-	/* cmd word 5-6 */
-	u8 ep2_type[16];
-};
-
-struct dprc_cmd_disconnect {
-	/* cmd word 0 */
-	__le32 id;
-	__le32 interface_id;
-	/* cmd word 1-2 */
-	u8 type[16];
-};
-
-struct dprc_cmd_get_connection {
-	/* cmd word 0 */
-	__le32 ep1_id;
-	__le32 ep1_interface_id;
-	/* cmd word 1-2 */
-	u8 ep1_type[16];
-};
-
-struct dprc_rsp_get_connection {
-	/* response word 0-2 */
-	__le64 pad[3];
-	/* response word 3 */
-	__le32 ep2_id;
-	__le32 ep2_interface_id;
-	/* response word 4-5 */
-	u8 ep2_type[16];
-	/* response word 6 */
-	__le32 state;
-};
-
-#endif /* _FSL_DPRC_CMD_H */
--- a/drivers/staging/fsl-mc/bus/dprc.h
+++ /dev/null
@@ -1,268 +0,0 @@
-/*
- * Copyright 2013-2016 Freescale Semiconductor Inc.
- *
- * Redistribution and use in source and binary forms, with or without
- * modification, are permitted provided that the following conditions are met:
- * * Redistributions of source code must retain the above copyright
- * notice, this list of conditions and the following disclaimer.
- * * Redistributions in binary form must reproduce the above copyright
- * notice, this list of conditions and the following disclaimer in the
- * documentation and/or other materials provided with the distribution.
- * * Neither the name of the above-listed copyright holders nor the
- * names of any contributors may be used to endorse or promote products
- * derived from this software without specific prior written permission.
- *
- *
- * ALTERNATIVELY, this software may be distributed under the terms of the
- * GNU General Public License ("GPL") as published by the Free Software
- * Foundation, either version 2 of that License or (at your option) any
- * later version.
- *
- * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
- * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
- * IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
- * ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDERS OR CONTRIBUTORS BE
- * LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
- * CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
- * SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
- * INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
- * CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
- * ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
- * POSSIBILITY OF SUCH DAMAGE.
- */
-#ifndef _FSL_DPRC_H
-#define _FSL_DPRC_H
-
-/*
- * Data Path Resource Container API
- * Contains DPRC API for managing and querying DPAA resources
- */
-
-struct fsl_mc_io;
-struct fsl_mc_obj_desc;
-
-int dprc_open(struct fsl_mc_io *mc_io,
-	      u32 cmd_flags,
-	      int container_id,
-	      u16 *token);
-
-int dprc_close(struct fsl_mc_io *mc_io,
-	       u32 cmd_flags,
-	       u16 token);
-
-/* IRQ */
-
-/* IRQ index */
-#define DPRC_IRQ_INDEX          0
-
-/* Number of dprc's IRQs */
-#define DPRC_NUM_OF_IRQS	1
-
-/* DPRC IRQ events */
-
-/* IRQ event - Indicates that a new object added to the container */
-#define DPRC_IRQ_EVENT_OBJ_ADDED		0x00000001
-/* IRQ event - Indicates that an object was removed from the container */
-#define DPRC_IRQ_EVENT_OBJ_REMOVED		0x00000002
-/* IRQ event - Indicates that resources added to the container */
-#define DPRC_IRQ_EVENT_RES_ADDED		0x00000004
-/* IRQ event - Indicates that resources removed from the container */
-#define DPRC_IRQ_EVENT_RES_REMOVED		0x00000008
-/*
- * IRQ event - Indicates that one of the descendant containers that opened by
- * this container is destroyed
- */
-#define DPRC_IRQ_EVENT_CONTAINER_DESTROYED	0x00000010
-
-/*
- * IRQ event - Indicates that on one of the container's opened object is
- * destroyed
- */
-#define DPRC_IRQ_EVENT_OBJ_DESTROYED		0x00000020
-
-/* Irq event - Indicates that object is created at the container */
-#define DPRC_IRQ_EVENT_OBJ_CREATED		0x00000040
-
-/**
- * struct dprc_irq_cfg - IRQ configuration
- * @paddr:	Address that must be written to signal a message-based interrupt
- * @val:	Value to write into irq_addr address
- * @irq_num:	A user defined number associated with this IRQ
- */
-struct dprc_irq_cfg {
-	     phys_addr_t paddr;
-	     u32 val;
-	     int irq_num;
-};
-
-int dprc_set_irq(struct fsl_mc_io *mc_io,
-		 u32 cmd_flags,
-		 u16 token,
-		 u8 irq_index,
-		 struct dprc_irq_cfg *irq_cfg);
-
-int dprc_get_irq(struct fsl_mc_io *mc_io,
-		 u32 cmd_flags,
-		 u16 token,
-		 u8 irq_index,
-		 int *type,
-		 struct dprc_irq_cfg *irq_cfg);
-
-int dprc_set_irq_enable(struct fsl_mc_io *mc_io,
-			u32 cmd_flags,
-			u16 token,
-			u8 irq_index,
-			u8 en);
-
-int dprc_get_irq_enable(struct fsl_mc_io *mc_io,
-			u32 cmd_flags,
-			u16 token,
-			u8 irq_index,
-			u8 *en);
-
-int dprc_set_irq_mask(struct fsl_mc_io *mc_io,
-		      u32 cmd_flags,
-		      u16 token,
-		      u8 irq_index,
-		      u32 mask);
-
-int dprc_get_irq_mask(struct fsl_mc_io *mc_io,
-		      u32 cmd_flags,
-		      u16 token,
-		      u8 irq_index,
-		      u32 *mask);
-
-int dprc_get_irq_status(struct fsl_mc_io *mc_io,
-			u32 cmd_flags,
-			u16 token,
-			u8 irq_index,
-			u32 *status);
-
-int dprc_clear_irq_status(struct fsl_mc_io *mc_io,
-			  u32 cmd_flags,
-			  u16 token,
-			  u8 irq_index,
-			  u32 status);
-
-/**
- * struct dprc_attributes - Container attributes
- * @container_id: Container's ID
- * @icid: Container's ICID
- * @portal_id: Container's portal ID
- * @options: Container's options as set at container's creation
- */
-struct dprc_attributes {
-	int container_id;
-	u16 icid;
-	int portal_id;
-	u64 options;
-};
-
-int dprc_get_attributes(struct fsl_mc_io *mc_io,
-			u32 cmd_flags,
-			u16 token,
-			struct dprc_attributes *attributes);
-
-int dprc_get_obj_count(struct fsl_mc_io *mc_io,
-		       u32 cmd_flags,
-		       u16 token,
-		       int *obj_count);
-
-int dprc_get_obj(struct fsl_mc_io *mc_io,
-		 u32 cmd_flags,
-		 u16 token,
-		 int obj_index,
-		 struct fsl_mc_obj_desc *obj_desc);
-
-int dprc_get_obj_desc(struct fsl_mc_io *mc_io,
-		      u32 cmd_flags,
-		      u16 token,
-		      char *obj_type,
-		      int obj_id,
-		      struct fsl_mc_obj_desc *obj_desc);
-
-int dprc_set_obj_irq(struct fsl_mc_io *mc_io,
-		     u32 cmd_flags,
-		     u16 token,
-		     char *obj_type,
-		     int obj_id,
-		     u8 irq_index,
-		     struct dprc_irq_cfg *irq_cfg);
-
-int dprc_get_obj_irq(struct fsl_mc_io *mc_io,
-		     u32 cmd_flags,
-		     u16 token,
-		     char *obj_type,
-		     int obj_id,
-		     u8 irq_index,
-		     int *type,
-		     struct dprc_irq_cfg *irq_cfg);
-
-int dprc_get_res_count(struct fsl_mc_io *mc_io,
-		       u32 cmd_flags,
-		       u16 token,
-		       char *type,
-		       int *res_count);
-
-/**
- * enum dprc_iter_status - Iteration status
- * @DPRC_ITER_STATUS_FIRST: Perform first iteration
- * @DPRC_ITER_STATUS_MORE: Indicates more/next iteration is needed
- * @DPRC_ITER_STATUS_LAST: Indicates last iteration
- */
-enum dprc_iter_status {
-	DPRC_ITER_STATUS_FIRST = 0,
-	DPRC_ITER_STATUS_MORE = 1,
-	DPRC_ITER_STATUS_LAST = 2
-};
-
-/* Region flags */
-/* Cacheable - Indicates that region should be mapped as cacheable */
-#define DPRC_REGION_CACHEABLE	0x00000001
-
-/**
- * enum dprc_region_type - Region type
- * @DPRC_REGION_TYPE_MC_PORTAL: MC portal region
- * @DPRC_REGION_TYPE_QBMAN_PORTAL: Qbman portal region
- */
-enum dprc_region_type {
-	DPRC_REGION_TYPE_MC_PORTAL,
-	DPRC_REGION_TYPE_QBMAN_PORTAL
-};
-
-/**
- * struct dprc_region_desc - Mappable region descriptor
- * @base_offset: Region offset from region's base address.
- *	For DPMCP and DPRC objects, region base is offset from SoC MC portals
- *	base address; For DPIO, region base is offset from SoC QMan portals
- *	base address
- * @size: Region size (in bytes)
- * @flags: Region attributes
- * @type: Portal region type
- */
-struct dprc_region_desc {
-	u32 base_offset;
-	u32 size;
-	u32 flags;
-	enum dprc_region_type type;
-};
-
-int dprc_get_obj_region(struct fsl_mc_io *mc_io,
-			u32 cmd_flags,
-			u16 token,
-			char *obj_type,
-			int obj_id,
-			u8 region_index,
-			struct dprc_region_desc *region_desc);
-
-int dprc_get_api_version(struct fsl_mc_io *mc_io,
-			 u32 cmd_flags,
-			 u16 *major_ver,
-			 u16 *minor_ver);
-
-int dprc_get_container_id(struct fsl_mc_io *mc_io,
-			  u32 cmd_flags,
-			  int *container_id);
-
-#endif /* _FSL_DPRC_H */
-
--- a/drivers/staging/fsl-mc/bus/irq-gic-v3-its-fsl-mc-msi.c
+++ b/drivers/staging/fsl-mc/bus/irq-gic-v3-its-fsl-mc-msi.c
@@ -13,6 +13,7 @@
 #include <linux/msi.h>
 #include <linux/of.h>
 #include <linux/of_irq.h>
+#include <linux/fsl/mc.h>
 #include "fsl-mc-private.h"
 
 static struct irq_chip its_msi_irq_chip = {
--- /dev/null
+++ b/include/linux/fsl/mc.h
@@ -0,0 +1,1029 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Freescale Management Complex (MC) bus public interface
+ *
+ * Copyright (C) 2014-2016 Freescale Semiconductor, Inc.
+ * Author: German Rivera <German.Rivera@freescale.com>
+ *
+ */
+#ifndef _FSL_MC_H_
+#define _FSL_MC_H_
+
+#include <linux/device.h>
+#include <linux/mod_devicetable.h>
+#include <linux/interrupt.h>
+#include <linux/cdev.h>
+#include <uapi/linux/fsl_mc.h>
+
+#define FSL_MC_VENDOR_FREESCALE	0x1957
+
+struct irq_domain;
+struct msi_domain_info;
+
+struct fsl_mc_device;
+struct fsl_mc_io;
+
+/**
+ * struct fsl_mc_driver - MC object device driver object
+ * @driver: Generic device driver
+ * @match_id_table: table of supported device matching Ids
+ * @probe: Function called when a device is added
+ * @remove: Function called when a device is removed
+ * @shutdown: Function called at shutdown time to quiesce the device
+ * @suspend: Function called when a device is stopped
+ * @resume: Function called when a device is resumed
+ *
+ * Generic DPAA device driver object for device drivers that are registered
+ * with a DPRC bus. This structure is to be embedded in each device-specific
+ * driver structure.
+ */
+struct fsl_mc_driver {
+	struct device_driver driver;
+	const struct fsl_mc_device_id *match_id_table;
+	int (*probe)(struct fsl_mc_device *dev);
+	int (*remove)(struct fsl_mc_device *dev);
+	void (*shutdown)(struct fsl_mc_device *dev);
+	int (*suspend)(struct fsl_mc_device *dev, pm_message_t state);
+	int (*resume)(struct fsl_mc_device *dev);
+};
+
+#define to_fsl_mc_driver(_drv) \
+	container_of(_drv, struct fsl_mc_driver, driver)
+
+#define to_fsl_mc_bus(_mc_dev) \
+	container_of(_mc_dev, struct fsl_mc_bus, mc_dev)
+
+/**
+ * enum fsl_mc_pool_type - Types of allocatable MC bus resources
+ *
+ * Entries in these enum are used as indices in the array of resource
+ * pools of an fsl_mc_bus object.
+ */
+enum fsl_mc_pool_type {
+	FSL_MC_POOL_DPMCP = 0x0,    /* corresponds to "dpmcp" in the MC */
+	FSL_MC_POOL_DPBP,	    /* corresponds to "dpbp" in the MC */
+	FSL_MC_POOL_DPCON,	    /* corresponds to "dpcon" in the MC */
+	FSL_MC_POOL_IRQ,
+
+	/*
+	 * NOTE: New resource pool types must be added before this entry
+	 */
+	FSL_MC_NUM_POOL_TYPES
+};
+
+/**
+ * struct fsl_mc_resource - MC generic resource
+ * @type: type of resource
+ * @id: unique MC resource Id within the resources of the same type
+ * @data: pointer to resource-specific data if the resource is currently
+ * allocated, or NULL if the resource is not currently allocated.
+ * @parent_pool: pointer to the parent resource pool from which this
+ * resource is allocated from.
+ * @node: Node in the free list of the corresponding resource pool
+ *
+ * NOTE: This structure is to be embedded as a field of specific
+ * MC resource structures.
+ */
+struct fsl_mc_resource {
+	enum fsl_mc_pool_type type;
+	s32 id;
+	void *data;
+	struct fsl_mc_resource_pool *parent_pool;
+	struct list_head node;
+};
+
+/**
+ * struct fsl_mc_device_irq - MC object device message-based interrupt
+ * @msi_desc: pointer to MSI descriptor allocated by fsl_mc_msi_alloc_descs()
+ * @mc_dev: MC object device that owns this interrupt
+ * @dev_irq_index: device-relative IRQ index
+ * @resource: MC generic resource associated with the interrupt
+ */
+struct fsl_mc_device_irq {
+	struct msi_desc *msi_desc;
+	struct fsl_mc_device *mc_dev;
+	u8 dev_irq_index;
+	struct fsl_mc_resource resource;
+};
+
+#define to_fsl_mc_irq(_mc_resource) \
+	container_of(_mc_resource, struct fsl_mc_device_irq, resource)
+
+/* Opened state - Indicates that an object is open by at least one owner */
+#define FSL_MC_OBJ_STATE_OPEN		0x00000001
+/* Plugged state - Indicates that the object is plugged */
+#define FSL_MC_OBJ_STATE_PLUGGED	0x00000002
+
+/**
+ * Shareability flag - Object flag indicating no memory shareability.
+ * the object generates memory accesses that are non coherent with other
+ * masters;
+ * user is responsible for proper memory handling through IOMMU configuration.
+ */
+#define FSL_MC_OBJ_FLAG_NO_MEM_SHAREABILITY	0x0001
+
+/**
+ * struct fsl_mc_obj_desc - Object descriptor
+ * @type: Type of object: NULL terminated string
+ * @id: ID of logical object resource
+ * @vendor: Object vendor identifier
+ * @ver_major: Major version number
+ * @ver_minor:  Minor version number
+ * @irq_count: Number of interrupts supported by the object
+ * @region_count: Number of mappable regions supported by the object
+ * @state: Object state: combination of FSL_MC_OBJ_STATE_ states
+ * @label: Object label: NULL terminated string
+ * @flags: Object's flags
+ */
+struct fsl_mc_obj_desc {
+	char type[16];
+	int id;
+	u16 vendor;
+	u16 ver_major;
+	u16 ver_minor;
+	u8 irq_count;
+	u8 region_count;
+	u32 state;
+	char label[16];
+	u16 flags;
+};
+
+/**
+ * Bit masks for a MC object device (struct fsl_mc_device) flags
+ */
+#define FSL_MC_IS_DPRC	0x0001
+
+/**
+ * struct fsl_mc_device - MC object device object
+ * @dev: Linux driver model device object
+ * @dma_mask: Default DMA mask
+ * @flags: MC object device flags
+ * @icid: Isolation context ID for the device
+ * @mc_handle: MC handle for the corresponding MC object opened
+ * @mc_io: Pointer to MC IO object assigned to this device or
+ * NULL if none.
+ * @obj_desc: MC description of the DPAA device
+ * @regions: pointer to array of MMIO region entries
+ * @irqs: pointer to array of pointers to interrupts allocated to this device
+ * @resource: generic resource associated with this MC object device, if any.
+ * @driver_override: Driver name to force a match
+ *
+ * Generic device object for MC object devices that are "attached" to a
+ * MC bus.
+ *
+ * NOTES:
+ * - For a non-DPRC object its icid is the same as its parent DPRC's icid.
+ * - The SMMU notifier callback gets invoked after device_add() has been
+ *   called for an MC object device, but before the device-specific probe
+ *   callback gets called.
+ * - DP_OBJ_DPRC objects are the only MC objects that have built-in MC
+ *   portals. For all other MC objects, their device drivers are responsible for
+ *   allocating MC portals for them by calling fsl_mc_portal_allocate().
+ * - Some types of MC objects (e.g., DP_OBJ_DPBP, DP_OBJ_DPCON) are
+ *   treated as resources that can be allocated/deallocated from the
+ *   corresponding resource pool in the object's parent DPRC, using the
+ *   fsl_mc_object_allocate()/fsl_mc_object_free() functions. These MC objects
+ *   are known as "allocatable" objects. For them, the corresponding
+ *   fsl_mc_device's 'resource' points to the associated resource object.
+ *   For MC objects that are not allocatable (e.g., DP_OBJ_DPRC, DP_OBJ_DPNI),
+ *   'resource' is NULL.
+ */
+struct fsl_mc_device {
+	struct device dev;
+	u64 dma_mask;
+	u16 flags;
+	u32 icid;
+	u16 mc_handle;
+	struct fsl_mc_io *mc_io;
+	struct fsl_mc_obj_desc obj_desc;
+	struct resource *regions;
+	struct fsl_mc_device_irq **irqs;
+	struct fsl_mc_resource *resource;
+	const char *driver_override;
+	struct device_link *consumer_link;
+};
+
+#define to_fsl_mc_device(_dev) \
+	container_of(_dev, struct fsl_mc_device, dev)
+
+struct mc_cmd_header {
+	u8 src_id;
+	u8 flags_hw;
+	u8 status;
+	u8 flags_sw;
+	__le16 token;
+	__le16 cmd_id;
+};
+
+enum mc_cmd_status {
+	MC_CMD_STATUS_OK = 0x0, /* Completed successfully */
+	MC_CMD_STATUS_READY = 0x1, /* Ready to be processed */
+	MC_CMD_STATUS_AUTH_ERR = 0x3, /* Authentication error */
+	MC_CMD_STATUS_NO_PRIVILEGE = 0x4, /* No privilege */
+	MC_CMD_STATUS_DMA_ERR = 0x5, /* DMA or I/O error */
+	MC_CMD_STATUS_CONFIG_ERR = 0x6, /* Configuration error */
+	MC_CMD_STATUS_TIMEOUT = 0x7, /* Operation timed out */
+	MC_CMD_STATUS_NO_RESOURCE = 0x8, /* No resources */
+	MC_CMD_STATUS_NO_MEMORY = 0x9, /* No memory available */
+	MC_CMD_STATUS_BUSY = 0xA, /* Device is busy */
+	MC_CMD_STATUS_UNSUPPORTED_OP = 0xB, /* Unsupported operation */
+	MC_CMD_STATUS_INVALID_STATE = 0xC /* Invalid state */
+};
+
+/*
+ * MC command flags
+ */
+
+/* High priority flag */
+#define MC_CMD_FLAG_PRI		0x80
+/* Command completion flag */
+#define MC_CMD_FLAG_INTR_DIS	0x01
+
+static inline u64 mc_encode_cmd_header(u16 cmd_id,
+				       u32 cmd_flags,
+				       u16 token)
+{
+	u64 header = 0;
+	struct mc_cmd_header *hdr = (struct mc_cmd_header *)&header;
+
+	hdr->cmd_id = cpu_to_le16(cmd_id);
+	hdr->token  = cpu_to_le16(token);
+	hdr->status = MC_CMD_STATUS_READY;
+	if (cmd_flags & MC_CMD_FLAG_PRI)
+		hdr->flags_hw = MC_CMD_FLAG_PRI;
+	if (cmd_flags & MC_CMD_FLAG_INTR_DIS)
+		hdr->flags_sw = MC_CMD_FLAG_INTR_DIS;
+
+	return header;
+}
+
+static inline u16 mc_cmd_hdr_read_token(struct fsl_mc_command *cmd)
+{
+	struct mc_cmd_header *hdr = (struct mc_cmd_header *)&cmd->header;
+	u16 token = le16_to_cpu(hdr->token);
+
+	return token;
+}
+
+struct mc_rsp_create {
+	__le32 object_id;
+};
+
+struct mc_rsp_api_ver {
+	__le16 major_ver;
+	__le16 minor_ver;
+};
+
+static inline u32 mc_cmd_read_object_id(struct fsl_mc_command *cmd)
+{
+	struct mc_rsp_create *rsp_params;
+
+	rsp_params = (struct mc_rsp_create *)cmd->params;
+	return le32_to_cpu(rsp_params->object_id);
+}
+
+static inline void mc_cmd_read_api_version(struct fsl_mc_command *cmd,
+					   u16 *major_ver,
+					   u16 *minor_ver)
+{
+	struct mc_rsp_api_ver *rsp_params;
+
+	rsp_params = (struct mc_rsp_api_ver *)cmd->params;
+	*major_ver = le16_to_cpu(rsp_params->major_ver);
+	*minor_ver = le16_to_cpu(rsp_params->minor_ver);
+}
+
+/**
+ * Bit masks for a MC I/O object (struct fsl_mc_io) flags
+ */
+#define FSL_MC_IO_ATOMIC_CONTEXT_PORTAL	0x0001
+
+/**
+ * struct fsl_mc_io - MC I/O object to be passed-in to mc_send_command()
+ * @dev: device associated with this Mc I/O object
+ * @flags: flags for mc_send_command()
+ * @portal_size: MC command portal size in bytes
+ * @portal_phys_addr: MC command portal physical address
+ * @portal_virt_addr: MC command portal virtual address
+ * @dpmcp_dev: pointer to the DPMCP device associated with the MC portal.
+ *
+ * Fields are only meaningful if the FSL_MC_IO_ATOMIC_CONTEXT_PORTAL flag is not
+ * set:
+ * @mutex: Mutex to serialize mc_send_command() calls that use the same MC
+ * portal, if the fsl_mc_io object was created with the
+ * FSL_MC_IO_ATOMIC_CONTEXT_PORTAL flag off. mc_send_command() calls for this
+ * fsl_mc_io object must be made only from non-atomic context.
+ *
+ * Fields are only meaningful if the FSL_MC_IO_ATOMIC_CONTEXT_PORTAL flag is
+ * set:
+ * @spinlock: Spinlock to serialize mc_send_command() calls that use the same MC
+ * portal, if the fsl_mc_io object was created with the
+ * FSL_MC_IO_ATOMIC_CONTEXT_PORTAL flag on. mc_send_command() calls for this
+ * fsl_mc_io object can be made from atomic or non-atomic context.
+ */
+struct fsl_mc_io {
+	struct device *dev;
+	u16 flags;
+	u32 portal_size;
+	phys_addr_t portal_phys_addr;
+	void __iomem *portal_virt_addr;
+	struct fsl_mc_device *dpmcp_dev;
+	union {
+		/*
+		 * This field is only meaningful if the
+		 * FSL_MC_IO_ATOMIC_CONTEXT_PORTAL flag is not set
+		 */
+		struct mutex mutex; /* serializes mc_send_command() */
+
+		/*
+		 * This field is only meaningful if the
+		 * FSL_MC_IO_ATOMIC_CONTEXT_PORTAL flag is set
+		 */
+		spinlock_t spinlock;	/* serializes mc_send_command() */
+	};
+};
+
+int mc_send_command(struct fsl_mc_io *mc_io, struct fsl_mc_command *cmd);
+
+#ifdef CONFIG_FSL_MC_BUS
+#define dev_is_fsl_mc(_dev) ((_dev)->bus == &fsl_mc_bus_type)
+#else
+/* If fsl-mc bus is not present device cannot belong to fsl-mc bus */
+#define dev_is_fsl_mc(_dev) (0)
+#endif
+
+/* Macro to check if a device is a container device */
+#define fsl_mc_is_cont_dev(_dev) (to_fsl_mc_device(_dev)->flags & \
+	FSL_MC_IS_DPRC)
+
+/* Macro to get the container device of a MC device */
+#define fsl_mc_cont_dev(_dev) (fsl_mc_is_cont_dev(_dev) ? \
+	(_dev) : (_dev)->parent)
+
+#define fsl_mc_is_dev_coherent(_dev) \
+	(!((to_fsl_mc_device(_dev))->obj_desc.flags & \
+	FSL_MC_OBJ_FLAG_NO_MEM_SHAREABILITY))
+
+/*
+ * module_fsl_mc_driver() - Helper macro for drivers that don't do
+ * anything special in module init/exit.  This eliminates a lot of
+ * boilerplate.  Each module may only use this macro once, and
+ * calling it replaces module_init() and module_exit()
+ */
+#define module_fsl_mc_driver(__fsl_mc_driver) \
+	module_driver(__fsl_mc_driver, fsl_mc_driver_register, \
+		      fsl_mc_driver_unregister)
+
+void fsl_mc_device_remove(struct fsl_mc_device *mc_dev);
+
+/*
+ * Macro to avoid include chaining to get THIS_MODULE
+ */
+#define fsl_mc_driver_register(drv) \
+	__fsl_mc_driver_register(drv, THIS_MODULE)
+
+int __must_check __fsl_mc_driver_register(struct fsl_mc_driver *fsl_mc_driver,
+					  struct module *owner);
+
+void fsl_mc_driver_unregister(struct fsl_mc_driver *driver);
+
+int __must_check fsl_mc_portal_allocate(struct fsl_mc_device *mc_dev,
+					u16 mc_io_flags,
+					struct fsl_mc_io **new_mc_io);
+
+void fsl_mc_portal_free(struct fsl_mc_io *mc_io);
+
+int fsl_mc_portal_reset(struct fsl_mc_io *mc_io);
+
+int __must_check fsl_mc_object_allocate(struct fsl_mc_device *mc_dev,
+					enum fsl_mc_pool_type pool_type,
+					struct fsl_mc_device **new_mc_adev);
+
+void fsl_mc_object_free(struct fsl_mc_device *mc_adev);
+
+struct irq_domain *fsl_mc_msi_create_irq_domain(struct fwnode_handle *fwnode,
+						struct msi_domain_info *info,
+						struct irq_domain *parent);
+
+int __must_check fsl_mc_allocate_irqs(struct fsl_mc_device *mc_dev);
+
+void fsl_mc_free_irqs(struct fsl_mc_device *mc_dev);
+
+extern struct bus_type fsl_mc_bus_type;
+
+extern struct device_type fsl_mc_bus_dprc_type;
+extern struct device_type fsl_mc_bus_dpni_type;
+extern struct device_type fsl_mc_bus_dpio_type;
+extern struct device_type fsl_mc_bus_dpsw_type;
+extern struct device_type fsl_mc_bus_dpdmux_type;
+extern struct device_type fsl_mc_bus_dpbp_type;
+extern struct device_type fsl_mc_bus_dpcon_type;
+extern struct device_type fsl_mc_bus_dpmcp_type;
+extern struct device_type fsl_mc_bus_dpmac_type;
+extern struct device_type fsl_mc_bus_dprtc_type;
+extern struct device_type fsl_mc_bus_dpseci_type;
+extern struct device_type fsl_mc_bus_dpdcei_type;
+extern struct device_type fsl_mc_bus_dpaiop_type;
+extern struct device_type fsl_mc_bus_dpci_type;
+extern struct device_type fsl_mc_bus_dpdmai_type;
+
+static inline bool is_fsl_mc_bus_dprc(const struct fsl_mc_device *mc_dev)
+{
+	return mc_dev->dev.type == &fsl_mc_bus_dprc_type;
+}
+
+static inline bool is_fsl_mc_bus_dpni(const struct fsl_mc_device *mc_dev)
+{
+	return mc_dev->dev.type == &fsl_mc_bus_dpni_type;
+}
+
+static inline bool is_fsl_mc_bus_dpio(const struct fsl_mc_device *mc_dev)
+{
+	return mc_dev->dev.type == &fsl_mc_bus_dpio_type;
+}
+
+static inline bool is_fsl_mc_bus_dpsw(const struct fsl_mc_device *mc_dev)
+{
+	return mc_dev->dev.type == &fsl_mc_bus_dpsw_type;
+}
+
+static inline bool is_fsl_mc_bus_dpdmux(const struct fsl_mc_device *mc_dev)
+{
+	return mc_dev->dev.type == &fsl_mc_bus_dpdmux_type;
+}
+
+static inline bool is_fsl_mc_bus_dpbp(const struct fsl_mc_device *mc_dev)
+{
+	return mc_dev->dev.type == &fsl_mc_bus_dpbp_type;
+}
+
+static inline bool is_fsl_mc_bus_dpcon(const struct fsl_mc_device *mc_dev)
+{
+	return mc_dev->dev.type == &fsl_mc_bus_dpcon_type;
+}
+
+static inline bool is_fsl_mc_bus_dpmcp(const struct fsl_mc_device *mc_dev)
+{
+	return mc_dev->dev.type == &fsl_mc_bus_dpmcp_type;
+}
+
+static inline bool is_fsl_mc_bus_dpmac(const struct fsl_mc_device *mc_dev)
+{
+	return mc_dev->dev.type == &fsl_mc_bus_dpmac_type;
+}
+
+static inline bool is_fsl_mc_bus_dprtc(const struct fsl_mc_device *mc_dev)
+{
+	return mc_dev->dev.type == &fsl_mc_bus_dprtc_type;
+}
+
+static inline bool is_fsl_mc_bus_dpseci(const struct fsl_mc_device *mc_dev)
+{
+	return mc_dev->dev.type == &fsl_mc_bus_dpseci_type;
+}
+
+static inline bool is_fsl_mc_bus_dpdcei(const struct fsl_mc_device *mc_dev)
+{
+	return mc_dev->dev.type == &fsl_mc_bus_dpdcei_type;
+}
+
+static inline bool is_fsl_mc_bus_dpaiop(const struct fsl_mc_device *mc_dev)
+{
+	return mc_dev->dev.type == &fsl_mc_bus_dpaiop_type;
+}
+
+static inline bool is_fsl_mc_bus_dpci(const struct fsl_mc_device *mc_dev)
+{
+	return mc_dev->dev.type == &fsl_mc_bus_dpci_type;
+}
+
+static inline bool is_fsl_mc_bus_dpdmai(const struct fsl_mc_device *mc_dev)
+{
+	return mc_dev->dev.type == &fsl_mc_bus_dpdmai_type;
+}
+
+/*
+ * Data Path Resource Container (DPRC) API
+ */
+
+/* Minimal supported DPRC Version */
+#define DPRC_MIN_VER_MAJOR			6
+#define DPRC_MIN_VER_MINOR			0
+
+/* DPRC command versioning */
+#define DPRC_CMD_BASE_VERSION			1
+#define DPRC_CMD_2ND_VERSION			2
+#define DPRC_CMD_ID_OFFSET			4
+
+#define DPRC_CMD(id)	(((id) << DPRC_CMD_ID_OFFSET) | DPRC_CMD_BASE_VERSION)
+#define DPRC_CMD_V2(id)	(((id) << DPRC_CMD_ID_OFFSET) | DPRC_CMD_2ND_VERSION)
+
+/* DPRC command IDs */
+#define DPRC_CMDID_CLOSE                        DPRC_CMD(0x800)
+#define DPRC_CMDID_OPEN                         DPRC_CMD(0x805)
+#define DPRC_CMDID_GET_API_VERSION              DPRC_CMD(0xa05)
+
+#define DPRC_CMDID_GET_ATTR                     DPRC_CMD(0x004)
+#define DPRC_CMDID_RESET_CONT                   DPRC_CMD(0x005)
+
+#define DPRC_CMDID_SET_IRQ                      DPRC_CMD(0x010)
+#define DPRC_CMDID_SET_IRQ_ENABLE               DPRC_CMD(0x012)
+#define DPRC_CMDID_SET_IRQ_MASK                 DPRC_CMD(0x014)
+#define DPRC_CMDID_GET_IRQ_STATUS               DPRC_CMD(0x016)
+#define DPRC_CMDID_CLEAR_IRQ_STATUS             DPRC_CMD(0x017)
+
+#define DPRC_CMDID_GET_CONT_ID                  DPRC_CMD(0x830)
+#define DPRC_CMDID_GET_OBJ_COUNT                DPRC_CMD(0x159)
+#define DPRC_CMDID_GET_OBJ                      DPRC_CMD(0x15A)
+#define DPRC_CMDID_GET_OBJ_REG                  DPRC_CMD_V2(0x15E)
+#define DPRC_CMDID_SET_OBJ_IRQ                  DPRC_CMD(0x15F)
+
+struct dprc_cmd_open {
+	__le32 container_id;
+};
+
+struct dprc_cmd_reset_container {
+	__le32 child_container_id;
+};
+
+struct dprc_cmd_set_irq {
+	/* cmd word 0 */
+	__le32 irq_val;
+	u8 irq_index;
+	u8 pad[3];
+	/* cmd word 1 */
+	__le64 irq_addr;
+	/* cmd word 2 */
+	__le32 irq_num;
+};
+
+#define DPRC_ENABLE		0x1
+
+struct dprc_cmd_set_irq_enable {
+	u8 enable;
+	u8 pad[3];
+	u8 irq_index;
+};
+
+struct dprc_cmd_set_irq_mask {
+	__le32 mask;
+	u8 irq_index;
+};
+
+struct dprc_cmd_get_irq_status {
+	__le32 status;
+	u8 irq_index;
+};
+
+struct dprc_rsp_get_irq_status {
+	__le32 status;
+};
+
+struct dprc_cmd_clear_irq_status {
+	__le32 status;
+	u8 irq_index;
+};
+
+struct dprc_rsp_get_attributes {
+	/* response word 0 */
+	__le32 container_id;
+	__le32 icid;
+	/* response word 1 */
+	__le32 options;
+	__le32 portal_id;
+};
+
+struct dprc_rsp_get_obj_count {
+	__le32 pad;
+	__le32 obj_count;
+};
+
+struct dprc_cmd_get_obj {
+	__le32 obj_index;
+};
+
+struct dprc_rsp_get_obj {
+	/* response word 0 */
+	__le32 pad0;
+	__le32 id;
+	/* response word 1 */
+	__le16 vendor;
+	u8 irq_count;
+	u8 region_count;
+	__le32 state;
+	/* response word 2 */
+	__le16 version_major;
+	__le16 version_minor;
+	__le16 flags;
+	__le16 pad1;
+	/* response word 3-4 */
+	u8 type[16];
+	/* response word 5-6 */
+	u8 label[16];
+};
+
+struct dprc_cmd_get_obj_region {
+	/* cmd word 0 */
+	__le32 obj_id;
+	__le16 pad0;
+	u8 region_index;
+	u8 pad1;
+	/* cmd word 1-2 */
+	__le64 pad2[2];
+	/* cmd word 3-4 */
+	u8 obj_type[16];
+};
+
+struct dprc_rsp_get_obj_region {
+	/* response word 0 */
+	__le64 pad0;
+	/* response word 1 */
+	__le32 base_offset;
+	__le32 pad1;
+	/* response word 2 */
+	__le32 size;
+	u8 type;
+	u8 pad2[3];
+	/* response word 3 */
+	__le32 flags;
+	__le32 pad3;
+	/* response word 4 */
+	__le64 base_addr;
+};
+
+struct dprc_cmd_set_obj_irq {
+	/* cmd word 0 */
+	__le32 irq_val;
+	u8 irq_index;
+	u8 pad[3];
+	/* cmd word 1 */
+	__le64 irq_addr;
+	/* cmd word 2 */
+	__le32 irq_num;
+	__le32 obj_id;
+	/* cmd word 3-4 */
+	u8 obj_type[16];
+};
+
+/*
+ * DPRC API for managing and querying DPAA resources
+ */
+int dprc_open(struct fsl_mc_io *mc_io,
+	      u32 cmd_flags,
+	      int container_id,
+	      u16 *token);
+
+int dprc_close(struct fsl_mc_io *mc_io,
+	       u32 cmd_flags,
+	       u16 token);
+
+/* DPRC IRQ events */
+
+/* IRQ event - Indicates that a new object added to the container */
+#define DPRC_IRQ_EVENT_OBJ_ADDED		0x00000001
+/* IRQ event - Indicates that an object was removed from the container */
+#define DPRC_IRQ_EVENT_OBJ_REMOVED		0x00000002
+/*
+ * IRQ event - Indicates that one of the descendant containers that opened by
+ * this container is destroyed
+ */
+#define DPRC_IRQ_EVENT_CONTAINER_DESTROYED	0x00000010
+
+/*
+ * IRQ event - Indicates that on one of the container's opened object is
+ * destroyed
+ */
+#define DPRC_IRQ_EVENT_OBJ_DESTROYED		0x00000020
+
+/* Irq event - Indicates that object is created at the container */
+#define DPRC_IRQ_EVENT_OBJ_CREATED		0x00000040
+
+/**
+ * struct dprc_irq_cfg - IRQ configuration
+ * @paddr:	Address that must be written to signal a message-based interrupt
+ * @val:	Value to write into irq_addr address
+ * @irq_num:	A user defined number associated with this IRQ
+ */
+struct dprc_irq_cfg {
+	     phys_addr_t paddr;
+	     u32 val;
+	     int irq_num;
+};
+
+int dprc_set_irq(struct fsl_mc_io *mc_io,
+		 u32 cmd_flags,
+		 u16 token,
+		 u8 irq_index,
+		 struct dprc_irq_cfg *irq_cfg);
+
+int dprc_set_irq_enable(struct fsl_mc_io *mc_io,
+			u32 cmd_flags,
+			u16 token,
+			u8 irq_index,
+			u8 en);
+
+int dprc_set_irq_mask(struct fsl_mc_io *mc_io,
+		      u32 cmd_flags,
+		      u16 token,
+		      u8 irq_index,
+		      u32 mask);
+
+int dprc_get_irq_status(struct fsl_mc_io *mc_io,
+			u32 cmd_flags,
+			u16 token,
+			u8 irq_index,
+			u32 *status);
+
+int dprc_clear_irq_status(struct fsl_mc_io *mc_io,
+			  u32 cmd_flags,
+			  u16 token,
+			  u8 irq_index,
+			  u32 status);
+
+/**
+ * struct dprc_attributes - Container attributes
+ * @container_id: Container's ID
+ * @icid: Container's ICID
+ * @portal_id: Container's portal ID
+ * @options: Container's options as set at container's creation
+ */
+struct dprc_attributes {
+	int container_id;
+	u32 icid;
+	int portal_id;
+	u64 options;
+};
+
+int dprc_get_attributes(struct fsl_mc_io *mc_io,
+			u32 cmd_flags,
+			u16 token,
+			struct dprc_attributes *attributes);
+
+int dprc_get_obj_count(struct fsl_mc_io *mc_io,
+		       u32 cmd_flags,
+		       u16 token,
+		       int *obj_count);
+
+int dprc_get_obj(struct fsl_mc_io *mc_io,
+		 u32 cmd_flags,
+		 u16 token,
+		 int obj_index,
+		 struct fsl_mc_obj_desc *obj_desc);
+
+int dprc_set_obj_irq(struct fsl_mc_io *mc_io,
+		     u32 cmd_flags,
+		     u16 token,
+		     char *obj_type,
+		     int obj_id,
+		     u8 irq_index,
+		     struct dprc_irq_cfg *irq_cfg);
+
+/* Region flags */
+/* Cacheable - Indicates that region should be mapped as cacheable */
+#define DPRC_REGION_CACHEABLE	0x00000001
+#define DPRC_REGION_SHAREABLE	0x00000002
+
+/**
+ * enum dprc_region_type - Region type
+ * @DPRC_REGION_TYPE_MC_PORTAL: MC portal region
+ * @DPRC_REGION_TYPE_QBMAN_PORTAL: Qbman portal region
+ */
+enum dprc_region_type {
+	DPRC_REGION_TYPE_MC_PORTAL,
+	DPRC_REGION_TYPE_QBMAN_PORTAL,
+	DPRC_REGION_TYPE_QBMAN_MEM_BACKED_PORTAL
+};
+
+/**
+ * struct dprc_region_desc - Mappable region descriptor
+ * @base_offset: Region offset from region's base address.
+ *	For DPMCP and DPRC objects, region base is offset from SoC MC portals
+ *	base address; For DPIO, region base is offset from SoC QMan portals
+ *	base address
+ * @size: Region size (in bytes)
+ * @flags: Region attributes
+ * @type: Portal region type
+ */
+struct dprc_region_desc {
+	u32 base_offset;
+	u32 size;
+	u32 flags;
+	enum dprc_region_type type;
+	u64 base_address;
+};
+
+int dprc_get_obj_region(struct fsl_mc_io *mc_io,
+			u32 cmd_flags,
+			u16 token,
+			char *obj_type,
+			int obj_id,
+			u8 region_index,
+			struct dprc_region_desc *region_desc);
+
+int dprc_get_api_version(struct fsl_mc_io *mc_io,
+			 u32 cmd_flags,
+			 u16 *major_ver,
+			 u16 *minor_ver);
+
+int dprc_get_container_id(struct fsl_mc_io *mc_io,
+			  u32 cmd_flags,
+			  int *container_id);
+
+int dprc_reset_container(struct fsl_mc_io *mc_io,
+			 u32 cmd_flags,
+			 u16 token,
+			 int child_container_id);
+
+/*
+ * Data Path Buffer Pool (DPBP) API
+ * Contains initialization APIs and runtime control APIs for DPBP
+ */
+
+int dpbp_open(struct fsl_mc_io *mc_io,
+	      u32 cmd_flags,
+	      int dpbp_id,
+	      u16 *token);
+
+int dpbp_close(struct fsl_mc_io *mc_io,
+	       u32 cmd_flags,
+	       u16 token);
+
+int dpbp_enable(struct fsl_mc_io *mc_io,
+		u32 cmd_flags,
+		u16 token);
+
+int dpbp_disable(struct fsl_mc_io *mc_io,
+		 u32 cmd_flags,
+		 u16 token);
+
+int dpbp_reset(struct fsl_mc_io *mc_io,
+	       u32 cmd_flags,
+	       u16 token);
+
+/**
+ * struct dpbp_attr - Structure representing DPBP attributes
+ * @id:		DPBP object ID
+ * @bpid:	Hardware buffer pool ID; should be used as an argument in
+ *		acquire/release operations on buffers
+ */
+struct dpbp_attr {
+	int id;
+	u16 bpid;
+};
+
+int dpbp_get_attributes(struct fsl_mc_io *mc_io,
+			u32 cmd_flags,
+			u16 token,
+			struct dpbp_attr *attr);
+
+/* Data Path Concentrator (DPCON) API
+ * Contains initialization APIs and runtime control APIs for DPCON
+ */
+
+/**
+ * Use it to disable notifications; see dpcon_set_notification()
+ */
+#define DPCON_INVALID_DPIO_ID		(int)(-1)
+
+int dpcon_open(struct fsl_mc_io *mc_io,
+	       u32 cmd_flags,
+	       int dpcon_id,
+	       u16 *token);
+
+int dpcon_close(struct fsl_mc_io *mc_io,
+		u32 cmd_flags,
+		u16 token);
+
+int dpcon_enable(struct fsl_mc_io *mc_io,
+		 u32 cmd_flags,
+		 u16 token);
+
+int dpcon_disable(struct fsl_mc_io *mc_io,
+		  u32 cmd_flags,
+		  u16 token);
+
+int dpcon_reset(struct fsl_mc_io *mc_io,
+		u32 cmd_flags,
+		u16 token);
+
+/**
+ * struct dpcon_attr - Structure representing DPCON attributes
+ * @id: DPCON object ID
+ * @qbman_ch_id: Channel ID to be used by dequeue operation
+ * @num_priorities: Number of priorities for the DPCON channel (1-8)
+ */
+struct dpcon_attr {
+	int id;
+	u16 qbman_ch_id;
+	u8 num_priorities;
+};
+
+int dpcon_get_attributes(struct fsl_mc_io *mc_io,
+			 u32 cmd_flags,
+			 u16 token,
+			 struct dpcon_attr *attr);
+
+/**
+ * struct dpcon_notification_cfg - Structure representing notification params
+ * @dpio_id:	DPIO object ID; must be configured with a notification channel;
+ *	to disable notifications set it to 'DPCON_INVALID_DPIO_ID';
+ * @priority:	Priority selection within the DPIO channel; valid values
+ *		are 0-7, depending on the number of priorities in that channel
+ * @user_ctx:	User context value provided with each CDAN message
+ */
+struct dpcon_notification_cfg {
+	int dpio_id;
+	u8 priority;
+	u64 user_ctx;
+};
+
+int dpcon_set_notification(struct fsl_mc_io *mc_io,
+			   u32 cmd_flags,
+			   u16 token,
+			   struct dpcon_notification_cfg *cfg);
+
+struct irq_domain;
+struct msi_domain_info;
+
+/**
+ * Maximum number of total IRQs that can be pre-allocated for an MC bus'
+ * IRQ pool
+ */
+#define FSL_MC_IRQ_POOL_MAX_TOTAL_IRQS	256
+
+/**
+ * struct fsl_mc_resource_pool - Pool of MC resources of a given
+ * type
+ * @type: type of resources in the pool
+ * @max_count: maximum number of resources in the pool
+ * @free_count: number of free resources in the pool
+ * @mutex: mutex to serialize access to the pool's free list
+ * @free_list: anchor node of list of free resources in the pool
+ * @mc_bus: pointer to the MC bus that owns this resource pool
+ */
+struct fsl_mc_resource_pool {
+	enum fsl_mc_pool_type type;
+	int max_count;
+	int free_count;
+	struct mutex mutex;	/* serializes access to free_list */
+	struct list_head free_list;
+	struct fsl_mc_bus *mc_bus;
+};
+
+/**
+ * struct fsl_mc_restool - information associated with a restool device file
+ * @cdev: struct char device linked to the root dprc
+ * @dev: dev_t for the char device to be added
+ * @device: newly created device in /dev
+ * @mutex: mutex lock to serialize the open/release operations
+ * @local_instance_in_use: local MC I/O instance in use or not
+ * @dynamic_instance_count: number of dynamically created MC I/O instances
+ */
+struct fsl_mc_restool {
+	struct cdev cdev;
+	dev_t dev;
+	struct device *device;
+	struct mutex mutex; /* serialize open/release operations */
+	bool local_instance_in_use;
+	u32 dynamic_instance_count;
+};
+
+/**
+ * struct fsl_mc_bus - logical bus that corresponds to a physical DPRC
+ * @mc_dev: fsl-mc device for the bus device itself.
+ * @resource_pools: array of resource pools (one pool per resource type)
+ * for this MC bus. These resources represent allocatable entities
+ * from the physical DPRC.
+ * @irq_resources: Pointer to array of IRQ objects for the IRQ pool
+ * @scan_mutex: Serializes bus scanning
+ * @dprc_attr: DPRC attributes
+ * @restool_misc: struct that abstracts the interaction with userspace restool
+ */
+struct fsl_mc_bus {
+	struct fsl_mc_device mc_dev;
+	struct fsl_mc_resource_pool resource_pools[FSL_MC_NUM_POOL_TYPES];
+	struct fsl_mc_device_irq *irq_resources;
+	struct mutex scan_mutex;    /* serializes bus scanning */
+	struct dprc_attributes dprc_attr;
+	struct fsl_mc_restool restool_misc;
+};
+
+int dprc_scan_objects(struct fsl_mc_device *mc_bus_dev,
+		      const char *driver_override,
+		      unsigned int *total_irq_count);
+
+int fsl_mc_find_msi_domain(struct device *mc_platform_dev,
+			   struct irq_domain **mc_msi_domain);
+
+int fsl_mc_populate_irq_pool(struct fsl_mc_bus *mc_bus,
+			     unsigned int irq_count);
+
+void fsl_mc_cleanup_irq_pool(struct fsl_mc_bus *mc_bus);
+
+void fsl_mc_init_all_resource_pools(struct fsl_mc_device *mc_bus_dev);
+
+void fsl_mc_cleanup_all_resource_pools(struct fsl_mc_device *mc_bus_dev);
+
+void fsl_mc_get_root_dprc(struct device *dev, struct device **root_dprc_dev);
+
+#endif /* _FSL_MC_H_ */
--- /dev/null
+++ b/include/uapi/linux/fsl_mc.h
@@ -0,0 +1,31 @@
+/* SPDX-License-Identifier: GPL-2.0 WITH Linux-syscall-note */
+/*
+ * Management Complex (MC) userspace public interface
+ *
+ * Copyright 2018 NXP
+ *
+ */
+#ifndef _UAPI_FSL_MC_H_
+#define _UAPI_FSL_MC_H_
+
+#define MC_CMD_NUM_OF_PARAMS	7
+
+/**
+ * struct fsl_mc_command - Management Complex (MC) command structure
+ * @header: MC command header
+ * @params: MC command parameters
+ *
+ * Used by RESTOOL_SEND_MC_COMMAND
+ */
+struct fsl_mc_command {
+	__u64 header;
+	__u64 params[MC_CMD_NUM_OF_PARAMS];
+};
+
+#define RESTOOL_IOCTL_TYPE	'R'
+#define RESTOOL_IOCTL_SEQ	0xE0
+
+#define RESTOOL_SEND_MC_COMMAND \
+	_IOWR(RESTOOL_IOCTL_TYPE, RESTOOL_IOCTL_SEQ, struct fsl_mc_command)
+
+#endif /* _UAPI_FSL_MC_H_ */
