From 0d988407afff02574ed649ff6776a77d322bbe72 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Wed, 14 Nov 2018 09:53:25 +0000
Subject: [PATCH 441/454] overlays: Remove superfluous #address/size-cells

Newer versions of dtc warn about unnecessary usage of #address-cells
and #size-cells, so remove them.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/overlays/adv7282m-overlay.dts | 4 ----
 arch/arm/boot/dts/overlays/ov5647-overlay.dts   | 4 ----
 arch/arm/boot/dts/overlays/tc358743-overlay.dts | 4 ----
 3 files changed, 12 deletions(-)

--- a/arch/arm/boot/dts/overlays/adv7282m-overlay.dts
+++ b/arch/arm/boot/dts/overlays/adv7282m-overlay.dts
@@ -34,13 +34,9 @@
 	fragment@1 {
 		target = <&csi1>;
 		__overlay__ {
-			#address-cells = <1>;
-			#size-cells = <0>;
 			status = "okay";
 
 			port {
-				#address-cells = <1>;
-				#size-cells = <0>;
 				csi1_ep: endpoint {
 					remote-endpoint = <&adv728x_0>;
 				};
--- a/arch/arm/boot/dts/overlays/ov5647-overlay.dts
+++ b/arch/arm/boot/dts/overlays/ov5647-overlay.dts
@@ -43,13 +43,9 @@
 	fragment@1 {
 		target = <&csi1>;
 		__overlay__ {
-			#address-cells = <1>;
-			#size-cells = <0>;
 			status = "okay";
 
 			port {
-				#address-cells = <1>;
-				#size-cells = <0>;
 				csi1_ep: endpoint {
 					remote-endpoint = <&ov5647_0>;
 				};
--- a/arch/arm/boot/dts/overlays/tc358743-overlay.dts
+++ b/arch/arm/boot/dts/overlays/tc358743-overlay.dts
@@ -42,13 +42,9 @@
 	fragment@1 {
 		target = <&csi1>;
 		__overlay__ {
-			#address-cells = <1>;
-			#size-cells = <0>;
 			status = "okay";
 
 			port {
-				#address-cells = <1>;
-				#size-cells = <0>;
 				csi1_ep: endpoint {
 					remote-endpoint = <&tc358743>;
 				};
