From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Subject: [PATCH] brcmfmac: get RAM info right before downloading PCIe firmware
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

It's important as brcmf_chip_get_raminfo() also makes sure that memory
is properly setup. Without it the firmware could report invalid RAM
address like 0x04000001.

During a normal brcmfmac lifetime brcmf_chip_get_raminfo() is called on
probe by the brcmf_chip_recognition(). This change allows implementing
further improvements like handling errors by resetting a device with
the brcmf_pcie_reset_device() and redownloading a firmware afterwards.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
---
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/chip.c | 6 ++++--
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/chip.h | 1 +
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/pcie.c | 6 ++++++
 3 files changed, 11 insertions(+), 2 deletions(-)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/chip.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/chip.c
@@ -696,8 +696,10 @@ static u32 brcmf_chip_tcm_rambase(struct
 	return 0;
 }
 
-static int brcmf_chip_get_raminfo(struct brcmf_chip_priv *ci)
+int brcmf_chip_get_raminfo(struct brcmf_chip *pub)
 {
+	struct brcmf_chip_priv *ci = container_of(pub, struct brcmf_chip_priv,
+						  pub);
 	struct brcmf_core_priv *mem_core;
 	struct brcmf_core *mem;
 
@@ -979,7 +981,7 @@ static int brcmf_chip_recognition(struct
 		brcmf_chip_set_passive(&ci->pub);
 	}
 
-	return brcmf_chip_get_raminfo(ci);
+	return brcmf_chip_get_raminfo(&ci->pub);
 }
 
 static void brcmf_chip_disable_arm(struct brcmf_chip_priv *chip, u16 id)
--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/chip.h
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/chip.h
@@ -69,6 +69,7 @@ struct brcmf_buscore_ops {
 	void (*activate)(void *ctx, struct brcmf_chip *chip, u32 rstvec);
 };
 
+int brcmf_chip_get_raminfo(struct brcmf_chip *pub);
 struct brcmf_chip *brcmf_chip_attach(void *ctx,
 				     const struct brcmf_buscore_ops *ops);
 void brcmf_chip_detach(struct brcmf_chip *chip);
--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/pcie.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/pcie.c
@@ -1770,6 +1770,12 @@ static void brcmf_pcie_setup(struct devi
 	nvram_len = fwreq->items[BRCMF_PCIE_FW_NVRAM].nv_data.len;
 	kfree(fwreq);
 
+	ret = brcmf_chip_get_raminfo(devinfo->ci);
+	if (ret) {
+		brcmf_err(bus, "Failed to get RAM info\n");
+		goto fail;
+	}
+
 	/* Some of the firmwares have the size of the memory of the device
 	 * defined inside the firmware. This is because part of the memory in
 	 * the device is shared and the devision is determined by FW. Parse
