From 81065f66dd99b3af58626a914b8c0fcff6b8b0ba Mon Sep 17 00:00:00 2001
From: Christian Lamparter <chunkeey@googlemail.com>
Date: Fri, 25 Aug 2017 15:47:15 +0200
Subject: [PATCH 02/25] crypto: crypto4xx - remove unused definitions and
 write-only variables

This patch removes several unused code and definitons
(structs, variables, ...).

Signed-off-by: Christian Lamparter <chunkeey@googlemail.com>
Signed-off-by: Herbert Xu <herbert@gondor.apana.org.au>
---
 drivers/crypto/amcc/crypto4xx_alg.c  |  6 ------
 drivers/crypto/amcc/crypto4xx_core.c |  2 +-
 drivers/crypto/amcc/crypto4xx_core.h | 16 ----------------
 3 files changed, 1 insertion(+), 23 deletions(-)

--- a/drivers/crypto/amcc/crypto4xx_alg.c
+++ b/drivers/crypto/amcc/crypto4xx_alg.c
@@ -75,7 +75,6 @@ int crypto4xx_encrypt(struct ablkcipher_
 	struct crypto4xx_ctx *ctx = crypto_tfm_ctx(req->base.tfm);
 
 	ctx->direction = DIR_OUTBOUND;
-	ctx->hash_final = 0;
 	ctx->is_hash = 0;
 	ctx->pd_ctl = 0x1;
 
@@ -89,7 +88,6 @@ int crypto4xx_decrypt(struct ablkcipher_
 	struct crypto4xx_ctx *ctx = crypto_tfm_ctx(req->base.tfm);
 
 	ctx->direction = DIR_INBOUND;
-	ctx->hash_final = 0;
 	ctx->is_hash = 0;
 	ctx->pd_ctl = 1;
 
@@ -136,7 +134,6 @@ static int crypto4xx_setkey_aes(struct c
 	}
 	/* Setup SA */
 	sa = (struct dynamic_sa_ctl *) ctx->sa_in;
-	ctx->hash_final = 0;
 
 	set_dynamic_sa_command_0(sa, SA_NOT_SAVE_HASH, (cm == CRYPTO_MODE_CBC ?
 				 SA_SAVE_IV : SA_NOT_SAVE_IV),
@@ -192,7 +189,6 @@ static int crypto4xx_hash_alg_init(struc
 
 	ctx->dev   = my_alg->dev;
 	ctx->is_hash = 1;
-	ctx->hash_final = 0;
 
 	/* Create SA */
 	if (ctx->sa_in_dma_addr || ctx->sa_out_dma_addr)
@@ -257,7 +253,6 @@ int crypto4xx_hash_update(struct ahash_r
 	struct crypto4xx_ctx *ctx = crypto_tfm_ctx(req->base.tfm);
 
 	ctx->is_hash = 1;
-	ctx->hash_final = 0;
 	ctx->pd_ctl = 0x11;
 	ctx->direction = DIR_INBOUND;
 
@@ -275,7 +270,6 @@ int crypto4xx_hash_digest(struct ahash_r
 {
 	struct crypto4xx_ctx *ctx = crypto_tfm_ctx(req->base.tfm);
 
-	ctx->hash_final = 1;
 	ctx->pd_ctl = 0x11;
 	ctx->direction = DIR_INBOUND;
 
--- a/drivers/crypto/amcc/crypto4xx_core.c
+++ b/drivers/crypto/amcc/crypto4xx_core.c
@@ -973,7 +973,7 @@ u32 crypto4xx_build_pd(struct crypto_asy
 
 	sa->sa_command_1.bf.hash_crypto_offset = 0;
 	pd->pd_ctl.w = ctx->pd_ctl;
-	pd->pd_ctl_len.w = 0x00400000 | (ctx->bypass << 24) | datalen;
+	pd->pd_ctl_len.w = 0x00400000 | datalen;
 	pd_uinfo->state = PD_ENTRY_INUSE;
 	wmb();
 	/* write any value to push engine to read a pd */
--- a/drivers/crypto/amcc/crypto4xx_core.h
+++ b/drivers/crypto/amcc/crypto4xx_core.h
@@ -72,7 +72,6 @@ struct pd_uinfo {
 struct crypto4xx_device {
 	struct crypto4xx_core_device *core_dev;
 	char *name;
-	u64  ce_phy_address;
 	void __iomem *ce_base;
 	void __iomem *trng_base;
 
@@ -127,21 +126,9 @@ struct crypto4xx_ctx {
 	u32 sa_len;
 	u32 offset_to_sr_ptr;           /* offset to state ptr, in dynamic sa */
 	u32 direction;
-	u32 next_hdr;
 	u32 save_iv;
-	u32 pd_ctl_len;
 	u32 pd_ctl;
-	u32 bypass;
 	u32 is_hash;
-	u32 hash_final;
-};
-
-struct crypto4xx_req_ctx {
-	struct crypto4xx_device *dev;	/* Device in which
-					operation to send to */
-	void *sa;
-	u32 sa_dma_addr;
-	u16 sa_len;
 };
 
 struct crypto4xx_alg_common {
@@ -172,9 +159,6 @@ static inline struct crypto4xx_alg *cryp
 
 extern int crypto4xx_alloc_sa(struct crypto4xx_ctx *ctx, u32 size);
 extern void crypto4xx_free_sa(struct crypto4xx_ctx *ctx);
-extern u32 crypto4xx_alloc_sa_rctx(struct crypto4xx_ctx *ctx,
-				   struct crypto4xx_ctx *rctx);
-extern void crypto4xx_free_sa_rctx(struct crypto4xx_ctx *rctx);
 extern void crypto4xx_free_ctx(struct crypto4xx_ctx *ctx);
 extern u32 crypto4xx_alloc_state_record(struct crypto4xx_ctx *ctx);
 extern u32 get_dynamic_sa_offset_state_ptr_field(struct crypto4xx_ctx *ctx);
