#!/bin/sh /etc/rc.common
# Copyright (C) 2012 OpenWrt.org

START=97
USE_PROCD=1

EXTRA_COMMANDS="status lucistat"
EXTRA_HELP="	status  Get DSL status information
	lucistat  Get status information if lua friendly format"

[ -f /lib/functions/lantiq_dsl.sh ] && . /lib/functions/lantiq_dsl.sh

annex_b=10_00_10_00_00_04_00_00
annex_bdmt=10_00_00_00_00_00_00_00
annex_b2=00_00_10_00_00_00_00_00
annex_b2p=00_00_00_00_00_04_00_00
annex_a=05_01_04_00_4C_01_04_00
annex_at1=01_00_00_00_00_00_00_00
annex_alite=00_01_00_00_00_00_00_00
annex_admt=04_00_00_00_00_00_00_00
annex_a2=00_00_04_00_00_00_00_00
annex_a2p=00_00_00_00_00_01_00_00
annex_l=00_00_00_00_0C_00_00_00
annex_m=00_00_00_00_40_00_04_00
annex_m2=00_00_00_00_40_00_00_00
annex_m2p=00_00_00_00_00_00_04_00
annex_j=10_00_10_40_00_04_01_00

service_triggers() {
	procd_add_reload_trigger network
}

start_service() {
	local annex
	local firmware
	local xtu
	config_load network
	config_get annex dsl annex
	config_get firmware dsl firmware

	eval "xtu=\"\${annex_$annex}\""

	[ -z "${firmware}" ] &&
		firmware=/lib/firmware/adsl.bin
	[ -f "${firmware}" ] || {
		echo failed to find $firmware
		return 1
	}

	procd_open_instance
	procd_set_param command /sbin/dsl_cpe_control \
			-i${xtu} \
			-n /sbin/dsl_notify.sh \
			-f ${firmware}
	procd_close_instance
}

stop_service() {
	DSL_NOTIFICATION_TYPE="DSL_INTERFACE_STATUS" \
	DSL_INTERFACE_STATUS="DOWN" \
		/sbin/dsl_notify.sh

	service_stop /sbin/dsl_cpe_control
}

