From b518bb159032aac33503fd4cf98706dc84cc1266 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Stefan=20Br=C3=BCns?= <stefan.bruens@rwth-aachen.de>
Date: Thu, 31 Aug 2017 01:06:37 +0200
Subject: [PATCH] arm64: allwinner: a64: add SPI nodes
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

The A64 SPI controllers are register compatible to the h3/h5 SPI
controllers.

The A64 has two SPI controllers, each with a single chip select.
The handles for the DMA channels (23/24 for SPI0/SPI1) are omitted,
as the A64 DMA support is currently missing.

Signed-off-by: Stefan Brüns <stefan.bruens@rwth-aachen.de>
Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi | 41 +++++++++++++++++++
 1 file changed, 41 insertions(+)

--- a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
@@ -325,6 +325,16 @@
 				drive-strength = <40>;
 			};
 
+			spi0_pins: spi0 {
+				pins = "PC0", "PC1", "PC2", "PC3";
+				function = "spi0";
+			};
+
+			spi1_pins: spi1 {
+				pins = "PD0", "PD1", "PD2", "PD3";
+				function = "spi1";
+			};
+
 			uart0_pins_a: uart0@0 {
 				pins = "PB8", "PB9";
 				function = "uart0";
@@ -470,6 +480,37 @@
 			};
 		};
 
+
+		spi0: spi@01c68000 {
+			compatible = "allwinner,sun8i-h3-spi";
+			reg = <0x01c68000 0x1000>;
+			interrupts = <GIC_SPI 65 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_SPI0>, <&ccu CLK_SPI0>;
+			clock-names = "ahb", "mod";
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi0_pins>;
+			resets = <&ccu RST_BUS_SPI0>;
+			status = "disabled";
+			num-cs = <1>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		spi1: spi@01c69000 {
+			compatible = "allwinner,sun8i-h3-spi";
+			reg = <0x01c69000 0x1000>;
+			interrupts = <GIC_SPI 66 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_SPI1>, <&ccu CLK_SPI1>;
+			clock-names = "ahb", "mod";
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi1_pins>;
+			resets = <&ccu RST_BUS_SPI1>;
+			status = "disabled";
+			num-cs = <1>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
 		gic: interrupt-controller@1c81000 {
 			compatible = "arm,gic-400";
 			reg = <0x01c81000 0x1000>,
