diff --git a/Documentation/devicetree/bindings/soc/qcom/qcom,gsbi.txt b/Documentation/devicetree/bindings/soc/qcom/qcom,gsbi.txt
index 4ce24d4..186e5f4 100644
--- a/Documentation/devicetree/bindings/soc/qcom/qcom,gsbi.txt
+++ b/Documentation/devicetree/bindings/soc/qcom/qcom,gsbi.txt
@@ -6,7 +6,8 @@ configuration settings.  The mode setting will govern the input/output mode of
 the 4 GSBI IOs.
 
 Required properties:
-- compatible: must contain "qcom,gsbi-v1.0.0" for APQ8064/IPQ8064
+- compatible:	Should contain "qcom,gsbi-v1.0.0"
+- cell-index:	Should contain the GSBI index
 - reg: Address range for GSBI registers
 - clocks: required clock
 - clock-names: must contain "iface" entry
@@ -16,6 +17,8 @@ Required properties:
 Optional properties:
 - qcom,crci : indicates CRCI MUX value for QUP CRCI ports.  Please reference
   dt-bindings/soc/qcom,gsbi.h for valid CRCI mux values.
+- syscon-tcsr: indicates phandle of TCSR syscon node.  Required if child uses
+  dma.
 
 Required properties if child node exists:
 - #address-cells: Must be 1
@@ -39,6 +42,7 @@ Example for APQ8064:
 
 	gsbi4@16300000 {
 		compatible = "qcom,gsbi-v1.0.0";
+		cell-index = <4>;
 		reg = <0x16300000 0x100>;
 		clocks = <&gcc GSBI4_H_CLK>;
 		clock-names = "iface";
@@ -48,6 +52,8 @@ Example for APQ8064:
 		qcom,mode = <GSBI_PROT_I2C_UART>;
 		qcom,crci = <GSBI_CRCI_QUP>;
 
+		syscon-tcsr = <&tcsr>;
+
 		/* child nodes go under here */
 
 		i2c_qup4: i2c@16380000 {
@@ -76,3 +82,9 @@ Example for APQ8064:
 		};
 	};
 
+	tcsr: syscon@1a400000 {
+		compatible = "qcom,apq8064-tcsr", "syscon";
+		reg = <0x1a400000 0x100>;
+	};
+
+
diff --git a/drivers/soc/qcom/Kconfig b/drivers/soc/qcom/Kconfig
index 7bd2c94..460b2db 100644
--- a/drivers/soc/qcom/Kconfig
+++ b/drivers/soc/qcom/Kconfig
@@ -4,6 +4,7 @@
 config QCOM_GSBI
         tristate "QCOM General Serial Bus Interface"
         depends on ARCH_QCOM
+        select MFD_SYSCON
         help
           Say y here to enable GSBI support.  The GSBI provides control
           functions for connecting the underlying serial UART, SPI, and I2C
diff --git a/drivers/soc/qcom/qcom_gsbi.c b/drivers/soc/qcom/qcom_gsbi.c
index 729425d..09c669e 100644
--- a/drivers/soc/qcom/qcom_gsbi.c
+++ b/drivers/soc/qcom/qcom_gsbi.c
@@ -18,22 +18,129 @@
 #include <linux/of.h>
 #include <linux/of_platform.h>
 #include <linux/platform_device.h>
+#include <linux/regmap.h>
+#include <linux/mfd/syscon.h>
+#include <dt-bindings/soc/qcom,gsbi.h>
 
 #define GSBI_CTRL_REG		0x0000
 #define GSBI_PROTOCOL_SHIFT	4
+#define MAX_GSBI		12
+
+#define TCSR_ADM_CRCI_BASE	0x70
+
+struct crci_config {
+	u32 num_rows;
+	const u32 (*array)[MAX_GSBI];
+};
+
+static const u32 crci_ipq8064[][MAX_GSBI] = {
+	{
+		0x000003, 0x00000c, 0x000030, 0x0000c0,
+		0x000300, 0x000c00, 0x003000, 0x00c000,
+		0x030000, 0x0c0000, 0x300000, 0xc00000
+	},
+	{
+		0x000003, 0x00000c, 0x000030, 0x0000c0,
+		0x000300, 0x000c00, 0x003000, 0x00c000,
+		0x030000, 0x0c0000, 0x300000, 0xc00000
+	},
+};
+
+static const struct crci_config config_ipq8064 = {
+	.num_rows = ARRAY_SIZE(crci_ipq8064),
+	.array = crci_ipq8064,
+};
+
+static const unsigned int crci_apq8064[][MAX_GSBI] = {
+	{
+		0x001800, 0x006000, 0x000030, 0x0000c0,
+		0x000300, 0x000400, 0x000000, 0x000000,
+		0x000000, 0x000000, 0x000000, 0x000000
+	},
+	{
+		0x000000, 0x000000, 0x000000, 0x000000,
+		0x000000, 0x000020, 0x0000c0, 0x000000,
+		0x000000, 0x000000, 0x000000, 0x000000
+	},
+};
+
+static const struct crci_config config_apq8064 = {
+	.num_rows = ARRAY_SIZE(crci_apq8064),
+	.array = crci_apq8064,
+};
+
+static const unsigned int crci_msm8960[][MAX_GSBI] = {
+	{
+		0x000003, 0x00000c, 0x000030, 0x0000c0,
+		0x000300, 0x000400, 0x000000, 0x000000,
+		0x000000, 0x000000, 0x000000, 0x000000
+	},
+	{
+		0x000000, 0x000000, 0x000000, 0x000000,
+		0x000000, 0x000020, 0x0000c0, 0x000300,
+		0x001800, 0x006000, 0x000000, 0x000000
+	},
+};
+
+static const struct crci_config config_msm8960 = {
+	.num_rows = ARRAY_SIZE(crci_msm8960),
+	.array = crci_msm8960,
+};
+
+static const unsigned int crci_msm8660[][MAX_GSBI] = {
+	{	/* ADM 0 - B */
+		0x000003, 0x00000c, 0x000030, 0x0000c0,
+		0x000300, 0x000c00, 0x003000, 0x00c000,
+		0x030000, 0x0c0000, 0x300000, 0xc00000
+	},
+	{	/* ADM 0 - B */
+		0x000003, 0x00000c, 0x000030, 0x0000c0,
+		0x000300, 0x000c00, 0x003000, 0x00c000,
+		0x030000, 0x0c0000, 0x300000, 0xc00000
+	},
+	{	/* ADM 1 - A */
+		0x000003, 0x00000c, 0x000030, 0x0000c0,
+		0x000300, 0x000c00, 0x003000, 0x00c000,
+		0x030000, 0x0c0000, 0x300000, 0xc00000
+	},
+	{	/* ADM 1 - B */
+		0x000003, 0x00000c, 0x000030, 0x0000c0,
+		0x000300, 0x000c00, 0x003000, 0x00c000,
+		0x030000, 0x0c0000, 0x300000, 0xc00000
+	},
+};
+
+static const struct crci_config config_msm8660 = {
+	.num_rows = ARRAY_SIZE(crci_msm8660),
+	.array = crci_msm8660,
+};
 
 struct gsbi_info {
 	struct clk *hclk;
 	u32 mode;
 	u32 crci;
+	struct regmap *tcsr;
+};
+
+static const struct of_device_id tcsr_dt_match[] = {
+	{ .compatible = "qcom,tcsr-ipq8064", .data = &config_ipq8064},
+	{ .compatible = "qcom,tcsr-apq8064", .data = &config_apq8064},
+	{ .compatible = "qcom,tcsr-msm8960", .data = &config_msm8960},
+	{ .compatible = "qcom,tcsr-msm8660", .data = &config_msm8660},
+	{ },
 };
 
 static int gsbi_probe(struct platform_device *pdev)
 {
 	struct device_node *node = pdev->dev.of_node;
+	struct device_node *tcsr_node;
+	const struct of_device_id *match;
 	struct resource *res;
 	void __iomem *base;
 	struct gsbi_info *gsbi;
+	int i;
+	u32 mask, gsbi_num;
+	const struct crci_config *config = NULL;
 
 	gsbi = devm_kzalloc(&pdev->dev, sizeof(*gsbi), GFP_KERNEL);
 
@@ -45,6 +152,32 @@ static int gsbi_probe(struct platform_device *pdev)
 	if (IS_ERR(base))
 		return PTR_ERR(base);
 
+	/* get the tcsr node and setup the config and regmap */
+	gsbi->tcsr = syscon_regmap_lookup_by_phandle(node, "syscon-tcsr");
+
+	if (!IS_ERR(gsbi->tcsr)) {
+		tcsr_node = of_parse_phandle(node, "syscon-tcsr", 0);
+		if (tcsr_node) {
+			match = of_match_node(tcsr_dt_match, tcsr_node);
+			if (match)
+				config = match->data;
+			else
+				dev_warn(&pdev->dev, "no matching TCSR\n");
+
+			of_node_put(tcsr_node);
+		}
+	}
+
+	if (of_property_read_u32(node, "cell-index", &gsbi_num)) {
+		dev_err(&pdev->dev, "missing cell-index\n");
+		return -EINVAL;
+	}
+
+	if (gsbi_num < 1 || gsbi_num > MAX_GSBI) {
+		dev_err(&pdev->dev, "invalid cell-index\n");
+		return -EINVAL;
+	}
+
 	if (of_property_read_u32(node, "qcom,mode", &gsbi->mode)) {
 		dev_err(&pdev->dev, "missing mode configuration\n");
 		return -EINVAL;
@@ -64,6 +197,25 @@ static int gsbi_probe(struct platform_device *pdev)
 	writel_relaxed((gsbi->mode << GSBI_PROTOCOL_SHIFT) | gsbi->crci,
 				base + GSBI_CTRL_REG);
 
+	/*
+	 * modify tcsr to reflect mode and ADM CRCI mux
+	 * Each gsbi contains a pair of bits, one for RX and one for TX
+	 * SPI mode requires both bits cleared, otherwise they are set
+	 */
+	if (config) {
+		for (i = 0; i < config->num_rows; i++) {
+			mask = config->array[i][gsbi_num - 1];
+
+			if (gsbi->mode == GSBI_PROT_SPI)
+				regmap_update_bits(gsbi->tcsr,
+					TCSR_ADM_CRCI_BASE + 4 * i, mask, 0);
+			else
+				regmap_update_bits(gsbi->tcsr,
+					TCSR_ADM_CRCI_BASE + 4 * i, mask, mask);
+
+		}
+	}
+
 	/* make sure the gsbi control write is not reordered */
 	wmb();
 
-- 
1.9.1

