/dts-v1/;

/include/ "bcm6358.dtsi"

/ {
	model = "BT Home Hub 2.0 Type A";
	compatible = "thomson,homehub2a", "brcm,bcm6358";

	spi-gpio {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "spi-gpio";

		gpio-mosi = <&gpio0 7 0>;
		gpio-sck = <&gpio0 6 0>;
		cs-gpios = <&gpio0 5 0>;
		num-chipselects = <1>;

		hc595: gpio-spi-controller@0 {
			compatible = "fairchild,74hc595";
			reg = <0>;
			registers-number = <2>;
			spi-max-frequency = <100000>;

			gpio-controller;
			#gpio-cells = <2>;
		};
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;
		debounce-interval = <60>;

		phone {
			label = "phone";
			gpios = <&gpio0 1 1>;
			linux,code = <169>;
		};
		reset {
			label = "reset";
			gpios = <&gpio0 9 1>;
			linux,code = <0x198>;
		};
		wps {
			label = "wps";
			gpios = <&gpio0 11 1>;
			linux,code = <0x211>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		power_red {
			label = "HOMEHUB2A:red:power";
			gpios = <&hc595 0 1>;
		};
		power_green {
			label = "HOMEHUB2A:green:power";
			gpios = <&hc595 1 1>;
			default-state = "on";
		};
		power_blue {
			label = "HOMEHUB2A:blue:power";
			gpios = <&hc595 2 1>;
		};
		broadband_red {
			label = "HOMEHUB2A:red:broadband";
			gpios = <&hc595 3 1>;
		};
		broadband_green {
			label = "HOMEHUB2A:green:broadband";
			gpios = <&hc595 4 1>;
		};
		broadband_blue {
			label = "HOMEHUB2A:blue:broadband";
			gpios = <&hc595 5 1>;
		};
		wireless_red {
			label = "HOMEHUB2A:red:wireless";
			gpios = <&hc595 6 1>;
		};
		wireless_green {
			label = "HOMEHUB2A:green:wireless";
			gpios = <&hc595 7 1>;
		};
		wireless_blue {
			label = "HOMEHUB2A:blue:wireless";
			gpios = <&hc595 8 1>;
		};
		phone_red {
			label = "HOMEHUB2A:red:phone";
			gpios = <&hc595 9 1>;
		};
		phone_green {
			label = "HOMEHUB2A:green:phone";
			gpios = <&hc595 10 1>;
		};
		phone_blue {
			label = "HOMEHUB2A:blue:phone";
			gpios = <&hc595 11 1>;
		};
		upgrading_red {
			label = "HOMEHUB2A:red:upgrading";
			gpios = <&hc595 12 1>;
		};
		upgrading_green {
			label = "HOMEHUB2A:green:upgrading";
			gpios = <&hc595 13 1>;
		};
		upgrading_blue {
			label = "HOMEHUB2A:blue:upgrading";
			gpios = <&hc595 14 1>;
		};
	};
};

&pflash {
	status = "ok";

	linux,part-probe = "bcm63xxpart";

	cfe@0 {
		label = "CFE";
		reg = <0x000000 0x020000>;
	};

	linux@20000 {
		label = "linux";
		reg = <0x020000 0xfc0000>;
	};

	nvram@fe0000 {
		label = "nvram";
		reg = <0xfe0000 0x020000>;
	};
};
