--- a/arch/arm/boot/dts/armada-xp.dtsi
+++ b/arch/arm/boot/dts/armada-xp.dtsi
@@ -88,12 +88,10 @@
 			};
 
 			i2c0: i2c@11000 {
-				compatible = "marvell,mv78230-i2c", "marvell,mv64xxx-i2c";
 				reg = <0x11000 0x100>;
 			};
 
 			i2c1: i2c@11100 {
-				compatible = "marvell,mv78230-i2c", "marvell,mv64xxx-i2c";
 				reg = <0x11100 0x100>;
 			};
 
