--- a/arch/arm/boot/dts/imx6qdl-gw51xx.dtsi
+++ b/arch/arm/boot/dts/imx6qdl-gw51xx.dtsi
@@ -89,6 +89,11 @@
 			enable-active-high;
 		};
 	};
+
+	gw16083: gw16083@52 {
+		compatible = "gateworks,gw16083";
+		reg = <0x52>;
+	};
 };
 
 &fec {
--- a/arch/arm/boot/dts/imx6qdl-gw52xx.dtsi
+++ b/arch/arm/boot/dts/imx6qdl-gw52xx.dtsi
@@ -266,6 +266,11 @@
 			};
 		};
 	};
+
+	gw16083: gw16083@52 {
+		compatible = "gateworks,gw16083";
+		reg = <0x52>;
+	};
 };
 
 &pcie {
--- a/arch/arm/boot/dts/imx6qdl-gw53xx.dtsi
+++ b/arch/arm/boot/dts/imx6qdl-gw53xx.dtsi
@@ -267,6 +267,11 @@
 			};
 		};
 	};
+
+	gw16083: gw16083@52 {
+		compatible = "gateworks,gw16083";
+		reg = <0x52>;
+	};
 };
 
 &pcie {
--- a/arch/arm/boot/dts/imx6qdl-gw54xx.dtsi
+++ b/arch/arm/boot/dts/imx6qdl-gw54xx.dtsi
@@ -308,6 +308,11 @@
 			};
 		};
 	};
+
+	gw16083: gw16083@52 {
+		compatible = "gateworks,gw16083";
+		reg = <0x52>;
+	};
 };
 
 &i2c3 {
